You are here: Using the Configurator > Configuring a System using a USB Key > Power Package GUIDs

# Power Package GUIDs

The optional /PowerPackage parameter enables you to define power management settings of the Intel AMT device during manual configuration. If not supplied, the default power settings defined by the manufacturer are used. This table gives the GUID values (in Hex 32 character format) per Intel AMT version.

Supported Power Package | GUID (Hex 32)
--- | ---
Intel AMT 6.x and higher (mobile)
ON in S0 | 763997110B56504388709812F391B560
ON in S0, ME Wake in S3/AC, S4-5/AC | 30800DEE09C07843AF287868A2DBBE3A
Intel AMT 6.x and higher (desktop)
ON in S0 | 944F8312FB104FDC968E1E232B0C9065
ON in S0, ME Wake in S3,S4-5 | 7322734623DC432FA98A13D37982D855
Intel AMT 5.x (desktop)
ON in S0 | 944F8312FB104FDC968E1E232B0C9065
ON in S0, S3 | A18600AB9A7F4C42A6E6BB243A295D9E
ON in S0, S3, S4-5 | 7286ABAC96B448E29B9E9B7DF91C7FD4
ON in S0, ME WoL in S3 | 7B32CD4D6BBE4389A62A4D7BD8DBD026
ON in S0, ME WoL in S3, S4-5 | 7322734623DC432FA98A13D37982D855
ON in S0, S3, S4-5, OFF After Power Loss | C519A4BA6E6F8D4DB227517F7E4595DB
ON in S0, ME WoL in S3,S4-5, OFF After Power Loss | D60BE3ED04C52C46B772D18018EE2FC4
Intel AMT 4.x (mobile)
ON in S0 | 763997110B56504388709812F391B560
ON in S0, S3/AC | 26D31C768708C74BBB5F38744315A5FF
ON in S0, S3/AC, S4-5/AC | 530E08DB6C0FD948B2D28958D3F1156E
ON in S0, ME Wake in S3/AC | 055DD5B64CA4874DA5A8B47C14DEDA5F
ON in S0, ME Wake in S3/AC, S4-5/AC | 30800DEE09C07843AF287868A2DBBE3A