You are here: Using the Configurator > Configurator Return Codes

# Configurator Return Codes

This table describes the return codes that are shown and recorded in the log file when running Configurator CLI commands. (For informational purposes, the list includes all return codes. Return codes related to remote configuration and the RCS should never occur when not using the RCS.)

# | Description
--- | ---
0 | The requested operation completed successfully
1 | Intel AMT is already configured on this system
2 | Intel AMT is already unconfigured on this system
3 | This system does not have Intel AMT (or it is disabled in the Intel MEBX, or the correct drivers are not installed or enabled)
4 | This system supports Intel® Small Business Advantage (Intel® SBA) and cannot be configured by Intel SCS components. Intel SBA systems were specifically designed for small businesses, and can only be configured using the software included with Intel SBA.
6 | The RCS failed to process the request
7 | The Intel AMT device does not have a PSK (prerequisite for the requested operation)
8 | Invalid command parameter
9 | The system is not in Intel AMT mode (check the manageability setting in the Intel MEBX)
10 | The manageability mode has been changed to “AMT”. You must reboot the system to complete this operation.
11 | Failed to change to Intel AMT mode (check the manageability setting in the Intel MEBX)
12 | An internal error has occurred in Intel AMT
16 | Invalid format used in the new Intel MEBX password parameter (refer to the documentation)
17 | Invalid format used in the current Intel MEBX password parameter (refer to the documentation)
18 | Cannot write the USB configuration data to file (possible reasons- the specified path does not exist; no write permissions; not enough free space).
19 | Failed to create the USB configuration file (invalid IP)
20 | Failed to create the USB configuration file (invalid power package)
21 | An internal error occurred when creating the USB configuration file
22 | An internal exception occurred when processing the request
25 | The system is already in Intel AMT mode
26 | The UsingDHCP parameter was supplied, but DHCP is not active on the host operating system
27 | Access denied. Make sure that the user has administrator permissions on the local host or in the Intel AMT device.
30 | This Intel AMT device does not support host-based configuration
31 | This Intel AMT device is in a state that does not support the ConfigAMT command
32 | The requested operation completed, but with warnings
33 | Failed to configure this Intel AMT device
34 | Failed to do the requested operation. The flash wear-out protection mechanism limits consecutive operations in a certain time period. Try the operation again later.
35 | A certificate request was sent to the Certification Authority but the created certificate was put into "Pending Requests" waiting for approval. Intel SCS does not support pending requests.
36 | Failed to request the certificate
37 | Failed to parse the XML file (possible reasons- the file does not exist or access to it is denied; the file contains incorrect parameters; incorrect or missing encryption password/parameter)
38 | Error with XML file (possible reasons- the file does not exist or access to it is denied; the file contains incorrect parameters; incorrect or missing encryption password/parameter; invalid data)
39 | The Intel AMT device is in a state that does not support disabling the Client Control mode
40 | This system was already unconfigured. The system was successfully put in the “Pre Provisioned” state and the Intel AMT interfaces are now closed.
41 | The certificate cannot be retrieved because access to the Certification Authority is denied
42 | Failed to write to the file. A possible reason is insufficient permissions in the selected folder.
43 | Failed to read from the given file. A possible reason is insufficient permissions in the selected folder.
44 | Memory Allocation Error
45 | Failed to unconfigure this Intel AMT device or Intel AMT unconfiguration failed
46 | Settings defined in the dedicated network settings XML file are not compatible with the network settings defined in the configuration profile
49 | Failed to do the requested maintenance tasks on this Intel AMT device
50 | The Intel AMT device is in a state that does not support the Maintenance command
51 | TLS cannot be configured because cryptography is disabled on this system
54 | The Intel AMT device cannot be set with the host FQDN and a dedicated FQDN
55 | The Intel AMT device cannot be set with the host IP and a dedicated IP
56 | An FQDN is mandatory for configuration (supply the FQDN in the NetworkSettings tag of the profile)
57 | Setting a static IP to the Intel AMT device from the host dynamic IP is not permitted
58 | When defining a static address, the IP and subnet mask parameters are mandatory
59 | Failed to find the host IP address and subnet mask to set in the Intel AMT device (possible reasons - the network card is disabled; the network connection is disabled; the network cable is unplugged)
60 | Dedicated FQDN is not permitted
61 | An invalid IP address was supplied in the parameter
62 | Cannot configure an AD object or certificates for the Intel AMT device without a valid FQDN
65 | Administrator credentials must be supplied in the XML or CLI to configure the Intel AMT device
66 | Failed to reissue certificates because the certificate data is missing in the profile
67 | Failed to renew the AD password because the AD data is missing in the profile
68 | Invalid parameter was found
70 | Failed to connect to the Intel AMT device (possible reasons: the system does not have Intel(R) AMT or is not responding; user access to it is denied)
71 | The buffer maximum size supplied in the function is too small
73 | Failed to put the system in the “Pre Provisioned” state (you can try to unconfigure the system using the Intel MEBX “Full Unprovision” option)
74 | Failed to complete the Setup operation on this Intel AMT device
75 | Failed to complete remote configuration of this Intel AMT device
76 | The file supplied in the FileToRun parameter returned an error when it was run
77 | Missing mandatory parameter
78 | Failed to put the Intel AMT device in the “In Provision” state. The Start Configuration operation failed. Examine the Intel MEBX settings to make sure remote configuration is enabled, or a TLS PSK pair is defined.
79 | Failed to connect to the Intel Management Engine Interface PTHI client
80 | Failed to complete the System Discovery
81 | Failed to run the file supplied in the FileToRun parameter
82 | The FileToRun parameter is not permitted for configuration methods using a Remote Configuration Server
83 | The Intel Management Engine Interface driver is not installed or cannot be accessed
84 | Invalid data in the profile
85 | Failed to move the Intel AMT device to Admin Control mode
86 | Failed to get the FQDN
87 | Failed to verify the signature of the file supplied in the FileToRun parameter. To cancel this verification, run the command using the LowSecurity global option.
88 | The requested operation was aborted because required file access failed
89 | The file supplied in the FileToRun parameter is not located in a trusted location. To cancel this prerequisite, run the command using the LowSecurity global option.
90 | Failed to get the Digest admin password to put in the Intel AMT device (calculated by the RCS using the Digest Master Password)
91 | Failed to get the Digest admin password that is configured in the Intel AMT device
92 | Failed to send the Hello Message to the RCS
93 | Failed to submit the certificate request to the Certification Authority
94 | Failed to get the certificate
95 | Failed to generate a TLS-PSK Pair
96 | Failed to generate the PKCS10 request
97 | Failed to get the FQDN of the Intel AMT device
98 | Failed to get the IP address of the Intel AMT device
99 | Failed to get the UUID of the Intel AMT device
100 | Failed to get the FQDN and the IP address of the Intel AMT device
101 | The remote configuration operation completed, but with warnings
102 | Failed to retrieve the PID from this Intel AMT device
103 | The requested functionality is not supported on this operating system
104 | Failed to renew the Digest admin password in the Intel AMT device because the administrator password is missing in the profile
105 | Failed to read data from the registry. A possible reason is that the registry value does not exist or access to it is denied.
106 | Failed to verify the hash of the file supplied in the FileToRun parameter against the Hash supplied in the FileHash parameter
107 | The Notify RCS operation failed
108 | This Intel AMT system already exists in the database
109 | Failed to connect to the RCS
110 | Failed to verify the file signature chain. Either connect the computer to the Internet, or manually download and install the root certificate update package from the Microsoft update catalog.