You are here: Introduction > Configuration Methods and Intel AMT Versions

# Configuration Methods and Intel AMT Versions

There are many different versions of Intel AMT. This table gives the configuration methods available for the different Intel AMT versions.

# | Configuration Method | Intel AMT Versions
--- | --- | ---
1 | Host-based Configuration | 6.2 and higher
2 | Manual Configuration | 6.x and higher
3 | One-Touch Configuration using PSK | 2.1 - 10
4 | Remote Configuration using PKI | 2.2, 2.6, 3.0 and higher
Note: TLS-PSK Configuration is not supported on Intel AMT 11 or later. Configuration methods #3 and #4 are not supported by the Configuration Utility. These configuration methods use the Remote configuration Service (RCS) component of Intel SCS. For more information about Intel SCS, refer to the Intel(R)_SCS_User_Guide.pdf.