You are here: Introduction > Configuration Methods and Intel AMT Versions > SMB/Manual Configuration

# Manual Configuration

The Manual configuration method lets you configure the Intel AMT device with basic configuration settings but it does require touching the device (to insert the USB key). However this puts Intel AMT into Admin Control Mode (ACM) and as such provides access to all AMT features, without mandatory requirement for user consent.

You can use the Configuration Utility to create the Setup.bin file. For more information, see:

- Manual Configuration

- Defining Manual Configuration (Multiple Systems)

Alternatively, you can use the ConfigViaUSB command of the Configurator (see Configuring a System using a USB Key).

Note:
This method is not available for systems with Intel AMT 2.x and 3.x because they cannot read the Setup.bin file.