=============================================================================
Intel(R) Server Board Platform Confidence Test Release Notes
=============================================================================
Intel Enterprise Platform & Services Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
=============================================================================
DATE:           Oct, 2017
TO:             Intel(R) server platform customers
SUBJECT:        Unified EFI Platform Confidence Test x64(PCTx64) 
=============================================================================
Information in this document is provided in connection with Intel products.
No license, express or implied, by estoppels or otherwise, to any intellectual
property rights are granted by this document. Except as provided in Intel's
Terms and Conditions of Sale for such products, Intel assumes no liability
whatsoever, and Intel disclaims any express or implied warranty, relating to
sale and/or use of Intel products including liability or warranties relating
to fitness for a particular purpose, merchantability, or infringement of any
patent, copyright or other intellectual property right. Intel Corporation may
have patents or pending patent applications, trademarks, copyrights, or other
intellectual property rights that relate to the presented subject matter. The
furnishing of documents and other materials and information does not provide
any license, express or implied, by estoppels or otherwise, to any such
patents, trademarks, copyrights, or other intellectual property rights. Intel
products are not intended for use in medical, life saving, or life sustaining
applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation.

*Other names and brands are the property of their respective owners.

Copyright (c) 2017 Intel Corporation.


=============================================================================
                              SET UP OF CD/DVD-ROM DRIVE
=============================================================================

Not supported at this time.

=============================================================================
                              SET UP OF USB FLASH DRIVE
=============================================================================

Unzip efi_pctx64_106.zip to root of USB Flash Drive.  

Insert USB Flash drive and boot the system.
BIOS Settings required for PCT, Press <F2> to enter Setup.
Upon entering BIOS press <F9> to load defaults.
Change the boot order so EFI Shell is the primary (#1) boot device.
Press <F10> to save BIOS setup settings and reboot to EFI.
Test should start automatically.
Pressing <F10> during tests will cause test to terminate.

It is recommended that after the comprehensive or comprehensive looping test 
you do a full AC power cycle (remove power from the system) before retesting.  
The reason for this is to ensure that all controllers are reset and in an 
expected mode.

Using Same PCT USB Flash Drive to test multiple systems.

Only Intel official released BIOS is supported by PCT.
===========================================
If you plan to use the same PCT USB drive to test multiple systems, boot the system
with the USB Flash Drive to start the test in EFI then wait until all the files are copied to the 
RAM drive, and test menu will display automatically, then remove the USB Flash Drive
before you start the PCT test. 
Note:
If the USB key is removed during or after starting the PCT test, it will cause the test to fail.


============================================================================
                         Supported Products
============================================================================
S1200SP

============================================================================
Date Released                   Version
============================================================================
8/21/2017
	1.06
    Update BMC/Drive/USB/RMM3/RTC/NPTM/HSC/GRAPHICS modules.


5/22/2017
	1.05
    Update Seriox64.

3/17/2017
	1.04
    Update PCIEx64, Add DMI predefined profiles for KBL support.update VPDx64.

1/11/2017
    Update TX64/Runtest/DISPSTAT/DISCFG/BIOSID/BMC/CACHE/CPU/DRIVE/GETINI
	GRAPHICS/GREP/HSCTEST/ICH/NPTM/PCIE
	PIC/PIT/RMM3TEST/RTC/SCAN/SERIO/SUPER IO/USB/VPD .

02/02/2016                       v1.02
    Update the DispCfgX64,DispStatX64,RuntestX64 and License Key.

12/04/2015                      V1.01
    Update the Graphics,VPD,Drive,ICHx,runtestx64,DispCfgx64,DispStatx64 and Seriox64 module 

08/05/2015			V1.00
	Initial release to support S1200SP.


	 

System requirements:
	
	USB/PS2 Keyboard 
	EFI Shell must be first Boot Option
	
Limitation:
- RTC.DATE_AND_TIME_KEEPING will affect the accuracy of the system time if Comprehensive test loop

Known Issue:
- Please use USB flash drive to run PCT. The test will run directly from USB flash drive. 
  UEFIx64 CD image is not available at this time.
- The Comprehensive test and Comprehensive test with looping takes ~1 hour to configure. 
=============================================================================
