=============================================================================
    Intel(R) Server Platform Canoe Pass FRU/SDR Update Release Notes
=============================================================================

INTEL Enterprise Platform & Services Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA

=============================================================================

DATE:   Feb 06, 2014

TO:     Intel(R) Server Platform Canoe Pass customers

SUBJECT:    IBMC(R) FRU/SDR update package S2600CP_FRUSDR_111 release notes

=============================================================================
                               LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products.
No license, express or implied, by estoppel or otherwise, to any intellectual
property rights is granted by this document. Except as provided in Intel's
Terms and Conditions of Sale for such products, Intel assumes no liability
whatsoever, and Intel disclaims any express or implied warranty, relating to
sale and/or use of Intel products including liability or warranties relating
to fitness for a particular purpose, merchantability, or infringement of any
patent, copyright or other intellectual property right. Intel Corporation may
have patents or pending patent applications, trademarks, copyrights, or other
intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not
provide any license, express or implied, by estoppel or otherwise, to any
such patents, trademarks, copyrights, or other intellectual property rights.
Intel products are not intended for use in medical, life saving, or life
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation.

*Other names and brands are the property of their respective owners.

Copyright (c) 2010 - 2014 Intel Corporation.


=============================================================================
                              ABOUT THIS RELEASE
=============================================================================

SDR file version:                   1.11
Baseboard FRU file version:         1.00
Master configuration file version:  1.11
FRUSDR utility version:             11.0 Build 20

=============================================================================
        SYSTEM HARDWARE & SOFTWARE REQUIREMENTS/REVISIONS
=============================================================================

- This FRU/SDR package has only been tested on Canoe Pass FAB3 baseboards.

- BMC firmware rev 1.17(or later) MUST be preinstalled prior to installing
  this FRU/SDR package.

- BIOS R1.06 or later

- MB Ver FB3

=============================================================================
                      IMPORTANT INSTALLATION NOTES
=============================================================================

- None

=============================================================================
            INSTALLATION PROCEDURE
=============================================================================

1. Ensure BMC release 1.17 or later is pre-installed before attempting this
   FRU/SDR update.

2. Copy all of the files in the S2600CP_FRUSDR_111.zip archive to a USB key,
   hard disk drive or floppy drive.
   All of the files in this zip archive must reside in the same directory.

3. Boot to EFI and then run the following command to display the
   contents of the baseboard FRU device:

    FRUSDR /d FRU

   If device is empty(which is the case for all new FAB3 baseboards) or corrupted, then
   execute the following command to program the empty FRU device:

   For Canoe Pass:
        FRUSDR /fru S2600CP.fru

4. Now execute the following command to bring up the main FRU/SDR load menu:

    FRUSDR /cfg master.cfg


5. Select the option which is applicable to what you want to do. On a brand
   new baseboard I would highly recommend to run option 3 to program both
   the FRU and SDR. By reprogramming the FRU you will be given the option
   to input data from the keyboard into various chassis, board and product
   areas. Ensure that you select the correct chassis from the chassis
   selection menu otherwise your fan sensors will not be configured
   properly.

6. Once the package has finished its installation, I would highly recommend
   to DC power off the system and cycle AC power.

=============================================================================
                           KNOWN ISSUES/WORKAROUNDS
=============================================================================

FCP_13:
- FRUSDR update FRU fail(frusdr 11.0 build02).

FCP_14:
- FRUSDR update FRU fail(frusdr 11.0 build02).

FCP_15:
- FRUSDR update FRU fail(frusdr 11.0 build02).

=============================================================================
                           FEATURES ADDED
=============================================================================
FCP_01:
- This package is only for PO builds.
- Update SDR as per CanoePass_CONFIG-FSC.xls(v1.1).

FCP_02:
- Follow Canoe Pass FSC config sheet Rev (1.5).

FCP_03:
- Follow Canoe Pass FSC config sheet Rev (1.7).
- Add auto SKU detection.
- Remove N12 voltage.
- Add ME FRUSDR.
- Add front panel FRUSDR.

FCP_04:
- Add SDR "ERR2 TimeOut".
- Add SDR "MSID Misatch".
- Add HDD status.
- Modify BB +1.5V & BB +1.35V Sensor Initialization to 0x3E.
- Modify FSC Global Clamp Tags.
- Modify PS FAN Low threshold.
 
FCP_05:
- Follow Canoe Pass FSC config sheet Rev (1.9).
- Modify the P1/P2 VRD HOT sensor Sensor Units 2 from 01 change to 00
- Add detect FP Board FRU.
- Add detect 4 port &  8 port BP Board.
- Modify HSBP Temp Assertion Event Mask & Deassertion Event Mask to 8532.
- Modify HSBP Temp Reading Mask & Settable / Readable Threshold Masks to 1B1B.
- Modify CP BMC fru Board Product Name.
- Modify SDR Entity Instance
- Fix PS REDUNDANCY.

FCP_06:
- Follow Canoe Pass FSC config sheet Rev (2.0).
- FRUSDR UTILITY upgrade to Version 10.0 Build 5.
- Add FRUSDR BIOS Post Error and BIOS Boot Event.
- Modify Front Panel FRU detect(if not detect Front Panel FRU then run USER SELECT mode).
- Modify MEM Thrm Trip 1/2/3/4 Sensor Type and Event reading type code to 0x01 and 0x03.
- Remove Union Peak M Non Redundant Fan 1/2 present.
- Modify power supply detect and HSBP detect.
- Add CPU detect.

FCP_07:
- Follow Canoe Pass FSC config sheet Rev (2.1).
- Modify BIOS SDR "Mem Conf Sensor" sensor number to 0x09.
- Add SDR :"System Airflow".
- Add SDR :"IBMC Watchdog".
- Add SDR :"VR WD Timer".
- Add SDR "P1 MEM01 VRD Hot","P1 MEM23 VRD Hot","P2 MEM01 VRD Hot","P2 MEM23 VRD Hot".
- Modify SDR HDD name : "HDD 1 Status" ~ "HDD 24 Status".

FCP_08:
- Follow Canoe Pass FSC config sheet Rev (2.1).
- Modify HSBP detected(MASTER.CFG).
- Modify Power Supply and HSBP prompt(MASTER.CFG).
- Modify "Mem Thrm Trip 2" Tag and del Mem Thrm Trip 3,Mem Thrm Trip 4.
- CPU1/2 Status(sensor number:0x70,0x71) Mask set "Processor disabled" to 1 = 0182h.
- disable sensor number:0x2F,0xB0,0xB1,0xB2,0xB3.
- Add "BMC System Management Health Monitoring"(sensor number:0x10) to SDR and disable the Sensor (code not ready).
- modify SPS FW Health(sensor number:0x17)Sensor type, Event/Reading Type Code to 0xDC, 0x75.
- Modify volatge scale.(ref config sheet 1.8).

FCP_09:
- Follow Canoe Pass FSC config sheet Rev (2.4).
- Modify auto detect 120mm Fan (Union Peak M Non Redundant). 
- Modify voltage nominal/max/min/uc/unc/lc/lnc value. 
- Modify "System Airflow" as config sheet 2.4.
- Add "Exit Air Temp"(sensor number:0x2E).
- Enable DIMM Aggregate Margin sensor number 0xb0 to 0xb3.
- Enable Baseboard NIC Temperature sensor number 0x2f.
- Enable BMC FW Health sensor number 0x10.
- Modify HSBP detected(MASTER.CFG).
- Modyfy UPM base power supply detect.

FCP_10:
- Follow Canoe Pass FSC config sheet Rev (2.5).
- Update MASTER.CFG front panel didn't auto detected as "Other Chassis".
- Modify 'BMC FW Health' Sensor Capabilities to 40h.
- add sensor:240VA Fault(sensor number 12h(disable)).

FCP_11:
- Follow Canoe Pass FSC config sheet Rev (2.6).
- System airflow Nominal reading & Normal Maximum value.

FCP_12:
- Follow Canoe Pass FSC config sheet Rev (2.6).
- Modify Domain 0 to 4,  FSC Sub-record Type = 04h (Advanced Fan Failure) and FSC Sub-record Type = 05h (Fans Off).

FCP_13:
- Follow Canoe Pass FSC config sheet Rev (2.7).
- Modify Entity ID 07 all Entity Instance = 01h.
- Add MTT CPU0/MTT CPU1 SDR.
- Update FRUSDR utility to FRUSDR11.0-Build02, and update FRUSDR.txt.

FCP_14:
- Follow Canoe Pass FSC config sheet Rev (2.8).
- Add P0/P1 MSID SDR,sensor number 0x81/0x87.
- Modify Union peak M Redundant SDR :FSC Record Type = 11h (System Airflow Formula).
- Exit Air Temp(0x2E) Add tag "EATEMP".
- Add MASTER.CFG power supply check to set "EATEMP" tag.
- Modify 0x34/0x35 MTT CPU0/CPU1 Owner/LUN from 00 change to 0x60.
- Modify DTS Look-up Table Record/Processor Parameters 22/DTS Slope to CB01.
- Change sensor name from "IBMC Watchdog"(0X0A) to "BMC Watchdog".
- Change sensor name from "BMC FW Health"(0X10) to "BMC Health".
- Modify Global Clamp:DIMM Thrm Mrgn 1(0xB0),DIMM Thrm Mrgn 2(0xB1),DIMM Thrm Mrgn 3(0xB2),DIMM Thrm Mrgn 4(0xB3) 
  Sensor Unavailable Control Value set to 0x00.

FCP_15:
- Follow Canoe Pass FSC config sheet Rev (2.9).
- Add SDR FW Update Status(0x12) and HSC 0/1/2 Status(0x69,0x6A,0x6B).
- MASTER.CFG shipping:Add CLEAR "PS_REDUNDANCY" and CLEAR "EATEMP".
- MASTER.CFG FCT and FCT2 :Add SET "EATEMP".
- Exit Air Temp(0x2E)Global Clamp Add tag 'EATEMP','UPM_BASE','UPM'
- Exit Air Temp(0x2E)SDR add tag 'UPM_BASE','UPM'
- Fan Redundancy (0x0C) add tag 'FCT'and 'FCT2'.
- Add SDR Fan 6 Present( 0x45).
- Add other chassis Redundant Fan 1 to 6 present taag (sensor number 40 to 45):
  OTHER_FAN_1,OTHER_FAN_2,OTHER_FAN_3,OTHER_FAN_4,OTHER_FAN_5,OTHER_FAN_6.
- Modify Fan Redundancy Map SDR Record Tag for 'OTHER','FCT','FCT2'.
- Add NM discovery sensor data record.

FCP_16:
- Follow Canoe Pass FSC config sheet Rev (2.9).
- MASTER.CFG Other chassis :add CLEAR "PS_REDUNDANCY" and CLEAR "EATEMP".
- MASTER.CFG other chassis :set fan redundancy sensor flag "FAN_REDUN_FLAG". 
- SDR: Fan Redundancy(0x0c)flag from "OTHER" flag chenge to "FAN_REDUN_FLAG"
- Modify Fan Redundancy Map SDR Record Tag from 'OTHER'change to 'FAN_REDUN_FLAG'
- SDR: Exit Air Temp remove tag "UPM_BASE" and "UPM".
- Global Clamp Header Record: Exit Air Temp remove tag "UPM_BASE" and "UPM".
- Global Clamp Header Record: Clamp ID 01  the ”„Clamp Flags”¦ = 11h.
- Modify VBAT SDR and VBAT scale.
- MASTER.CFG: Modify HSBP check FRU PN(Product Name).

FCP_17:
- Follow Canoe Pass FSC config sheet Rev (3.2).
- Modify MASTER.CFG FCT/FCT2 SET "EATEMP" to CLEAR "EATEMP"
- Modify SDR sensor name "Chs Intrusion"(04h) change to "Physical Scrty".
- Modify SDR sensor name "VR WD Timer"(0Bh) change to "VR Watchdog".
- Modify SDR sensor name "BB CPU1 VR Temp "(24h) change to "BB P2 VR Temp"(Thermal engineer will change to "BB P2 VR Temp").
- Modify SDR sensor name all fans change change(30H~38H) to "System Fan xx".
- Modify SDR sensor name "CPU1 Status"(70h) change to "P1 Status".
- Modify SDR sensor name "CPU2 Status"(71h) change to "P2 Status".
- Modify SDR sensor name "P1 ERR2 TimeOut"(7Ch) change to "P1 ERR2".
- Modify SDR sensor name "P2 ERR2 TimeOut"(7Dh) change to "P2 ERR2".
- Modify SDR sensor name "P1 MSID Mismatch"(81h) change to "P1 MSID Misatch".
- Modify SDR sensor name "P2 MSID Mismatch"(87h) change to "P2 MSID Misatch".
- Modify SDR sensor name "CPU1 VRD Hot"(90h) change to "P1 VRD Hot".
- Modify SDR sensor name "CPU2 VRD Hot"(91h) change to "P2 VRD Hot".
- Modify SDR sensor name "Mem Thrm Trip 1"(C0h) change to "Mem P1 Thrm Trip".
- Modify SDR sensor name "Mem Thrm Trip 2"(C1h) change to "Mem P2 Thrm Trip".
- add SDR Chassis ID and FAN FRU LED Mapping(UPM BASE/UPM/Other Chassis/FCT/FCT2).
- Modify New PS Fan SDRs (sensor number: A0/A1/A4/A5).

FCP_18:
- Follow Canoe Pass FSC config sheet Rev (3.4).

FCP_19:
- Follow Canoe Pass FSC config sheet Rev (3.5).
- Modify "P0 MSID Misatch" to "P0 MSID Mismatch"(81),"P1 MSID Misatch" to "P1 MSID Mismatch"(87).
- Modify Agg Thrm Mgn 1 ~ 5 Assertion/Deassertion Event Mask to 0000.

FCP_20:
- Follow Canoe Pass FSC config sheet Rev (3.7).
- Modify Global Stepwise Records/unque ID:0,determine number:4/ area for human readable values for LCC/PWM initial speed point:9
  from 19%(13h) change to  25%(19h).
- Add 'OTHER' tag to Global Stepwise Records "BB EDGE Temp"(20).
- Add 'OTHER' tag to Global Clamp Headers "P1 Therm Margin"(74),DIMM Thrm Mrgn 1(B0),DIMM Thrm Mrgn 2(B1),
  BB EDGE Temp(20),BB CPU1 VR Temp(24),BB BMC Temp(23),BB MEM VR Temp(25),LAN NIC Temp(2F),SSB Temp(22),P1 DTS Therm Mgn(83).
- Modify VBAT(DE) SDR. 
- Modify SDR name 'MTT CPU0' to 'P1 MTT'.
- Modify SDR name 'MTT CPU1' to 'P2 MTT'.
- Modify SDR name 'P0 MSID Mismatch' to 'P1 MSID Mismatch'
- Modify SDR name 'P1 MSID Mismatch' to 'P2 MSID Mismatch'
- Modify MASTER.CFG detect PS_REDUNDANCY.
- Add P1 MTT/P2 MTT tag.
- MASTER.CFG: delete OTHER chassis fan redundancy sensor detect tag "FAN_REDUN_FLAG".
- MASTER.CFG: Modify FCT/FCT2 "OTHER_FAN_6" change to "FCT_FAN_6".
- SDR: Fan Redundancy (0x0C) remove 'FAN_REDUN_FLAG' tag.
- SDR: System Fan 6' add 'FCT_FAN_6' tag.
- SDR: Fan 1 Present (0x40) remove 'OTHER_FAN_1' tag.
- SDR: Fan 2 Present (0x41) remove 'OTHER_FAN_2' tag.
- SDR: Fan 3 Present (0x42) remove 'OTHER_FAN_3' tag.
- SDR: Fan 4 Present (0x43) remove 'OTHER_FAN_4' tag.
- SDR: Fan 5 Present (0x44) remove 'OTHER_FAN_5' tag.
- SDR: Fan 5 Present (0x45) 'OTHER_FAN_6' change to 'FCT_FAN_6'.
- SDR: Fan Redundancy Map SDR Record remove 'FAN_REDUN_FLAG' tag.

FCP_21:
- Follow Canoe Pass FSC config sheet Rev (3.8).
- SDR: Modify Global Clamp Record P2 DTS Margin(0x84) Clamp Flags CPU Number=1.
- SDR: remove SAS Mod Temp clamp tag 'UPM'.
- SDR: FP NMI Diag Int add tag 'FP_NMI'.
- MASTER.CFG: FCT2, SET "PS_REDUNDANCY" change to CLEAR "PS_REDUNDANCY".
- MASTER.CFG: FCT2, SET "750_PS2" change to CLEAR "750_PS2".
- MASTER.CFG: OTHER chassis prompt "Does the front panel support a NMI button?".
- MASTER.CFG: UP-M NR,UP-M R,Shipping,FCT,FCT2 add SET "FP_NMI".
- Modify FRUSDR utility version 11 duild 5.

FCP_22:
- Follow Canoe Pass FSC config sheet Rev (4.0).
- MASTER.CFG: Shipping/FCT/FCT2 remove SET "FP_NMI".
- SDR: Modify P1 Mem Thrm Trip(0xC0)/P2 Mem Thrm Trip(0xC1) Sensor Type to 0C, Event / Reading Base Type to 6F.

S2600CP_FRUSDR_23:
- Follow Canoe Pass FSC config sheet Rev (4.2).
- Modify FRU file name, version update to 0.04.
- master.cfg: Modify FRU and SDR file name.
- S2600CP.sdr: Modify Exit Air Temp(0x2E) OEM to 0x47.

S2600CP_FRUSDR_24:
- Follow Canoe Pass FSC config sheet Rev (4.4).
- S2600CP.sdr: Modify System Airflow(0x11) Analog characteristic flags from 00 change to 07.
- S2600CP.sdr: BMC Health(0x10) Deassertion Event Mask from 1000 change to 0000.
- S2600CP.sdr: Modify DOMAIN 0 to DOMAIN 7.

S2600CP_FRUSDR_25:
- Follow Canoe Pass FSC config sheet Rev (4.5).
- master.cfg: Add "NO_CHASSIS_INTRU" tag for Other chassis and shipping.
- S2600CP.sdr: Sensor number 0x04:into two, one is with chassis intrusion event mask, another is not.
- S2600CP.sdr: Sensor number 0x2F:entity id change to 07h and instance change to 01h.
- S2600CP,sdr: CPU VR (24h) fan clamp threshold from 88 to 72.

S2600CP_FRUSDR_26:
- Follow Canoe Pass FSC config sheet Rev (4.5).
- S2600CP.sdr: Modify Global Stepwise/other chassis/Stepwise Curve ID 100/Domain Max - bit 7 from 0 change to 1.
- S2600CP.sdr: 'Mem Rdnc Sensor' Sensor Owner ID from 1 change to 0x33.
- S2600CP.sdr: 'Mem Conf Sensor' Sensor Number from 9 change to 2,
               Event / Reading Base Type from 0x6F change to 0x09.
- S2600CP.sdr: add SDR 'QPI Link Width'(0x09).
- S2600CP.sdr: add SDR 'Sparing Rdnc'(0x11).
- S2600CP.sdr: 'Rdnc Mod Sensor'(0x12) Sensor Owner ID from 0x33 change to 0x01.
- S2600CP.sdr: add SDR 'Mmry Parity Err'(0x13).
- S2600CP.sdr: 'PCIe Fat Sensor' Sensor Number from 0x04 change to 0x14,
               Event / Reading Base Type from 0x70 change to 0x76.
- S2600CP.sdr: 'QPI Fatl Sensor' Sensor Number from 0x07 change to 0x17,
               Event / Reading Base Type from 0x73 change to 0x74.
- S2600CP.sdr: add SDR 'BIOS Evt Sensor'(0x83)(two BIOS Evt Sensor).

S2600CP_FRUSDR_100:
- Follow Canoe Pass FSC config sheet Rev (4.6).
- S2600CP.sdr: add SDR'PCIe Fat Sensor'(0x04)(two PCIe Fat Sensor).
- FRUSDR UTILITY upgrade to Version 11.0 Build 6.

S2600CP_FRUSDR_101:
- Follow Canoe Pass FSC config sheet Rev (4.7).
- S2600CP.sdr: modify FCT/FCT2 FAN FRU LED Mapping Number of mapping pairs.
- S2600CP.sdr: modify SDR Entity Instance.
- S2600CP.sdr: Global clamp records add IO Module Temp and SAS Module Temp.
- S2600CP.sdr: Add I/O MODULE , I/O MODULE FRU and clamp record.
- S2600CP.sdr: Add SAS MODULE , SAS MODULE FRU and clamp record.
- S2600CP.sdr: modify SDR Exit Air Temp(0x2E) Assertion/Deassertion Event Mask and Reading Mask & Settable to 0000.      

S2600CP_FRUSDR_102:
- Follow Canoe Pass FSC config sheet Rev (4.8).
- S2600CP.sdr: Modify SDR sensor name "Pwr Unit Status"(0x01),"SMI Timeout"(0x06),"BMC FW Health"(0x10),"PS1 Power In"(0x54),
  "PS2 Power In"(0x55).

S2600CP_FRUSDR_103:
- Follow Canoe Pass FSC config sheet Rev (5.1).

S2600CP_FRUSDR_104:
- Follow Canoe Pass FSC config sheet Rev (5.1).
- Master.cfg : change chassis code name to product name.
- Master.cfg : change copyright 2011-->2012.

S2600CP_FRUSDR_105:
- Follow Canoe Pass FSC config sheet Rev (5.2).
- S2600CP.sdr: Front Panel temp sensor entity ID from 0x0C to 0x40 in SDR to solve DCMI issue.
- S2600CP.sdr: Modify "front panel" FRU Entity ID from 0x07 change to 0x0C.
- S2600CP.sdr: Modify "front panel" FRU Entity Instance from 0x37 change to 0x01.
- S2600CP.sdr: Modify "Baseboard" FRU Entity Instance from 0x36 change to 0x01.
- S2600CP.sdr: Modify "SAS Module" FRU Entity Instance from 0x31 change to 0x01.
- S2600CP.sdr: Add SDR Type 11 Record "Pwr Supply 1 FRU".
- S2600CP.sdr: Add SDR Type 11 Record "Pwr Supply 2 FRU".
- S2600CP.sdr: Add SDR Type 11 Record "HS Backplane 1".
- S2600CP.sdr: Add SDR Type 11 Record "HS Backplane 2".
- S2600CP.sdr: Add SDR Type 11 Record "HS Backplane 3".

S2600CP_FRUSDR_106:
- Follow Canoe Pass FSC config sheet Rev (5.2).
- Update FRUSDR utility Version 11.0 Build 9.
- S2600CP.sdr: Modify HDD number.

S2600CP_FRUSDR_107:
- Follow Canoe Pass FSC config sheet Rev (5.4).
- Update FRUSDR utility Version 11.0 Build 11.
- S2600CP.sdr: Power unit redundancy sensor "Capabilities" change to 00.

S2600CP_FRUSDR_108:
- Follow Canoe Pass FSC config sheet Rev (5.4).
- S2600CP.sdr: Modify sensor number 02 "Pwr Unit Redund" Remove De-assertion event from FF00 change to 0000.
- S2600CP.sdr: Modify sensor number 70/71 "P1 Status"/"P2 Status" Assertion Event Mask/Deassertion Event Mask/Reading Mask to 8200.
- S2600CP.sdr: Modify sensor number 90/91 P1 VRD Hot/P2 VRD Hot Sensor Capabilities to 40.
- S2600CP.sdr: Modify sensor number 94~97 P1 MEM01 VRD Hot/P1 MEM23 VRD Hot/P2 MEM01 VRD Hot/P2 MEM23 VRD Hot Sensor Capabilities to 40.
- S2600CP.sdr: Modify sensor number F0~FE,60~68 HDD 0 Status to HDD 23 Status Assertion Event Mask/Deassertion Event Mask/Reading Mask to 8300.
- S2600CP.sdr: Modify sensor number 34/35 'P1 MTT"/"P2 MTT" M = 0x05, B=0x00, Rexp/Bexp = 0xF0.
- Update FRUSDR utility Version 11.0 Build 14.

S2600CP_FRUSDR_109:
- Follow Canoe Pass FSC config sheet Rev (5.6).
- S2600CP.sdr: Update upper critical and upper noncritical for exit air temperature in sys config tab.

S2600CP_FRUSDR_110:
- Follow Canoe Pass FSC config sheet Rev (5.6).
- FRUSDR UTILITY upgrade to Version 11.0 Build 19.

S2600CP_FRUSDR_111:
- Follow Canoe Pass FSC config sheet Rev (5.6).
- S2600CP.sdr: Add sensor number 66/67 PSU1 Status/PSU2 Status SDR.

=============================================================================
                           ISSUES FIXED
=============================================================================
FCP_01:
- None.

FCP_02:
EPSD100011519-FRUSDR update didn't have "Other chassis" can be choose.
EPSD100011517-System Fan3 (#0x31) sensor reading always 0x00.

FCP_03:
EPSD100011518-Voltage /BB +1.1V STBY (#0xDD) lower non-critical event logged while system boot up. 
EPSD100011759-No 550W power supply can be choose for FRUSDR 02 updated.

FCP_04:
EPSD100011946-No define MSID sensor in FCP_03 / CP_BMC.SDR file.
EPSD100011947-No define ERR2 sensor in FCP_03 / CP_BMC.SDR file.

FCP_05:
none

FCP_06:
EPSD100011979-After OS watchdog timeout failed on last boot, but there was no error message in the SEL log.
EPSD100012043-[EWS]MEM Thrm Trip (0xC0, 0xC1, 0xC2, 0xC3) sensor Health always show "Unknow".

FCP_07:
EPSD100219643-SDR file has two BIOS records with the same generator ID and sensor number.

FCP_08:
EPSD100219958-Canoe Pass FRU/SDR package FCP_07 loads DIMM thermal trip sensors for processors 3 & 4.
EPSD100012166-Issue Get SM signal command to get fan power/speed got response 0x64 (full speed).

FCP_09:
none.

FCP_10:
EPSD100013577-Update FRUSDR with non-FRU front panel, update utility didn't auto detected as "Other Chassis".
EPSD100220565-DIMM Air velocity records lacking in SDR.
EPSD100220564-DTS Lookup tables missing in SDR.

FCP_11:
none.

FCP_12:
none.

FCP_13:
EPSD100014114-Smash Enter show /system1/sensor*: Target Not Found.
EPSD100220986-SDR record lacking for MEM thortting.
EPSD100221121-Advanced Fan Failure sub-records are not used correctly.

FCP_14:
EPSD100221121-Advanced Fan Failure sub-records are not used correctly.
EPSD100221366-Exit Air Temp sensor 0x2e should only be installed when PMBUSpower supply detected.
EPSD100014433-The init sensor scanning bit is not cleared as it is expected to be.
EPSD100014214-Exit Air Temp(0x2E) Sensor status always show 0xE0 (Not available).

FCP_15:
EPSD100220686-No SEL entry found for successfull FW Update after successfully updating FW using .nsh file.
EPSD100220687-No SEL entry found for FW Update Failure.

FCP_16:
EPSD100221878-Incorrect Clamp Flags in P2 Therm Margin FSC clamp record.
EPSD100015016-Update FRUSDR got message "Hot Swap Backplane 1 FRU is invalid".

FCP_17:
EPSD100221962-Critical fan tach events occur when fans are driven at Normal Control Value PWM.

FCP_18:
none.

FCP_19:
EPSD100222920-Global Aggregate Thermal Margin sensors have incorrect event masks.

FCP_20:
EPSD100221962-Critical fan tach events occur when fans are driven at Normal Control Value PWM.
EPSD100016120-Execute FSC script LinearStepwise_003.tcl always got fail result.
EPSD100016187-Fans are running on full speed after FRUSDR flashed for Other chassis setting.

FCP_21:
none.

FCP_22:
none.

S2600CP_FRUSDR_23:
none.

S2600CP_FRUSDR_24:
none.

S2600CP_FRUSDR_25:
None.

S2600CP_FRUSDR_26:
None.

S2600CP_FRUSDR_100:
None.

S2600CP_FRUSDR_101:
None.

S2600CP_FRUSDR_102:
None.

S2600CP_FRUSDR_103:
None.

S2600CP_FRUSDR_104:
None.

S2600CP_FRUSDR_105:
None.

S2600CP_FRUSDR_106:
None.

S2600CP_FRUSDR_107:
None

S2600CP_FRUSDR_108:
None

S2600CP_FRUSDR_109:
None

S2600CP_FRUSDR_110:
None

S2600CP_FRUSDR_111:
None

=============================================================================
                             REFERENCE MATERIAL
=============================================================================
CanoePass_CONFIG-FSC Rev 5.6 datasheet.
[END OF RELEASE NOTES]