=============================================================================
       Intel(R) Server Platform S1600JP FRU/SDR Update Release Notes
=============================================================================

INTEL Enterprise Platform & Services Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA

=============================================================================

DATE:   Sep 30, 2017

TO:     Intel(R) Server Platform S1600JP Pass customers

SUBJECT:    IBMC(R) FRU/SDR update package S1600JP_FRUSDR_1.07 release notes

=============================================================================
                               LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products.
No license, express or implied, by estoppel or otherwise, to any intellectual
property rights is granted by this document. Except as provided in Intel's
Terms and Conditions of Sale for such products, Intel assumes no liability
whatsoever, and Intel disclaims any express or implied warranty, relating to
sale and/or use of Intel products including liability or warranties relating
to fitness for a particular purpose, merchantability, or infringement of any
patent, copyright or other intellectual property right. Intel Corporation may
have patents or pending patent applications, trademarks, copyrights, or other
intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not
provide any license, express or implied, by estoppel or otherwise, to any
such patents, trademarks, copyrights, or other intellectual property rights.
Intel products are not intended for use in medical, life saving, or life
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation.

*Other names and brands are the property of their respective owners.

Copyright (c) 2010 - 2014 Intel Corporation.


=============================================================================
                           ABOUT THIS RELEASE
=============================================================================

SDR file version: 1.07
Baseboard FRU file version: 0.01
Master configuration file version: 1.07
FRUSDR utility version: v11.0_Build19

=============================================================================
                           SYSTEM HARDWARE & SOFTWARE REQUIREMENTS/REVISIONS
=============================================================================

- This FRU/SDR package has only been tested on S1600JP FAB1 baseboards.

- BMC firmware rev 1.17.4151 (or later) MUST be preinstalled prior to
  installing this FRU/SDR package.

- BIOS SE5C600.86B.99.99.x058

=============================================================================
                           IMPORTANT INSTALLATION NOTES
=============================================================================

- None

=============================================================================
                           INSTALLATION PROCEDURE
=============================================================================

1. Ensure BMC release 1.17.4151 or later is pre-installed before attempting this
   FRU/SDR update.

2. Copy all of the files in the S1600JP_FRUSDR_1.07.zip archive to a USB key,
   hard disk drive or floppy drive.
   All of the files in this zip archive must reside in the same directory.

3. Boot to EFI and then run the following command to display the
   contents of the baseboard FRU device:

    FRUSDR /d FRU

   If device is empty(which is the case for all new FAB1 baseboards) or 
   corrupted, then execute the following command to program the empty FRU 
   device:

   For S1600JP:
        FRUSDR /fru S1600JP.fru

4. Now execute the following command to bring up the main FRU/SDR load menu:

    FRUSDR /cfg master.cfg

5. Select the option which is applicable to what you want to do. On a brand
   new baseboard I would highly recommend to run option 3 to program both
   the FRU and SDR. By reprogramming the FRU you will be given the option
   to input data from the keyboard into various chassis, board and product
   areas. Ensure that you select the correct chassis from the chassis
   selection menu otherwise your fan sensors will not be configured
   properly.

6. Once the package has finished its installation, I would highly recommend
   to DC power off the system and cycle AC power.

=============================================================================
                           KNOWN ISSUES/WORKAROUNDS
=============================================================================
- Known issue: The first time to update FRU will fail. Please use another
  method to update FRU the first time you update FRU. 
  Frusdr.efi /fru S1600JP.fru.
 
=============================================================================
                           FEATURES ADDED
=============================================================================
S1600JP_FRUSDR_1.07:
- Add supporting for 450W PSU with new model name start with "DPS-500WB-2 "

S1600JP_FRUSDR_1.06:
- Add PSU status SDR entry for ME, sensor number is 0x66, 0x67.
- Follow Jackson Pass FSC Config Sheet Rev 1.6.xlsm.

S1600JP_FRUSDR_1.05:
- Change FRUSDR utility to v11.0_Build19.
- Follow Jackson Pass FSC Config Sheet Rev 1.6.xlsm.

S1600JP_FRUSDR_1.04:
- Change OEM from 0x00 to 0x25 for sensor number D3h.
- Follow Jackson Pass FSC Config Sheet Rev 1.6.xlsm.

S1600JP_FRUSDR_1.03:
- Update sku name.
- Follow Jackson Pass FSC Config Sheet Rev 1.6.xlsm.

S1600JP_FRUSDR_1.02:
- Update C1 and C2 for 4Fan sku.
- Update ramp coefficient LSB for clamp ID C4.
- Follow Jackson Pass FSC Config Sheet Rev 1.6.xlsm.

S1600JP_FRUSDR_1.01:
- Add MIC status sensor for sensor number A3h.
- Add MIC margin sensor for sensor number C5h.
- Add MIC margin sensor for clamp header ID C5h.
- Update LCC for 4Fan and 5Fan SKU.
- Add FSC for MIC SKU.
- Follow Jackson Pass FSC Config Sheet Rev 1.5.xlsm.

S1600JP_FRUSDR_1.00:
- Modify Deassertion Event Mask 0xFF00 to be 0x0000 for sensor number 02h.
- Separate acoustic setting and performance setting.
- Update some values for 4*4056 fan SKU.
- Update temperature byte for clamp ID: 20h, 23h - 28h, and 2Ch - 2Fh.
- Update some sensors' clamping value.
- Add clamp sensor of 94h.
- Change riser sensor's name GPU Mod Temp to be GPU Riser Temp.
- Change riser sensor's name FhFl Mod Temp to be Fhfl Riser Temp.
- Modify M 0x01 to be 0x05 and R exp, B exp 0x00 to be 0xf0 for P1 MTT.
- Update the MiniERP 450W PSU MN.
- Update DC 450W PSU Product Name YM-2451D to be SUNNY451DM.
- Change FRUSDR utility to v11.0_Build14.
- Follow Jackson Pass FSC Config Sheet Rev 1.4.xlsm.

S1600JP_FRUSDR_0.07:
- Add one more sensor(28H) for SAS Modules with two thermal devices.
- Assign 26h/2Dh into domain 1 for two skus.
- Modify rule of detect SAS module temperature.
- Modify rule of detect SAS module FRU.
- Modify rule of detect I/O module temperature.
- Modify auto re-arm to be manual re-arm for sensor number 0Eh and 0Fh.
- Remove event offset trigger 08 (processor disabled) for sensor number 70h.
- Remove event offset triggers 02, 03, 05 and 08 for sensor number F0h - FEh and 60h - 68h.
- Follow Jackson Pass FSC Config Sheet Rev 1.33.xlsm.

S1600JP_FRUSDR_0.06:
- Modify PSU FRU name YM-2451DAR to be YM-2451D in master.cfg.
- Update rule for detecting I/O Mod temperature.
- Map PSU zone with zone 0/1/2.
- Change sensor 2E's Assertion and Deassertion mask value to 0000h in Sys Config tab.
- Update Fan fault boost value from FFh to 100%.
- Set Sensor-reading-unavailable Control Value of 2Fh to 0%.
- Modify manual re-arm to be auto re-arm for P1 VRD Hot.
- Follow Jackson Pass FSC Config Sheet Rev 1.32.xlsm.

S1600JP_FRUSDR_0.05:
- Modify sensor names for sensor number: 24h and 25h.
- Modify Sensor Capabilities for sensor number: 02h.
- Modify LCC of Power Supply.
- Remove clamp ID 5Dh for FSC in PS domain.
- Modify DIMM air velocity bit9 - bit11 and bit18 - bit20.
- Modify System Airflow Formula bit5 - bit9.
- Map PSU with zone 0/1 in stepwise header record.
- Follow Jackson Pass FSC Config Sheet Rev 1.30.xlsm.

S1600JP_FRUSDR_0.04:
- Add temperature sensors number: 27h and 2Ch on risers.
- Add clamp header and fan speed control for sensor number 27h and 2Ch.
- Modify temperature bit in clamp header for sensor number 2Dh.
- Modify the fan fault LED GPIO number.
- Change FRUSDR utility to v11.0_Build11.
- Follow Jackson Pass FSC Config Sheet Rev 1.23.xlsm.

S1600JP_FRUSDR_0.03:
- Modify global clamp header record Sensor-reading-unavailable Control Value, record ID: 0xB1, 0xB2.
- Remove tags of "SAS_MODULE" for FCT use in master.cfg.
- Modify some tags for every chassis/sku what it need.
- Add another product name of 450W mini-ERP PSU in master.cfg.
- Rename sensor name, record ID: 0x60 - 0x68, 0xF0 - 0xFE.
- Remove all sensors which related with 600W Fix Power Supply.
- Modify configurtion error bit for P1 status.
- Modify system fan tags for standard sku in master.cfg and S1600JP.sdr.
- Modify entity ID to 0x40 for sensor number 0x21.
- Rearrange display message for PSU in master.cfg.
- Follow Jackson Pass FSC Config Sheet Rev 1.20.xlsm.

S1600JP_FRUSDR_0.02:
- Modify product name of 450W mini-ERP PSU in master.cfg.
- Remove all chassis domain 2 to reference fans-off in S1600JP.sdr.
- Rename tags for PSU in master.cfg and S1600JP.sdr.
- Rearrange display message for PSU in master.cfg.
- Add type 11 SDRs for FRU Device ID: 02h, 03h, 05h, 06h, 07h, 09h, and 0Ah in S1600JP.sdr.
- Modify auto detection for 450W mini-ERP PSU in master.cfg.
- Add two SDRs, sensor number 0E and 0F in S1600JP.sdr.
- Modify configurtion error bit for P1 status.
- Change FRUSDR utility to v11.0_Build9.
- Follow Jackson Pass FSC Config Sheet Rev 1.15.xlsm.

S1600JP_FRUSDR_0.01:
- Update SDR as per Jackson Pass FSC Config Sheet Rev 1.10.xlsm.

=============================================================================
                           ISSUES FIXED
=============================================================================
S1600JP_FRUSDR_1.07:
- None.

S1600JP_FRUSDR_1.06:
- None.

S1600JP_FRUSDR_1.05:
- None.

S1600JP_FRUSDR_1.04:
- None.

S1600JP_FRUSDR_1.03:
- None.

S1600JP_FRUSDR_1.02:
- None.

S1600JP_FRUSDR_1.01:
- None.

S1600JP_FRUSDR_1.00:
- None.

S1600JP_FRUSDR_0.07:
- None.

S1600JP_FRUSDR_0.06:
- None.

S1600JP_FRUSDR_0.05:
- None.

S1600JP_FRUSDR_0.04:
- EPSD100021670 - JKP fan fault LED did not match with system fan.

S1600JP_FRUSDR_0.03:
- EPSD100020794 - The 450W AC redundant PSU FRU is invalid.

S1600JP_FRUSDR_0.02:
- EPSD100020790 - Execute FTF script BAT_FSC_RecordCheck_003.tcl has fail result.
- EPSD100020791 - Execute FTF script BAT_FSC_Functional_003.tcl has fail result.
- EPSD100020794 - The 450W AC redundant PSU FRU is invalid.

S1600JP_FRUSDR_0.01:
- None.

=============================================================================
                           REFERENCE MATERIAL
=============================================================================
Jackson Pass FSC Config Sheet Rev 1.6.xlsm datasheet

[END OF RELEASE NOTES]