=============================================================================
    Intel(R) Server Platform S2400EP FRU/SDR Update Release Notes
=============================================================================

INTEL Enterprise Platform & Services Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA

=============================================================================

DATE:   Feb 10, 2014

TO:	    Intel(R) Server Platform S2400EP customers

SUBJECT:    Integrate BMC(R) FRU/SDR update package S2400EP_FRUSDR_104 release notes

=============================================================================
                               LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products.
No license, express or implied, by estoppel or otherwise, to any intellectual
property rights is granted by this document. Except as provided in Intel's
Terms and Conditions of Sale for such products, Intel assumes no liability
whatsoever, and Intel disclaims any express or implied warranty, relating to
sale and/or use of Intel products including liability or warranties relating
to fitness for a particular purpose, merchantability, or infringement of any
patent, copyright or other intellectual property right. Intel Corporation may
have patents or pending patent applications, trademarks, copyrights, or other
intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not
provide any license, express or implied, by estoppel or otherwise, to any
such patents, trademarks, copyrights, or other intellectual property rights.
Intel products are not intended for use in medical, life saving, or life
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation.

*Other names and brands are the property of their respective owners.

Copyright (c) 2010 - 2014 Intel Corporation.


=============================================================================
                              ABOUT THIS RELEASE
=============================================================================

SDR file version: 1.04
Baseboard FRU file version: 0.01
Master configuration file version: 1.04
FRUSDR UTILITY Version: 11.0 Build 20

=============================================================================
        SYSTEM HARDWARE & SOFTWARE REQUIREMENTS/REVISIONS
=============================================================================

- This FRU/SDR package has only been tested on S2400EP FAB1 baseboards

- BMC firmware rev 01.16 (or later) MUST be preinstalled prior to installing
  this FRU/SDR package

- BIOS R0102 or later
- MB Ver Fab1

=============================================================================
                      IMPORTANT INSTALLATION NOTES
=============================================================================

- None

=============================================================================
            INSTALLATION PROCEDURE
=============================================================================

1. Ensure BMC release 01.16 or later is pre-installed before attempting this
   FRU/SDR update.

2. Copy all of the files in the S2400EP_FRUSDR_104.zip archive to a USB key,
   hard disk drive or floppy drive.
   All of the files in this zip archive must reside in the same directory.

3. Boot to EFI and then run the following command to display the
   contents of the baseboard FRU device:

    FRUSDR /d FRU

   If device is empty(which is the case for all new FAB1 baseboards) or corrupted, then
   execute the following command to program the empty FRU device:

   For S2400EP:
        FRUSDR /fru S2400EP.fru

4. Now execute the following command to bring up the main FRU/SDR load menu:

    FRUSDR /cfg master.cfg


5. Select the option which is applicable to what you want to do. On a brand
   new baseboard I would highly recommend to run option 3 to program both
   the FRU and SDR. By reprogramming the FRU you will be given the option
   to input data from the keyboard into various chassis, board and product
   areas. Ensure that you select the correct chassis from the chassis
   selection menu otherwise your fan sensors will not be configured
   properly.

6. Once the package has finished its installation, I would highly recommend
   to DC power off the system and cycle AC power.

=============================================================================
                           KNOWN ISSUES/WORKAROUNDS
=============================================================================

- None

=============================================================================
                           FEATURES ADDED
=============================================================================

S2400EP_FRUSDR_104:
- Add the ME sensor "PSU1 STATUS" and "PSU2 STATUS".

S2400EP_FRUSDR_103:
- None.

S2400EP_FRUSDR_102:
- Update exit air temperature and system air flow settings
- Update some temperature sensor normal minum setting and low critical and low non critical setting

S2400EP_FRUSDR_101:
- Remove the chassis intrusion feature from BFP21_NR and BFP15_NR
- Modify processor vrd hot sensor to auto re-arm
- Modify the flow of detect IO module and SAS module
- Rename s#B0 s#B2

S2400EP_FRUSDR_100:
- Update Aggregate sensor configuration Record

S2400EP_FRUSDR_04:
- Update system airflow formula Record
- Update fan normal control value
- Add Global Clamp Records 64h,65h,94h,95h
- Add Texit and system airflow for BFP15" chassis
- Update Global Stepwise Records

S2400EP_FRUSDR_03:
- Modify all Drive Status sensors' TAG
- Add s# 29h 2Ah 2Bh
- Add HSBP detection in master.cfg file 
- Add a TAG to 'Exit Air Temp' sensor
- Modify Sensor Maximum Reading of s#83 and s#84 from 00 to 7F
- Remove 600W PSU Iout current%
- Add Baseboard NIC Temperature sensor clamp
- Add IO module and SAS module temperature sensor clamp
- Add PS domain in FSC
- Update fans-off and low speed sub-record
- Update fan normal value

S2400EP_FRUSDR_02:
- Correct all entity instance of entity ID 07
- Update PS FRU in Master file
- Update LCC in "Stepwise sub-record" in each chassis (BFP21_NR & BFP15_NR)
- Delete all 'BFP21_R' tag (fan redundant sku)
- Delete DTS parameter record
- Delete DTS lookup record
- Remove fan redundancy record

S2400EP_FRUSDR_01:
- Update SDR as per S2400EP FSC Config Sheet.xls(v1.1)


=============================================================================
                           ISSUES FIXED
=============================================================================

S2400EP_FRUSDR_104:
- None

S2400EP_FRUSDR_103:
- Update FRUSDR utility to 11 build 20.

S2400EP_FRUSDR_102:
- None

S2400EP_FRUSDR_101:
- None

S2400EP_FRUSDR_100:
- None

S2400EP_FRUSDR_04:
- EPSD100021608:The values of "Type/Length Code" and "Sensor Capabilities" in sensor#34/35 are incorrect 

S2400EP_FRUSDR_03:
- EPSD100021270:Upper threshold values for sensors "P1/P2 DTS Therm Mgn" in EWS are
  not consistent with the valus read via CMDTOOL.EXE
- EPSD100020595:The version 0f FRUSDR_02 it can't detected the HSBP automatically
- EPSD100020476:There is no HSC temperature sensor in EWS
- EPSD100020474:EWS show eight HDD status sensors for 3.5'HSBP
- EPSD100019755:Sensor"Exit Air Temp"(2E) health show"Unknow"in EWS

S2400EP_FRUSDR_02:
- None

S2400EP_FRUSDR_01:
- None

=============================================================================
                             REFERENCE MATERIAL
=============================================================================

S2400EP FSC Config Sheet.xls(v1.6)


[END OF RELEASE NOTES]