This release note and the software that accompanies it are copyright (c) 2018, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported RAID Controllers
==========================
This download supports Intel(R) RAID controllers with LSI3316 ROC using MR software stack:
RMS3AC160


===================
Package Information
===================
Flash package = v24.22.0-0023


==========
Attention!
==========
Intel recommends to loading Factory Default setting after the firmware upgrade which will not affect data on any existing array. To do so:
1. Reboot the system and login to the RAID BIOS Console. 
2. Select the controller and select 'Adapter Properties'->'Next'
3. Set the 'Set Factory Defaults' setting to 'Yes' and submit the change.
4. Reboot the system (the default settings are applied).
5. Re-configure to the desired settings in RAID Web Console2.

---------------------------------------
Firmware downgrade notice
---------------------------------------
Intel does not recommend to downgrade the factory installed firmware on your RAID module or controller, it has important enhancements and bug fixes you may lose when going to a previous version.
If you need to install an older firmware version, please contact Intel for instructions on how to perform this action.


==================
Known Restrictions
==================
1) This download does NOT support EFI v1.1 environment. Please use the EFI shell command “ver" which will display the EFI version, to identify the EFI version.
2) When 2 or more VDs are created, VD cache settings must be the same.

**************************************************************************************************************************
***********PLEASE READ BEFORE DOWNGRADING FROM THIS FIRMWARE VERSION TO ANY PRIOR FIRMWARE VERSION************************
**************************************************************************************************************************
Online Firmware Update should not be performed when downgrading from this release to a prior release.  Please refer to the 240_VD_Feature_Limitations_Known_Issues_Addendum_v1.0.pdf document included with this package for additional details.
**************************************************************************************************************************
**************************************************************************************************************************


=======================
Contents on the package 
=======================
The following files are included in this zip:

Name:                                                                      Description:
COPYING.NEWLIB.txt                                                         License Agreement
3316-MR_FWPKG_v24.22.0-0023_Readme.txt                                     This file
MR_614p1_3316.rom                                                          Firmware binary
License_v2.pdf                                                             License Agreement
update.nsh                                                                 UEFI firmware update batch file
240_VD_Feature_Limitations_Known_Issues_Addendum_v1.0.pdf                  Advisory Addendum from Avago
StorCLI\*                                                                  StorCLI CLI tool for EFI shell environment


==========================
Installation instructions:
==========================

UEFI shell instructions for updating RAID Firmware:
-----------------
   1. Download and extract all files to a USB flash drive.
   2. Boot the target system to EFI shell. 
   3. Change directory to the local drive and directory containing the flash update files and the firmware image file.
   4. Type "update.nsh" and press <Enter> to execute the command
   5. Wait for the flash to complete. Do NOT reboot the system during the update.

You can also use RAID Web Console 2 or OS version of StorCLI to update the RAID firmware.  For more detail, please refer to the Intel(R) RAID Software User's Guide.


=============================
Package Details/Fixes/Updates 
=============================

Version Numbers:
===============
Firmware Package:24.22.0-0023 (MR 6.14 point release 1)
	Firmware 4.740.00-8288
	ROMENV 1.09
	BootBlock 3.10.01.00-0003
	NVDATA  4.1705.00-0004
	UEFI_Driver 0x06180202 (SIGNED)
	Hii 03.25.05.04 (SIGNED)
	FCODE 4.19.08.00
	BIOS  6.36.00.2
	CTRL-R 5.19-0602	

Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ01268412 - Unable to access device PD (SSD)
SCGCQ01287286 - OS hung and iMR FW reset when do delete and create VD from previous powersave PD (Spindowned)
SCGCQ01343017 - No amber LED when a configured disk is removed
SCGCQ01348114 - Controller fails to boot up when migrated from 6.13 to 6.14 FW for Specific OEM
SCGCQ01350295 - Value defined for the DDR turning parameter DP_IO_VREF_1_2 is wrong for invader boards
SCGCQ01368845 - 4G DDR tuning value has to be changed in MR FW.
SCGCQ01375977 - Controller Disappear during clean shutdown on OEM server
SCGCQ01378970 - FW breaks into montask with pinned cache and foreign configuration
SCGCQ01395084 - FW reported tmm Date of Manufacture 15/25/6
SCGCQ01399701 - Interrupting Offload will Lead to Next offload cycle to fail
SCGCQ01440768 - Parameter Page Invalid, Setting channel count based on DDR Size.
SCGCQ01446811 - Addressing PCIe credit free issue.
SCGCQ01455133 - Firmware upgrade/downgrade operation failing on iMR controller
SCGCQ01455949 - On iMR & for 2 enclosures connected in cascaded multi path , power off and then power on the 1st enclosure, PDs not getting detected
SCGCQ01465727 - 6.14 : Reverting the sysDma changes
SCGCQ01473188 - SED Drive become UBad during secure erase on MegaRAID 9361-8i controller
SCGCQ01347858 - Found invalid event
SCGCQ01375071 - Placement of an image checkword at data area of NOR flash leads to controller crash
SCGCQ01394288 - MR : Cache data Lost when Term Log is set to "on" and grown bad blocks are there in the controller
SCGCQ01400807 - Learn cycle shown as active when Learn cycle fails
SCGCQ01403292 - Firmware allows to add bad blcoks beyond actual number of blocks.
SCGCQ01472217 - linker error resolved
SCGCQ01395724 - NVCache state not transitioning from 'Faulty' to 'Ok' until after reboot
SCGCQ01439651 - Porting of firmware download fixes
SCGCQ01446965 - SSD SATA JBOD discovered as 0.0MB after re-loading the same driver.
SCGCQ01264142 - New fault code for routine synchronous reset
SCGCQ01459161 - Integrate phase 14 PL - 14.00.08.00 with MR 6.14
SCGCQ01452102 - customer request for GPIO support.
SCGCQ01401110 - PL 14.00.07.00 integration to MR 6.14
SCGCQ01386225 - Integrate phase 14 PL - 14.00.06.00 with MR 6.14
SCGCQ01373161 - FW not responding to PWR_REQ in time. Request to up the number of TURs sent before timing out drive.
SCGCQ01369359 - Disable OOB communication via I2C
SCGCQ01334112 - PL phase 13.0007.00 integration with MR 6.13
SCGCQ01276465 - PL integration 12.00.10.00 with MR 6.12
SCGCQ01268897 - Integrated PL 12.0.9.0 with MR 6.12
SCGCQ01188711 - Define interface to support firmware assisted VD/JBOD properties(max IO size, device queue depth..)
SCGCQ01221705 - 24i/28i : Need to identify Controller has onboard Enclosure through NVDATA.
SCGCQ01472061 - CacheCade: IO performance need to be improved for WB SVD and WB CCVD combination for specific PnP ID
SCGCQ01403814 - FW breaks into montask with pinned cache and foreign configuration
SCGCQ01394348 - Boot message string change for BOOT_MSG_CACHE_DISCARD
SCGCQ01384265 - PL 14.00.05.00 Integration with Invader MR 6.14
SCGCQ01466802 - Setting DDR flag for ROMB design having new DDR for an OEM
SCGCQ01394920 - Block OCR after Clearing NVRAM
SCGCQ01351442 - Firmware hits montask while reconstruction when drive is pulled out
SCGCQ01349420 - Cache data lost event seen for WT vds
SCGCQ01421934 - Check Consistency doesn't identify double media errors once aborting and starting CC again
SCGCQ01350347 - Kill adapater observed while running IO's on 240 Volumes
SCGCQ01291340 - RAID10 VD goes to failed state after performing RLM
SCGCQ01446983 - PL considers Timer Handle=0 and invalid, MR FW did not.
SCGCQ01339330 - MR 6.14 Beta: MonTask: line 245 in file ../../raid/1078int.c while running reboot test with background operations
SCGCQ01334365 - MR_6.14: PCI Trapping ISR incorrect logic for config trap address
SCGCQ01331892 - Driver crashed after FW update via UCSM 
SCGCQ01326394 - HW workaround implementation for SCGCQ00830272 and SCGCQ01048567
SCGCQ01306491 - Firmware:- Request to change 9361-8i) to permanently disable SDS Mode and JBOD Mode
SCGCQ01280567 - MR_6.13:FW flash pack -30 with reboot , result to Controller hang at bios level (Power PC)
SCGCQ01260889 - Firmware halts upon changing controller personality to JBOD mode with MCTP enabled
SCGCQ01356192 - IOMMU fault at address 0x80360000
SCGCQ01311731 - 6.14 : To fix IOPATH overflow during linking
SCGCQ01412827 - Controller hang at DCR Err Logg Address 29e02.
SCGCQ01351052 - FC: 0 CS: 0 offload meta signature not valid, ffffffff observed in FW logs on a system restart.
SCGCQ01334334 - Controller hangs in primary core on reboot in OEM server
SCGCQ01446963 - Revert the DDR tuning values back to default value
SCGCQ01351559 - MR 6.13: Blocked Spin down Pass thru command for configured drives.
SCGCQ01350771 - No amber LED when a configured disk is removed
SCGCQ01304919 - PL Fault 0000601e observed while running multipath on/off script in JBOD mode.
SCGCQ01290418 - Storcli Failed to create single PD R0 from UGood drive which has replaced a UBAD foreign drive
SCGCQ01289194 - IN FAILED ARRAY bit is not being set when a VD is cleared
SCGCQ01255837 - RDM in Use-RDm Error & crashed into Montask during boot
SCGCQ01367331 - LSA hangs when user try to change drive security key.
SCGCQ01447780 - Controller crash observed while running OLTP workload (4K and 16K 16QD)
SCGCQ01304921 - PL Fault 0000601e observed while running multipath on/off script in JBOD mode.
SCGCQ01348658 - Firmware crashes during medium error recovery and Rebuild
SCGCQ01402828 - MR7.3: 4k PD Configuration can't be imported from iMR to MR Controller. However, it can be imported from MR to iMR
SCGCQ01328038 - Controller hang with FDE Drive
SCGCQ01415424 - Parameter Page Reads fail during ONFI bringup.

CTRL-R
SCGCQ01497428 - Firmware crash when trying to traverse through Ctrl-H tabs when cable is removed
SCGCQ01382063 - Data Abort Exception while entering CTRL R

BIOS
SCGCQ01379365 - System reset is initiated twice in BIOS
SCGCQ01379238 - Drive ID shown in BIOS POST is more than 1000+, even thought the total drives is only about 160
SCGCQ01379284 - Reset Type and customer messaging for system resets initiated by controller oprom
SCGCQ01446924 - System stops at post in legacy mode boot in the multi controllers configuration where-in one of the controller is in fault state

UEFI Driver
SCGCQ01383115 - With pinned cache generated, HII is auto launched during system Boot when BIOS Mode is set to Ignore Errors.
SCGCQ01349431 - Firmware Management Protocol - Firmware update fails with inappropriate message when trying to update an unsigned component
SCGCQ01376694 - Issues in UEFI driver when FW is in fault state
SCGCQ01376714 - Debug print shown on the console from the UEFI Driver error path.
SCGCQ01379235 - Cursor below text and in center of line on the system reset request screen.
SCGCQ01376551 - Reset Type and customer messaging for system resets initiated by controller OpROM
SCGCQ01351615 - Change the logic for reentering to main entry point in UEFI Driver

HII
SCGCQ01384295 - HII in "Create Logical Drive" page shows JBOD present in the system , even if there are no JBODs present
SCGCQ01376636 - Use SetMem before filling drive name
SCGCQ01376606 - For SuperCap, HII has the primitive 'Remaining Capacity' which is different compared to other host utilites
SCGCQ01446905 - MR HII will jump to some form unexpectedly when import foreigh configuration
SCGCQ01446899 - change Default setting in Select Media Type in HII from HDD to Both
SCGCQ01407034 - Check All is not working in Assign Dedicated HotSpare form
SCGCQ01348102 - Click on "OK" button after completing any operation doesn't have any effect in the screen
SCGCQ01446908 - Use SetBrowserData for VD and PD Mngt Refresh functions.
SCGCQ01401537 - The physical drive operation % increase in progress is not getting updated
SCGCQ01373600 - Delay seen during boot in case of 240 PD configuration.
SCGCQ01356100 - Save Debug log: Free the memory in error path
SCGCQ01349342 - Foreign Configuration Preview screen also has entries of virtual drives that are optimal in state.
SCGCQ01356104 - HII - Fast Init progress shows 0% despite it already completed
SCGCQ01356102 - RSOD seen when user browse to Enclosure Management Page
SCGCQ01443719 - Virtual Drive information is incorrect in preview foreign configuration form in HII.
SCGCQ01407038 - Check All option is not working properly in Make JBOD form
SCGCQ01356098 - Replace hardcoded SDV Part number with Mass Production Part Number
SCGCQ01349369 - Customize the configuration help message.
SCGCQ01376658 - HII shows wrong Temperature value when Sensor status is "Not Installed"
SCGCQ01376653 - Foreign configuration page seen after changing profile to NVMe.
SCGCQ01356101 - HII produces "Success" page for unsuccessful operation when saving controller events



Version Numbers:
===============
Firmware Package:24.22.0-0013 (MR 6.14)
	Firmware 4.740.00-8247
	ROMENV 1.09
	BootBlock 3.10.01.00-0003
	NVDATA  4.1705.00-0004
	UEFI_Driver 0x06180200 (SIGNED)
	Hii 03.25.05.00 (SIGNED)
	FCODE 4.19.08.00
	BIOS  6.36.00.0
	CTRL-R 5.19-0600

Bug Fixes and Enhancements:
===========================
Firmware:

SCGCQ00857533 - (Resolved) - Kill adapter in line 1272 in file ../../raid/1078dma.c after pulling enclosure cable with IOs running on 240VD, JBOD
SCGCQ01083581 - (Closed) - Activity LED is always ON even when no drives are present.
SCGCQ01201958 - (Closed) - MR 6.13: Blocked Spin down Pass thru command for configured drives.
SCGCQ01213915 - (Closed) - In RAID personality, MR_DCMD_CFG_AUTOCFG DCMD is disabled in non-240 VD environment.
SCGCQ01215003 - (Closed) - Setting all the ldtoTgtId with 0xff beyond 240 entries.
SCGCQ01223284 - (Closed) - MR_EVT_PD_ERROR_STATS events are logged when drive is moved to REBUILD/UNCONFIGURED BAD/ONLINE/OFFLINE. Also correct DCMD
SCGCQ01227115 - (Closed) - FW crashes when FW update(OFU) is done with faluty onfi
SCGCQ01230560 - (Closed) - Coverity issues:fixed the coverity defects.
SCGCQ01230749 - (Closed) - MR6.12 NVRAM Overflow - incomplete FW logs
SCGCQ01232275 - (Closed) - Update the MAXTransferLength properly for Driver enabled 1MB support feature
SCGCQ01235505 - (Closed) - Assertion failure in ../../dm/mpt2/mptrec.c at line 3139, while performing cable pull/push operation.
SCGCQ01236287 - (Closed) - corrected the span index
SCGCQ01241568 - (Closed) - Coverity issue 15748 and 17765
SCGCQ01241680 - (Closed) - Drive Strength values are incorrect for last 8 phys of 24i Controller
SCGCQ01242817 - (Closed) - Change Slew Rate on dual rank 24i Boards to fix ECC Errors.
SCGCQ01252243 - (Closed) - Firmware halts upon changing controller personality to JBOD mode with MCTP enabled
SCGCQ01256120 - (Closed) - 'C0:mr_wakeup: mem 45569e20, cache line ffffffff' observed while running BGI on RAID 5 Volume with media errors.
SCGCQ01258563 - (Closed) - Assertion failure in ../../raid/2108vI2o.c at line 2398 on flashing firmware
SCGCQ01282181 - (Closed) - Storcli Failed to create single PD R0 from UGood drive which has replaced a UBAD foreign drive
SCGCQ01285595 - (Closed) - Coverity reported an uninitialized variable
SCGCQ01288297 - (Closed) - Reboot the system with 240 R0 Volumes and changing the mode->JBOD is hitting Montask.
SCGCQ01288781 - (Closed) - PL Fault 0000601e observed while running multipath on/off script in JBOD mode.
SCGCQ01289147 - (Closed) - erase types and startSecureEraseNonSED is set accordingly
SCGCQ01290201 - (Closed) - Modify NVDATA boot message to rename 'NVDATA image' to 'firmware image'
SCGCQ01313607 - (Closed) - Cache data lost event seen for WT vds
SCGCQ01313950 - (Closed) - Kill adapater observed while running IO's on 240 Volumes
SCGCQ01316152 - (Closed) - Coverity: Fixing Coverity defect 16148
SCGCQ01318465 - (Closed) - Fixing the coverity raised issue
SCGCQ01319291 - (Closed) - Coverity issue 19341
SCGCQ01323607 - (Closed) - HW workaround implementation for SCGCQ00830272 and SCGCQ01048567
SCGCQ01323848 - (Closed) - auto config is not happening in some cases after issuing storcli /cx set autopdcache=r0
SCGCQ01332706 - (Closed) - MR 6.14 Beta: MonTask: line 245 in file ../../raid/1078int.c while running reboot test with background operations
SCGCQ01332947 - (Closed) - MR_6.14: 3316 PCI Trapping ISR incorrect logic for config trap address
SCGCQ01334292 - (Closed) - ntruder: Fix the 3316 Boot Block compilation and warning issue.
SCGCQ01342601 - (Closed) - Imr 3108 FW crashes while upgrading from Pkg 24.18.0-0021 to Pkg 24.21.0-0007.
SCGCQ01351483 - (Resolved) - MR_3108_WORKAROUND_PCIE_IGNORE_REPLY_PARITY_ERROR macro definition missing
SCGCQ01204592 - (Closed) - Fatal Firmware error when connecting to straight without Group ID support.
SCGCQ01221549 - (Closed) - FW does not fail unsupported erase type for a PD
SCGCQ01222318 - (Closed) - Allow Cyrpto erase on non-System PD's and non RAID PDs(ISE capable drives) and monitor the erase progress.
SCGCQ01227079 - (Closed) - Fix coverity reported issue
SCGCQ01230441 - (Closed) - FW is not updating EPDs list exposed to host after drives removal event is posted which is causing dev nodes are not getting deleted on drive removal
SCGCQ01235661 - (Closed) - Diagnostics report of iMR 3108 contains information about R6 and R60 is set to 0
SCGCQ01237252 - (Closed) - Enable MR_DCMD_PD_ERROR_STATS and the event MR_EVT_PD_ERROR_STATS only for direct attached drives
SCGCQ01252111 - (Closed) - DATA TLB ERROR, While connecting controller each Port to Back-Plane sequentially.
SCGCQ01256005 - (Closed) - MR 6.13.1Alpha:Probable Drive/cable issue Event not printed in firmwarelogs on triggering drive/cable error when connected BP
SCGCQ01280181 - (Closed) - Controller cache discarded due to memory/battery problem
SCGCQ01283507 - (Closed) - Perf-Win:Performance drop of -24% is seen in OLTP for IO size-128K, QD[1]-R6 16DC, 6G-SATA HDD
SCGCQ01299214 - (Closed) - Coverity issues 19244, 19245, 19246 and 19248
SCGCQ01299482 - (Closed) - MR 6.14 3316(Vail): 3316 Controller hangs in primary core on reboot in Dell Power Edge T620 server.
SCGCQ01300678 - (Closed) - Fix coverity issue 19253 Structurally dead code in checkCacheOffloadStatus, raid/1078init.c
SCGCQ01300689 - (Closed) - coverity defects fixed
SCGCQ01317039 - (Closed) - To fix coverity issue 17759
SCGCQ01299424 - (Closed) - FC: 0 CS: 0 offload meta signature not valid, ffffffff observed in FW logs on a system restart.
SCGCQ01285311 - (Opened) - High DB and Log write-latency issues with 3316 for R0 in MS-Jetstress benchmarking
SCGCQ01300667 - (Closed) - MR 6.14 - Fix coverity issue 19238
SCGCQ01301658 - (Closed) - Coverity issue 15356
SCGCQ01209605 - (Closed) - update the boundary values in UpdateFeatureSetValues()
SCGCQ01250342 - (Closed) - FW hang finaly leading to kill adatper with inBox driver
SCGCQ01114969 - (Closed) - MR 7.2: Add API support to make application work with Cachecade3.0 on 3516 (Public)
SCGCQ01341925 - (Implemented) - Integrate 3316 PL 14.00.04.00 with MR 6.14
SCGCQ01330898 - (Implemented) - PL integration
SCGCQ01307233 - (Implemented) - Integrate PL phase 14.00.02.00 with MR 6.14
SCGCQ01260431 - (Implemented) - PR State Machine Clean up during Patrol Read/Check Consistency Conflicts
SCGCQ01258853 - (Implemented) - Firmware:- Request to change OEM (9361-8i) to permanently disable SDS Mode and JBOD Mode
SCGCQ01255385 - (Closed) - Enable JBOD support in MR6.x for OEMID=9 ONLY for the Sebastian (9361-8i) PCI IDs.
SCGCQ01253696 - (Implemented) - Revert the DDR tuning changes for specific PCI IDs.
SCGCQ01238286 - (Closed) - Integrate 3316 PL 13.00.04.00 (SCGCQ01237533)
SCGCQ01238126 - (Closed) - Integrate PL 13.00.04.00 to MR_FW_SAS3_6.13_4G_DDR
SCGCQ01231972 - (Closed) - MR 6.12: Adding 3316 PL library Version 12.0.5.0
SCGCQ01228949 - (Closed) - Open up MR_DCMD_CFG_AUTOCFG for iMR for GET operation
SCGCQ01224232 - (Closed) - Revert the DDR tuning changes for specific PCI IDs.
SCGCQ01223351 - (Closed) - Integrating PL - SCGCQ01169053 into 6.1_Patch new It stream.
SCGCQ01222700 - (Closed) - API changes for CR55 - PCIe lane/link speed
SCGCQ01222698 - (Closed) - API change for Simplified RAID10 Creation
SCGCQ01218406 - (Closed) - API Changes Required for Specific OEM Backplane functionality
SCGCQ01215397 - (Closed) - Customer requesting digitally signed FW packages on their 3316 controller
SCGCQ01215334 - (Closed) - API changes for PR SCGCQ01139678 - Method for determining bad ONFI flash in storcli
SCGCQ01203751 - (Closed) - API changes for PR SCGCQ01127742 - Isolating faulty cable issue from bad drive issue
SCGCQ01194361 - (Closed) - Integrating PL (SCGCQ01189907) 10.00.11.00 3108 6.10
SCGCQ01188725 - (Closed) - Define CurrentFwNvmePageSize element in new MFI_REG_STATE_EXT3 register
SCGCQ01213092 - (Closed) - MR7.1. Add MR API bit to indicate the profile is NVMe Only profile
SCGCQ01304141 - (Closed) - Integrate 13.00.06.00 PL to MR 6.13
SCGCQ01273435 - (Closed) - PL Checkin for phase 13.00.05.00 - PL RO SCGCQ01273246
SCGCQ01254954 - (Closed) - Add additional sense data to firmware tracker list
SCGCQ01219862 - (Closed) - Method for determining bad ONFI flash via Storcli & SNMP trap upon NAND flash failure for 3108 and 3316
SCGCQ01137359 - (Implemented) - IN FAILED ARRAY bit is not being set when a VD is cleared
SCGCQ01215270 - (Closed) - Isolating faulty cable issue from bad drive issue
SCGCQ01268896 - (Implemented) - PL integration
SCGCQ00893669 - (Port_Complete) - Medium error correction events were not reported
SCGCQ00895474 - (Port_Complete) - 3108 6.9: FW breaks MonTask: line 245 in file ../../raid/1078int.c with IOs on max VD configured and BGOps
SCGCQ00895481 - (Port_Complete) - 3108 6.9: FW breaks MonTask: line 245 in file ../../raid/1078int.c with IOs on max VD configured and BGOps
SCGCQ00895482 - (Port_Complete) - 3108 6.9: FW breaks MonTask: line 245 in file ../../raid/1078int.c with IOs on max VD configured and BGOps
SCGCQ00946612 - (Port_Complete) - Sanity check for handling the cases where event length comes up as zero/ rPtr goes beyond iptr
SCGCQ01093890 - (Port_Complete) - Storecli not showing vd after personality switch from sds to raid
SCGCQ01149764 - (Port_Complete) - iMR: Drives with configuration is getting converted to JBOD if system already has maximum configurable drives.
SCGCQ01180873 - (Port_Complete) - Function in FW (injectParityErr) doesn't work to generate i-cache parity error
SCGCQ01186523 - (Port_Complete) - iEEESGL flag was not getting set for IO request in SES DCDB handler
SCGCQ01191484 - (Port_Complete) - MR 6.12 Solaris 11.3 X86: "MonTask: line 2357 in file ../../raid/2108vI2o.c" while running IO's on 64 VD's with OCR.
SCGCQ01198744 - (Port_Complete) - Unexpected all device insert event causes logical state change and VD deletion
SCGCQ01219839 - (Port_Complete) - L2/L3 Cache error was detected on the RAID controller during boot (24 hours after shutdown hang)
SCGCQ01219897 - (Port_Complete) - IMR_6.13: Drive is not marked as Foreign upon OCR when controller already has max configured PD's
SCGCQ01219985 - (Port_Complete) - MR6.10_FW : CRC mismatch and invalid log event found while querying for Controller properties and learn cycle in parallel.
SCGCQ01220128 - (Port_Complete) - Rebuild Error on PD (Error f0) with iMR 9341-8i (SAS3008)
SCGCQ01220159 - (Port_Complete) - FW pkg 23.22.0-0017 and later initialize drives ~50% slower
SCGCQ01229234 - (Port_Complete) - 3316_2G DDR Write Timeouts with Medusa DM discovery issue
SCGCQ01229929 - (Port_Complete) - MR7.1_NVMe: After foreign import of 64 R0 VDs, operating system unable to discover the VDs
SCGCQ01232073 - (Port_Not_Required) - In RAID personality, MR_DCMD_CFG_AUTOCFG DCMD is disabled in non-240 VD environment.
SCGCQ01232103 - (Port_Complete) - Open up MR_DCMD_CFG_AUTOCFG for iMR for GET operation
SCGCQ01235056 - (Port_Complete) - FW crashes when FW update(OFU) is done with faluty onfi
SCGCQ01237142 - (Port_Complete) - In RAID personality, MR_DCMD_CFG_AUTOCFG DCMD is disabled in non-240 VD environment.
SCGCQ01238262 - (Port_Complete) - iEEESGL flag was not getting set for IO request in SES DCDB handler
SCGCQ01238639 - (Port_Complete) - Storecli not showing vd after personality switch from sds to raid
SCGCQ01241870 - (Port_Complete) - Storcli failed to stop drives LED locating with a range
SCGCQ01242590 - (Port_Complete) - iEEESGL flag was not getting set for IO request in SES DCDB handler
SCGCQ01242592 - (Port_Complete) - iEEESGL flag was not getting set for IO request in SES DCDB handler
SCGCQ01242596 - (Port_Complete) - iEEESGL flag was not getting set for IO request in SES DCDB handler
SCGCQ01242597 - (Port_Complete) - iEEESGL flag was not getting set for IO request in SES DCDB handler
SCGCQ01242649 - (Port_Complete) - MR6.12 NVRAM Overflow - incomplete FW logs
SCGCQ01242650 - (Port_Complete) - MR6.12 NVRAM Overflow - incomplete FW logs
SCGCQ01242651 - (Port_Complete) - MR6.12 NVRAM Overflow - incomplete FW logs
SCGCQ01242766 - (Port_Complete) - MR7.1_NVMe: After foreign import of 64 R0 VDs, operating system unable to discover the VDs
SCGCQ01243833 - (Port_Complete) - Local storage admin config FSM failure on setting TR on 64 VDs
SCGCQ01243834 - (Port_Complete) - Local storage admin config FSM failure on setting TR on 64 VDs
SCGCQ01245596 - (Port_Complete) - unable to encrypt disk when using no pass-phrase on WebBIOS
SCGCQ01245782 - (Port_Complete) - Offline Marked DG (RAID0) appearing in RHEL 7 install
SCGCQ01247063 - (Port_Complete) - Cache Offload test fails with Armstrong controllers in Intel Servers.
SCGCQ01247264 - (Port_Complete) - SAS2208 card reset in DataCenter due to unknown reason
SCGCQ01255838 - (Port_Complete) - RDM in Use-RDm Error & crashed into Montask during boot (SCGCQ01147739 OEM DU issue)
SCGCQ01256109 - (Port_Complete) - MR7.0 - DC when a PD is made offline during RLM of single Dr. R0 to 4 Dr. R1 (PRL11)
SCGCQ01256178 - (Port_Complete) - Make GPIO drive strengths configurable via NVDATA.
SCGCQ01262837 - (Port_Complete) - FD33xD issues in VMWare
SCGCQ01263811 - (Port_Complete) - FD33xD issues in VMWare
SCGCQ01265413 - (Port_Complete) - OEM 32MB Image doesn't boot on PP boards
SCGCQ01266168 - (Port_Complete) - 'C0:mr_wakeup: mem 45569e20, cache line ffffffff' observed while running BGI on RAID 5 Volume with media errors.
SCGCQ01266169 - (Port_Complete) - 'C0:mr_wakeup: mem 45569e20, cache line ffffffff' observed while running BGI on RAID 5 Volume with media errors.
SCGCQ01266300 - (Port_Complete) - FD33xD issues in VMWare
SCGCQ01267801 - (Port_Complete) - In RAID personality, MR_DCMD_CFG_AUTOCFG DCMD is disabled in non-240 VD environment.
SCGCQ01267851 - (Port_Complete) - Cache data Lost when Term Log is set to "on"
SCGCQ01268059 - (Port_Complete) - Handling of DCR errors in MSS core
SCGCQ01269779 - (Port_Complete) - Auto refresh is not happening when LD is deleted during rebuild is in progress
SCGCQ01274496 - (Port_Complete) - In RAID personality, MR_DCMD_CFG_AUTOCFG DCMD is disabled in non-240 VD environment.
SCGCQ01287082 - (Port_Complete) - unable to encrypt disk when using no pass-phrase on WebBIOS
SCGCQ01291492 - (Port_Complete) - Controller cache discarded due to memory/battery problem
SCGCQ01294884 - (Port_Complete) - Cannot stop patrol read on PD with medium errors by the stop cmd
SCGCQ01297666 - (Port_Complete) - Code review: turn off the onfi when bbu is bad
SCGCQ01299260 - (Port_Complete) - Code review: turn off the onfi when bbu is bad
SCGCQ01300759 - (Port_Complete) - Perf-Win:Performance drop of -24% is seen in OLTP for IO size-128K, QD[1]-R6 16DC, 6G-SATA HDD
SCGCQ01326069 - (Port_Complete) - OS hung and iMR FW reset when do delete and create VD from previous powersave PD (Spindowned)
SCGCQ01332726 - (Port_Complete) - driver crashed after FW update via UCSM (UCSM bundle 2.2(8fS2)A/B to 3.1(2.163)A/B)
SCGCQ01351614 - (Port_Not_Required) - Controller fails to boot up when migrated from 6.13 to 6.14 FW for Specific OEM
SCGCQ00945335 - (Port_Complete) - Sanity check for handling the cases where event length comes up as zero/ rPtr goes beyond iptr
SCGCQ01219901 - (Port_Complete) - Controller became unresponsive after hitting OCM error
SCGCQ01232131 - (Port_Complete) - 3108 6.13-Beta: MonTask: line 3386 in file ../../dm/src/devmgr.c while running JBOD IO on SAS SSD with cable pull push
SCGCQ01241869 - (Port_Complete) - Invalid date for next learn cycle is set due to invalid date from OEM server (STF: Next learn time is 1970-01-28)
SCGCQ01243832 - (Port_Complete) - Local storage admin config FSM failure on setting TR on 64 VDs
SCGCQ01243836 - (Port_Complete) - Local storage admin config FSM failure on setting TR on 64 VDs
SCGCQ01248969 - (Port_Complete) - MR6.12 NVRAM Overflow - incomplete FW logs
SCGCQ01261095 - (Port_Complete) - FD33xD issues in VMWare
SCGCQ01265514 - (Port_Complete) - MR_EVT_ARGS_PD_INQ structure giving wrong PD side as part of the event
SCGCQ01273187 - (Port_Complete) - Configuration lost and system crashed on having a stale configuration connected
SCGCQ01273960 - (Port_Complete) - MR_6.13:FW flash pack -30 with reboot , result to 3316 Controller hang at bios level (Power PC)
SCGCQ01223113 - (Port_Complete) - Request not to reset the Idle Timers.
SCGCQ01235753 - (Port_Complete) - 16i - All 10T SAS HDDs can't be detected after setting spinupdrivecount=4
SCGCQ01311439 - (Port_Complete) - SAS2208 card reset in DataCenter due to unknown reason
SCGCQ01247082 - (Port_Complete) - Drive Strength values are incorrect for last 8 phys of 24i Controller
SCGCQ01282285 - (Port_Complete) - Firmware hits montask while reconstruction when drive is pulled out
SCGCQ01299219 - (Port_Complete) - Code review: turn off the onfi when bbu is bad
SCGCQ01265445 - (Port_Complete) - GetAllLDAllowedOperation call in Storelib is not returning Allowed operations when some LDs are deleted
SCGCQ01288845 - (Port_Complete) - Controller does not boot up while performing cache offload .

NVDATA:
SCGCQ01295563 - (Closed) - rectified ctrlId from 0128 to 0122
SCGCQ01273446 - (Closed) - 24i Locate LED not working for slots on port 4 and port 5
SCGCQ01341920 - (Closed) - MR _6.14 :  Drive inserted print in FW , not matching to the physically drive inserted in the Backplane.
SCGCQ01282187 - (Closed) - Oracle: Ability to set persistent FW log as default via NVData

CTRL-R
SCGCQ01317176 - (Closed) - CTRLH: Sorting the Pds and Hot Spare drives in VD management
SCGCQ01210262 - (Closed) - MR6.13_Storcli: Storcli throws wrong error message and also shows Dual error messages in detailed status
SCGCQ01300711 - (Closed) - Code changes for Big Endian servers for OS detection on the VD
SCGCQ01273421 - (Closed) - Port to Enclosure mapping is not correct in CTRL-R.
SCGCQ01283497 - (Closed) - Handle memory leaks in getSortedPdList
SCGCQ01278705 - (Closed) - Change Write Policy when create CacheCade VD in CtrlR Utility cannot show customer chose policy
SCGCQ01317174 - (Closed) - Sorting the Pds and Hot Spare drives in VD management
SCGCQ01325051 - (Closed) - CTRL-H: Online and UG drives are not sorted in the PD management screen.
SCGCQ01312072 - (Closed) - LibMods: Sort the connector names, when the names are not in Port 0 -3 format
SCGCQ01264142 - (Closed) - New fault code for routine synchronous reset
SCGCQ01114969 - (Closed) - MR 7.2: Add API support to make application work with Cachecade3.0 on 3516 (Public)
SCGCQ01222700 - (Closed) - API changes for CR55 - PCIe lane/link speed
SCGCQ01222698 - (Closed) - API change for Simplified RAID10 Creation
SCGCQ01218406 - (Closed) - API Changes Required for Specific OEM Backplane functionality
SCGCQ01215334 - (Closed) - API changes for PR SCGCQ01139678 - Method for determining bad ONFI flash in storcli
SCGCQ01203751 - (Closed) - API changes for PR SCGCQ01127742 - Isolating faulty cable issue from bad drive issue
SCGCQ01188725 - (Closed) - Define CurrentFwNvmePageSize element in new MFI_REG_STATE_EXT3 register
SCGCQ01213092 - (Closed) - MR7.1. Add MR API bit to indicate the profile is NVMe Only profile
SCGCQ01307257 - (Closed) - Disk sorting based on connector name, slot and position
SCGCQ01282293 - (Closed) - LibMods changes - Add OpenSSL v1.0.2i to StorCLI
SCGCQ01214425 - (Closed) - Windows Server 2016 Nanoserver GCA version validation for MR and IT -- MR 6.13/SAS3 Phase 13/14
SCGCQ01307232 - (Closed) - CTRL-R: Sort the disk based on connector name, position and slot
SCGCQ01242802 - (Port_Complete) - OEM chassis in Ctrl-R utility Foreign View tab shows RAID - 00 as RAID - 1
SCGCQ01245523 - (Port_Complete) - Drive Group Id in Foreign view tab is wrongly displayed
SCGCQ01232037 - (Port_Complete) - 3108 2GB MR card BIOS CTrl-H: disks list in VD Mgmt incorrect.
SCGCQ01249538 - (Port_Complete) - Libmods: SCGCQ01214152 - Storcli fails with segmentation fault (core dumped) with foreign import
SCGCQ01267606 - (Port_Complete) - (Libmods) Isolating faulty cable issue from bad drive issue for controllers (3108 and 3316)
SCGCQ01283479 - (Port_Complete) - Prepare To Transport
SCGCQ01176928 - (Port_Complete) - Updated the string from "Instant Secure Erase" to "Cryptographic Erase"
SCGCQ01300789 - (Port_Complete) - Libmods: Second OCR request not triggered, fired when first OCR request about to finish, but O/P shows success(SCGCQ01290216)
SCGCQ01290430 - (Port_Complete) - Displays reboot message, on launching CTRL-R with controller in safe mode and Secured foreign drive.
SCGCQ01283458 - (Port_Complete) - Disable security gives wrong error message when SECURE PD and Transport ready VD is present
SCGCQ01283457 - (Port_Complete) - Manage Ded. HS option should not be shown when Drive Group is Transport Ready State.
SCGCQ01268885 - (Port_Complete) - Solaris Sparc 11.3:After enabling largeiosupport from storcli, largeiosupport not enabled in CTRL Property.
SCGCQ01300707 - (Port_Complete) - storclif64 can not create prl11 across 2 enclosure using 32 pds
SCGCQ01283446 - (Port_Complete) - Rearrange Transport Ready form
SCGCQ01283450 - (Port_Complete) - "Undo Prepare for Removal" needs to be removed from TR PDs
SCGCQ01294079 - (Port_Complete) - CacheCade VD association returns error in Config Utility (Ctrl-R)
SCGCQ01283447 - (Port_Complete) - Add Hidden field and block the Hideen VD and Transport VD in Boot Device
SCGCQ01283441 - (Port_Complete) - Prepare To Transport
SCGCQ01283543 - (Port_Complete) - CSCuw42102: Ctrl-R showing blank enclosure detail
SCGCQ01356244 - (Port_Complete) - Ctrl-H hang during foreign import along with app tab toggling.
SCGCQ01279496 - (Port_Complete) - Ctrl-R showing blank enclosure detail
SCGCQ01291519 - (Port_Complete) - 3516 B0 controller cannot delete Foreign config drives.

BIOS
SCGCQ01379238 (Port Of Defect SCGCQ01292708)-FW displays the ID in BIOS during boot up more than 1000+, even total drives is only about 160PDs
SCGCQ01379365 (Port Of Defect SCGCQ01379327)-System reset is initiated twice in BIOS
SCGCQ01379284 (Port Of EnhancementRequest SCGCQ01293535) - Headline: Reset Type and customer messaging for system resets initiated by controller oprom

UEFI Driver
SCGCQ00883008 - (Closed) - Profile Mgmt API Changes
SCGCQ00886417 - (Closed) - MR_RAID_CTX_G35 has one too many bits
SCGCQ00927738 - (Closed) - Reintroduce numSGEExt Field in Raid Context for 3108 to support 1MB IO
SCGCQ00948535 - (Closed) - The code had events with repetitive ID and some structures clashing
SCGCQ01001936 - (Closed) - CtrlInfo.adapterOperations3.supportProfileChange is missing in 3516 Dev API baseline dated 2015-12-23
SCGCQ01014835 - (Closed) - CtrlInfo.adapterOperations3.supportProfileChange is missing in 3516 Dev API baseline dated 2015-12-23 has been added back again
into adapteroperations 4
SCGCQ01242633 - (Closed) - Driver health shows as Failed even after handling the boot message.
SCGCQ01289887 - (Closed) - When user unloads UEFI Driver nullify pHiiHandShakeProtocol and ask platform to free HII (memory and image handle)
SCGCQ01264142 - (Closed) - New fault code for routine synchronous reset
SCGCQ01114969 - (Closed) - MR 7.2: Add API support to make application work with Cachecade3.0 on 3516 (Public)
SCGCQ01222700 - (Closed) - API changes for CR55 - PCIe lane/link speed
SCGCQ01222698 - (Closed) - API change for Simplified RAID10 Creation
SCGCQ01218406 - (Closed) - API Changes Required for Specific OEM Backplane functionality
SCGCQ01215334 - (Closed) - API changes for PR SCGCQ01139678 - Method for determining bad ONFI flash in storcli
SCGCQ01203751 - (Closed) - API changes for PR SCGCQ01127742 - Isolating faulty cable issue from bad drive issue
SCGCQ01146597 - (Closed) - MR 6.12 - Add JBOD mode personality to MR_CTRL_PERSONALITY
SCGCQ01141251 - (Closed) - MR 7.0: Add supportPdMapTargetId flag in MR_CTRL_INFO and MFI_CAPABILITIES
SCGCQ01139344 - (Closed) - MR 6.13: Add API support for TFM/SCAP _MR_BBU_VPD_INFO_FIXED parameters
SCGCQ01137627 - (Closed) - MR 6.13: Add a new control command to fetch ROC temperature data over I2C
SCGCQ00867953 - (Closed) - profile management API
SCGCQ00875328 - (Closed) - Mega API modifications needed for RMW-FP and Cache bypass features in 3516
SCGCQ00883262 - (Closed) - Merging api_overrides mega_api files with the files in the Mega_API development stream
SCGCQ00941620 - (Closed) - 3516: de-feature AHCI
SCGCQ01023741 - (Closed) - MR_CTRL_INFO expansion from 2K to 4K
SCGCQ01059740 - (Closed) - mega api changes for ibuttonless PR
SCGCQ01075821 - (Closed) - Profile Management Changes to support requestedProfileID and optimisedProfile
SCGCQ01094549 - (Closed) - MEGA_API Changes to incorporate new IO subtype to support redirect cached IO
SCGCQ01133839 - (Closed) - MR 7.0: Add MR_RAID_FLAGS_IO_SUB_TYPE_LDIO_BW_LIMIT = 7 to mfi.h file
SCGCQ01188725 - (Closed) - Define CurrentFwNvmePageSize element in new MFI_REG_STATE_EXT3 register
SCGCQ01213092 - (Closed) - MR7.1. Add MR API bit to indicate the profile is NVMe Only profile
SCGCQ01245780 - (Port_Complete) - EFI driver test Red-screen-of-death
SCGCQ01310866 - (Port_Complete) - Return EFI_UNSUPPORTED if UEFI Driver already manages one controller.

HII
SCGCQ01242633 - (Closed) - Driver health shows as Failed even after handling the boot message.
SCGCQ01287605 - (Closed) - When user unloads UEFI Driver nullify pHiiHandShakeProtocol and ask platform to free HII (memory and image handle)
SCGCQ01325212 - (Closed) - HEFU: Don't check the return value for the function to get connector index and sorted connnector index
SCGCQ01342734 - (Closed) - Incorrect Drive Group numbering in "Create Virtual Drive" menu
SCGCQ01282322 - (Closed) - UseSetMem instaed of UnicodeSprint (L"")
SCGCQ01312071 - (Closed) - HEFU: Sort the connector names, when the names are not in Port 0 -3 format
SCGCQ01264142 - (Closed) - New fault code for routine synchronous reset
SCGCQ01114969 - (Closed) - MR 7.2: Add API support to make application work with Cachecade3.0 on 3516 (Public)
SCGCQ01234371 - (Closed) - HEFU - Sort the disk based on connector name, slot and position
SCGCQ01222700 - (Closed) - API changes for CR55 - PCIe lane/link speed
SCGCQ01222698 - (Closed) - API change for Simplified RAID10 Creation
SCGCQ01218406 - (Closed) - API Changes Required for Specific OEM Backplane functionality
SCGCQ01215334 - (Closed) - API changes for PR SCGCQ01139678 - Method for determining bad ONFI flash in storcli
SCGCQ01203751 - (Closed) - API changes for PR SCGCQ01127742 - Isolating faulty cable issue from bad drive issue
SCGCQ01188725 - (Closed) - Define CurrentFwNvmePageSize element in new MFI_REG_STATE_EXT3 register
SCGCQ01213092 - (Closed) - MR7.1. Add MR API bit to indicate the profile is NVMe Only profile
SCGCQ01145318 - (Port_Complete) - Prepare To Transport
SCGCQ01245780 - (Port_Complete) - EFI driver test Red-screen-of-death
SCGCQ01293975 - (Port_Complete) - Cannot perform RLM in HII in certain scenario
SCGCQ01282444 - (Port_Complete) - Undo Prepare for Removal" needs to be removed from TR PDs
SCGCQ01333898 - (Port_Complete) - A wrong message displayed in HII reconstruction browser while trying to trigger reconstruction again
SCGCQ01293002 - (Port_Complete) - For security key, the length must be upto 32 not 256
SCGCQ01293502 - (Port_Complete) - The 6G SSD Negotiated Link speed=12G in HII
SCGCQ01333896 - (Port_Complete) - Need to correct the spelling mistake in the help message under the drive management page in HII
SCGCQ01286463 - (Port_Complete) - MR 7.0.1 No fast/full init after creation of profile based VDs
SCGCQ01293444 - (Port_Complete) - Show "Port 4-7 & Port 0-3" for all drives in the HII Drive Management when the controller uses x8 SAS link to expander
SCGCQ01245896 - (Port_Complete) - MegaRAID option is listed in dashboard menu, with no options listed.
SCGCQ01245792 - (Port_Complete) - 9460-16i - HDD information show messy code in BIOS when HDDs connected in LSI RAID card
SCGCQ01274030 - (Port_Complete) - Fix sorting and SupportMorethan16Phys issue
SCGCQ01293971 - (Port_Complete) - Unable to reconfigure RAID 0 VD to RAID 1 in HII when sufficient unconfigured good drive exists in the system.
SCGCQ01282448 - (Port_Complete) - Disable security gives wrong error message when SECURE PD and Transport ready VD is presnet
SCGCQ01293974 - (Port_Complete) - PCI/VPD data to be populated for MR cards-short term solution to hard code the values in Hii for Purley Launch
SCGCQ01293999 - (Port_Complete) - HPE: Firmware Flash is not closed properly after the flash.	

Firmware Package:24.19.0-0047 (MR 6.13)
	Firmware 4.720.00-8218
	ROMENV 1.09
	BootBlock 3.10.01.00-0000
	NVDATA  4.2510.01-0051
	UEFI_Driver v0x06160200 (SIGNED)
	Hii v03.23.06.00 (SIGNED w/correct Size)
	FCODE 4.19.08.00
	BIOS  6.34.01.0
	CTRL-R 5.18-0403

Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ01111615 - (Closed) - Changing RAID FoD key(Add/Remove) through customer application will make original VD to foreign
SCGCQ01111966 - (Closed) - LSA displays discrepant information for empty backplanes
SCGCQ01116419 - (Closed) - With controller operating in least latency mode, FW hits montask upon running IOs
SCGCQ01117839 - (Closed) - MRFW : Exception in Core 0 while importing Foreign Config with enclosure connections swapped.
SCGCQ01126892 - (Closed) - On performing DIF R6 rebuild operation result in DIF errors
SCGCQ01130036 - (Closed) - PR fails to continue on PD after a USER paused Patrol read is resumed after OCR.
SCGCQ01136710 - (Closed) - To fix compilation issue in 6.13
SCGCQ01139294 - (Closed) - CTRL-H allowing user to enable protection
SCGCQ01144627 - (Closed) - FW hits to montask with mutipath push/pull operation
SCGCQ01150161 - (Closed) - Don't allow SESVPDAssociationTypeInMultiPathCfg to change for OEM via controller property
SCGCQ01151384 - (Closed) - Build the Flash Component List only if any of the image is flashed.
SCGCQ01152599 - (Closed) - Assertion failure in ../../dm/mpt2/mptcmd.c at line 1418 during PD offline on R5 using DIF drives.
SCGCQ01154299 - (Closed) - Dev defect: kill adapter debugging information are missing in the crash dump collection path.
SCGCQ01161841 - (Closed) - IMR FW fails to support 32 configured good drives, during JBOD to good and array removal step.
SCGCQ01162896 - (Closed) - In case of Raid 6 and medium error on the drives, if the driver state is manually changed to OFFLINE, FW hits a DMA error
SCGCQ01169202 - (Closed) - MR_6.13 : Issuing Hibernation during rebuild with IO result to Assertion failure
SCGCQ01169780 - (Closed) - After performing FW upgrade to MR 6.13 from MR 6.12, fails to enable ctrl property enable PI.
SCGCQ01177023 - (Closed) - Default behavior is not set to JBOD during personality switch from EPD to JBOD
SCGCQ01177948 - (Closed) - MR_6.13_FW: Kill Adapter on running multipath push pull
SCGCQ01180459 - (Closed) - VD with 4Kn drives, performance is slow with 6.10/6.11. Issue not seen on 6.9
SCGCQ01187677 - (Closed) - Update the macro name as appropriate
SCGCQ01191412 - (Closed) - OEM HDD LED issues
SCGCQ01192863 - (Closed) - MR 6.13 Alpha OEL 7.2:MonTask: line 538 in file ../../dm/mpt2/mptcmd.c while running multipath cable breaker script
SCGCQ01193231 - (Closed) - -6% to -15% Perf drop in all IO size with Higher QD in 12G SAS HDD [x16EC,x24EC,x40EC]
SCGCQ01196132 - (Closed) - cachecade feature is enabled through FOD key,is not entertained unless reboot/reset the controlller
SCGCQ01208120 - (Closed) - Foreign config import boundary conditions
SCGCQ01208490 - (Closed) - DDR Write Timeouts with DM discovery issue
SCGCQ01213918 - (Closed) - 3108 6.13-Beta: MonTask: line 3386 in file ../../dm/src/devmgr.c while running JBOD IO on SAS SSD with cable pull push
SCGCQ01225116 - (Closed) - MRIntru6.13RC-Win/Lin:~38% drops SW 4/8/16/32/64/128K QD(1-256) R0/R5/R6/R10 40D/24DEC/16DC 12G-SASHDD/6G-SATAHDD/12G SAS SSD
SCGCQ01226439 - (Closed) - FW crash with more than 64 VD's while performing RAID->JBOD/JBOD->RAID switch
SCGCQ01240031 - (Closed) - Cache Offload test fails with controllers in OEM Servers.
SCGCQ01253076 - (Closed) - Cache Data lost if power loss happens during descriptor preparation.
SCGCQ01260609 - (Closed) - Dev defect to address action items identified during  ONFI Review
SCGCQ01261213 - (Closed) - Dev defect to handle HW action items identified during  Onfi Review.
SCGCQ01261426 - (Closed) - Cache data Lost when Term Log is set to "on"
SCGCQ01262834 - (Closed) - 6.13 ONFI_PORT: If power loss occurs after OCR, FW might lose tty log.
SCGCQ01262883 - (Closed) - 6.13_ONFI_PORT: Program the erase and wait count values during ONFI Initialization.
SCGCQ01262884 - (Closed) - 6.13 ONFI PORT :Set bit 0 in global Interrupt Register so that host will receive an interrupt.
SCGCQ01267220 - (Closed) - Flash File System Reads fail after system reset.
SCGCQ01267700 - (Closed) - FW does not remember user induced bad blocks across boots.
SCGCQ01268066 - (Closed) - MR 6.13: Performance: Drops up to 30% seen across many profiles for Sequential writes for 24 SAS HDD R0
SCGCQ01273216 - (Closed) - MR_6.13:FW flash pack -30 with reboot , result to Controller hang at bios level (Power PC)
SCGCQ01274494 - (Closed) - Cache Restore fails if supercap is removed while cache offload is in Progress.
SCGCQ01278512 - (Closed) - Unable to set termlog on/off from storcli intermittently
SCGCQ01282319 - (Closed) - After Termlog Toggling with power cycle, result to ERROR: Dirty disk cache data has been lost
SCGCQ01283719 - (Closed) - Modify Read Eye Training Algorithm to make it spec compliant.
SCGCQ01128576 - (Closed) - 6.13_SDS: Handling the SYNC_CACHE command for WB EPDs
SCGCQ01132432 - (Closed) - Security is disabled on a OEM controller after a FOD key is added or removed until next reboot.
SCGCQ01135815 - (Closed) - FW fails to import DIF arrays, after changing enable PI controller property 0 -> 1
SCGCQ01149312 - (Closed) - Dev defect: number of messages in the VDM queue is not initialized with proper values
SCGCQ01155893 - (Closed) - Dev defect: To check-in specific params page update changes.
SCGCQ01163849 - (Closed) - IMR_6.13: Drive is not marked as Foreign upon OCR when controller already has max configured PD's
SCGCQ01167814 - (Closed) - For hidden VDs incorrect VD access Policy shown in the LSA
SCGCQ01201595 - (Closed) - FW crashes during SSC VD import on a system having certain VDs
SCGCQ01204801 - (Closed) - Fix the coverity issue
SCGCQ01204802 - (Closed) - Fix coverity defects
SCGCQ01208167 - (Closed) - Windows MR6.13 Alpha-eSDS 3108:-7 to -13% Perf Drops SR IO Sizes-4K,8K,16K QD(8) SATA SSD x8,x16,x24 PD,EPD (Coalescing)
SCGCQ01208304 - (Closed) - Read timeouts observed during Cache Restore on 4gig boards.
SCGCQ01263110 - (Closed) - Handling of DCR errors in MSS core
SCGCQ01278480 - (Closed) - Controller does not boot up while performing cache offload .
SCGCQ01117827 - (Closed) - MRFW : OCR disabled while fw downgrade from 6.12 to 6.4
SCGCQ01137690 - (Closed) - Controller exports 1 MB as IO size irrespective of its type/mode.
SCGCQ01172369 - (Closed) - FW is observing Kill Adapter while CCVD disassociate in progress
SCGCQ01188556 - (Closed) - Coverity defects CID 15746, 18327 and 18574
SCGCQ01191216 - (Closed) - FW crashes when LDs were deleted during rebuild operation.
SCGCQ01199711 - (Closed) - FW crashes upon firing storcli show all command
SCGCQ01204471 - (Closed) - Termlog is not persistent across boots when tty hist is ON.
SCGCQ01208906 - (Closed) - Aborted Erase is resumed after OCR in SDS & RAID mode .
SCGCQ01297565 - (Closed) - Code review: turn off the onfi when bbu is bad
SCGCQ01156908 - (Closed) - PD not displayed by StorCLI, does not allow to change state of the PD as well.
SCGCQ01163865 - (Closed) - MR FW returning invalid return code while setting link speed.
SCGCQ01180987 - (Closed) - MR 6.13 PA3:DATA TLB Error MonTask: line 245 in file ../../raid/1078int.c after disabling multipath bit and OCR
SCGCQ01187690 - (Closed) - Coverity tool issue: Code indention and Unintentional integer overflow issues
SCGCQ01117190 - (Closed) - Kill Adapter on running multipath push pull
SCGCQ01170701 - (Closed) - Configuration lost and system crashed on having a stale configuration connected
SCGCQ01188437 - (Closed) - Fix for coverity defects CD: 17745 and CD: 18227
SCGCQ01190895 - (Closed) - RDM in Use-RDm Error & crashed into Montask during boot 
SCGCQ01185882 - (Closed) - Coverity Issues
SCGCQ01185858 - (Closed) - Coverity : Array Out-of-bounds access error reported
SCGCQ01190905 - (Closed) - Win/Lin Upto ~30% drops are observed SW for 4k/8K/16k/32K/64K/128K QD(1-256) for R0/R5/R10 for 12G SAS HDD.
SCGCQ01196090 - (Closed) - Copy-Back resumes from Zero after foreign import with reboot.
SCGCQ01262698 - (Closed) - Shift IOPATH code by 4 cache lines to workaround performance issue.
SCGCQ01226974 - (Implemented) - Check in PL version 13.00.03.00
SCGCQ01216305 - (Implemented) - MR6.13: Disable SDS personality mode
SCGCQ01187730 - (Closed) - Integrating PL(SCGCQ01183279) 13.00.01.00 in 6.13
SCGCQ01170212 - (Closed) - Autoconfig feature support for 64 VD mode.
SCGCQ01156969 - (Closed) - Firmware does not turn fault LED for drives with size < 512MB
SCGCQ01155304 - (Closed) - The security key lifecycle management for EKMS
SCGCQ01150052 - (Closed) - Change DDR Tuning Settings in Response to ECC errors
SCGCQ01141427 - (Closed) - Enable SDS personality mode
SCGCQ01139341 - (Closed) - WG: Instance Validation issues pertaining to Energy pack (GET).
SCGCQ01134167 - (Closed) - Need MCTP over PCIe enabled for 3108 design - unblock current MCTP/PCIe level
SCGCQ01134165 - (Closed) - Adding the function that changing flag of full initialize completion
SCGCQ01085797 - (Implemented) - User can save the FoD key to TMM through the MSM pop-up advanced software options.
SCGCQ01265401 - (Closed) - Integrate PL 13.00.05.00 (RO SCGCQ01263844)
SCGCQ01188995 - (Implemented) - Make GPIO drive strengths configurable via NVDATA.
SCGCQ01156825 - (Closed) - Integrating PL(SCGCQ01140801) 13.00.00.00 to 6.13
SCGCQ01082117 - (Closed) - Change DDR Tuning Settings in Response to ECC errors
SCGCQ01213219 - (Closed) - Integrating PL SCGCQ01210438 (13.00.02.00) into 6.13 .
SCGCQ01210265 - (Closed) - Integrating PL (SCGCQ01208895) to 6.13 3108
SCGCQ01199671 - (Closed) - MegaRAID 3108 ROMB with 2GB DDR3 for cachevault single write mode (FW Change)
SCGCQ01156111 - (Closed) - Integrating PL(SCGCQ01140806) 13.00.00.00 to MR 6.13
SCGCQ01129378 - (Closed) - SCSI SANITIZE/Crypto on JBOD Drives under MR
SCGCQ01181178 - (Implemented) - Investigate on unalligned IO's for 512E drives with background operation
SCGCQ00829979 - (Port_Complete) - FW upgrade from non 240VD FW to 240VD FW when OS is behind the controller results in BSOD
SCGCQ00829980 - (Port_Complete) - FW upgrade from non 240VD FW to 240VD FW when OS is behind the controller results in BSOD
SCGCQ00988970 - (Port_Complete) - PDs are getting swapped and starts rebuild on wrong VD after the enclosure power cycle
SCGCQ01033483 - (Port_Complete) - Exception handler table is always addressed to primary FW region in iMR controller.
SCGCQ01082876 - (Port_Complete) - Upgraded to MR5.14, still see "I2C 4 PID 10 SCL STUCK Low! while I2C Rx receiving data intStatus 00008000" in fw log.
SCGCQ01130999 - (Port_Complete) - I/O failures observed on 4kn VD with data Protection Enabled
SCGCQ01131001 - (Port_Complete) - I/O failures observed on 4kn VD with data Protection Enabled
SCGCQ01132984 - (Port_Complete) - Improve performance of of Cachecade associated SVDs for 512K 100% RW FIO Workload
SCGCQ01133565 - (Port_Complete) - FDE Error messages were seen due to incorrect handling of sense data
SCGCQ01134074 - (Port_Complete) - Request for FW to disable all PI, and not allow to be re-enabled
SCGCQ01136062 - (Port_Complete) - Data Miscompare found during recovery of CacheCade pinned windows across OCR/Reboot or discard of CacheCade pinned windows while CacheCade degrade flush in progress
SCGCQ01136063 - (Port_Complete) - Data Miscompare found during recovery of CacheCade pinned windows across OCR/Reboot or discard of CacheCade pinned windows while CacheCade degrade flush in progress
SCGCQ01139844 - (Port_Complete) - FW crashes when setting fwtermlog bbu=on to a card with bad NAND flash
SCGCQ01140902 - (Port_Complete) - Security is disabled on a MR Flatwoods controller after a FOD key is added or removed until next reboot.
SCGCQ01141456 - (Port_Complete) - CTRL-H allowing user to enable protection .
SCGCQ01145325 - (Port_Complete) - Need MCTP over PCIe enabled for 3108 design - unblock current MCTP/PCIe level
SCGCQ01146497 - (Port_Complete) - EPD's are not created when pd erase is in progresss on one/more of the drive s after system reboot
SCGCQ01149762 - (Port_Complete) - iMR: Drives with configuration is getting converted to JBOD if system already has maximum configurable drives.
SCGCQ01149763 - (Port_Complete) - iMR: Drives with configuration is getting converted to JBOD if system already has maximum configurable drives.
SCGCQ01150028 - (Port_Complete) - Dev defect: number of messages in the VDM queue is not initialized with proper values
SCGCQ01150067 - (Port_Complete) - FW:Add capability to expose each SAS Expander-attached SEP as a separate Enclosure PD
SCGCQ01150173 - (Port_Complete) - Request for NVdata change on 9361-8i to make the minimum stripe size 16K (instead of 64K)
SCGCQ01152709 - (Port_Complete) - FW crashes when setting fwtermlog bbu=on to a card with bad NAND flash
SCGCQ01155380 - (Port_Complete) - SCSI SANITIZE/Crypto on JBOD Drives under MR
SCGCQ01155454 - (Port_Complete) - L2/L3 Cache error was detected on the RAID controller during boot (24 hours after shutdown hang)
SCGCQ01158838 - (Port_Complete) - iEEESGL flag was not getting set for IO request in SES DCDB handler
SCGCQ01163258 - (Port_Complete) - LUID gets changed during foreing import from non-240VD FW to 240VD FW
SCGCQ01174094 - (Port_Complete) - Fake the progress response to application until background operation resumes
SCGCQ01174409 - (Port_Complete) - Enhance code to catch Stack Overflow problem as soon as it occurs.
SCGCQ01175616 - (Active) - New Erase Type CRYPTO ERASE is supported for ISE capable drives via DCMDs.
SCGCQ01180170 - (Port_Complete) - Controller exports 1 MB as IO size irrespective of its type/mode.
SCGCQ01180872 - (Port_Complete) - Function in FW (injectParityErr) doesn't work to generate i-cache parity error
SCGCQ01184957 - (Port_Complete) - xIOV_Step2.5 : BladeErrorIsrTask while running IO's.
SCGCQ01201996 - (Port_Complete) - MR7.0 - DC when a PD is made offline during RLM of single Dr. R0 to 4 Dr. R1 (PRL11)
SCGCQ01202625 - (Port_Complete) - Assertion failure in ../../raid/cache.c at line 2495: during RHEL 7.1 OS boot after VDs are created
SCGCQ01205307 - (Port_Complete) - Rebuild does not start when "useunconfiggoodforemergency" feature is enabled and one "prepare for removal" drive is undone.
SCGCQ01205341 - (Port_Complete) - Memory size and CacheVault Flash size show wierd values
SCGCQ01205429 - (Port_Complete) - iEEESGL flag was not getting set for IO request in SES DCDB handler
SCGCQ01206978 - (Port_Complete) - FW trying ld sync for target ID beyond 63 when non-240 driver is installed
SCGCQ01232058 - (Port_Complete) - FW does not fail unsupported erase type for a PD
SCGCQ01235529 - (Port_Complete) - Update the MAXTransferLength properly for Driver enabled 1MB support feature
SCGCQ01259337 - (Port_Complete) - ONFI: To properly handle the OCR case with RESET Status Register.
SCGCQ01260470 - (Port_Complete) - COL disarmed, VDs remain in WB mode, no Administrative Messages to bad flash part.
SCGCQ01260995 - (Port_Complete) - Infinite loop in onfiSyncModeEnter
SCGCQ01261425 - (Port_Complete) - FW crashes when setting fwtermlog bbu=on to a card with bad NAND flash
SCGCQ01263212 - (Port_Complete) - Insertion of the boot messages and the evets for montoring the ONFI backup capacity.
SCGCQ01263800 - (Port_Complete) - 'C0:mr_wakeup: mem 45569e20, cache line ffffffff' observed while running BGI on RAID 5 Volume with media errors.
SCGCQ01263859 - (Port_Complete) - Handling of DCR errors in MSS core
SCGCQ01264476 - (Port_Complete) - Invalid date for next learn cycle is set due to invalid date from OEM server (STF: Next learn time is 1970-01-28)
SCGCQ01288848 - (Port_Complete) - Controller cache discarded due to memory/battery problem
SCGCQ01063833 - (Port_Complete) - DC Reboot Caused an LTO Drive Attached to Controller to Load a Tape.
SCGCQ01131000 - (Port_Complete) - I/O failures observed on 4kn VD with data Protection Enabled
SCGCQ01131002 - (Port_Complete) - I/O failures observed on 4kn VD with data Protection Enabled
SCGCQ01149114 - (Port_Complete) - Kill-adapter during rebuild, recon, and drive pull
SCGCQ01170646 - (Port_Complete) - Local storage admin config FSM failure on setting TR on 64 VDs
SCGCQ01180171 - (Active) - Controller exports 1 MB as IO size irrespective of its type/mode.
SCGCQ01180864 - (Port_Complete) - For SES enclosures, now we call a wrapper function to get the correct slot number before setting the bad slot bitmap.
SCGCQ01184451 - (Port_Complete) - Copyback not automatically initiating when manually setting drives to Unconfigured_Good
SCGCQ01202208 - (Port_Complete) - IMR_6.13: Drive is not marked as Foreign upon OCR when controller already has max configured PD's
SCGCQ01205397 - (Port_Complete) - Configuration lost and system crashed on having a stale configuration connected
SCGCQ01255374 - (Port_Complete) - Activity LED is always ON even when no drives are present.
SCGCQ01263759 - (Port_Complete) - issues in VMWare
SCGCQ01289123 - (Port_Complete) - RAID10 VD goes to failed state after performing RLM
SCGCQ01163768 - (Port_Complete) - LUID gets changed during foreing import from non-240VD FW to 240VD FW
SCGCQ01297497 - (Port_Complete) - Performance drop of -24% is seen in OLTP for IO size-128K, QD[1]-R6 16DC, 6G-SATA HDD
SCGCQ01131003 - (Port_Complete) - I/O failures observed on 4kn VD with data Protection Enabled
SCGCQ01141508 - (Port_Complete) - xIOV:PL Fault 0000d073/0000d101 for shutting down the host during IO in SDS,1660 in file ../../dm/pl2/pliopi.c
SCGCQ01176519 - (Port_Complete) - xIOV:PL Fault 0000d073 for running IO on shared EPDs across hots with Heavy load.
SCGCQ01203802 - (Port_Complete) - MR7.0 - DC when a PD is made offline during RLM of single Dr. R0 to 4 Dr. R1 (PRL11)
SCGCQ01014121 - (Port_Complete) - B22 M3 LSI Controller in configuration lost state
SCGCQ01158573 - (Port_Complete) - Request not to reset the Idle Timers.
SCGCQ01168218 - (Port_Complete) - Raid controller stuck in montask after multiple hard reboots - (SCGCQ01118632

NVDATA:
SCGCQ01255383 - (Closed) - Activity LED is always ON even when no drives are present.
SCGCQ01241685 - (Closed) - Drive Strength values are incorrect for last 8 ports in some boards.
SCGCQ01185624 - (Resolved) - MR_6.13 : Product name for the board should display as 9361-24i instead of 9361-16i
SCGCQ01227599 - (Closed) - Activity LED is always ON even when no drives are present.
SCGCQ01241479 - (Closed) - MR 6.x: Enable LDBBM by default for Channel Controllers.
SCGCQ01245534 - (Closed) - MR9361-16i physical wide port numeration differs from labels and documentation
SCGCQ01271659 - (Closed) - enabled LARGEIOSUPPORT for OEM nvdata
SCGCQ01204501 - (Closed) - Change default drive strength values.
SCGCQ01273348 - (Closed) - 9361-24i NVDATA changes
SCGCQ01294598 - (Closed) - ctrl Id has been added to xml files
SCGCQ01255546 - (Closed) - Correct the Man page 6 and Man Page 43 settings for channel controller.
SCGCQ01268892 - (Closed) - OEM NVDATA xml modification
SCGCQ01269720 - (Closed) - Disable JBOD personality(mode) for OEM
SCGCQ01186255 - (Closed) - Change ManPage12 flags to let PL control LED as needed by PL.
SCGCQ01245611 - (Port_Complete) - MR9361-16i physical wide port numeration differs from labels and documentation

UEFI Driver:
SCGCQ01134128 - (Closed) - The security key lifecycle management for EKMS
SCGCQ01191839 - (Port_Complete) - RSOD encountered on reboot system
SCGCQ01205305 - (Port_Complete) - EFI driver test Red-screen-of-death

HII:
SCGCQ01193228 - (Closed) - HII provides an option Full initialization for R60 DIF array during array creation
SCGCQ01164506 - (Closed) - Title for select drive form is shown as HF030 when creating vd in raid mode
SCGCQ01143300 - (Closed) - Fix HII issues related to EKMA
SCGCQ00883008 - (Closed) - Profile Mgmt API Changes
SCGCQ00886417 - (Closed) - MR_RAID_CTX_G35 has one too many bits
SCGCQ00927738 - (Closed) - Reintroduce numSGEExt Field in Raid Context to support 1MB IO
SCGCQ00948535 - (Closed) - The code had events with repetitive ID and some structures clashing
SCGCQ01001936 - (Closed) - CtrlInfo.adapterOperations3.supportProfileChange is missing in Dev API baseline dated 2015-12-23
SCGCQ01014835 - (Closed) - CtrlInfo.adapterOperations3.supportProfileChange is missing in Dev API baseline dated 2015-12-23 has been added back again
into adapteroperations 4
SCGCQ01196215 - (Closed) - ASSERT text seen on screen when entering system menu
SCGCQ01138815 - (Closed) - HII- Add warning message before we change the behavior mode and it's parameters
SCGCQ01164510 - (Closed) - Form title for convert JBOD s to UG when creating a vd is shown as HF041 on the confirmation page .
SCGCQ01122925 - (Closed) - Error Displayed which HII Dashboard form is launched
SCGCQ01214389 - (Closed) - "Check all" does not select drives during creation of VD
SCGCQ01195985 - (Closed) - Create SSC VD option displayed when max VDs are configured
SCGCQ01156878 - (Closed) - Switching Personality is not showing in HII
SCGCQ01145633 - (Closed) - HII exits when attempted preview foreign configuration while the drives are pulled out
SCGCQ01176614 - (Closed) - UCM 2.0 is not fully supported
SCGCQ01167163 - (Closed) - HII:handle coverity defects
SCGCQ01208732 - (Closed) - Junk value seen in JBOD to UG conversion form
SCGCQ01146597 - (Closed) - MR 6.12 - Add JBOD mode personality to MR_CTRL_PERSONALITY
SCGCQ01141251 - (Closed) - MR 7.0: Add supportPdMapTargetId flag in MR_CTRL_INFO and MFI_CAPABILITIES
SCGCQ01139344 - (Closed) - MR 6.13: Add API support for TFM/SCAP _MR_BBU_VPD_INFO_FIXED parameters
SCGCQ01137627 - (Closed) - MR 6.13: Add a new control command to fetch ROC temperature data over I2C
SCGCQ00867953 - (Closed) - profile management API
SCGCQ00875328 - (Closed) - Mega API modifications needed for RMW-FP and Cache bypass features
SCGCQ00883262 - (Closed) - Merging api_overrides mega_api files with the files in the Mega_API development stream
SCGCQ00941620 - (Closed) - de-feature AHCI
SCGCQ01023741 - (Closed) - MR_CTRL_INFO expansion from 2K to 4K
SCGCQ01059740 - (Closed) - mega api changes for ibuttonless PR
SCGCQ01075821 - (Closed) - Profile Management Changes to support requestedProfileID and optimisedProfile
SCGCQ01094549 - (Closed) - MEGA_API Changes to incorporate new IO subtype to support redirect cached IO
SCGCQ01133839 - (Closed) - MR 7.0: Add MR_RAID_FLAGS_IO_SUB_TYPE_LDIO_BW_LIMIT = 7 to mfi.h file
SCGCQ01144381 - (Implemented) - HII to support UCM 2.0 for (9361-8i) based controllers
SCGCQ01134128 - (Closed) - The security key lifecycle management for EKMS
SCGCQ01145284 - (Closed) - HII: Rename HBA mode to JBOD mode
SCGCQ01140914 - (Port_Complete) - "Autoconfigure Raid 0" option is available in HII even in absence of ready HDDs
SCGCQ01140915 - (Port_Complete) - PRL-11 VD expansion fails
SCGCQ01166472 - (Port_Complete) - Form title for convert JBOD s to UG when creating a vd is shown as HF041 on the confirmation page .
SCGCQ01204956 - (Port_Not_Required) - Import Foreign Config menu option is shown in HII when in HBA mode
SCGCQ01204962 - (Port_Complete) - Battery Temperature is listed as High in Battery Management menu in HII when temp is 29C/84F.
SCGCQ01140917 - (Port_Complete) - HII Profile VD performs a BGI after created, but displays a Default Initialization of Full or Fast at time of creation
SCGCQ01204964 - (Port_Complete) - HII - Unable to change task rates with "+/-"
SCGCQ01205277 - (Port_Not_Required) - HII - "Check All" does NOT select all drives when creating VD
SCGCQ01169018 - (Port_Complete) - With large VDs creating from Free Space will fail on first attempt
SCGCQ01205298 - (Port_Complete) - 9460-16i - Unable to migrate RAID6 to RAID5
SCGCQ01206747 - (Port_Complete) - OEM controller giving a Question Value Mismatch trying to add another VD using free space from a degraded VD.
SCGCQ01191839 - (Port_Complete) - RSOD encountered on reboot system
SCGCQ01205299 - (Port_Complete) - HII requires for user to enter security key three times to disable/enable pass pharse at the boot time.
SCGCQ01140910 - (Port_Complete) - Incorrect drop down menu of VDs while initiating RLM for the second time in HII.
SCGCQ01140911 - (Port_Complete) - With no ready disk, no. of Eligible NonRaid pds to convert to ready state shows zero
SCGCQ01180959 - (Port_Complete) - Dont allow user to set 4K JBOD as a boot device from PD management
SCGCQ01205305 - (Port_Complete) - EFI driver test Red-screen-of-death
SCGCQ01146029 - (Port_Complete) - HII: Rename HBA mode to JBOD mode
SCGCQ01166525 - (Port_Complete) - Title for select drive form is shown as HF030 when creating vd in raid mode
SCGCQ01167058 - (Port_Complete) - VD creation fails with available free capacity in single disk group
SCGCQ01204953 - (Port_Complete) - HII exits when attempted preview foreign configuration while the drives are pulled out

BIOS:
SCGCQ01200478 - (Port_Complete) - Check hostMemRequired bit at appropriate place in INT15Trapper()

CTRL-R:
SCGCQ01185730 - (Closed) - With controller in JBOD mode try to create VDs R1 and R0 from CTRL_H the FW breaks with Data TLB error.
SCGCQ01033486 - (Closed) - Adpinfo doesn't show detail Pending Flash FW info via storcli
SCGCQ01210262 - (Closed) - Storcli throws wrong error message and also shows Dual error messages in detailed status
SCGCQ01281203 - (Closed) - Displays reboot message, on launching CTRL-R with controller in safe mode and Secured foreign drive.
SCGCQ01064480 - (Closed) - MFI Frame alignment
SCGCQ01155309 - (Closed) - Storcli SegFault -HUU update utility doesn't detect SBMezz if Foreign Config PD exist
SCGCQ01184721 - (Resolved) - StorcliO Cavium CentOS : Displays Errorcode 255 for controller information (c0 show)
SCGCQ01185690 - (Closed) - Removed Missing return values in Libmods
SCGCQ01193194 - (Closed) - storcli crashes while trying to load configuration
SCGCQ01196471 - (Closed) - Regardless of Drive availability, Ctrl-R Create vd gave an option to create array.
SCGCQ01185184 - (Closed) - Removing the logically dead code from CLI.
SCGCQ01185673 - (Closed) - Removing the logically dead code from Libmods
SCGCQ01136658 - (Closed) - CTRL-H: Add new checkbox [Use existing security Key ] in Change security key
SCGCQ01093152 - (Closed) - Correcting error messages for transport errors.
SCGCQ01109142 - (Closed) - SWR_1.50 RHEL 6.8: Storcli /c0 show all is not displaying OS driver version.
SCGCQ01112673 - (Closed) - Storcli needs to be fixed for maximum TR info in ctrl show all
SCGCQ01138814 - (Closed) - CTRL-H- Add warning message before we change the behavior mode and it's parameters
SCGCQ01264552 - (Closed) - CacheCade VD association returns error in Config Utility (Ctrl-R)
SCGCQ00942269 - (Closed) - eSDS Alpha : LibMod Ctrl-R is allowing to enable and disable JBOD on the controller in SDS Mode
SCGCQ01146002 - (Closed) - Ctrl-H: Overlap of config parameters in JBOD behavior mode
SCGCQ01079824 - (Closed) - eSDS_1.1_HSW_Beta: Storcli after Saving and Restoring configuration using file doesn't list EPD and JBOD in PDlist type
SCGCQ01139839 - (Closed) - Ctrl-R doesnt prompt for hot spare drive selection while creating Vd
SCGCQ01194348 - (Closed) - Create Virtual Drive" enabled after reaching max config
SCGCQ01136661 - (Closed) - CTRLH- Add error Handling for prepare for removal and undo prepare for removal
SCGCQ01185187 - (Closed) - CTRL-H:handle coverity defects
SCGCQ01264142 - (Closed) - New fault code for routine synchronous reset
SCGCQ01222700 - (Closed) - API changes for CR55 - PCIe lane/link speed
SCGCQ01222698 - (Closed) - API change for Simplified RAID10 Creation
SCGCQ01218406 - (Closed) - API Changes Required for Specific OEM Backplane functionality
SCGCQ01203751 - (Closed) - API changes for PR SCGCQ01127742 - Isolating faulty cable issue from bad drive issue
SCGCQ01141462 - (Closed) - LibMods : Adding the function that changing flag of full initialize completion
SCGCQ01188725 - (Closed) - Define CurrentFwNvmePageSize element in new MFI_REG_STATE_EXT3 register
SCGCQ01213092 - (Closed) - MR7.1. Add MR API bit to indicate the profile is NVMe Only profile
SCGCQ01114969 - (Closed) - MR 7.2: Add API support to make application work with Cachecade3.0 (Public)
SCGCQ01215334 - (Closed) - API changes for PR SCGCQ01139678 - Method for determining bad ONFI flash in storcli
SCGCQ01112370 - (Implemented) - Contains Libmods changes for FRU implementation (CLI ER: SCGCQ01097099 )
SCGCQ00907898 - (Implemented) - LibMod:Add ISA and MR Personality Mode Support
SCGCQ00950485 - (Closed) - Do not allow VD creation on Removal Ready PD
SCGCQ01214425 - (Closed) - Windows Server 2016 Nanoserver GCA version validation for MR and IT -- MR 6.13/SAS3 Phase 13/14
SCGCQ01134132 - (Implemented) - Add support for new version OpenSSL1.02g to support "DROWN" - CVE-2016-0800
SCGCQ00879989 - (Implemented) - LibMod Changes: Add ISA and MR Personality Mode Support
SCGCQ01145285 - (Implemented) - Ctrl-H - LibMods: Rename HBA mode to JBOD mode
SCGCQ01245523 - (Port_Complete) - Drive Group Id in Foreign view tab is wrongly displayed
SCGCQ01242802 - (Port_Complete) - Double Decker chassis in Ctrl-R utility Foreign View tab shows RAID - 00 as RAID - 1
SCGCQ01030217 - (Port_Complete) - storcli64 Emulated Physical Drive section shows incorrect capacity for 2TB 4k HDDs
SCGCQ01232037 - (Port_Complete) - 3108 2GB MR card BIOS CTrl-H: disks list in VD Mgmt incorrect.
SCGCQ01139832 - (Port_Complete) - SED-Ctrl-R-Security/Confirm Key is being displayed in plain text format
SCGCQ00995143 - (Port_Complete) - Connector name is not in sorted state when queried from storcli .
SCGCQ01046049 - (Port_Complete) - -Memory coruption message with SWR, with "eall show" command
SCGCQ01176928 - (Port_Complete) - Updated the string from "Instant Secure Erase" to "Cryptographic Erase"
SCGCQ00928044 - (Port_Complete) - Inconsistency in showing controller status between MSM and StorCLI for Fake Flash errors
SCGCQ00928097 - (Port_Complete) - LibMod: Display connector and Enclosure information for backplane drives
SCGCQ01141291 - (Port_Complete) - Ctrl-R doesnt prompt for hot spare drive selection while creating Vd
SCGCQ01289083 - (Port_Complete) - CSCuw42102: Ctrl-R showing blank enclosure detail
SCGCQ01279497 - (Port_Complete) - Ctrl-R showing blank enclosure detail
SCGCQ01146026 - (Port_Complete) - Ctrl-H: Overlap of config parameters in JBOD behavior mode
SCGCQ00928099 - (Port_Complete) - Checking-in Libmod changes for defect-SCGCQ00914834
SCGCQ01123359 - (Port_Complete) - EPMR10: CLI Checkin for PPC Little Endian Compilation.
SCGCQ01144779 - (Port_Complete) - Libmod changes: Adding CLI command to display/toggle new controller property.(SCGCQ01106982)
SCGCQ01276430 - (Port_Complete) - Port to Enclosure mapping is not correct in CTRL-R.
SCGCQ01146785 - (Port_Complete) - Added the code to display the JBOD personality and switch between the JBOD and RAID personalities
SCGCQ00928098 - (Port_Complete) - LibMods: Add support to enable/Disable of Large IO Support - 1 MB IO
SCGCQ00939845 - (Port_Complete) - Buffer is not incremented when reading sector of the drive
SCGCQ00942788 - (Port_Complete) - eSDS Alpha : LibMod Ctrl-R is allowing to enable and disable JBOD on the controller in SDS Mode
SCGCQ01146028 - (Port_Complete) - Ctrl-H - LibMods: Rename HBA mode to JBOD mode
SCGCQ01146783 - (Port_Complete) - FW crashes when setting fwtermlog bbu=on to a card with bad NAND flash
SCGCQ00928090 - (Port_Complete) - Missing WB Option
SCGCQ01201335 - (Port_Complete) - sparc version storcli tool can not execute storcli /cx show for card



Firmware Package:24.17.0-0084 (MR 6.12)
	Firmware 4.660.01.8103
	ROMENV 1.09
	BootBlock 3.07.00.00-0003
	NVDATA  3.1605.00-0009
	UEFI_Driver 0x06150500(signed)
	Hii 03.21.14.00(signed)
	FCODE 4.17.08.00
	BIOS 6.32.02.0
	Ctrl-R v5.17-1300
	PCLI 1.07.05
	
Bug Fixes and Enhancements:
	Firmware:
		Defects (1)
		SCGCQ01159064	Firmware uses bad blocks for Cache Offload
	BIOS:
		Enhancements(1)
		SCGCQ01048324	Handle passthrough and JBOD functionality for SDS Mode for iMR and MR with 3108, 3316, and 3008 solutions


*Third-party trademarks are the property of their respective owners.


