Component:
=========
SAS MegaRAID Firmware Release Notes for MegaRAID Controllers
Release date: 05/04/18


Version Numbers:	
===============
Current Package Details:
Firmware Package: 50.5.2-1326 (MR 7.5p2)
Firmware 5.050.00-1367
ROMENV 1.12
BootBlock 7.02.00.00-0017
NVDATA  5.0500.04-0004
UEFI_Driver  v0x07050400 (SIGNED)
Hii v07.05.06.00 (SIGNED)
FCODE 4.17.08.00
BIOS 7.05.02.0
SBR: 5.0500.01-0334

Previous Package Details:
Firmware Package: 50.2.1-0589 (MR 7.2)
Firmware  5.020.00-0838
ROMENV 1.12
BootBlock 7.02.00.00-0015
NVDATA  7.02.00.00-0016
UEFI_Driver  0x07020400 (Signed)
Hii 07.02.05.00 (SIGNED)
FCODE 4.17.08.00
BIOS 07.02.03.0
SBR: 268


Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ01566087 - JBOD devices were dropped after unloading driver and reloading driver in linux
SCGCQ01571588 - backend PCIe: 4311 fault (part 3)
SCGCQ01577475 - 9440-8i card: drop out UG drive, error LED always ON. Error LED turns off only upon reinsertion of the drive.
SCGCQ01583517 - sysDMA attempted on core1 cause FW crash
SCGCQ01605610 - Task Management due to SATA init failure results in resource error message
SCGCQ01575182 - BIOS Handshake breaks Manufacturing Environment, need change in TTY and/or add timeout in FW for BIOS Handshake
SCGCQ01614688 - 7.5 R1 performance change request.
SCGCQ01574924 - pl: backend PCIe: 4311 fault (part 3)
SCGCQ01581911 - Fixing the issues during bringup of the universal backplane.
SCGCQ01582240 - To fix issues for back plane configuration validation and LED control for the UBM backplane.
SCGCQ01582246 - To fix the LED issue, VPP data and moving to change detect poll state
SCGCQ01582497 - Event with enclose 0x00 slot 0 during the system boot when a command is timed out (Command timeout on PD 12(e0x00/s0))
SCGCQ01582503 - STP Passthru commands end up with blank FiS response buffer
SCGCQ01582535 - 9460-8i is reporting Chip Temperature of 255 when the ambient temp is about 0 C
SCGCQ01598554 - Slot status LED updates to certain slots on NVMe backplane may fail
SCGCQ01599743 - Restrict FW update based on NVMe external clock oscillator support of current SBR and inbound SBR image
SCGCQ01602617 - Add logging messages in addition to changes for SCGCQ01520443
SCGCQ01615762 - Enclosures is not exposed to Host even if exposeEnclosureToHost is set.
SCGCQ01582244 - To fix the phy to slot mapping issue for the UBM backplane
SCGCQ01582532 - CC doesn't start on special built OEM firmware
SCGCQ01593192 - (SATA Only) SCSI Unmap command to some SATA drives are timing out.
SCGCQ01540362 - Linux driver incorrect issuing MR_DCMD_DEV_GET_TARGET_PROP to enclosure devices
SCGCQ01601702 - pl: NVMe: Write Long (10) fails when LBA exceeds 0x7FFFFFFF
SCGCQ01627798 - divert bitmap not enabled on R5/R6 WT Vds
SCGCQ01454613 - Pausing progress operation and resuming shows it starting from 0 again and abruptly moves to actual progress after a while
SCGCQ01478170 - Direct attached NVME drives are not getting associated with vSES in Microsoft Storage Spaces Direct.
SCGCQ01479406 - Drive addition in OS takes longer time when Drives are connected with certain backplanes to the controller
SCGCQ01484382 - improved fix for 6001 fault
SCGCQ01485060 - (SATA Only) Format of SATA SSD takes long time
SCGCQ01485441 - Firmware Download does not protect user from downgrading to firmware
SCGCQ01486695 - Host application hangs waiting for completion of IO issued after NVMe device is removed
SCGCQ01487291 - switch attached devices not detected under Windows
SCGCQ01491291 - OOB SLT get errror when getting send, getobjstatus and getttylog.
SCGCQ01498117 - Controller fail to be detected by BIOS and OS after FW downgrade MR73 with COL.
SCGCQ01502112 - Hit Assertion failure in ../../hw/pce/fusion.c at line 1847 after loading the driver & reboot
SCGCQ01502700 - Report Zone for very large data of 4MB takes ~2 seconds for processing
SCGCQ01503262 - FW may fault on single bit correctable ECC errors in IOA Local RAM
SCGCQ01504284 - additional phy hardware cleanup on link down and hot reset
SCGCQ01504310 - LTSSM state wait during hot reset
SCGCQ01504936 - New Event required for individual PD PR completion
SCGCQ01507024 - FW hit assertion failure when booting up with enclosure attached
SCGCQ01509537 - Auto rebuild does not start when HS has PF
SCGCQ01509632 - (SATA Only) SCT Error Recovery Control read using ATA Passthrough is not returning correct values.
SCGCQ01509791 - Assertion failure in ../../cpu/arm/exceptions.c at line 938 observed, while destaging preserved cache on R0 DG
SCGCQ01510251 - Fix Temperature Throttling
SCGCQ01518712 - FW incorrectly reports LD unit attention pending irrespective of the scsi op code
SCGCQ01519732 - 4311 fault with NVMe enabled
SCGCQ01522342 - 4311 fault with NVMe enabled (part 2)
SCGCQ01522362 - Firmware asserted at memory.h at line 443: isInAddressibleRange when push/pull JBOD NVMe drives
SCGCQ01522492 - Address performance issue for CPU intensive profiles.
SCGCQ01522509 - Firmware reports iopiTimedOutIOFound when running IO on NVMe JBOD drives
SCGCQ01529400 - Spin up large config drives by load the config file while they are in POWERSAVE, caused FW hit DrvSpinup.c @line 1362
SCGCQ01531736 - SR, RR, and OLTP regressions up to -90% on 24 Single Drive R0 Config
SCGCQ01545274 - Change CmdIgnoreLdUnitAttention() from _IOPATH to static inline
SCGCQ01548923 - system hangs during the reboot test at boot.
SCGCQ01561552 - OOB slt can not see the imr controller
SCGCQ01563926 - OEM name Characters seen in HII Drive management instead of port information.
SCGCQ01566825 - Changing personality between RAID and JBOD resulted in firmware assertion
SCGCQ01566954 - Change UNMAP support from enable to disable
SCGCQ01334586 - Task Management request of Abort Task to an NVMe device completes with failure status 
SCGCQ01406527 - PL 00005851 hit while issuing OCRs with IO
SCGCQ01451278 - link may fail to come up after link break
SCGCQ01487866 - Intermittent Update firmware failed with M0 using EFI StorCLI
SCGCQ01489030 - Global HDD LED may not indicate IO activity for NVMe or SAS drives
SCGCQ01494379 - 0x7C41 Fault doing IOs and Task Managements on a mixed SAS/NVMe topology.
SCGCQ01496842 - port enable may time out on spinup failure
SCGCQ01505392 - Slot LEDs on SGPIO based backplane may not blink
SCGCQ01509362 - Firmware asserted at ddf/ddf.c at line 1377: ld == vdRec->Populated_VDEs when insert NVMe drives
SCGCQ01511995 - OEM Drive Activity LED Stays On
SCGCQ01516975 - Firmware hang during power up after power failure with COL
SCGCQ01525140 - Firmware hangs due to DISM not completing
SCGCQ01555097 - Firmware asserted during cable pull with IO on JBODs and taskmgmt reset
SCGCQ01561897 - After VD erase, In the Action menu, It is not changing from Stop Erase to Erase
SCGCQ01502102 - Assertion failure in ../../dm/mpt2/mptframe.c at line 1250: mptIo!=NULL
SCGCQ01503916 - erroneously called bvdInfoSort() in DDF_ConfigRead() causes DDF to be corrupted
SCGCQ01505522 - Cannot set Foreign UBad to Foreign UGood with a config of 31 VDs and iMR 9441-8i
SCGCQ01519710 - Dump pending driver IO completions from task context during kill adapter debug
SCGCQ01531146 - Kill Adapter when create vd
SCGCQ01538991 - Enable MR code for generating firmware not compatible with profile event
SCGCQ01468157 - RAID Personality - R0 WB SW 4/8K all QD regression RHEL
SCGCQ01484398 - RAID-5 Hardware Key No Longer Functional 
SCGCQ01488410 - 30% to 35% JetstressDB Average Write Latency regression found in R5
SCGCQ01509463 - fw got data abort when connect more enclosure than max in iMR.
SCGCQ01518446 - pdCOD content is being overwritten when using storelibtest to issue SCAN FOREIGN
SCGCQ01522814 - All VDs are not getting deleted after the vd erase operation with 'delete VD after erase' option is selected
SCGCQ01505906 - passCount not incremented for Ctlr Self Diag Link Test
SCGCQ01512359 - web UI is exposing personality change option for iMR controller
SCGCQ01436268 - Add Test Link Diagnostic API
SCGCQ01459401 - Cleanup MR FW log
SCGCQ01531388 - Disable deallocation support
SCGCQ01559697 - Provide print in termlog that shows which I2C address is used for the LED signaling of NVMe drives
SCGCQ01459375 - Use Sense Data from SATA Log Page 10 when querying Log Page 10
SCGCQ01506822 - Resetting discovered flag when prepare for endpoint discovery control command.
SCGCQ01558893 - FBU345 should show as CVPM05
SCGCQ01512568 - Remove deallocation support
SCGCQ01468156 - Limit printing a SGL chain to only 15 elements.
SCGCQ01481032 - SSD can not show the "Part Number"/ "FRU Number" information 
SCGCQ01481034 - CATERR reported on front panel LCD and SUT hang at the windows logo page
SCGCQ01496768 - System will pop up “Cannot communicate with iButton to …” during reboot with OEM custom card
SCGCQ01501951 - Switching back and forth between profile 10 and 12 with data cable pull results in foreign config not importable
SCGCQ01505077 - 0x265D Fault Observed on Cold Boot of Customer Server with Misconfigured Controller NVDATA
SCGCQ01505080 - SCSI Write Buffer Mode 7 Command Incorrectly Failed by Firmware
SCGCQ01508067 - Slave response mode fails to return response to I2C read
SCGCQ01508156 - Controller hangs after warm reboot in presence of pinned cache
SCGCQ01510341 - Preserved Cache doesn't flush back during Foreign Import
SCGCQ01511969 - controller reset seen while importing 32 VD foreign config
SCGCQ01514262 - Fault State (0x265d) is Observed While Connecting an Enclosure with Fully Populated SATA Drives
SCGCQ01516692 - iMR-FW Drive Fault LED will light at some frequency when a JBOD drive is pulled out
SCGCQ01519802 - workaround timer may trigger after too short of an interval
SCGCQ01522339 - Controller hang when updating PD fw
SCGCQ01522511 - rapid device removal/add with a specific vendor backplane
SCGCQ01523550 - 4311 fault with NVMe enabled (part 2)
SCGCQ01529383 - non-NVMe endpoint not cleaned up on removal
SCGCQ01529512 - Fault 0x5862 seen when host buffer size is smaller than allocation length in CDB
SCGCQ01538948 - Sles12 SP3 OS is getting stuck during first boot
SCGCQ01539840 - PL Fault 0000ecdd LR 01403837 during initial discovery
SCGCQ01540255 - Initiate ocr when FW enters MonTask
SCGCQ01540360 - Termlog/UARTlog - messages sometimes missed in Termlog
SCGCQ01556426 - switch attached discovery takes too long
SCGCQ01561914 - Jbod become Ugood sometimes after reboot
SCGCQ01562034 - Controller hung, when updating the drive firmware
SCGCQ01562098 - Performance Improvements
SCGCQ01567485 - Check Consistency doesn't identify double media errors once aborting and starting CC again
SCGCQ01581266 - Turn off GPIOA19 (global fault LED installed) correctly at boot time
SCGCQ01421231 - I2C traces shows partial response/zero’ed out packet response from the HBA
SCGCQ01481100 - 930-24i/9460-24i and 930-8i/9460-8i create raid1 with 4 HDD, can't expand VD in UEFI
SCGCQ01511224 - Raid card loss during Test
SCGCQ01512617 - PL owned mids are not getting released even after removing drives (SATA)
SCGCQ01519729 - hardware does not like the IOP enable method used here.
SCGCQ01520063 - storcli show phyerror will return error in some test in some scenario
SCGCQ01521377 - MR FW is setting GPIO_SET_BBU_ENABLE(GPIOA8) wrongly in OCR case.
SCGCQ01524353 - (SATA Only) LBPRZ bit in VPD page 0xB2 is never set for SATA devices
SCGCQ01524448 - MegaRAID BIOS didnot timeout and cause Server boot hung when Controller Boot Fail because of bad SPD
SCGCQ01526202 - iMR FW locks up and PSOD seen while trying to flash MR7.2.1 FW ROP
SCGCQ01530310 - Controller is not detecting in the storelib, after changing the mode from "set mode oob" command
SCGCQ01533267 - EC0D fault
SCGCQ01556893 - link workaround not sufficiently coordinated with SAS link establishment
SCGCQ01561912 - storcli shows 8ports controller as 9 ports
SCGCQ01574395 - System hangs after performed Cryptographic Erase on SAS ISE drive
SCGCQ01499168 - Enhance SAS3 FW to pass PCIeCV PCIe Configuration Validation TD_1_28 Vital Product Data Capability Test
SCGCQ01505145 - When upgrading from 678 10.0 to 10.1 886 and switching to 240VD, unable to create 240VD
SCGCQ01520574 - 4311 fault with NVMe enabled
SCGCQ01521373 - Controller can not correctly detected smart error SATAA HDD.
SCGCQ01524638 - (SATA Only) Security Protocol In command complete without data transfer for allocation length not a multiple of 512
SCGCQ01527219 - PCIe reconfiguration may occur during NVMe controller reset
SCGCQ01558211 - Continuous error( MptHostCmdDone cmdId=fe lmid=8a2:1851b400 tid 04 devH ..) in firmware log when run I/O on NVMe drive
SCGCQ01559005 - Revised "Avoid Duplicate Mid" Feature Code Could Incorrectly Allow IO to Start Through PL Firmware Path
SCGCQ01561911 - Assertion failure in ../../mros/mem.c : mb->tag==tag
SCGCQ01577461 - Fault LED behavior is not consistent between PD direct attached vs connected via expander
SCGCQ01516689 - storcli /c0 show termlog didnot get termlog sometimes
SCGCQ01530305 - Get VDM Support command does not have VendorID and VendorAddInfo fields properly populated
SCGCQ01504375 - Disable write cache to default
SCGCQ01520061 - OCR is disabled by default is RC build, even NVDATA if it is enabled.
SCGCQ01540335 - FW automatically delete and create the EPD's with assigning EPD no 3f indefinitely.
SCGCQ01530478 - DUP failure on OEM controller while I/O is running in background
SCGCQ01503207 - Add method to determine Ring Buffer Overflow in RMC
SCGCQ01459626 - Assertion failure in ../../raid/taskman.c at line 342 while running TM sg_reset on SATA drives
SCGCQ01467284 - Optimize abort handling in command block context.
SCGCQ01467357 - Firmware crash when format drive to PI support
SCGCQ01473186 - To check if NVRAM changes related to upgrade/downgrade issue is present
SCGCQ01473242 - Firmware needs block certain user initiated operaations while it is in pending transition from one profile or personality to another
SCGCQ01450092 - MR RAID-mode profile 10 create vd cause pds for that vd offline
SCGCQ01454233 - WG:LSA in JBOD mode supports creating VD with "Always WriteBack" write policy
SCGCQ01476342 - Assert can occur when applying iButton/iButtonless Licensing settings that is typically done in a manufacturing environment.
SCGCQ01478714 - Unable to set RAID profile 11 & 12 (ROP 820 and newer affected)
SCGCQ01482688 - Additional changes needed for SCGCQ01470741: 16i Cannot Spinup HDD During System Power On.
SCGCQ01473960 - Block personality change when EPD security is not safestore managed.
SCGCQ01484398 - RAID-5 Hardware Key No Longer Functional(ROP 834 & earlier is okay)
SCGCQ01463522 - New feature to disable JBOD through NVDATA change if requested by customer
SCGCQ01464952 - Support for disabling personality modes
SCGCQ01474267 - Disallow mixture of NVMe drives and SAS/SATA drives in VD creation
SCGCQ01458621 - PL: EnclMgmt: Move ownership of SES Page 0x0A slot mapping from devices to PHYs
SCGCQ01487260 - MPI SEP request to Slots with invalid SES Page 0A element index may not complete
SCGCQ01479658 - pl: NVMe: port enable may complete before devices link up
SCGCQ01478827 - pl: NVMe: issues related to port enable completion
SCGCQ01461851 - PL trying to perform memory move using address which is in the non-addressable range
SCGCQ01459637 - pl: backend PCIe: erroneous address pool copy
SCGCQ01460622 - ONFI Device param page checksum calculation is not correct.
SCGCQ01466376 - Fast Path IO is not failed for LDBBM table entries
SCGCQ01473774 - I2C controller hang is observed with repeated LD create and delete script from BMC
SCGCQ01474118 - Max supported disk of Raid 50 and Raid 60 is showing 138
SCGCQ01482233 - 9460-8i card connect drive through direct-attached backplane: error LED not on when drop out a drive.
SCGCQ01483186 - Factory default restore required to set the controller properties after FW upgrade
SCGCQ01496629 - Global HDD LED may not indicate IO activity for NVMe or SAS drives
SCGCQ01459785 - Uncorrectable Medium / DIF Errors are not being handled correctly with pi enabled VDs.
SCGCQ01459793 - Fatal FW Error during CopyBack and partial VD creations on a spanned VD.
SCGCQ01466377 - IO Stress Automation test failed while trying to delete VDs; OCR seen in TTY
SCGCQ01474091 - Inserting enclosures results in unconfigured good PDs changing to R0 automatically and should not
SCGCQ01474449 - Assertion failure in ../../raid/cache.c found while running multipath push/pull with IO'
SCGCQ01478865 - 16i Cannot Spinup HDD During System Power On
SCGCQ01482228 - Fixed the issue with older ibutton
SCGCQ01470577 - Controller hangs after updating to latest ROP 676
SCGCQ01458055 - OS hung and iMR FW reset when do delete and create VD from previous powersave PD (Spindowned)
SCGCQ01459797 - Replace Member PD failed to copy back on a 4KN data protected VD
SCGCQ01473796 - set jbod on a Faulty disk will take several minutes to go to bad state
SCGCQ01487806 - Disable T10 Protection Information support
SCGCQ01404432 - Update nvram.h with correct size for curAdpPersonality
SCGCQ01415120 - Raid Map and Pd sync are updated for every OCR
SCGCQ01408312 - Reduce number of block-pairs used for 8GB offload
SCGCQ01418180 - NVDATA: Change Default SGPIO electrical driving strength from 50 to 66 Ohm 
SCGCQ01421427 - Data abort exception during OCR with JBODs
SCGCQ01424266 - Revert SCGCQ01418180 for 3616 and 3508 XSD, 3408 and 3416 remains the same.
SCGCQ01425554 - Integrate MR PL-SCS Libs
SCGCQ01388735 - Store the RAID SubDevID in NVRAM to have a reference to original RAID-ID - NVRAM changes
SCGCQ01373260 - [NVRAM] Warning removal 1295
SCGCQ01421154 - Prevent Improper Flash from ISSI Supported SBR/FW to non-ISSI Supported SBR/FW when Board has ISSI Chip
SCGCQ01413785 - Parameter Page Reads fail during ONFI bringup.
SCGCQ01412186 - pdRef filled incorrectly in bvd->Physical_Disk_Sequence[] causing DDF to skip added PD in Recon
SCGCQ01421154 - Prevent Improper Flash from ISSI Supported SBR/FW to non-ISSI Supported SBR/FW when Board has ISSI Chip
SCGCQ01411024 - Flash write Failed with err code 5
SCGCQ01411329 - Shutdown command received from host" missed in tty log

UEFI_Driver:
SCGCQ00883008 - Profile Mgmt API Changes
SCGCQ00927738 - Reintroduce numSGEExt Field in Raid Context to support 1MB IO
SCGCQ01405242 - Enable WB support via API
SCGCQ00948535 - The code had events with repetitive ID and some structures clashing
SCGCQ01403193 - Form set title displayed as <> in HII
SCGCQ01407043 - If waitForKey is False suppress "Enter Your Input Here:" string
SCGCQ01452207 - UEFI Driver skips showing boot message when FW sets Wait For Key Variable with 0
SCGCQ01264142 - New fault code for routine synchronous reset
SCGCQ00867953 - profile management API
SCGCQ01023741 - MR_CTRL_INFO expansion from 2K to 4K
SCGCQ01059740 - mega api changes for ibuttonless PR
SCGCQ01075821 - Profile Management Changes to support requestedProfileID and optimisedProfile
SCGCQ01407767 - If waitForKey is False suppress "Enter Your Input Here:" string
SCGCQ01384314 - With pinned cache generated, HII is auto launched during system Boot when BIOS Mode is set to Ignore Errors.
SCGCQ01447716 - UEFI Driver: For STP Frame data buffer is not copied
SCGCQ01384316 - With pinned cache generated, HII is auto launched during system Boot when BIOS Mode is set to Ignore Errors.
SCGCQ01447720 - UEFI Driver : System Hangs on running SCT test
SCGCQ01452207 - UEFI Driver skips showing boot message when FW sets Wait For Key Variable  with 0
SCGCQ00867953 - profile management API
SCGCQ00875328 - Mega API modifications needed for RMW-FP and Cache bypass features 
SCGCQ00941620 - de-feature AHCI
SCGCQ01023741 - MR_CTRL_INFO expansion from 2K to 4K
SCGCQ01059740 - mega api changes for ibuttonless PR
SCGCQ01203751 - Isolating faulty cable issue from bad drive issue
SCGCQ01227051 - New events for PR/CC conflicts and sector size mismatch
SCGCQ01447718 - UEFI Driver: For STP Frame data buffer is not copied
SCGCQ01474307 - UEFI driver to handle applications NOT setting direction flag
SCGCQ01558862 - SCSI frame length not matching with SGL count
SCGCQ01452594 - UEFI Driver skips showing boot message when FW sets Wait For Key Variable  with 0
SCGCQ01447716 - For STP Frame data buffer is not copied
SCGCQ01447723 - System Hangs on running SCT test
SCGCQ01478749 - Remove FMP Support From UEFI Driver
SCGCQ01447720 - System Hangs on running SCT test
SCGCQ01407043 - If waitForKey is False suppress "Enter Your Input Here:" string
SCGCQ01345378 - MR7 PNP additions
SCGCQ01351616 - Change the logic for reentering to main entry point in UEFI Driver
SCGCQ01384314 - With pinned cache generated, HII is auto launched during system Boot when BIOS Mode is set to Ignore Errors.
SCGCQ01321203 - Reset Type and customer messaging for system resets initiated by controller OpROM
SCGCQ01321228 - When user unloads UEFI Driver nullify pHiiHandShakeProtocol and ask platform to free HII (memory and image handle)
SCGCQ01301650 - Cursor below text and in center of line on the system reset request screen.
SCGCQ01309119 - Debug print shown on the console from the UEFI Driver error path.
SCGCQ01349428 - Firmware Management Protocol - Firmware update fails with inappropriate message when trying to update an unsigned
component

Hii:
SCGCQ01447718 - For STP Frame data buffer is not copied
SCGCQ01449687 - JBOD Mode – SAS/SATA Large Topology Support (240 PD/VD) (WT for VDs)
SCGCQ01474307 - UEFI driver to handle applications NOT setting direction flag
SCGCQ01558862 - SCSI frame length not matching with SGL count
SCGCQ01491187 - Attached Enclosures/PDs do not enumerate correctly in HII.
SCGCQ01452594 - UEFI Driver skips showing boot message when FW sets Wait For Key Variable  with 0
SCGCQ01486435 - PCIe PD interface type still showing as an option for OEM Controller
SCGCQ01524609 - Add Device Speed options for PCIe drives
SCGCQ01558992 - Unable to select Option to discard preserved cache in HII.
SCGCQ01447723 - System Hangs on running SCT test
SCGCQ01478749 - Remove FMP Support From UEFI Driver
SCGCQ01478752 - Profile management: Do not show "Max PCIe Count" if MR_CTRL_INFO.adapterOperations5.supportPCIe is set to 0
SCGCQ01397706 - Check All option is not working properly in Make JBOD form
SCGCQ01403193 - Form set title displayed as <> in HII
SCGCQ01404248 - HII: Controller Name is not shown in the HII Formset title
SCGCQ01407043 - If waitForKey is False suppress "Enter Your Input Here:" string
SCGCQ01388767 - HII is showing the internal backplane drives in triplet format instead of duplet.
SCGCQ01401629 - Secure Virtual Disk checkbox not selected by default when Security is Enabled on the controller
SCGCQ01405002 - HII Controller mode[JBOD] :Check All option not available to Make JBOD
SCGCQ01405359 - Question value mismatch in profile management
SCGCQ01413295 - HII: Read VPD and display SN in HII accordingly and update the Inventory data with default values when keyword is missing in VPD
SCGCQ01445619 - HBA (Host Bus Adapter) String is used twice instead of SDS (Software Defined Storage)
SCGCQ01397564 - The physical drive operation % increase in progress is not getting updated
SCGCQ01427258 - Suppress Emulation Type for 4k VD
SCGCQ01452207 - UEFI Driver skips showing boot message when FW sets Wait For Key Variable with 0
SCGCQ01376325 - An empty page is seen when reconstruction is triggered.
SCGCQ01404996 - HII Controller mode[JBOD] :Warning massage is not displayed in Make JBOD
SCGCQ01387373 - "The requested command has invalid arguments" message is seen after importing 150+ virtual drives.
SCGCQ01388677 - Connector Name is truncated in the "Disk Name string" in Disk Management
SCGCQ01396828 - Unable to convert all UG drives to JBOD while 2 enclosure connected
SCGCQ01406386 - Internal Backplane is showing as an enclosure in HII Dashboard View
SCGCQ01407025 - Check All is not working in Assign Dedicated HotSpare form
SCGCQ01411539 - Use SetBrowserData for VD and PD Mngt Refresh functions.
SCGCQ01412729 - HII - Select Span option shown after creating a VD with no Unconfigured drives remaining
SCGCQ01405000 - HII Controller mode[JBOD] :Error massage displayed upon converting UG to JBOD
SCGCQ01406429 - HII shows junk characters instead of serial number when you go to Controller Management Page.
SCGCQ01289924 - Add "Incompatible with Profile" event
SCGCQ01445048 - Add a new structure to provide OEMs ability to switch to select either I2C or PCIe as an out of band transport
SCGCQ01386211 - UEFI Driver: MR/iMR PCI Generic Information Retrieval from MPB Entry
SCGCQ01406093 - JBOD Mode – SAS/SATA (64 Physical Drive/Virtual DriveD) (Write back for Virtual Drives)
SCGCQ01336996 - HII: MR/iMR PCI Generic Information Retrieval from MPB Entry
SCGCQ01394969 - JBOD Mode – SAS/SATA Large Topology Support (240 PD/VD) (WT for VDs)
SCGCQ01400115 - The physical drive operation % increase in progress is not getting updated
SCGCQ01447705 - Submit Fail for Form: Dashboard view for HII/Storage management forms
SCGCQ01419755 - HII - Select Span option shown after creating a VD with no Unconfigured drives remaining
SCGCQ01407767 - If waitForKey is False suppress "Enter Your Input Here:" string
SCGCQ01392392 - Connector Name is truncated in the "Disk Name string" in Disk Management
SCGCQ01389130 - In the 'Manage SAS Storage Link Speed' form, not able to move the cursor to the next entry.
SCGCQ01385162 - For SuperCap, HII has the primitive 'Remaining Capacity' which is different compared to other host utilites
SCGCQ01454099 - Not able to change Security passphrase after selecting the check box "use existing passphrase".
SCGCQ01452578 - RLM option not listing for Raid 0 VD created on SSD when there is existing R1 VD with HDD
SCGCQ01449677 - Enclosure count is wrong in HII Dashboard form
SCGCQ01402885 - Unable to convert all UG drives to JBOD while 2 enclosure connected
SCGCQ01388946 - "The requested command has invalid arguments" message is seen after importing 150+ virtual drives.
SCGCQ01426500 - Per HII NGM design doc rev 1.3, HII not to show Connection field under basic pd prop page for OEM BP
SCGCQ01402889 - HII is showing the H745P MX internal backplane drives in triplet format instead of duplet.
SCGCQ01402883 - Check All option is not working properly in Make JBOD form
SCGCQ01384314 - With pinned cache generated, HII is auto launched during system Boot when BIOS Mode is set to Ignore Errors.
SCGCQ01447677 - SATA PD information is missing on OEM controller in HII
SCGCQ01447658 - help String change request for "Select Raid Level" for RAID 60
SCGCQ01407030 - Check All is not working in Assign Dedicated HotSpare form
SCGCQ01423426 - Internal Backplane is showing as an enclosure in HII Dashboard View
SCGCQ01416004 - Add Device Speed under Advanced PD properties page
SCGCQ01389129 - In the 'Manage SAS Storage Link Speed' form, not able to move the cursor to the next entry.
SCGCQ01447716 - UEFI Driver: For STP Frame data buffer is not copied
SCGCQ01386799 - Not able to disable JBOD mode when there is file system/operating system present on the controller configuration.
SCGCQ01426465 - HII - PD ordering is based on slot id rather than enclosure id
SCGCQ01386798 - Not able to disable JBOD mode when there is file system/operating system present on the controller configuration.
SCGCQ01384316 - With pinned cache generated, HII is auto launched during system Boot when BIOS Mode is set to Ignore Errors.
SCGCQ01422005 - change Default setting in Select Media Type in HII from HDD to Both
SCGCQ01422002 - iMR HII will jump to some form unexpectedly when import foreigh configuration
SCGCQ01491729 - Attached Enclosures/PDs do not enumerate correctly in HII.
SCGCQ01464680 - Unable to create a R10 in HII but can with CLI
SCGCQ01447734 - Issue with Uneven Span
SCGCQ01447720 - UEFI Driver : System Hangs on running SCT test
SCGCQ01447698 - HII : System Hangs with Assert on running SCT test
SCGCQ01447088 - Question value mismatch when converting JBODs to UGs during VD creation
SCGCQ01467531 - Create Virtual Drive: The Yes option that user chose gets retained for Disable Background Initialization
SCGCQ01330410 - Add Requeted Profile ID field in Profile Management form.
SCGCQ01397706 - Check All option is not working properly in Make JBOD form
SCGCQ01407043 - If waitForKey is False suppress "Enter Your Input Here:" string
SCGCQ01388767 - HII is showing internal backplane drives in triplet format instead of duplet.
SCGCQ01401629 - Secure Virtual Disk checkbox not selected by default when Security is Enabled on the controller
SCGCQ01343778 - Question ID assignment for item under suppressif TRUE and the same item that gets created at runtime
SCGCQ01344008 - HEFU: Delay seen during boot in case of 240 PD configuration.
SCGCQ01344658 - Customize the configuration help message.
SCGCQ01355025 - Silence Alarm: Use tech pub suggested help string
SCGCQ01379764 - HII Advanced VD properties shows "CacheCade Type" primitive
SCGCQ01376325 - An empty page is seen when reconstruction is triggered.
SCGCQ01372698 - LockKeyFailed is set with junk value from Controller info
SCGCQ01387373 - "The requested command has invalid arguments" message is seen after importing 150+ virtual drives.
SCGCQ01388677 - Connector Name is truncated in the "Disk Name string" in Disk Management
SCGCQ01396828 - Unable to convert all UG drives to JBOD while 2 enclosure connected
SCGCQ01406386 - Internal Backplane is showing as an enclosure in HII Dashboard View
SCGCQ01352041 - RSOD seen when user browse to Enclosure Management Page
SCGCQ01354659 - HII Create Virtual Disk option is selectable even before choosing drives for the VD
SCGCQ01412729 - HII - Select Span option shown after creating a VD with no Unconfigured drives remaining
SCGCQ01348156 - Foreign Configuration Preview screen also has entries of virtual drives that are optimal in state.
SCGCQ01337568 - HII: Enumeration of drives
SCGCQ01335254 - Prompt string should be unique
SCGCQ01345617 - Remove unsupported features from the HII Main Menu Help tab
SCGCQ01359020 - Add new card support in HII
SCGCQ01325348 - With secured foreign SED, it is asking you to enter the Passphrase/password.
SCGCQ01291052 - User must be warned when they create a VD across the front backplane and enclosures behind the switch
SCGCQ01376269 - Internal bpis showing up as an encl which causes HII to show the enumeration incorrectly - implement new MR API
SCGCQ01345378 - MR7 PNP additions
SCGCQ01350528 - Select RAID level using QID under suppressif TRUE and then same primtiive generated at runtime
SCGCQ01321222 - HEFU: Sort the connector names, when the names are not in Port 0 -3 format
SCGCQ01344341 - Incorrect Drive Group numbering in "Create Virtual Drive" menu
SCGCQ01351616 - Change the logic for reentering to main entry point in UEFI Driver
SCGCQ01385162 - For SuperCap, HII has the primitive 'Remaining Capacity' which is different compared to other host utilites
SCGCQ01400115 - The physical drive operation % increase in progress is not getting updated
SCGCQ01321208 - When user unloads UEFI Driver nullify pHiiHandShakeProtocol and ask platform to free HII (memory and image handle)
SCGCQ01333899 - Inappropriate message shown when the Reconstruction is initiated again while the previous reconstruction is in progress.
SCGCQ01384314 - With pinned cache generated, HII is auto launched during system Boot when BIOS Mode is set to Ignore Errors.
SCGCQ01321189 - Foreign configuration page seen after changing profile to NVMe.
SCGCQ01321203 - Reset Type and customer messaging for system resets initiated by controller OpROM
SCGCQ01389129 - In the 'Manage SAS Storage Link Speed' form, not able to move the cursor to the next entry.
SCGCQ01407030 - Check All is not working in Assign Dedicated HotSpare form
SCGCQ01334156 - HEFU: Don't check the return value for the function to get connector index and sorted connnector index
SCGCQ01321185 - HII shows wrong Temperature value when Sensor status is "Not Installed"
SCGCQ01334144 - Not able to select check box in some forms
SCGCQ01386798 - Not able to disable JBOD mode when there is file system/operating system present on the controller configuration.
SCGCQ01321210 - HEFU - Sort the disk based on connector name, slot and position
SCGCQ01301650 - Cursor below text and in center of line on the system reset request screen.
SCGCQ01309119 - Debug print shown on the console from the UEFI Driver error path.
SCGCQ01348104 - Click on "OK" button after completing any operation doesn't have any effect in the screen
SCGCQ01349428 - Firmware Management Protocol - Firmware update fails with inappropriate message when trying to update an unsigned
component

BIOS:
SCGCQ01402877 - Legacy BIOS: JBOD Mode – SAS/SATA Large Topology Support
SCGCQ01424581 - System stops at post in legacy mode boot in the multi controllers configuration where-in one of the controller is in fault state
SCGCQ01292708 - Drive ID shown in BIOS POST is more than 1000+, even thought the total drives is only about 160
SCGCQ01379327 - System reset is initiated twice in BIOS
SCGCQ01321554 - Reset Type and customer messaging for system resets initiated by controller optrom

Boot Block:
SCGCQ01357917 - Boot Block Accesses PCI_LINK_CONFIG while PCE Core is Reset




