//****************************************************************************
//                   INTEL CORPORATION PROPRIETARY INFORMATION
//       This software is supplied under the terms of a license agreement or
//       nondisclosure agreement with Intel Corporation and may not be copied
//       or disclosed except in accordance with the terms of that agreement.
//         Copyright (c) 2018 Intel Corporation. All Rights Reserved.
//***************************************************************************
//
// Data in this file is based on the BNP FSC Auto-SDR Config Sheet rev2.1_Candidate.xlsm (20180829) spreadsheet.
//

// SDR tag usage

//====================================================================//
// (1) Chassis related TAG
//====================================================================//
// _SDR_TAG    'BCP_2U4N'               // SDRs for 2U4N chassis
// _SDR_TAG    '2U4N_BP_X35'            // SDRs for 3.5" HDD-BP
// _SDR_TAG    '24HDDHSBP'              // SDRs for 2.5" HDD-BP
// _SDR_TAG    'EBCP-BNP'               // SDRs for EBCP-BNP
// _SDR_TAG    'BP_X35_LC'              // SDRs for 3.5" HDD-BP if S2600BPL populated
// _SDR_TAG    '24HDD_LC'               // SDRs for 2.5" HDD-BP if S2600BPL populated
// _SDR_TAG    'EBCP-LC'                // SDRs for EBCP-BNP    if S2600BPL populated
// _SDR_TAG    'TEST_PLATE'             // SDRs for Test Plate for NPI: PO Kit
// _SDR_TAG    'OTHER'                  // SDRs for OTHER chassis

//====================================================================//
// (2) Processor related sensors
//====================================================================//
// Processor support tags:
//      PROCESSOR_2     = Second CPU in a dual processor system
//


//====================================================================//
// (3) Fan sensors
//====================================================================//
// _SDR_TAG    'SYS_FAN_2U4N'           //System Fan 2U4N SKU
// _SDR_TAG    'SYSTEM_FAN_1A'          //System Fan SYSTEM_FAN_1A
// _SDR_TAG    'SYSTEM_FAN_1B'          //System Fan SYSTEM_FAN_1B
// _SDR_TAG    'SYSTEM_FAN_2A'          //System Fan SYSTEM_FAN_2A
// _SDR_TAG    'SYSTEM_FAN_2B'          //System Fan SYSTEM_FAN_2B
// _SDR_TAG    'SYSTEM_FAN_3A'          //System Fan SYSTEM_FAN_3A
// _SDR_TAG    'SYSTEM_FAN_3B'          //System Fan SYSTEM_FAN_3B
// _SDR_TAG    'SYSTEM_FAN_4A'          //System Fan SYSTEM_FAN_4A
// _SDR_TAG    'SYSTEM_FAN_4B'          //System Fan SYSTEM_FAN_4B
// _SDR_TAG    'SYSTEM_FAN_5A'          //System Fan SYSTEM_FAN_5A
// _SDR_TAG    'SYSTEM_FAN_5B'          //System Fan SYSTEM_FAN_5B
// _SDR_TAG    'SYSTEM_FAN_6A'          //System Fan SYSTEM_FAN_6A
// _SDR_TAG    'SYSTEM_FAN_6B'          //System Fan SYSTEM_FAN_6B
// _SDR_TAG    'SYSTEM_FAN_7'           //System Fan SYSTEM_FAN_7
// _SDR_TAG    'SYSTEM_FAN_8'           //System Fan SYSTEM_FAN_8
// _SDR_TAG    'OTHER_FAN_1A'           //System Fan OTHER_FAN_1A
// _SDR_TAG    'OTHER_FAN_1B'           //System Fan OTHER_FAN_1B
// _SDR_TAG    'OTHER_FAN_2A'           //System Fan OTHER_FAN_2A
// _SDR_TAG    'OTHER_FAN_2B'           //System Fan OTHER_FAN_2B
// _SDR_TAG    'OTHER_FAN_3A'           //System Fan OTHER_FAN_3A
// _SDR_TAG    'OTHER_FAN_3B'           //System Fan OTHER_FAN_3B
// _SDR_TAG    'OTHER_FAN_4A'           //System Fan OTHER_FAN_4A
// _SDR_TAG    'OTHER_FAN_4B'           //System Fan OTHER_FAN_4B
// _SDR_TAG    'OTHER_FAN_5A'           //System Fan OTHER_FAN_5A
// _SDR_TAG    'OTHER_FAN_5B'           //System Fan OTHER_FAN_5B
// _SDR_TAG    'OTHER_FAN_6A'           //System Fan OTHER_FAN_6A
// _SDR_TAG    'OTHER_FAN_6B'           //System Fan OTHER_FAN_6B
// _SDR_TAG    'OTHER_FAN_6'            //System Fan OTHER_FAN_6
// _SDR_TAG    'OTHER_FAN_7'            //System Fan OTHER_FAN_7
//====================================================================//
// (4) Power Supply related sensors
//====================================================================//
// _SDR_TAG    'STICKY_PS1_VALID'       // PS1 has valid FRU
// _SDR_TAG    'STICKY_PS2_VALID'       // PS2 has valid FRU
// _SDR_TAG    'STICKY_PS1_2130W'       // 2130W Power Supply 1
// _SDR_TAG    'STICKY_PS2_2130W'       // 2130W Power Supply 2
// _SDR_TAG    'STICKY_REDUNDANT_PS'    // Power Supply Redundancy
//
//====================================================================//
// (5) Others
//====================================================================//
// Miscellaneous support tags:
// _SDR_TAG    'CHASSIS_INTRU'          // Physical Security sensor
// _SDR_TAG    'LAN_LEASH'              // Physical Security sensor
// _SDR_TAG    'IFT_RISER1_AC'          // IFT Carrier populated on Riser 1 with Addr AC
// _SDR_TAG    'IFT_RISER1_A4'          // IFT Carrier populated on Riser 1 with Addr A4
// _SDR_TAG    'IFT_RISER2_AC'          // IFT Carrier populated on Riser 2 with Addr AC
// _SDR_TAG    'IFT_RISER2_A4'          // IFT Carrier populated on Riser 2 with Addr A4

//
// File Header Information
//

_LF_NAME       'BUCHANAN_PASS.SDR'
_LF_VERSION    '1.39'
_LF_FMT_VER    '0.01'
_IPMI_VERSION  '2.00'

//
// SDR Header Information
//

_SDR (
_START_ADDR    0000
_DATA_LEN      0000
_NVS_TYPE      'IMBDEVICE'
_DEV_BUS       FF
_DEV_ADDRESS   20

_SDR_TYPE  01
_REC_LEN  003D
    // Sensor Record Header
    0001            // Record ID
    51              // SDR Version
    01              // Record Type
    38              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    20              // Sensor Number
 
    // Record Body Bytes
    37              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    2D              // Nominal Reading
    37              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    41              // Upper critical
    3C              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CD              // Type/Length Code
    'BB Inlet Temp'// String Bytes

_SDR_TYPE  01
_REC_LEN  003B
    // Sensor Record Header
    0002            // Record ID
    51              // SDR Version
    01              // Record Type
    36              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    23              // Sensor Number
 
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    50              // Nominal Reading
    50              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    5A              // Upper critical
    55              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CB              // Type/Length Code
    'BB BMC Temp'// String Bytes

_SDR_TYPE  01
_REC_LEN  003F
    // Sensor Record Header
    0003            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    24              // Sensor Number
 
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    50              // Nominal Reading
    69              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    73              // Upper critical
    6E              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CF              // Type/Length Code
    'BB CPU1 VR Temp'// String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_REC_LEN    003F
 
    // Sensor Record Header
    0100            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
  
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    26              // Sensor Number
  
    // Record Body Bytes
    07              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    50              // Nominal Reading
    69              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    73              // Upper critical
    6E              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CF              // Type/Length Code
    'BB CPU2 VR Temp'// String Bytes

 
_SDR_TYPE  01
_SDR_TAG    'S2600BPP'
_SDR_TAG    'S2600BPQ'
_SDR_TAG    'S2600BPL'
_REC_LEN  003F
    // Sensor Record Header
    0004            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
     
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    14              // Sensor Number
     
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    50              // Nominal Reading
    69              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    73              // Upper critical
    6E              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CF              // Type/Length Code
    'BB MISC VR Temp'// String Bytes


_SDR_TYPE  01
_REC_LEN  003E
    // Sensor Record Header
    0005            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    25              // Sensor Number
 
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    50              // Nominal Reading
    69              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    73              // Upper critical
    6E              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CE              // Type/Length Code
    'BB Outlet Temp'// String Bytes


_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_REC_LEN    003E
    
    // Sensor Record Header
    0006            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    11              // Sensor Number
 
    // Record Body Bytes
    17              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    63              // Sensor Capabilities
    0B              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    11              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    02              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    14              // Nominal Reading
    28              // Normal Maximum
    00              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    00              // Positive hysteresis value
    00              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CE              // Type/Length Code
    'System Airflow'// String Bytes


_SDR_TYPE  01
_SDR_TAG  'LSISAS3008'
_SDR_TAG  'LSISAS3008_6PORT'
_REC_LEN  003C
    // Sensor Record Header
    0007            // Record ID
    51              // SDR Version
    01              // Record Type
    37              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    9E              // Sensor Number
 
    // Record Body Bytes
    17              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    63              // Sensor Capabilities
    0B              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    28              // Nominal Reading
    5F              // Normal Maximum
    0F              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    69              // Upper critical
    64              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    00              // Positive hysteresis value
    00              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CC              // Type/Length Code
    'LSI3008 Temp'// String Bytes


_SDR_TYPE  01
_SDR_TAG  'LSISAS3008_6PORT'
_REC_LEN  003F
    // Sensor Record Header
    0008            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    93              // Sensor Number
 
    // Record Body Bytes
    17              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    63              // Sensor Capabilities
    0B              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    28              // Nominal Reading
    4B              // Normal Maximum
    0F              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    55              // Upper critical
    50              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    00              // Positive hysteresis value
    00              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CF              // Type/Length Code
    'LSI3008 VR Temp'// String Bytes


_SDR_TYPE  01
_SDR_TAG  'LSISAS3408'
_REC_LEN  003C
    // Sensor Record Header
    0009            // Record ID
    51              // SDR Version
    01              // Record Type
    37              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    9E              // Sensor Number
 
    // Record Body Bytes
    17              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    63              // Sensor Capabilities
    0B              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    28              // Nominal Reading
    5F              // Normal Maximum
    05              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    69              // Upper critical
    64              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    05              // Lower non-critical
    00              // Positive hysteresis value
    00              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CC              // Type/Length Code
    'LSI3408 Temp'// String Bytes


_SDR_TYPE  01
_SDR_TAG  'LSISAS3408'
_REC_LEN  003F
    // Sensor Record Header
    000A            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    93              // Sensor Number
 
    // Record Body Bytes
    17              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    63              // Sensor Capabilities
    0B              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    28              // Nominal Reading
    4B              // Normal Maximum
    0F              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    55              // Upper critical
    50              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    00              // Positive hysteresis value
    00              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CF              // Type/Length Code
    'LSI3408 VR Temp'// String Bytes


_SDR_TYPE   01
_REC_LEN    0038
    
    // Sensor Record Header
    000E            // Record ID
    51              // SDR Version
    01              // Record Type
    33              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    22              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    50              // Nominal Reading
    5D              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    67              // Upper critical
    62              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    C8              // Type/Length Code
    'SSB Temp'      // String Bytes


_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'HSBP_TEMP'
_REC_LEN    0039

    
    // Sensor Record Header
    000F            // Record ID
    51              // SDR Version
    01              // Record Type
    34              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    29              // Sensor Number
    
    // Record Body Bytes
    0F              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    19              // Nominal Reading
    2D              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    6E              // Upper critical
    69              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    C9              // Type/Length Code
    'HSBP PSOC'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_REC_LEN    003D
    
    // Sensor Record Header
    0010            // Record ID
    51              // SDR Version
    01              // Record Type
    38              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    2E              // Sensor Number
 
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    37              // Nominal Reading
    4B              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    55              // Upper critical
    50              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CD              // Type/Length Code
    'Exit Air Temp' // String Bytes


_SDR_TYPE   01
_SDR_TAG    'S2600BPP'
_SDR_TAG    'S2600BPQ'
_SDR_TAG    'S2600BPL'
_REC_LEN    003C
    
    // Sensor Record Header
    0011            // Record ID
    51              // SDR Version
    01              // Record Type
    37              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    2F              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    50              // Nominal Reading
    6E              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    78              // Upper critical
    73              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CC              // Type/Length Code
    'LAN NIC Temp'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_1A'
_REC_LEN    003A
    
    // Sensor Record Header
    0012            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    30              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    62              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    84              // Nominal Reading
    FF              // Normal Maximum
    0A              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    08              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 1A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN  003A
    
    // Sensor Record Header
    0013            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    30              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    08              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    5A              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    85              // Nominal Reading
    FF              // Normal Maximum
    0B              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    09              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CA              // Type/Length Code
    'Sys Fan 1A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_1A'
_REC_LEN    003A
    
    // Sensor Record Header
    0122            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    30              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    3E              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    87              // Nominal Reading
    FF              // Normal Maximum
    0F              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    0B              // Lower critical
    0C              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 1A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_1B'
_REC_LEN    003A
    
    // Sensor Record Header
    0015            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    31              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    62              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    84              // Nominal Reading
    FF              // Normal Maximum
    0A              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    08              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 1B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN  003A
    
    // Sensor Record Header
    0016            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    31              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    09             // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    5D              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    85              // Nominal Reading
    FF              // Normal Maximum
    0C              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    08              // Lower critical
    09              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CA              // Type/Length Code
    'Sys Fan 1B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_1B'
_REC_LEN    003A
    
    // Sensor Record Header
    0123            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    31              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    3C              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    87              // Nominal Reading
    FF              // Normal Maximum
    10              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    0B              // Lower critical
    0D              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 1B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_2A'
_REC_LEN    003A
    
    // Sensor Record Header
    0018            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    32              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    03              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    62              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    84              // Nominal Reading
    FF              // Normal Maximum
    0A              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    08              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 2A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN  003A
    
    // Sensor Record Header
    0019            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    32              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    0A              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    5A              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    85              // Nominal Reading
    FF              // Normal Maximum
    0B              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    09              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CA              // Type/Length Code
    'Sys Fan 2A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_2A'
_REC_LEN    003A
    
    // Sensor Record Header
    0124            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    32              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    03              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    3E              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    87              // Nominal Reading
    FF              // Normal Maximum
    0F              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    0B              // Lower critical
    0C              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 2A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_2B'
_REC_LEN    003A
    
    // Sensor Record Header
    001B            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    33              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    04              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    62              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    84              // Nominal Reading
    FF              // Normal Maximum
    0A              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    08              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 2B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN  003A
    
    // Sensor Record Header
    001C            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    33              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    0B              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    5D              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    85              // Nominal Reading
    FF              // Normal Maximum
    0C              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    08              // Lower critical
    09              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CA              // Type/Length Code
    'Sys Fan 2B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_2B'
_REC_LEN    003A
    
    // Sensor Record Header
    0125            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    33              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    04              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    3C              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    87              // Nominal Reading
    FF              // Normal Maximum
    10              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    0B              // Lower critical
    0D              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 2B'    // String Bytes


_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   001E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   63                 // Sensor Initialization
   B8                 // Sensor Capabilities
   0C                 // Sensor Type -- Memory
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask (not event logging)
   3F3F               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   05                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   F0                 // R exp, B exp
   00                 // Analog characteristic flags
   00                 // Normal Reading 
   00                 // Normal Maximum 
   00                 // Normal Minimum 
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical
   00                 // Upper non-critical 
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'MTT CPU1'         // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_3A'
_REC_LEN    003A
    
    // Sensor Record Header
    001F            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    34              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    05              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    62              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    84              // Nominal Reading
    FF              // Normal Maximum
    0A              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    08              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 3A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN  003A
    
    // Sensor Record Header
    0020            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    34              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    0C              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    5A              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    85              // Nominal Reading
    FF              // Normal Maximum
    0B              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    09              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CA              // Type/Length Code
    'Sys Fan 3A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_3A'
_REC_LEN    003A
    
    // Sensor Record Header
    0126            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    34              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    05              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    3E              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    87              // Nominal Reading
    FF              // Normal Maximum
    0F              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    0B              // Lower critical
    0C              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 3A'    // String Bytes


_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   0022               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   63                 // Sensor Initialization
   B8                 // Sensor Capabilities
   0C                 // Sensor Type -- Memory
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   3F3F               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   05                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   F0                 // R exp, B exp
   00                 // Analog characteristic flags
   00                 // Normal Reading 
   00                 // Normal Maximum 
   00                 // Normal Minimum 
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical
   00                 // Upper non-critical 
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'MTT CPU2'         // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_3B'
_REC_LEN    003A
    
    // Sensor Record Header
    0023            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    35              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    06              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    62              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    84              // Nominal Reading
    FF              // Normal Maximum
    0A              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    08              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 3B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN  003A
    
    // Sensor Record Header
    0024            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    35              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    0D              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    5D              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    85              // Nominal Reading
    FF              // Normal Maximum
    0C              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    08              // Lower critical
    09              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CA              // Type/Length Code
    'Sys Fan 3B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_3B'
_REC_LEN    003A
    
    // Sensor Record Header
    0127            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    35              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    06              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    3C              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    87              // Nominal Reading
    FF              // Normal Maximum
    10              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    0B              // Lower critical
    0D              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 3B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_4A'
_REC_LEN    003A
    
    // Sensor Record Header
    0026            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    30              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    07              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    62              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    84              // Nominal Reading
    FF              // Normal Maximum
    0A              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    08              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 4A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_4A'
_REC_LEN    003A
    
    // Sensor Record Header
    0128            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    30              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    07              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    3E              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    87              // Nominal Reading
    FF              // Normal Maximum
    0F              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    0B              // Lower critical
    0C              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 4A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_4B'
_REC_LEN    003A
    
    // Sensor Record Header
    0028            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    31              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    08              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    62              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    84              // Nominal Reading
    FF              // Normal Maximum
    0A              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    08              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 4B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_4B'
_REC_LEN    003A
    
    // Sensor Record Header
    0129            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    31              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    08              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    3C              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    87              // Nominal Reading
    FF              // Normal Maximum
    10              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    0B              // Lower critical
    0D              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 4B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_5A'
_REC_LEN    003A
    
    // Sensor Record Header
    002A            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    32              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    09              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    62              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    84              // Nominal Reading
    FF              // Normal Maximum
    0A              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    08              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 5A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_5A'
_REC_LEN    003A
    
    // Sensor Record Header
    012A            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    32              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    09              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    3E              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    87              // Nominal Reading
    FF              // Normal Maximum
    0F              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    0B              // Lower critical
    0C              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 5A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_5B'
_REC_LEN    003A
    
    // Sensor Record Header
    002C            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    33              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    0A              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    62              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    84              // Nominal Reading
    FF              // Normal Maximum
    0A              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    08              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 5B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_5B'
_REC_LEN    003A
    
    // Sensor Record Header
    012B            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    33              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    0A              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    3C              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    87              // Nominal Reading
    FF              // Normal Maximum
    10              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    0B              // Lower critical
    0D              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 5B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_6A'
_REC_LEN    003A
    
    // Sensor Record Header
    002E            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    34              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    0B              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    62              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    84              // Nominal Reading
    FF              // Normal Maximum
    0A              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    08              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 6A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_6A'
_REC_LEN    003A
    
    // Sensor Record Header
    012C            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    34              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    0B              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    3E              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    87              // Nominal Reading
    FF              // Normal Maximum
    0F              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    0B              // Lower critical
    0C              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 6A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_6B'
_REC_LEN    003A
    
    // Sensor Record Header
    0030            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    35              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    0C              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    62              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    84              // Nominal Reading
    FF              // Normal Maximum
    0A              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    08              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 6B'    // String Bytes
 
 
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_6B'
_REC_LEN    003A
    
    // Sensor Record Header
    012D            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    35              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    0C              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    3C              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    87              // Nominal Reading
    FF              // Normal Maximum
    10              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    0B              // Lower critical
    0D              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Fan 6B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG   'S2600BPL'
_REC_LEN   003A
    
    // Sensor Record Header
    0024            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    3C              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    0D              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    0A              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    1A              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    8B              // Nominal Reading
    FF              // Normal Maximum
    85              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    FF              // Upper critical
    B7              // Upper non-critical
    00              // Lower non-recoverable
    0C              // Lower critical
    71              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Pump 1'// String Bytes


_SDR_TYPE  01
_SDR_TAG   'OTHER_FAN_6'

_REC_LEN  0039
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    01              // Record Type
    34              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    36              // Sensor Number
 
    // Record Body Bytes
    1D              // Entity ID
    0C              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    27              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    8C              // Nominal Reading
    FF              // Normal Maximum
    19              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    11              // Lower critical
    14              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    C9              // Type/Length Code
    'Sys Fan 6'// String Bytes
 

_SDR_TYPE  01
_SDR_TAG   'SYSTEM_FAN_6'
_REC_LEN   0039

    // Sensor Record Header
    012E            // Record ID
    51              // SDR Version
    01              // Record Type
    34              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    36              // Sensor Number
 
    // Record Body Bytes
    1D              // Entity ID
    0C              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    27              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    8C              // Nominal Reading
    FF              // Normal Maximum
    19              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    11              // Lower critical
    14              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    C9              // Type/Length Code
    'Sys Fan 6'// String Bytes


_SDR_TYPE   01
_SDR_TAG   'S2600BPL'
_REC_LEN   003A
    
    // Sensor Record Header
    0024            // Record ID
    51              // SDR Version
    01              // Record Type
    35              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    3D              // Sensor Number
    
    // Record Body Bytes
    1D              // Entity ID
    0D              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    0A              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    1A              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    8B              // Nominal Reading
    FF              // Normal Maximum
    85              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    FF              // Upper critical
    B7              // Upper non-critical
    00              // Lower non-recoverable
    0C              // Lower critical
    71              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    CA              // Type/Length Code
    'Sys Pump 2'// String Bytes


_SDR_TYPE  01
_SDR_TAG   'OTHER_FAN_7'

_REC_LEN  0039
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    01              // Record Type
    34              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    37              // Sensor Number
 
    // Record Body Bytes
    1D              // Entity ID
    0C              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    27              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    8C              // Nominal Reading
    FF              // Normal Maximum
    19              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    11              // Lower critical
    14              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    C9              // Type/Length Code
    'Sys Fan 7'// String Bytes
 

_SDR_TYPE  01
_SDR_TAG   'SYSTEM_FAN_7'
_REC_LEN   0039

    // Sensor Record Header
    012F            // Record ID
    51              // SDR Version
    01              // Record Type
    34              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    37              // Sensor Number
 
    // Record Body Bytes
    1D              // Entity ID
    0C              // Entity Instance
    7F              // Sensor Initialization
    28              // Sensor Capabilities
    04              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    12              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    27              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    8C              // Nominal Reading
    FF              // Normal Maximum
    19              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    11              // Lower critical
    14              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    45              // OEM
    C9              // Type/Length Code
    'Sys Fan 7'// String Bytes
 

_SDR_TYPE  01
_SDR_TAG   'STICKY_PS1_2130W'
_SDR_TAG   'STICKY_PS1'
_REC_LEN  003F
    // Sensor Record Header
    0032            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    54              // Sensor Number
 
    // Record Body Bytes
    0A              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    0B              // Sensor Type
    01             // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    06              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    0D              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    5A              // Nominal Reading
    B4              // Normal Maximum
    00              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    D5              // Upper critical
    C4              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    00              // Positive hysteresis value
    00              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CF              // Type/Length Code
    'PS1 Input Power'// String Bytes


_SDR_TYPE  01
_SDR_TAG   'STICKY_PS2_2130W'
_SDR_TAG   'STICKY_PS2'
_REC_LEN  003F
    // Sensor Record Header
    0033            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    55              // Sensor Number
 
    // Record Body Bytes
    0A              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    0B              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    06              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    0D              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    5A              // Nominal Reading
    B4              // Normal Maximum
    00              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    D5              // Upper critical
    C4              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    00              // Positive hysteresis value
    00              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CF              // Type/Length Code
    'PS2 Input Power'// String Bytes


_SDR_TYPE  01
_SDR_TAG   'STICKY_PS1_2130W'
_SDR_TAG   'STICKY_PS1'
_REC_LEN  003E
    // Sensor Record Header
    0034            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    58              // Sensor Number
 
    // Record Body Bytes
    0A              // Entity ID
    03              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    03              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    01              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    32              // Nominal Reading
    64              // Normal Maximum
    00              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    75              // Upper critical
    64              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    00              // Positive hysteresis value
    00              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CE              // Type/Length Code
    'PS1 Curr Out %'// String Bytes


_SDR_TYPE  01
_SDR_TAG   'STICKY_PS2_2130W'
_SDR_TAG   'STICKY_PS2'
_REC_LEN  003E
    // Sensor Record Header
    0035            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    59              // Sensor Number
 
    // Record Body Bytes
    0A              // Entity ID
    04              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    03              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    01              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    32              // Nominal Reading
    64              // Normal Maximum
    00              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    75              // Upper critical
    64              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    00              // Positive hysteresis value
    00              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CE              // Type/Length Code
    'PS2 Curr Out %'// String Bytes


_SDR_TYPE  01
_SDR_TAG   'STICKY_PS1_2130W'
_SDR_TAG   'STICKY_PS1'
_REC_LEN  003F
    // Sensor Record Header
    0036            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    5C              // Sensor Number
 
    // Record Body Bytes
    0A              // Entity ID
    05              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    1C              // Nominal Reading
    37              // Normal Maximum
    05              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    41              // Upper critical
    3C              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CF              // Type/Length Code
    'PS1 Temperature'// String Bytes


_SDR_TYPE  01
_SDR_TAG   'STICKY_PS2_2130W'
_SDR_TAG   'STICKY_PS2'
_REC_LEN  003F
    // Sensor Record Header
    0037            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    5D              // Sensor Number
 
    // Record Body Bytes
    0A              // Entity ID
    06              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    1C              // Nominal Reading
    37              // Normal Maximum
    05              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    41              // Upper critical
    3C              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CF              // Type/Length Code
    'PS2 Temperature'// String Bytes


_SDR_TYPE   01
_REC_LEN    003F
    
    // Sensor Record Header
    0038            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    74              // Sensor Number
    
    // Record Body Bytes
    03              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    F1              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CF              // Type/Length Code
    'P1 Therm Margin'// String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_REC_LEN    003F
    
    // Sensor Record Header
    0039            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    75              // Sensor Number
    
    // Record Body Bytes
    03              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    F1              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CF              // Type/Length Code
    'P2 Therm Margin'// String Bytes


_SDR_TYPE   01
_REC_LEN    003F
    
    // Sensor Record Header
    003A            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    78              // Sensor Number
    
    // Record Body Bytes
    03              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    01              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    00              // Nominal Reading
    14              // Normal Maximum
    00              // Normal Minimum
    64              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    32              // Upper critical
    1E              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CF              // Type/Length Code
    'P1 Therm Ctrl %'// String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_REC_LEN    003F
    
    // Sensor Record Header
    003B            // Record ID
    51              // SDR Version
    01              // Record Type
    3A              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    79              // Sensor Number
    
    // Record Body Bytes
    03              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    01              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    00              // Nominal Reading
    14              // Normal Maximum
    00              // Normal Minimum
    64              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    32              // Upper critical
    1E              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CF              // Type/Length Code
    'P2 Therm Ctrl %'// String Bytes


_SDR_TYPE   01
_REC_LEN    0040
    
    // Sensor Record Header
    003C            // Record ID
    51              // SDR Version
    01              // Record Type
    3B              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    83              // Sensor Number
    
    // Record Body Bytes
    03              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    F1              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    0F              // Upper critical
    0A              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    D0              // Type/Length Code
    'P1 DTS Therm Mgn'// String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_REC_LEN    0040
    
    // Sensor Record Header
    003D            // Record ID
    51              // SDR Version
    01              // Record Type
    3B              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    84              // Sensor Number
    
    // Record Body Bytes
    03              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    F1              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    0F              // Upper critical
    0A              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    D0              // Type/Length Code
    'P2 DTS Therm Mgn'// String Bytes


_SDR_TYPE   01
_REC_LEN    003E
    
    // Sensor Record Header
    003E            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    85              // Sensor Number
    
    // Record Body Bytes
    03              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    F1              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    0F              // Upper critical
    0A              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysterisis value
    02              // Negative hysterisis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM used for filtering [7:5]=Type(001=Median, 010=Mean)[4:0]=Sample Count
    CE              // Type/Length Code
    'P1 Temperature'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_REC_LEN    003E
    
    // Sensor Record Header
    003F            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    86              // Sensor Number
    
    // Record Body Bytes
    03              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    F1              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    0F              // Upper critical
    0A              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysterisis value
    02              // Negative hysterisis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM used for filtering [7:5]=Type(001=Median, 010=Mean)[4:0]=Sample Count
    CE              // Type/Length Code
    'P2 Temperature'   // String Bytes


_SDR_TYPE   01
_REC_LEN  003E
    
    // Sensor Record Header
    0040            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    B0              // Sensor Number
    
    // Record Body Bytes
    08              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    EC              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    0A              // Upper critical
    05              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CE              // Type/Length Code
    'P1 DIMM Thrm 1'// String Bytes


_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'OTHER'
_SDR_TAG    'TEST_PLATE'
_REC_LEN  003E
    
    // Sensor Record Header
    0041            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    B1              // Sensor Number
    
    // Record Body Bytes
    08              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    EC              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    0A              // Upper critical
    05              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CE              // Type/Length Code
    'P1 DIMM Thrm 2'// String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_REC_LEN  003E
    
    // Sensor Record Header
    0042            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    B2              // Sensor Number
    
    // Record Body Bytes
    08              // Entity ID
    03              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8002            // Assertion Event Mask
    8032            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    EC              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    0A              // Upper critical
    05              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CE              // Type/Length Code
    'P2 DIMM Thrm 1'// String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_REC_LEN  003E
    
    // Sensor Record Header
    0043            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    B3              // Sensor Number
    
    // Record Body Bytes
    08              // Entity ID
    04              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    1818            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    EC              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    0A              // Upper critical
    05              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CE              // Type/Length Code
    'P2 DIMM Thrm 2'// String Bytes


_SDR_TYPE   01
_SDR_TAG  'BCP_2U4N'
_REC_LEN    0040
    
    // Sensor Record Header
    0046            // Record ID
    51              // SDR Version
    01              // Record Type
    3B              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    C8              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    EC              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    D0              // Type/Length Code
    'Agg Therm Mrgn 1'// String Bytes


_SDR_TYPE   01
_SDR_TAG  'BCP_2U4N'
_REC_LEN    0040
    
    // Sensor Record Header
    013E            // Record ID
    51              // SDR Version
    01              // Record Type
    3B              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    C9              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    EC              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    D0              // Type/Length Code
    'Agg Therm Mrgn 2'// String Bytes


_SDR_TYPE  01
_SDR_TAG  'BCP_2U4N'
_SDR_TAG  'TEST_PLATE'
_REC_LEN  0039
    // Sensor Record Header
    0047            // Record ID
    51              // SDR Version
    01              // Record Type
    34              // Record Length
 
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    21              // Sensor Number
 
    // Record Body Bytes
    0F              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    FE              // B
    C0              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    1B              // Nominal Reading
    2F              // Normal Maximum
    11              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    39              // Upper critical
    34              // Upper non-critical
    00              // Lower non-recoverable
    07              // Lower critical
    0C              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    C9              // Type/Length Code
    'HSBP Temp'// String Bytes

_SDR_TYPE   01
_SDR_TAG    'RISER_1_FRU'
_REC_LEN    003C
    
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    01              // Record Type
    37              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    27              // Sensor Number
    
    // Record Body Bytes
    10              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    28              // Nominal Reading
    46              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    50              // Upper critical
    4B              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CC              // Type/Length Code
    'Riser 1 Temp'  // String Bytes

_SDR_TYPE   01
_SDR_TAG    'RISER_2_FRU'
_REC_LEN    003C
    
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    01              // Record Type
    37              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    2C              // Sensor Number
    
    // Record Body Bytes
    10              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    28              // Nominal Reading
    46              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    50              // Upper critical
    4B              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CC              // Type/Length Code
    'Riser 2 Temp'  // String Bytes


_SDR_TYPE   01
_REC_LEN    0039
    
    // Sensor Record Header
    0048            // Record ID
    51              // SDR Version
    01              // Record Type
    34              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    D0              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    37              // M
    00              // M, Tolerance
    26              // B
    C0              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    D0              // R exp, B exp
    07              // Analog characteristic flags
    E0              // Nominal Reading
    EB              // Normal Maximum
    D5              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    C6              // Lower critical
    CC              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    C9              // Type/Length Code
    'BB +12.0V'     // String Bytes


_SDR_TYPE   01
_REC_LEN    003D
    
    // Sensor Record Header
    0049            // Record ID
    51              // SDR Version
    01              // Record Type
    38              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    DE              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0530            // Assertion Event Mask
    0500            // Deassertion Event Mask
    0303            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    82              // M
    00              // M, Tolerance
    41              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    C0              // R exp, B exp
    07              // Analog characteristic flags
    E5              // Nominal Reading
    F1              // Normal Maximum
    C3              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    00              // Upper non-recoverable
    FC              // Upper critical
    FA              // Upper non-critical
    00              // Lower non-recoverable
    A3              // Lower critical
    BC              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    25              // OEM
    CD              // Type/Length Code
    'BB +3.3V Vbat' // String Bytes


_SDR_TYPE   01
_REC_LEN    003E
 
    // Sensor Record Header
    011F            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
  
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    45              // Sensor Number
  
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    50              // Nominal Reading
    69              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    73              // Upper critical
    6E              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CE              // Type/Length Code
    'Mem 1 VRD Temp'// String Bytes

 
_SDR_TYPE   01
_REC_LEN    003E
 
    // Sensor Record Header
    0120            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
  
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    46              // Sensor Number
  
    // Record Body Bytes
    07              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    50              // Nominal Reading
    69              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    73              // Upper critical
    6E              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    CE              // Type/Length Code
    'Mem 2 VRD Temp'// String Bytes
 
 
_SDR_TYPE  01
_REC_LEN  003E

    // Sensor Record Header
    0121            // Record ID
    51              // SDR Version
    01              // Record Type
    39              // Record Length
     
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    44              // Sensor Number
     
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    8532            // Assertion Event Mask
    8532            // Deassertion Event Mask
    1B1B            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    50              // Nominal Reading
    69              // Normal Maximum
    0F              // Normal Minimum
    7F              // Sensor Maximum Reading
    80              // Sensor Minimum Reading
    00              // Upper non-recoverable
    73              // Upper critical
    6E              // Upper non-critical
    00              // Lower non-recoverable
    05              // Lower critical
    0A              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte
    25              // OEM
    CE              // Type/Length Code
    'EV CPU1VR Temp'// String Bytes


_SDR_TYPE   02
_REC_LEN    002F
    
    // Sensor Record Header
    004A            // Record ID
    51              // SDR Version
    02              // Record Type
    2A              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    01              // Sensor Number
    
    // Record Body Bytes
    15              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    09              // Sensor Type
    6F              // Event / Reading Base Type
    7500            // Assertion Event Mask
    7500            // Deassertion Event Mask
    7500            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'Pwr Unit Status'// String Bytes


_SDR_TYPE   02
_SDR_TAG    'STICKY_REDUNDANT_PS'
_REC_LEN    002F
    
    // Sensor Record Header
    004B            // Record ID
    51              // SDR Version
    02              // Record Type
    2A              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    02              // Sensor Number
    
    // Record Body Bytes
    15              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    00              // Sensor Capabilities
    09              // Sensor Type
    0B              // Event / Reading Base Type
    FF00            // Assertion Event Mask
    FF00            // Deassertion Event Mask
    FF00            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'Pwr Unit Redund'// String Bytes


_SDR_TYPE   02
_REC_LEN    002D
    
    // Sensor Record Header
    004C            // Record ID
    51              // SDR Version
    02              // Record Type
    28              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    03              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    23              // Sensor Type
    6F              // Event / Reading Base Type
    0F01            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0F01            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CD              // Type/Length Code
    'IPMI Watchdog' // String Bytes


_SDR_TYPE   02
_SDR_TAG    'INTRUSION'
_REC_LEN    002E
    
    // Sensor Record Header
    004D            // Record ID
    51              // SDR Version
    02              // Record Type
    29              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    04              // Sensor Number
    
    // Record Body Bytes
    17              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    05              // Sensor Type
    6F              // Event / Reading Base Type
    1100            // Assertion Event Mask
    1100            // Deassertion Event Mask
    1100            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CE              // Type/Length Code
    'Physical Scrty'// String Bytes


_SDR_TYPE   02
_SDR_TAG    'NO_INTRUSION'
_REC_LEN    002E
    
    // Sensor Record Header
    004E            // Record ID
    51              // SDR Version
    02              // Record Type
    29              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    04              // Sensor Number
    
    // Record Body Bytes
    17              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    05              // Sensor Type
    6F              // Event / Reading Base Type
    1000            // Assertion Event Mask
    1000            // Deassertion Event Mask
    1000            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CE              // Type/Length Code
    'Physical Scrty'// String Bytes


_SDR_TYPE   02
_SDR_TAG    'FP_NMI'
_REC_LEN    002F
    
    // Sensor Record Header
    004F            // Record ID
    51              // SDR Version
    02              // Record Type
    2A              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    05              // Sensor Number
    
    // Record Body Bytes
    0C              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    13              // Sensor Type
    6F              // Event / Reading Base Type
    0100            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0100            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'FP NMI Diag Int'// String Bytes


_SDR_TYPE   02
_REC_LEN    002B
    
    // Sensor Record Header
    0050            // Record ID
    51              // SDR Version
    02              // Record Type
    26              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    06              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    F3              // Sensor Type
    03              // Event / Reading Base Type
    0200            // Assertion Event Mask
    0200            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CB              // Type/Length Code
    'SMI Timeout'   // String Bytes


_SDR_TYPE   02
_REC_LEN    0030
    
    // Sensor Record Header
    0051            // Record ID
    51              // SDR Version
    02              // Record Type
    2B              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    07              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    10              // Sensor Type
    6F              // Event / Reading Base Type
    0400            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0400            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    D0              // Type/Length Code
    'System Event Log'// String Bytes


_SDR_TYPE   02
_REC_LEN    002C
    
    // Sensor Record Header
    0052            // Record ID
    51              // SDR Version
    02              // Record Type
    27              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    08              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    12              // Sensor Type
    6F              // Event / Reading Base Type
    1000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    1000            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'System Event'  // String Bytes


_SDR_TYPE   02
_REC_LEN    0026
    
    // Sensor Record Header
    0053            // Record ID
    51              // SDR Version
    02              // Record Type
    21              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    09              // Sensor Number
    
    // Record Body Bytes
    0C              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    14              // Sensor Type
    6F              // Event / Reading Base Type
    0500            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0500            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    C6              // Type/Length Code
    'Button'        // String Bytes


_SDR_TYPE   02
_REC_LEN    002C
    
    // Sensor Record Header
    0054            // Record ID
    51              // SDR Version
    02              // Record Type
    27              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    0A              // Sensor Number
    
    // Record Body Bytes
    2E              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    28              // Sensor Type
    03              // Event / Reading Base Type
    0200            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'BMC Watchdog'  // String Bytes


_SDR_TYPE   02
_REC_LEN    002B
    
    // Sensor Record Header
    0055            // Record ID
    51              // SDR Version
    02              // Record Type
    26              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    0B              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    00              // Sensor Capabilities
    02              // Sensor Type
    03              // Event / Reading Base Type
    0200            // Assertion Event Mask
    0200            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CB              // Type/Length Code
    'VR Watchdog'   // String Bytes


_SDR_TYPE   02
_REC_LEN    002E
    
    // Sensor Record Header
    0056            // Record ID
    51              // SDR Version
    02              // Record Type
    29              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    0D              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    00              // Sensor Capabilities
    19              // Sensor Type (chipset)
    6F              // Event / Reading Base Type
    0200            // Assertion Event Mask
    0200            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CE              // Type/Length Code
    'SSB Therm Trip'// String Bytes


_SDR_TYPE   02
_REC_LEN    002D
    
    // Sensor Record Header
    0059            // Record ID
    51              // SDR Version
    02              // Record Type
    28              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    10              // Sensor Number
    
    // Record Body Bytes
    2E              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    28              // Sensor Type
    6F              // Event / Reading Base Type
    1000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    1000            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CD              // Type/Length Code
    'BMC FW Health' // String Bytes


_SDR_TYPE   02
_REC_LEN    002F
    
    // Sensor Record Header
    005A            // Record ID
    51              // SDR Version
    02              // Record Type
    2A              // Record Length
    
    // Record Key Bytes
    2C              // Sensor Owner ID
    60              // Sensor Owner LUN
    1A              // Sensor Number
    
    // Record Body Bytes
    2E              // Entity ID
    02              // Entity Instance
    41              // Sensor Initialization
    C3              // Sensor Capabilities
    DC              // Sensor Type
    74              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0700            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0000            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'NM Capabilities'// String Bytes


_SDR_TYPE   02
_REC_LEN    002D
  
    // Sensor Record Header
    0063            // Record ID
    51              // SDR Version
    02              // Record Type
    28              // Record Length
  
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    B8              // Sensor Number
  
    // Record Body Bytes
    15              // Entity ID
    03              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    09              // Sensor Type
    03              // Event / Reading Base Type
    0200            // Assertion Event Mask   --State asserted =0200
    0200            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CD              // Type/Length Code
    'Auto Shutdown' // String Bytes


_SDR_TYPE   02
_SDR_TAG    'STICKY_PS1_2130W'
_SDR_TAG    'STICKY_PS1'
_REC_LEN    002A
    
    // Sensor Record Header
    005B            // Record ID
    51              // SDR Version
    02              // Record Type
    25              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    50              // Sensor Number
    
    // Record Body Bytes
    0A              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    08              // Sensor Type
    6F              // Event / Reading Base Type
    4F00            // Assertion Event Mask
    4F00            // Deassertion Event Mask
    4F00            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CA              // Type/Length Code
    'PS1 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'STICKY_PS2_2130W'
_SDR_TAG    'STICKY_PS2'
_REC_LEN    002A
    
    // Sensor Record Header
    005C            // Record ID
    51              // SDR Version
    02              // Record Type
    25              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    51              // Sensor Number
    
    // Record Body Bytes
    0A              // Entity ID
    02              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    08              // Sensor Type
    6F              // Event / Reading Base Type
    4F00            // Assertion Event Mask
    4F00            // Deassertion Event Mask
    4F00            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CA              // Type/Length Code
    'PS2 Status'    // String Bytes


_SDR_TYPE   02
_REC_LEN    0029
    
    // Sensor Record Header
    005D            // Record ID
    51              // SDR Version
    02              // Record Type
    24              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    70              // Sensor Number
    
    // Record Body Bytes
    03              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    00              // Sensor Capabilities
    07              // Sensor Type
    6F              // Event / Reading Base Type
    A300            // Assertion Event Mask
    A300            // Deassertion Event Mask
    A300            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    C9              // Type/Length Code
    'P1 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_REC_LEN    0029
    
    // Sensor Record Header
    005E            // Record ID
    51              // SDR Version
    02              // Record Type
    24              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    71              // Sensor Number
    
    // Record Body Bytes
    03              // Entity ID
    02              // Entity Instance
    67              // Sensor Initialization
    00              // Sensor Capabilities
    07              // Sensor Type
    6F              // Event / Reading Base Type
    A300            // Assertion Event Mask
    A300            // Deassertion Event Mask
    A300            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    C9              // Type/Length Code
    'P2 Status'     // String Bytes


_SDR_TYPE   02
_REC_LEN    0028
    
    // Sensor Record Header
    005F            // Record ID
    51              // SDR Version
    02              // Record Type
    23              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    7C              // Sensor Number
    
    // Record Body Bytes
    03              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    41              // Sensor Capabilities
    07              // Sensor Type
    03              // Event / Reading Base Type
    0200            // Assertion Event Mask
    0200            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    C8              // Type/Length Code
    'CPU ERR2'      // String Bytes


_SDR_TYPE   02
_REC_LEN    002B
    
    // Sensor Record Header
    0061            // Record ID
    51              // SDR Version
    02              // Record Type
    26              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    82              // Sensor Number
    
    // Record Body Bytes
    03              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    00              // Sensor Capabilities
    07              // Sensor Type
    03              // Event / Reading Base Type
    0200            // Assertion Event Mask
    0200            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CB              // Type/Length Code
    'CPU Missing'   // String Bytes


_SDR_TYPE   02
_REC_LEN    0027
    
    // Sensor Record Header
    0062            // Record ID
    51              // SDR Version
    02              // Record Type
    22              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    90              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    01              // Sensor Type
    05              // Event / Reading Base Type
    0200            // Assertion Event Mask
    0200            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    C7              // Type/Length Code
    'VRD Hot'       // String Bytes


_SDR_TYPE   01
_SDR_TAG    'ENABLE_NVME_FUNCTIONS'
_REC_LEN    0040
    
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    01              // Record Type
    3B              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    91              // Sensor Number
    
    // Record Body Bytes
    0C              // Entity ID
    02              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    01              // Sensor Type
    01              // Event / Reading Base Type
    0002            // Assertion Event Mask
    0002            // Deassertion Event Mask
    1010            // Reading Mask & Settable / Readable Threshold Masks
    80              // Sensor Units 1
    01              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    01              // M
    00              // M, Tolerance
    00              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    00              // R exp, B exp
    07              // Analog characteristic flags
    EC              // Nominal Reading
    00              // Normal Maximum
    BA              // Normal Minimum
    7F              // Sensor Maximum Reading
    82              // Sensor Minimum Reading
    00              // Upper non-recoverable
    00              // Upper critical
    00              // Upper non-critical
    00              // Lower non-recoverable
    00              // Lower critical
    00              // Lower non-critical
    02              // Positive hysteresis value
    02              // Negative hysteresis value
    00              // Reserved Byte
    00              // Reserved Byte 
    00              // OEM
    D0              // Type/Length Code
    'NVMe 1 Therm Mgn'// String Bytes


_SDR_TYPE   02
_SDR_TAG    'ENABLE_NVME_FUNCTIONS'
_REC_LEN    0030
    
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    02              // Record Type
    2B              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    94              // Sensor Number
    
    // Record Body Bytes
    0F              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    0D              // Sensor Type
    73              // Event / Reading Base Type
    FF00            // Assertion Event Mask
    FF00            // Deassertion Event Mask
    FF00            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    D0              // Type/Length Code
    'NVMe 1 Crit Warn'// String Bytes


_SDR_TYPE   02
_SDR_TAG    'STICKY_PS1_2130W'
_SDR_TAG    'STICKY_PS1'
_REC_LEN    002D
    
    // Sensor Record Header
    0063            // Record ID
    51              // SDR Version
    02              // Record Type
    28              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    A0              // Sensor Number
    
    // Record Body Bytes
    0A              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    00              // Sensor Capabilities
    04              // Sensor Type
    03              // Event / Reading Base Type
    0200            // Assertion Event Mask
    0200            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CD              // Type/Length Code
    'PS1 Fan1 Fail' // String Bytes


_SDR_TYPE   02
_SDR_TAG    'STICKY_PS1_2130W'
_SDR_TAG    'STICKY_PS1'
_REC_LEN    002D
    
    // Sensor Record Header
    0063            // Record ID
    51              // SDR Version
    02              // Record Type
    28              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    A1              // Sensor Number
    
    // Record Body Bytes
    0A              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    00              // Sensor Capabilities
    04              // Sensor Type
    03              // Event / Reading Base Type
    0200            // Assertion Event Mask
    0200            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CD              // Type/Length Code
    'PS1 Fan2 Fail' // String Bytes


_SDR_TYPE   02
_SDR_TAG    'STICKY_PS2_2130W'
_SDR_TAG    'STICKY_PS2'
_REC_LEN    002D
    
    // Sensor Record Header
    0068            // Record ID
    51              // SDR Version
    02              // Record Type
    28              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    A4              // Sensor Number
    
    // Record Body Bytes
    0A              // Entity ID
    03              // Entity Instance
    67              // Sensor Initialization
    00              // Sensor Capabilities
    04              // Sensor Type
    03              // Event / Reading Base Type
    0200            // Assertion Event Mask
    0200            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CD              // Type/Length Code
    'PS2 Fan1 Fail' // String Bytes


_SDR_TYPE   02
_SDR_TAG    'STICKY_PS2_2130W'
_SDR_TAG    'STICKY_PS2'
_REC_LEN    002D
    
    // Sensor Record Header
    0068            // Record ID
    51              // SDR Version
    02              // Record Type
    28              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    A5              // Sensor Number
    
    // Record Body Bytes
    0A              // Entity ID
    03              // Entity Instance
    67              // Sensor Initialization
    00              // Sensor Capabilities
    04              // Sensor Type
    03              // Event / Reading Base Type
    0200            // Assertion Event Mask
    0200            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CD              // Type/Length Code
    'PS2 Fan2 Fail' // String Bytes


_SDR_TYPE   02
_REC_LEN    0030
    
    // Sensor Record Header
    0069            // Record ID
    51              // SDR Version
    02              // Record Type
    2B              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    C0              // Sensor Number
    
    // Record Body Bytes
    20              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    00              // Sensor Capabilities
    0C              // Sensor Type
    6F              // Event / Reading Base Type
    0004            // Assertion Event Mask
    0004            // Deassertion Event Mask
    0004            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    D0              // Type/Length Code
    'Mem P1 Thrm Trip'// String Bytes


_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_REC_LEN    0030
    
    // Sensor Record Header
    006A            // Record ID
    51              // SDR Version
    02              // Record Type
    2B              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    C1              // Sensor Number
    
    // Record Body Bytes
    20              // Entity ID
    02              // Entity Instance
    67              // Sensor Initialization
    00              // Sensor Capabilities
    0C              // Sensor Type
    6F              // Event / Reading Base Type
    0004            // Assertion Event Mask
    0004            // Deassertion Event Mask
    0004            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    D0              // Type/Length Code
    'Mem P2 Thrm Trip'// String Bytes


_SDR_TYPE   02
_REC_LEN    002D
    
    // Sensor Record Header
    006B            // Record ID
    51              // SDR Version
    02              // Record Type
    28              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    D1              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    02              // Sensor Type
    03              // Event / Reading Base Type
    0200            // Assertion Event Mask
    0200            // Deassertion Event Mask
    0200            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CD              // Type/Length Code
    'Voltage Fault' // String Bytes

_SDR_TYPE   02
_REC_LEN    002C
    
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    02              // Record Type
    27              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    DB              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    67              // Sensor Initialization
    40              // Sensor Capabilities
    DB              // Sensor Type
    7B              // Event / Reading Base Type
    1F00            // Assertion Event Mask
    1F00            // Deassertion Event Mask
    1F00            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'Remote Debug'  // String Bytes


_SDR_TYPE   02
_SDR_TAG    'BCP_2U4N'
_REC_LEN    002C
    
    // Sensor Record Header
    006C            // Record ID
    51              // SDR Version
    02              // Record Type
    27              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    F0              // Sensor Number
    
    // Record Body Bytes
    04              // Entity ID
    01              // Entity Instance
    6D              // Sensor Initialization
    40              // Sensor Capabilities
    0D              // Sensor Type
    6F              // Event / Reading Base Type
    8300            // Assertion Event Mask
    8300            // Deassertion Event Mask
    8300            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'HDD 0 Status'  // String Bytes


_SDR_TYPE   02
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '24HDDHSBP'
_SDR_TAG    'BP_X35_LC'
_SDR_TAG    '24HDD_LC'
_REC_LEN    002C
    
    // Sensor Record Header
    006D            // Record ID
    51              // SDR Version
    02              // Record Type
    27              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    F1              // Sensor Number
    
    // Record Body Bytes
    04              // Entity ID
    02              // Entity Instance
    6D              // Sensor Initialization
    40              // Sensor Capabilities
    0D              // Sensor Type
    6F              // Event / Reading Base Type
    8300            // Assertion Event Mask
    8300            // Deassertion Event Mask
    8300            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'HDD 1 Status'  // String Bytes


_SDR_TYPE   02
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '24HDDHSBP'
_SDR_TAG    'BP_X35_LC'
_SDR_TAG    '24HDD_LC'
_REC_LEN    002C
    
    // Sensor Record Header
    006E            // Record ID
    51              // SDR Version
    02              // Record Type
    27              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    F2              // Sensor Number
    
    // Record Body Bytes
    04              // Entity ID
    03              // Entity Instance
    6D              // Sensor Initialization
    40              // Sensor Capabilities
    0D              // Sensor Type
    6F              // Event / Reading Base Type
    8300            // Assertion Event Mask
    8300            // Deassertion Event Mask
    8300            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'HDD 2 Status'  // String Bytes


_SDR_TYPE   02
_SDR_TAG    '24HDDHSBP'
_SDR_TAG    '24HDD_LC'
_REC_LEN    002C
    
    // Sensor Record Header
    006F            // Record ID
    51              // SDR Version
    02              // Record Type
    27              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    F3              // Sensor Number
    
    // Record Body Bytes
    04              // Entity ID
    04              // Entity Instance
    6D              // Sensor Initialization
    40              // Sensor Capabilities
    0D              // Sensor Type
    6F              // Event / Reading Base Type
    8300            // Assertion Event Mask
    8300            // Deassertion Event Mask
    8300            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'HDD 3 Status'  // String Bytes


_SDR_TYPE   02
_SDR_TAG    '24HDDHSBP'
_SDR_TAG    '24HDD_LC'
_REC_LEN    002C
    
    // Sensor Record Header
    0070            // Record ID
    51              // SDR Version
    02              // Record Type
    27              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    F4              // Sensor Number
    
    // Record Body Bytes
    04              // Entity ID
    05              // Entity Instance
    6D              // Sensor Initialization
    40              // Sensor Capabilities
    0D              // Sensor Type
    6F              // Event / Reading Base Type
    8300            // Assertion Event Mask
    8300            // Deassertion Event Mask
    8300            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'HDD 4 Status'  // String Bytes


_SDR_TYPE   02
_SDR_TAG    '24HDDHSBP'
_SDR_TAG    '24HDD_LC'
_REC_LEN    002C
    
    // Sensor Record Header
    0071            // Record ID
    51              // SDR Version
    02              // Record Type
    27              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    F5              // Sensor Number
    
    // Record Body Bytes
    04              // Entity ID
    06              // Entity Instance
    6D              // Sensor Initialization
    40              // Sensor Capabilities
    0D              // Sensor Type
    6F              // Event / Reading Base Type
    8300            // Assertion Event Mask
    8300            // Deassertion Event Mask
    8300            // Reading Mask & Settable / Readable Threshold Masks
    C0              // Sensor Units 1
    00              // Sensor Units 2
    00              // Sensor Units 3
    0100            // Sensor Record Sharing
    00              // Positive-going Threshold Hysteresis
    00              // Negative-going Threshold Hysteresis
    00              // Reserved
    00              // Reserved
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'HDD 5 Status'  // String Bytes




_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0107            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    01              // Sensor Number
    
    // Record Body Bytes
    22              // Entity ID
    01              // Entity Instance
    0C              // Sensor Type
    0B              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'Mem Rdnc Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0073            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    02              // Sensor Number
    
    // Record Body Bytes
    20              // Entity ID
    01              // Entity Instance
    0C              // Sensor Type
    6F              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'Mmry ECC Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0074            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    01              // Sensor Owner ID
    00              // Sensor Owner LUN
    02              // Sensor Number
    
    // Record Body Bytes
    20              // Entity ID
    01              // Entity Instance
    0C              // Sensor Type
    09              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'Mem Conf Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0075            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    03              // Sensor Number
    
    // Record Body Bytes
    30              // Entity ID
    01              // Entity Instance
    13              // Sensor Type
    6F              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'PCI Lgcy Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    0021
    
    // Sensor Record Header
    0076            // Record ID
    51              // SDR Version
    03              // Record Type
    1C              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    04              // Sensor Number
    
    // Record Body Bytes
    31              // Entity ID
    01              // Entity Instance
    13              // Sensor Type
    70              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    D0              // Type/Length Code
    'PCIe Fatal Error'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0077            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    05              // Sensor Number
    
    // Record Body Bytes
    31              // Entity ID
    01              // Entity Instance
    13              // Sensor Type
    71              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'PCIe Cor Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0078            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    01              // Sensor Owner ID
    00              // Sensor Owner LUN
    06              // Sensor Number
    
    // Record Body Bytes
    22              // Entity ID
    01              // Entity Instance
    0F              // Sensor Type
    6F              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'POST Err Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0079            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    06              // Sensor Number
    
    // Record Body Bytes
    2B              // Entity ID
    01              // Entity Instance
    13              // Sensor Type
    72              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'UPI Corr Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    007A            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    07              // Sensor Number
    
    // Record Body Bytes
    2B              // Entity ID
    01              // Entity Instance
    13              // Sensor Type
    73              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'UPI Fatl Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    001F
    
    // Sensor Record Header
    007B            // Record ID
    51              // SDR Version
    03              // Record Type
    1A              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    08              // Sensor Number
    
    // Record Body Bytes
    31              // Entity ID
    01              // Entity Instance
    19              // Sensor Type
    75              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CE              // Type/Length Code
    'Chipset Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    001F
    
    // Sensor Record Header
    007C            // Record ID
    51              // SDR Version
    03              // Record Type
    1A              // Record Length
    
    // Record Key Bytes
    01              // Sensor Owner ID
    00              // Sensor Owner LUN
    09              // Sensor Number
    
    // Record Body Bytes
    2B              // Entity ID
    05              // Entity Instance
    13              // Sensor Type
    77              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CE              // Type/Length Code
    'UPI Link Width'// String Bytes


_SDR_TYPE   03
_REC_LEN    001F
    
    // Sensor Record Header
    007D            // Record ID
    51              // SDR Version
    03              // Record Type
    1A              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    10              // Sensor Number
    
    // Record Body Bytes
    20              // Entity ID
    01              // Entity Instance
    0C              // Sensor Type
    7F              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CE              // Type/Length Code
    'Mem err Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    001D
    
    // Sensor Record Header
    007E            // Record ID
    51              // SDR Version
    03              // Record Type
    18              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    11              // Sensor Number
    
    // Record Body Bytes
    2B              // Entity ID
    01              // Entity Instance
    0C              // Sensor Type
    0B              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'Sparing Rdnc'  // String Bytes


_SDR_TYPE   03
_REC_LEN    0021
    
    // Sensor Record Header
    007F            // Record ID
    51              // SDR Version
    03              // Record Type
    1C              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    12              // Sensor Number
    
    // Record Body Bytes
    2E              // Entity ID
    01              // Entity Instance
    2B              // Sensor Type
    70              // Event/Reading Type Code
    0000            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    D0              // Type/Length Code
    'FW Update Status'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0080            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    01              // Sensor Owner ID
    00              // Sensor Owner LUN
    12              // Sensor Number
    
    // Record Body Bytes
    2B              // Entity ID
    01              // Entity Instance
    0C              // Sensor Type
    09              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'Rdnc Mod Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0081            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    13              // Sensor Number
    
    // Record Body Bytes
    20              // Entity ID
    01              // Entity Instance
    0C              // Sensor Type
    6F              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'Mmry Parity Err'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0082            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    14              // Sensor Number
    
    // Record Body Bytes
    31              // Entity ID
    01              // Entity Instance
    13              // Sensor Type
    76              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'PCIe Fat Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    001E
    
    // Sensor Record Header
    0083            // Record ID
    51              // SDR Version
    03              // Record Type
    19              // Record Length
    
    // Record Key Bytes
    2C              // Sensor Owner ID
    60              // Sensor Owner LUN
    17              // Sensor Number
    
    // Record Body Bytes
    2E              // Entity ID
    02              // Entity Instance
    DC              // Sensor Type
    75              // Event/Reading Type Code
    0000            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CD              // Type/Length Code
    'SPS FW Health' // String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0084            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    17              // Sensor Number
    
    // Record Body Bytes
    2B              // Entity ID
    01              // Entity Instance
    13              // Sensor Type
    74              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'UPI Fatl Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    001D
    
    // Sensor Record Header
    0085            // Record ID
    51              // SDR Version
    03              // Record Type
    18              // Record Length
    
    // Record Key Bytes
    2C              // Sensor Owner ID
    60              // Sensor Owner LUN
    18              // Sensor Number
    
    // Record Body Bytes
    2E              // Entity ID
    02              // Entity Instance
    DC              // Sensor Type
    72              // Event/Reading Type Code
    0000            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'NM Exception'  // String Bytes


_SDR_TYPE   03
_REC_LEN    001A
    
    // Sensor Record Header
    0086            // Record ID
    51              // SDR Version
    03              // Record Type
    15              // Record Length
    
    // Record Key Bytes
    2C              // Sensor Owner ID
    60              // Sensor Owner LUN
    19              // Sensor Number
    
    // Record Body Bytes
    2E              // Entity ID
    02              // Entity Instance
    DC              // Sensor Type
    73              // Event/Reading Type Code
    0000            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    C9              // Type/Length Code
    'NM Health'     // String Bytes


_SDR_TYPE   03
_REC_LEN    001D
    
    // Sensor Record Header
    0087            // Record ID
    51              // SDR Version
    03              // Record Type
    18              // Record Length
    
    // Record Key Bytes
    2C              // Sensor Owner ID
    60              // Sensor Owner LUN
    1B              // Sensor Number
    
    // Record Body Bytes
    2E              // Entity ID
    02              // Entity Instance
    DC              // Sensor Type
    72              // Event/Reading Type Code
    0000            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'NM Threshold'  // String Bytes


_SDR_TYPE   03
_REC_LEN    001F
    
    // Sensor Record Header
    0088            // Record ID
    51              // SDR Version
    03              // Record Type
    1A              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    81              // Sensor Number
    
    // Record Body Bytes
    2E              // Entity ID
    01              // Entity Instance
    28              // Sensor Type
    03              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CE              // Type/Length Code
    'MTM Lvl Change'// String Bytes


_SDR_TYPE   03
_REC_LEN    001C

    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    03              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    1A              // Sensor Number
   
    // Record Body Bytes
    2E              // Entity ID
    01              // Entity Instance
    C3              // Sensor Type
    71              // Event/Reading Type Code
    0000            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CB              // Type/Length Code
    'FW Security'   // String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    01              // Sensor Owner ID
    00              // Sensor Owner LUN
    83              // Sensor Number
    
    // Record Body Bytes
    22              // Entity ID
    01              // Entity Instance
    12              // Sensor Type
    6F              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'BIOS Evt Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0089            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    83              // Sensor Number
    
    // Record Body Bytes
    22              // Entity ID
    01              // Entity Instance
    12              // Sensor Type
    6F              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'BIOS Evt Sensor'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0089            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    33              // Sensor Owner ID
    00              // Sensor Owner LUN
    83              // Sensor Number
    
    // Record Body Bytes
    2B              // Entity ID
    01              // Entity Instance
    12              // Sensor Type
    6F              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'BIOS Evt Sensor'// String Bytes


_SDR_TYPE   03
_SDR_TAG 'BCP_2U4N'
_SDR_TAG 'TEST_PLATE'
_REC_LEN    001F
    
    // Sensor Record Header
    008A            // Record ID
    51              // SDR Version
    03              // Record Type
    1A              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    87              // Sensor Number
    
    // Record Body Bytes
    2E              // Entity ID
    01              // Entity Instance
    28              // Sensor Type
    03              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CE              // Type/Length Code
    'AutoCfg Status'// String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    008B            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    2C              // Sensor Owner ID
    60              // Sensor Owner LUN
    B2              // Sensor Number
    
    // Record Body Bytes
    2E              // Entity ID
    02              // Entity Instance
    DC              // Sensor Type
    03              // Event/Reading Type Code
    0000            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'SmaRT-CLST Stat'// String Bytes


_SDR_TYPE   03
_REC_LEN    001D
    
    // Sensor Record Header
    008C            // Record ID
    51              // SDR Version
    03              // Record Type
    18              // Record Length
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    D7              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    2A              // Sensor Type
    6F              // Event/Reading Type Code
    0000            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CC              // Type/Length Code
    'Bad User PWD'  // String Bytes


_SDR_TYPE   03
_REC_LEN    0020
    
    // Sensor Record Header
    0072            // Record ID
    51              // SDR Version
    03              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    41              // Sensor Owner ID
    00              // Sensor Owner LUN
    00              // Sensor Number
    
    // Record Body Bytes
    21              // Entity ID
    01              // Entity Instance
    20              // Sensor Type
    04              // Event/Reading Type Code
    0100            // Sensor Record Sharing
    00              // Reserved
    00              // OEM
    CF              // Type/Length Code
    'OS Event Sensor'// String Bytes


_SDR_TYPE   11
_REC_LEN    0019
    
    // Sensor Record Header
    008D            // Record ID
    51              // SDR Version
    11              // Record Type
    14              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    00              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    07              // FRU Entity ID
    01              // FRU Entity Instance
    00              // OEM
    C9              // Type/Length Code
    'Baseboard'     // String Bytes


_SDR_TYPE   11
_SDR_TAG    'BCP_2U4N'
_REC_LEN    001C
    
    // Sensor Record Header
    008E            // Record ID
    51              // SDR Version
    11              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    08              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    0F              // FRU Entity ID
    01              // FRU Entity Instance
    00              // OEM
    CC              // Type/Length Code
    'HS Backplane'// String Bytes


_SDR_TYPE   11
_SDR_TAG    'RISER_1_FRU'
_REC_LEN    001C
    
    // Sensor Record Header
    0090            // Record ID
    51              // SDR Version
    11              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    0B              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    10              // FRU Entity ID
    01              // FRU Entity Instance
    00              // OEM
    CC              // Type/Length Code
    'PCIe Riser 1'  // String Bytes


_SDR_TYPE   11
_SDR_TAG    'RISER_2_FRU'
_REC_LEN    001C
    
    // Sensor Record Header
    0091            // Record ID
    51              // SDR Version
    11              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    0C              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    10              // FRU Entity ID
    02              // FRU Entity Instance
    00              // OEM
    CC              // Type/Length Code
    'PCIe Riser 2'  // String Bytes


_SDR_TYPE   11
_SDR_TAG  'LSISAS3008_6PORT'
_REC_LEN    001E
    
    // Sensor Record Header
    0105            // Record ID
    51              // SDR Version
    11              // Record Type
    19              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    0D              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    10              // FRU Entity ID
    03              // FRU Entity Instance
    00              // OEM
    CE              // Type/Length Code
    '3008 Bdg Board'  // String Bytes


_SDR_TYPE   11
_SDR_TAG  'LSISAS3408'
_REC_LEN    001E
    
    // Sensor Record Header
    0092            // Record ID
    51              // SDR Version
    11              // Record Type
    19              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    0D              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    10              // FRU Entity ID
    03              // FRU Entity Instance
    00              // OEM
    CE              // Type/Length Code
    '3408 Bdg Board'  // String Bytes


_SDR_TYPE   11
_SDR_TAG  'PT_BRIDGE'
_REC_LEN    001C
    
    // Sensor Record Header
    0092            // Record ID
    51              // SDR Version
    11              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    0D              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    10              // FRU Entity ID
    03              // FRU Entity Instance
    00              // OEM
    CC              // Type/Length Code
    'PT Bdg Board'  // String Bytes


_SDR_TYPE   11
_SDR_TAG  'IFT_RISER1_AC'
_REC_LEN    001B
    
    // Sensor Record Header
    0092            // Record ID
    51              // SDR Version
    11              // Record Type
    16              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    10              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    10              // FRU Entity ID
    03              // FRU Entity Instance
    00              // OEM
    CB              // Type/Length Code
    'IFT Carrier'  // String Bytes


_SDR_TYPE   11
_SDR_TAG  'IFT_RISER1_A4'
_REC_LEN    001B
    
    // Sensor Record Header
    0092            // Record ID
    51              // SDR Version
    11              // Record Type
    16              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    11              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    10              // FRU Entity ID
    03              // FRU Entity Instance
    00              // OEM
    CB              // Type/Length Code
    'IFT Carrier'  // String Bytes


_SDR_TYPE   11
_SDR_TAG  'IFT_RISER2_AC'
_REC_LEN    001B
    
    // Sensor Record Header
    0092            // Record ID
    51              // SDR Version
    11              // Record Type
    16              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    12              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    10              // FRU Entity ID
    03              // FRU Entity Instance
    00              // OEM
    CB              // Type/Length Code
    'IFT Carrier'  // String Bytes


_SDR_TYPE   11
_SDR_TAG  'IFT_RISER2_A4'
_REC_LEN    001B
    
    // Sensor Record Header
    0092            // Record ID
    51              // SDR Version
    11              // Record Type
    16              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    13              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    10              // FRU Entity ID
    03              // FRU Entity Instance
    00              // OEM
    CB              // Type/Length Code
    'IFT Carrier'  // String Bytes


_SDR_TYPE   11
_SDR_TAG    'STICKY_PS1_2130W'
_SDR_TAG    'STICKY_PS1'
_REC_LEN    0020
    
    // Sensor Record Header
    0095            // Record ID
    51              // SDR Version
    11              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    02              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    0A              // FRU Entity ID
    01              // FRU Entity Instance
    00              // OEM
    D0              // Type/Length Code
    'Pwr Supply 1 FRU'// String Bytes


_SDR_TYPE   11
_SDR_TAG    'STICKY_PS2_2130W'
_SDR_TAG    'STICKY_PS2'
_REC_LEN    0020
    
    // Sensor Record Header
    0096            // Record ID
    51              // SDR Version
    11              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    03              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    0A              // FRU Entity ID
    02              // FRU Entity Instance
    00              // OEM
    D0              // Type/Length Code
    'Pwr Supply 2 FRU'// String Bytes


_SDR_TYPE   11
_SDR_TAG    'SSD_AIC_1'
_REC_LEN    001E
    
    // Sensor Record Header
    0098            // Record ID
    51              // SDR Version
    11              // Record Type
    19              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    12              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    0B              // FRU Entity ID
    01              // FRU Entity Instance
    00              // OEM
    CE              // Type/Length Code
    'PCIe SSD AIC 1'// String Bytes


_SDR_TYPE   11
_SDR_TAG    'SSD_AIC_2'
_REC_LEN    001E
    
    // Sensor Record Header
    0099            // Record ID
    51              // SDR Version
    11              // Record Type
    19              // Record Length
    
    // Record Key Bytes
    20              // Device Access Address
    13              // FRU Device ID / Device Slave Address
    80              // Access LUN / Bus ID
    00              // Channel Number
    
    // Record Body Bytes
    00              // Reserved
    10              // Device Type
    00              // Device Type Modifier
    0B              // FRU Entity ID
    02              // FRU Entity Instance
    00              // OEM
    CE              // Type/Length Code
    'PCIe SSD AIC 2'// String Bytes


_SDR_TYPE   12
_REC_LEN    0020
    
    // Sensor Record Header
    009C            // Record ID
    51              // SDR Version
    12              // Record Type
    1B              // Record Length
    
    // Record Key Bytes
    20              // Device Slave Address
    00              // Channel Number
    
    // Record Body Bytes
    08              // Power state notification
    BF              // Device capabilities
    00              // Reserved
    00              // Reserved
    00              // Reserved
    2E              // Entity ID
    01              // Entity instance
    00              // OEM
    D0              // Type/Length Code
    'Basbrd Mgmt Ctlr'// String Bytes


_SDR_TYPE   12
_REC_LEN    001B
    
    // Sensor Record Header
    009D            // Record ID
    51              // SDR Version
    12              // Record Type
    16              // Record Length
    
    // Record Key Bytes
    2C              // Device Slave Address
    06              // Channel Number
    
    // Record Body Bytes
    24              // Power state notification
    21              // Device capabilities
    00              // Reserved
    00              // Reserved
    00              // Reserved
    2E              // Entity ID
    02              // Entity instance
    00              // OEM
    CB              // Type/Length Code
    'Mgmt Engine'   // String Bytes


_SDR_TYPE   C0
_SDR_TAG    'STICKY_REDUNDANT_PS'
_REC_LEN    000E
    
    // Sensor Record Header
    009E            // Record ID
    51              // SDR Version
    C0              // Record Type
    09              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    02              // Record Subtype Value
    02              // Power Unit Redundancy sensor number
    00              // Bits [7:1]-Reserved; Bit[0]-1=No monitorable supplies present
    01              // The number of present and operational
    50              // Power Supply Status 1 Sensor Number
    51              // Power Supply Status 2 Sensor Number


_SDR_TYPE   C0
_REC_LEN    0018
    
    // Sensor Record Header
    00A3            // Record ID
    51              // SDR Version
    C0              // Record Type
    13              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    05              // Record Subtype Value
    
    // Fan Redundancy Map Record
    FF              // Fan Redundancy Sensor Number
    00              // Flags; [7:1]-Reserved; [0]-persistently stored event state, 1= store tis event state persistently
    0404            // Failed Event State Mask
    01              // Redundant Fan Count
    30              // Fan Speed Sensor
    00              // Fan Presence Sensor 
    32              // Fan Speed Sensor
    00              // Fan Presence Sensor 
    34              // Fan Speed Sensor
    00              // Fan Presence Sensor 
    36              // Fan Speed Sensor
    00              // Fan Presence Sensor 
    38              // Fan Speed Sensor
    00              // Fan Presence Sensor 


_SDR_TYPE   C0
_REC_LEN    0010
    
    // Sensor Record Header
    00A6            // Record ID
    51              // SDR Version
    C0              // Record Type
    0B              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    09              // Record Subtype Value
    
    // Voltage Sensor Scaling
    02              // Number of entries following
    D0              // Voltage Sensor Number
    7F06            // Scale Factor (LSB MSB)
    DE              // Voltage Sensor Number
    4C1D            // Scale Factor (LSB MSB)


_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0027
    
    // Sensor Record Header
    00A7            // Record ID
    51              // SDR Version
    C0              // Record Type
    22              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0A              // Record Subtype Value
    
    // Fan Sensor Scaling
    00              // Format - Bit fields, 1 == Raw time, 0 = RPM
    00              // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
    8062            // Sys Fan 1A Max RPM (Sensor 30) **(M = 5C)**
    2862            // Sys Fan 1B Max RPM (Sensor 31) **(M = 5F)**
    8062            // Sys Fan 2A Max RPM (Sensor 32) **(M = 5C)**
    2862            // Sys Fan 2B Max RPM (Sensor 33) **(M = 5F)**
    8062            // Sys Fan 3A Max RPM (Sensor 34) **(M = 5C)**
    2862            // Sys Fan 3B Max RPM (Sensor 35) **(M = 5F)**
    8062            // Sys Fan 4A Max RPM (Sensor 36) **(M = 5C)**
    2862            // Sys Fan 4B Max RPM (Sensor 37) **(M = 5F)**
    8062            // Sys Fan 5A Max RPM (Sensor 38) **(M = 5C)**
    2862            // Sys Fan 5B Max RPM (Sensor 39) **(M = 5F)**
    8062            // Sys Fan 6A Max RPM (Sensor 3A) **(M = 5C)**
    2862            // Sys Fan 6B Max RPM (Sensor 3B) **(M = 5F)**
    3462            // CPU Fan 01 Max RPM (Sensor 3C) **Not Used**
    3462            // CPU Fan 02 Max RPM (Sensor 3D) **Not Used**


_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_REC_LEN    0027
    
    // Sensor Record Header
    00A8            // Record ID
    51              // SDR Version
    C0              // Record Type
    22              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0A              // Record Subtype Value
    
    // Fan Sensor Scaling
    00              // Format - Bit fields, 1 == Raw time, 0 = RPM
    00              // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
    005C            // Sys Fan 1A Max RPM (Sensor 30) **(M = 5C)**
    005F            // Sys Fan 1B Max RPM (Sensor 31) **(M = 5F)**
    005C            // Sys Fan 2A Max RPM (Sensor 32) **(M = 5C)**
    005F            // Sys Fan 2B Max RPM (Sensor 33) **(M = 5F)**
    005C            // Sys Fan 3A Max RPM (Sensor 34) **(M = 5C)**
    005F            // Sys Fan 3B Max RPM (Sensor 35) **(M = 5F)**
    005C            // Sys Fan 4A Max RPM (Sensor 36) **(M = 5C)**
    005F            // Sys Fan 4B Max RPM (Sensor 37) **(M = 5F)**
    005C            // Sys Fan 5A Max RPM (Sensor 38) **(M = 5C)**
    005F            // Sys Fan 5B Max RPM (Sensor 39) **(M = 5F)**
    005C            // Sys Fan 6A Max RPM (Sensor 3A) **(M = 5C)**
    005F            // Sys Fan 6B Max RPM (Sensor 3B) **(M = 5F)**
    0001            // CPU Fan 01 Max RPM (Sensor 3C) **Not Used**
    0001            // CPU Fan 02 Max RPM (Sensor 3D) **Not Used**


_SDR_TYPE   C0
_SDR_TAG    'TEST_PLATE'
_REC_LEN    0027
    
    // Sensor Record Header
    00AB            // Record ID
    51              // SDR Version
    C0              // Record Type
    22              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0A              // Record Subtype Value
    
    // Fan Sensor Scaling
    00              // Format - Bit fields, 1 == Raw time, 0 = RPM
    00              // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
    3421            // Sys Fan 1A Max RPM (Sensor 30) **(M = 5C)**
    0100            // Sys Fan 1B Max RPM (Sensor 31) **(M = 5F)**
    3421            // Sys Fan 2A Max RPM (Sensor 32) **(M = 5C)**
    0100            // Sys Fan 2B Max RPM (Sensor 33) **(M = 5F)**
    3421            // Sys Fan 3A Max RPM (Sensor 34) **(M = 5C)**
    0100            // Sys Fan 3B Max RPM (Sensor 35) **(M = 5F)**
    3421            // Sys Fan 4A Max RPM (Sensor 36) **(M = 5C)**
    0100            // Sys Fan 4B Max RPM (Sensor 37) **(M = 5F)**
    0100            // Sys Fan 5A Max RPM (Sensor 38) **(M = 5C)**
    0100            // Sys Fan 5B Max RPM (Sensor 39) **(M = 5F)**
    0100            // Sys Fan 6A Max RPM (Sensor 3A) **(M = 5C)**
    0100            // Sys Fan 6B Max RPM (Sensor 3B) **(M = 5F)**
    0100            // CPU Fan 01 Max RPM (Sensor 3C) **Not Used**
    0100            // CPU Fan 02 Max RPM (Sensor 3D) **Not Used**


_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00AC            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    74              // Clamp Header ID
    74              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    1A              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    F4              // Clamp Control Coefficient LSB (Slow)
    01              // Clamp Control Coefficient MSB (Slow)
    A0              // Clamp Control Coefficient LSB (Fast)
    0F              // Clamp Control Coefficient MSB (Fast)
    58              // Clamp Control Coefficient LSB (derivative)
    1B              // Clamp Control Coefficient MSB (Derivative)
    FC              // Clamp Temperature
    01              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00AD            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    75              // Clamp Header ID
    75              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    F4              // Clamp Control Coefficient LSB (Slow)
    01              // Clamp Control Coefficient MSB (Slow)
    A0              // Clamp Control Coefficient LSB (Fast)
    0F              // Clamp Control Coefficient MSB (Fast)
    58              // Clamp Control Coefficient LSB (derivative)
    1B              // Clamp Control Coefficient MSB (Derivative)
    FC              // Clamp Temperature
    11              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00AE            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    B0              // Clamp Header ID
    B0              // Input Sensor Number
    00              // Entity Presence Sensor Number
    00              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    00              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    80              // Clamp Control Coefficient LSB (Slow)
    00              // Clamp Control Coefficient MSB (Slow)
    D0              // Clamp Control Coefficient LSB (Fast)
    01              // Clamp Control Coefficient MSB (Fast)
    58              // Clamp Control Coefficient LSB (derivative)
    1B              // Clamp Control Coefficient MSB (Derivative)
    FC              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00AF            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    B1              // Clamp Header ID
    B1              // Input Sensor Number
    00              // Entity Presence Sensor Number
    00              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    00              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    80              // Clamp Control Coefficient LSB (Slow)
    00              // Clamp Control Coefficient MSB (Slow)
    D0              // Clamp Control Coefficient LSB (Fast)
    01              // Clamp Control Coefficient MSB (Fast)
    58              // Clamp Control Coefficient LSB (derivative)
    1B              // Clamp Control Coefficient MSB (Derivative)
    FC              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00B0            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    B2              // Clamp Header ID
    B2              // Input Sensor Number
    00              // Entity Presence Sensor Number
    00              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    00              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    80              // Clamp Control Coefficient LSB (Slow)
    00              // Clamp Control Coefficient MSB (Slow)
    D0              // Clamp Control Coefficient LSB (Fast)
    01              // Clamp Control Coefficient MSB (Fast)
    58              // Clamp Control Coefficient LSB (derivative)
    1B              // Clamp Control Coefficient MSB (Derivative)
    FC              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00B1            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    B3              // Clamp Header ID
    B3              // Input Sensor Number
    00              // Entity Presence Sensor Number
    00              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    00              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    80              // Clamp Control Coefficient LSB (Slow)
    00              // Clamp Control Coefficient MSB (Slow)
    D0              // Clamp Control Coefficient LSB (Fast)
    01              // Clamp Control Coefficient MSB (Fast)
    58              // Clamp Control Coefficient LSB (derivative)
    1B              // Clamp Control Coefficient MSB (Derivative)
    FC              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)

_SDR_TYPE  C0
_REC_LEN  001B
    // Sensor Record Header
    00B2            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
 
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    44              // Clamp Header ID
    44              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    46              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B

    // Sensor Record Header
    00B3            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    23              // Clamp Header ID
    23              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    4A              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)

_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00B4            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    25              // Clamp Header ID
    25              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    80              // Clamp Control Coefficient LSB (Slow)
    00              // Clamp Control Coefficient MSB (Slow)
    D0              // Clamp Control Coefficient LSB (Fast)
    01              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    41              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00B5            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    22              // Clamp Header ID
    22              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    53              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00B6            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    14              // Clamp Header ID
    14              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    5A              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)

_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00B7            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    2F              // Clamp Header ID
    2F              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    5A              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B

    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
 
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    27              // Clamp Header ID
    27              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    37              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B

    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
 
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    2C              // Clamp Header ID
    2C              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    37              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)

_SDR_TYPE   C0
_REC_LEN    001B
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
 
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    24              // Clamp Header ID
    24              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    5A              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)

_SDR_TYPE   C0
_REC_LEN    001B
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
 
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    26              // Clamp Header ID
    26              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    5A              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
 
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    45              // Clamp Header ID
    45              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    5A              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
 
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    46              // Clamp Header ID
    46              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    5A              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)

_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00B8            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    5C              // Clamp Header ID
    5C              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    32              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00B9            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    5D              // Clamp Header ID
    5D              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    32              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00BA            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    29              // Clamp Header ID
    29              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    70              // Clamp Control Coefficient LSB (Fast)
    17              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    2D              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)

_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00BB            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    83              // Clamp Header ID
    83              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    F4              // Clamp Control Coefficient LSB (Slow)
    01              // Clamp Control Coefficient MSB (Slow)
    D0              // Clamp Control Coefficient LSB (Fast)
    07              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    FC              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00BC            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    84              // Clamp Header ID
    84              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    00              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    F4              // Clamp Control Coefficient LSB (Slow)
    01              // Clamp Control Coefficient MSB (Slow)
    D0              // Clamp Control Coefficient LSB (Fast)
    07              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    FC              // Clamp Temperature
    10              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B
    
    // Sensor Record Header
    00BD            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    2E              // Clamp Header ID
    2E              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    10              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    E8              // Clamp Control Coefficient LSB (Slow)
    03              // Clamp Control Coefficient MSB (Slow)
    D0              // Clamp Control Coefficient LSB (Fast)
    01              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    42              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE  C0
_REC_LEN  001B
    
    // Sensor Record Header
    00BE            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
 
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    9E              // Clamp Header ID
    9E              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    80              // Clamp Control Coefficient LSB (Slow)
    00              // Clamp Control Coefficient MSB (Slow)
    D0              // Clamp Control Coefficient LSB (Fast)
    01              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    50              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE  C0
_REC_LEN  001B
    
    // Sensor Record Header
    00BF            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
 
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    93              // Clamp Header ID
    93              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    80              // Clamp Control Coefficient LSB (Slow)
    00              // Clamp Control Coefficient MSB (Slow)
    D0              // Clamp Control Coefficient LSB (Fast)
    01              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    41              // Clamp Temperature
    00              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B

    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
 
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    94              // Clamp Header ID
    83              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    1A              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    80              // Clamp Control Coefficient LSB (Slow)
    00              // Clamp Control Coefficient MSB (Slow)
    D0              // Clamp Control Coefficient LSB (Fast)
    07              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    F3              // Clamp Temperature
    01              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_REC_LEN    001B

    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
 
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    03              // FSC version
    00              // FSC Record type
    
    // Global Clamp Header Record
    95              // Clamp Header ID
    84              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    28              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
    80              // Clamp Control Coefficient LSB (Slow)
    00              // Clamp Control Coefficient MSB (Slow)
    D0              // Clamp Control Coefficient LSB (Fast)
    07              // Clamp Control Coefficient MSB (Fast)
    D0              // Clamp Control Coefficient LSB (derivative)
    07              // Clamp Control Coefficient MSB (Derivative)
    F3              // Clamp Temperature
    11              // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 0 (not TControl)


_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   00C0           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   C3             // Domain Mask
   1F             // Acoustic Fan Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = no change)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   00             // Sensor Exclusion Count (1h = 1 sensor to exclude)
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5B             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID


_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   00C1           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   C3             // Domain Mask
   E0             // Performance Fan Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   28             // Normal Control Value (28h = 40%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = no change)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   00             // Sensor Exclusion Count (1h = 1 sensor to exclude)
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5C             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID


_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0033

   // Sensor Record Header
   00C2           // Record ID
   51             // SDR Version
   C0             // Record Type
   2E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   14             // Clamp ID
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   27             // Clamp ID
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   2C             // Clamp ID
   // Clamp Sub-Record 18
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID
   // Clamp Sub-Record 19
   03             // FSC Sub-Record Type (03h = Clamp)
   44             // Clamp ID
   // Clamp Sub-Record 20
   03             // FSC Sub-Record Type (03h = Clamp)
   45             // Clamp ID
   // Clamp Sub-Record 21
   03             // FSC Sub-Record Type (03h = Clamp)
   46             // Clamp ID


_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0033

   // Sensor Record Header
   00C3           // Record ID
   51             // SDR Version
   C0             // Record Type
   2E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   14             // Clamp ID
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   27             // Clamp ID
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   2C             // Clamp ID
   // Clamp Sub-Record 18
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID
   // Clamp Sub-Record 19
   03             // FSC Sub-Record Type (03h = Clamp)
   44             // Clamp ID
   // Clamp Sub-Record 20
   03             // FSC Sub-Record Type (03h = Clamp)
   45             // Clamp ID
   // Clamp Sub-Record 21
   03             // FSC Sub-Record Type (03h = Clamp)
   46             // Clamp ID


_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0033

   // Sensor Record Header
   00C3           // Record ID
   51             // SDR Version
   C0             // Record Type
   2E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   40             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   14             // Clamp ID
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   27             // Clamp ID
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   2C             // Clamp ID
   // Clamp Sub-Record 18
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID
   // Clamp Sub-Record 19
   03             // FSC Sub-Record Type (03h = Clamp)
   44             // Clamp ID
   // Clamp Sub-Record 20
   03             // FSC Sub-Record Type (03h = Clamp)
   45             // Clamp ID
   // Clamp Sub-Record 21
   03             // FSC Sub-Record Type (03h = Clamp)
   46             // Clamp ID


_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0033

   // Sensor Record Header
   00C3           // Record ID
   51             // SDR Version
   C0             // Record Type
   2E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   80             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   14             // Clamp ID
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   27             // Clamp ID
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   2C             // Clamp ID
   // Clamp Sub-Record 18
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID
   // Clamp Sub-Record 19
   03             // FSC Sub-Record Type (03h = Clamp)
   44             // Clamp ID
   // Clamp Sub-Record 20
   03             // FSC Sub-Record Type (03h = Clamp)
   45             // Clamp ID
   // Clamp Sub-Record 21
   03             // FSC Sub-Record Type (03h = Clamp)
   46             // Clamp ID


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C4            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    00              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    1E              // PWM % Value 1
    1E              // Temperature 2
    23              // PWM % Value 2
    28              // Temperature 3
    28              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C5            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    01              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    21              // PWM % Value 1
    1E              // Temperature 2
    25              // PWM % Value 2
    28              // Temperature 3
    2F              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C6            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    02              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    28              // PWM % Value 1
    1E              // Temperature 2
    2D              // PWM % Value 2
    28              // Temperature 3
    32              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C7            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    03              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    2D              // PWM % Value 1
    1E              // Temperature 2
    32              // PWM % Value 2
    28              // Temperature 3
    37              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C8            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    04              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    32              // PWM % Value 1
    1E              // Temperature 2
    37              // PWM % Value 2
    28              // Temperature 3
    42              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C9            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    05              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    37              // PWM % Value 1
    1E              // Temperature 2
    41              // PWM % Value 2
    28              // Temperature 3
    47              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00CA            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    06              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    3C              // PWM % Value 1
    1E              // Temperature 2
    46              // PWM % Value 2
    28              // Temperature 3
    4B              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00CB            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    07              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    41              // PWM % Value 1
    1E              // Temperature 2
    4B              // PWM % Value 2
    28              // Temperature 3
    50              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00CC            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    08              // Stepwise curve ID
    84              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    64              // PWM % Value 1
    1E              // Temperature 2
    64              // PWM % Value 2
    28              // Temperature 3
    64              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00CD            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    09              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    1B              // PWM % Value 1
    1E              // Temperature 2
    1E              // PWM % Value 2
    28              // Temperature 3
    28              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00CE            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    0A              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    21              // PWM % Value 1
    1E              // Temperature 2
    25              // PWM % Value 2
    28              // Temperature 3
    2F              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00CF            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    0B              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    28              // PWM % Value 1
    1E              // Temperature 2
    2D              // PWM % Value 2
    28              // Temperature 3
    32              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00D0            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    0C              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    2D              // PWM % Value 1
    1E              // Temperature 2
    32              // PWM % Value 2
    28              // Temperature 3
    37              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00D1            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    0D              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    32              // PWM % Value 1
    1E              // Temperature 2
    37              // PWM % Value 2
    28              // Temperature 3
    42              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00D2            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    0E              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    37              // PWM % Value 1
    1E              // Temperature 2
    41              // PWM % Value 2
    28              // Temperature 3
    47              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00D3            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    0F              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    3C              // PWM % Value 1
    1E              // Temperature 2
    46              // PWM % Value 2
    28              // Temperature 3
    4B              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00D4            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    10              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    41              // PWM % Value 1
    1E              // Temperature 2
    4B              // PWM % Value 2
    28              // Temperature 3
    50              // PWM % Value 3
    32              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0013
    
    // Sensor Record Header
    00D5            // Record ID
    51              // SDR Version
    C0              // Record Type
    0E              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    11              // Stepwise curve ID
    83              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    64              // PWM % Value 1
    1E              // Temperature 2
    64              // PWM % Value 2
    28              // Temperature 3
    64              // PWM % Value 3


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00D6            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    12              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    23              // PWM % Value 1
    1E              // Temperature 2
    23              // PWM % Value 2
    28              // Temperature 3
    23              // PWM % Value 3
    34              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00D7            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    13              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    19              // PWM % Value 1
    1E              // Temperature 2
    19              // PWM % Value 2
    28              // Temperature 3
    19              // PWM % Value 3
    34              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0017
    
    // Sensor Record Header
    00D8            // Record ID
    51              // SDR Version
    C0              // Record Type
    12              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    // Global Stepwise Curve Record
    14              // Stepwise curve ID
    05              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    4B              // PWM % Value 1
    1E              // Temperature 2
    4B              // PWM % Value 2
    21              // Temperature 3
    4B              // PWM % Value 3
    26              // Temperature 4
    4B              // PWM % Value 4
    28              // Temperature 5
    4B              // PWM % Value 5

_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C4            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    15              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    1B              // PWM % Value 1
    19              // Temperature 2
    1E              // PWM % Value 2
    23              // Temperature 3
    28              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C4            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    16              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    21              // PWM % Value 1
    19              // Temperature 2
    25              // PWM % Value 2
    23              // Temperature 3
    2F              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C4            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    17              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    28              // PWM % Value 1
    19              // Temperature 2
    2D              // PWM % Value 2
    23              // Temperature 3
    32              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C4            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    18              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    2D              // PWM % Value 1
    19              // Temperature 2
    32              // PWM % Value 2
    23              // Temperature 3
    37              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C4            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    19              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    32              // PWM % Value 1
    19              // Temperature 2
    37              // PWM % Value 2
    23              // Temperature 3
    42              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4
  

_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C4            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    1A              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    37              // PWM % Value 1
    19              // Temperature 2
    41              // PWM % Value 2
    23              // Temperature 3
    47              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4
  

_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C4            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    1B              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    3C              // PWM % Value 1
    19              // Temperature 2
    46              // PWM % Value 2
    23              // Temperature 3
    4B              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4
  

_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    00C4            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    1C              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    41              // PWM % Value 1
    19              // Temperature 2
    4B              // PWM % Value 2
    23              // Temperature 3
    50              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0013
    
    // Sensor Record Header
    00C4            // Record ID
    51              // SDR Version
    C0              // Record Type
    0E              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    1D              // Stepwise curve ID
    83              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    64              // PWM % Value 1
    1E              // Temperature 2
    64              // PWM % Value 2
    28              // Temperature 3
    64              // PWM % Value 3


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0141            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    1E              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    1B              // PWM % Value 1
    19              // Temperature 2
    1E              // PWM % Value 2
    23              // Temperature 3
    28              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0142            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    1F              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    21              // PWM % Value 1
    19              // Temperature 2
    25              // PWM % Value 2
    23              // Temperature 3
    2F              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0143            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    20              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    28              // PWM % Value 1
    19              // Temperature 2
    2D              // PWM % Value 2
    23              // Temperature 3
    32              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0144            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    21              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    2D              // PWM % Value 1
    19              // Temperature 2
    32              // PWM % Value 2
    23              // Temperature 3
    37              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0145            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    22              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    32              // PWM % Value 1
    19              // Temperature 2
    37              // PWM % Value 2
    23              // Temperature 3
    42              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0146            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    23              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    37              // PWM % Value 1
    19              // Temperature 2
    41              // PWM % Value 2
    23              // Temperature 3
    47              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0147            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    24              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    3C              // PWM % Value 1
    19              // Temperature 2
    46              // PWM % Value 2
    23              // Temperature 3
    4B              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0148            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    25              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    41              // PWM % Value 1
    19              // Temperature 2
    4B              // PWM % Value 2
    23              // Temperature 3
    50              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0013
    
    // Sensor Record Header
    0149            // Record ID
    51              // SDR Version
    C0              // Record Type
    0E              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    26              // Stepwise curve ID
    83              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    64              // PWM % Value 1
    1E              // Temperature 2
    64              // PWM % Value 2
    28              // Temperature 3
    64              // PWM % Value 3


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0003            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    27              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    1B              // PWM % Value 1
    19              // Temperature 2
    1E              // PWM % Value 2
    23              // Temperature 3
    28              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0004            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    28              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    21              // PWM % Value 1
    19              // Temperature 2
    25              // PWM % Value 2
    23              // Temperature 3
    2F              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0005            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    29              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    23              // PWM % Value 1
    19              // Temperature 2
    28              // PWM % Value 2
    23              // Temperature 3
    2D              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0006            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    2A              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    28              // PWM % Value 1
    19              // Temperature 2
    2D              // PWM % Value 2
    23              // Temperature 3
    32              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0007            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    2B              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    2A              // PWM % Value 1
    19              // Temperature 2
    2F              // PWM % Value 2
    23              // Temperature 3
    34              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0008            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    2C              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    2D              // PWM % Value 1
    19              // Temperature 2
    32              // PWM % Value 2
    23              // Temperature 3
    37              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0009            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    2D              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    2F              // PWM % Value 1
    19              // Temperature 2
    34              // PWM % Value 2
    23              // Temperature 3
    39              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    000A            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    2E              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    32              // PWM % Value 1
    19              // Temperature 2
    37              // PWM % Value 2
    23              // Temperature 3
    3C              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0013
    
    // Sensor Record Header
    000B            // Record ID
    51              // SDR Version
    C0              // Record Type
    0E              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    2F              // Stepwise curve ID
    83              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    64              // PWM % Value 1
    1E              // Temperature 2
    64              // PWM % Value 2
    28              // Temperature 3
    64              // PWM % Value 3


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    000C            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    30              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    20              // PWM % Value 1
    19              // Temperature 2
    23              // PWM % Value 2
    23              // Temperature 3
    2D              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    000D            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    31              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    26              // PWM % Value 1
    19              // Temperature 2
    2A              // PWM % Value 2
    23              // Temperature 3
    34              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    000E            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    32              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    28              // PWM % Value 1
    19              // Temperature 2
    2D              // PWM % Value 2
    23              // Temperature 3
    32              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    000F            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    33              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    2D              // PWM % Value 1
    19              // Temperature 2
    32              // PWM % Value 2
    23              // Temperature 3
    37              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0010            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    34              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    2F              // PWM % Value 1
    19              // Temperature 2
    34              // PWM % Value 2
    23              // Temperature 3
    39              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0011            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    35              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    32              // PWM % Value 1
    19              // Temperature 2
    37              // PWM % Value 2
    23              // Temperature 3
    3C              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0012            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    36              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    34              // PWM % Value 1
    19              // Temperature 2
    39              // PWM % Value 2
    23              // Temperature 3
    3E              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    0013            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    37              // Stepwise curve ID
    04              // Domain Maximum/Control Pair Count (N)
    0F              // Temperature 1
    37              // PWM % Value 1
    19              // Temperature 2
    3C              // PWM % Value 2
    23              // Temperature 3
    41              // PWM % Value 3
    2D              // Temperature 4
    64              // PWM % Value 4


_SDR_TYPE   C0
_REC_LEN    0013
    
    // Sensor Record Header
    0014            // Record ID
    51              // SDR Version
    C0              // Record Type
    0E              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    38              // Stepwise curve ID
    83              // Domain Maximum/Control Pair Count (N)
    14              // Temperature 1
    64              // PWM % Value 1
    1E              // Temperature 2
    64              // PWM % Value 2
    28              // Temperature 3
    64              // PWM % Value 3


_SDR_TYPE   C0
_REC_LEN    0011
    
    // Sensor Record Header
    00D9            // Record ID
    51              // SDR Version
    C0              // Record Type
    0C              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    5B              // Stepwise curve ID
    02              // Domain Maximum/Control Pair Count (N)
    1E              // Temperature 1
    19              // PWM % Value 1
    41              // Temperature 2
    36              // PWM % Value 2


_SDR_TYPE   C0
_REC_LEN    0011
    
    // Sensor Record Header
    00D8            // Record ID
    51              // SDR Version
    C0              // Record Type
    0C              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    5C              // Stepwise curve ID
    02              // Domain Maximum/Control Pair Count (N)
    1E              // Temperature 1
    28              // PWM % Value 1
    41              // Temperature 2
    64              // PWM % Value 2


_SDR_TYPE   C0
_REC_LEN    0011
    
    // Sensor Record Header
    00D9            // Record ID
    51              // SDR Version
    C0              // Record Type
    0C              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    02              // FSC Record type
    
    // Global Stepwise Curve Record
    64              // Stepwise curve ID
    82              // Domain Maximum/Control Pair Count (N)
    1E              // Temperature 1
    64              // PWM % Value 1
    3C              // Temperature 2
    64              // PWM % Value 2


_SDR_TYPE   C0
_REC_LEN    0013
    
    // Sensor Record Header
    00DA            // Record ID
    51              // SDR Version
    C0              // Record Type
    0E              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    21              // FSC Record type
    
    // Global Stepwise Header Record
    00              // Stepwise Header ID
    21              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    50              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0


_SDR_TYPE   C0
_REC_LEN    0013
    
    // Sensor Record Header
    00DB            // Record ID
    51              // SDR Version
    C0              // Record Type
    0E              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    21              // FSC Record type
    
    // Global Stepwise Header Record
    01              // Stepwise Header ID
    20              // Input Sensor Number
    00              // Entity Presence Sensor Number
    64              // Sensor Disabled Control Value
    64              // Sensor Fail Control Value
    64              // Sensor Unavailable Control Value
    00              // Sleep Control Value
    50              // Sleep State and Hysteresis [7:6]-Sleep State Support (0=ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    001C
    
    // Sensor Record Header
    00DC            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    01              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    00              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    08              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    001C
    
    // Sensor Record Header
    00DD            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    02              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    01              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    08              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    001C
    
    // Sensor Record Header
    00DE            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    04              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    02              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    08              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    001C
    
    // Sensor Record Header
    00DF            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    08              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    03              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    08              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    001C
    
    // Sensor Record Header
    00E0            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    10              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    04              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    08              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    001C
    
    // Sensor Record Header
    00E1            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    20              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    05              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    08              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    001C
    
    // Sensor Record Header
    00E2            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    40              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    06              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    08              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    001C
    
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    80              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    07              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    08              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    0037
    
    // Sensor Record Header
    00E3            // Record ID
    51              // SDR Version
    C0              // Record Type
    32              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    1F              // Fan Profile Support

    // Clamp sub-record 1
    03              // FSC Sub-record type
    83              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-record type
    84              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-record type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-record type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-record type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-record type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-record type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-record type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-record type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-record type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-record type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-record type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-record type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-record type
    14              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-record type
    9E              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-record type
    27              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-record type
    2C              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-record type
    29              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-record type
    44              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-record type
    45              // Global Clamp ID
    // Clamp sub-record 22
    03              // FSC Sub-record type
    46              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    0037
    
    // Sensor Record Header
    00DC            // Record ID
    51              // SDR Version
    C0              // Record Type
    32              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    E0              // Fan Profile Support

    // Clamp sub-record 1
    03              // FSC Sub-record type
    94              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-record type
    95              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-record type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-record type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-record type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-record type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-record type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-record type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-record type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-record type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-record type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-record type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-record type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-record type
    14              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-record type
    9E              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-record type
    27              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-record type
    2C              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-record type
    29              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-record type
    44              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-record type
    45              // Global Clamp ID
    // Clamp sub-record 22
    03              // FSC Sub-record type
    46              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    0022
    
    // Sensor Record Header
    00E4            // Record ID
    51              // SDR Version
    C0              // Record Type
    1D              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    18              // FSC Record type

    // Record Body Bytes
    04              // Domain Support
    FF              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    2D              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    12              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    08              // Global Stepwise curve ID
    // Clamp sub-record 1
    03              // FSC Sub-record type
    29              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-record type
    5C              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-record type
    5D              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    0016
    
    // Sensor Record Header
    00E5            // Record ID
    51              // SDR Version
    C0              // Record Type
    11              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    0F              // Fan Profile Support

    // Advanced fan failure sub-record
    04              // FSC Sub-record type
    64              // Domain 0 Fan failure value 
    FF              // Domain 1 Fan failure value 
    FF              // Domain 2 Fan failure value 
    FF              // Domain 3 Fan failure value
    FF              // Domain 4 Fan failure value
    FF              // Domain 5 Fan failure value
    FF              // Domain 6 Fan failure value
    FF              // Domain 7 Fan failure value


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    0016
    
    // Sensor Record Header
    00E6            // Record ID
    51              // SDR Version
    C0              // Record Type
    11              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    18              // FSC Record type

    // Record Body Bytes
    04              // Domain Support
    0F              // Fan Profile Support

    // Advanced fan failure sub-record
    04              // FSC Sub-record type
    FF              // Domain 0 Fan failure value 
    FF              // Domain 1 Fan failure value 
    64              // Domain 2 Fan failure value 
    FF              // Domain 3 Fan failure value
    FF              // Domain 4 Fan failure value
    FF              // Domain 5 Fan failure value
    FF              // Domain 6 Fan failure value
    FF              // Domain 7 Fan failure value


_SDR_TYPE   C0
_SDR_TAG  '2U4N_BP_X35'
_REC_LEN    0012
    
    // Sensor Record Header
    00E7            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    0F              // Fan Profile Support

    // Fans-off and Low Speed sub-record
    05              // FSC Sub-record type
    C8              // Sensor Number
    C4              // Fans-off control value 
    0A              // Hysteresis
    19              // Fans-off PWM offset


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    001C
    
    // Sensor Record Header
    00E8            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    01              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    09              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    11              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    001C
    
    // Sensor Record Header
    00E9            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    02              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    0A              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    11              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    001C
    
    // Sensor Record Header
    00EA            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    04              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    0B              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    11              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    001C
    
    // Sensor Record Header
    00EB            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    08              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    0C              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    11              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    001C
    
    // Sensor Record Header
    00EC            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    10              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    0D              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    11              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    001C
    
    // Sensor Record Header
    00E5            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    20              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    0E              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    11              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    001C
    
    // Sensor Record Header
    00E6            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    40              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    0F              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    11              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    001C
    
    // Sensor Record Header
    00E7            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    80              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    10              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    11              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    0039
    
    // Sensor Record Header
    00EF            // Record ID
    51              // SDR Version
    C0              // Record Type
    34              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    1F              // Fan Profile Support

    // Clamp sub-record 1
    03              // FSC Sub-record type
    83              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-record type
    84              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-record type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-record type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-record type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-record type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-record type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-record type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-record type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-record type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-record type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-record type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-record type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-record type
    14              // Global Clamp ID
    // Clamp sub-record 15
    03              // FSC Sub-record type
    9E              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-record type
    93              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-record type
    27              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-record type
    2C              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-record type
    29              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-record type
    44              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-record type
    45              // Global Clamp ID
    // Clamp sub-record 22
    03              // FSC Sub-record type
    46              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    0039
    
    // Sensor Record Header
    00E8            // Record ID
    51              // SDR Version
    C0              // Record Type
    34              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    E0              // Fan Profile Support

    // Clamp sub-record 1
    03              // FSC Sub-record type
    94              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-record type
    95              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-record type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-record type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-record type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-record type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-record type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-record type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-record type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-record type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-record type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-record type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-record type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-record type
    14              // Global Clamp ID
    // Clamp sub-record 15
    03              // FSC Sub-record type
    9E              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-record type
    93              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-record type
    27              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-record type
    2C              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-record type
    29              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-record type
    44              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-record type
    45              // Global Clamp ID
    // Clamp sub-record 22
    03              // FSC Sub-record type
    46              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    0022
    
    // Sensor Record Header
    00F0            // Record ID
    51              // SDR Version
    C0              // Record Type
    1D              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    18              // FSC Record type

    // Record Body Bytes
    04              // Domain Support
    FF              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    2D              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    13              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    11              // Global Stepwise curve ID
    // Clamp sub-record 1
    03              // FSC Sub-record type
    29              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-record type
    5C              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-record type
    5D              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    0016
    
    // Sensor Record Header
    00F1            // Record ID
    51              // SDR Version
    C0              // Record Type
    11              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    0F              // Fan Profile Support

    // Advanced fan failure sub-record
    04              // FSC Sub-record type
    64              // Domain 0 Fan failure value 
    FF              // Domain 1 Fan failure value 
    FF              // Domain 2 Fan failure value 
    FF              // Domain 3 Fan Failure Value
    FF              // Domain 4 Fan Failure Value
    FF              // Domain 5 Fan Failure Value
    FF              // Domain 6 Fan Failure Value
    FF              // Domain 7 Fan Failure Value


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    0016
    
    // Sensor Record Header
    00F2            // Record ID
    51              // SDR Version
    C0              // Record Type
    11              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    18              // FSC Record type

    // Record Body Bytes
    04              // Domain Support
    0F              // Fan Profile Support

    // Advanced fan failure sub-record
    04              // FSC Sub-record type
    FF              // Domain 0 Fan failure value 
    FF              // Domain 1 Fan failure value 
    64              // Domain 2 Fan failure value 
    FF              // Domain 3 Fan Failure Value
    FF              // Domain 4 Fan Failure Value
    FF              // Domain 5 Fan Failure Value
    FF              // Domain 6 Fan Failure Value
    FF              // Domain 7 Fan Failure Value    


_SDR_TYPE   C0
_SDR_TAG  '24HDDHSBP'
_REC_LEN    0012
    
    // Sensor Record Header
    00F3            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    0F              // Fan Profile Support

    // Fans-off and Low Speed sub-record
    05              // FSC Sub-record type
    C8              // Sensor Number
    C4              // Fans-off control value 
    0A              // Hysteresis
    19              // Fans-off PWM offset


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    001C
    
    // Sensor Record Header
    00DC            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    01              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    15              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1D              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    001C
    
    // Sensor Record Header
    00DD            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    02              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    16              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1D              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    001C
    
    // Sensor Record Header
    00DE            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    04              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    17              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1D              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    001C
    
    // Sensor Record Header
    00DF            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    08              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    18              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1D              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    001C
    
    // Sensor Record Header
    00E0            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    10              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    19              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1D              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    001C
    
    // Sensor Record Header
    00E1            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    20              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1A              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1D              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    001C
    
    // Sensor Record Header
    00E2            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    40              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1B              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1D              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    001C
    
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    80              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1C              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1D              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    0037
    
    // Sensor Record Header
    00E3            // Record ID
    51              // SDR Version
    C0              // Record Type
    32              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    1F              // Fan Profile Support

    // Clamp sub-record 1
    03              // FSC Sub-record type
    83              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-record type
    84              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-record type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-record type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-record type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-record type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-record type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-record type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-record type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-record type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-record type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-record type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-record type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-record type
    14              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-record type
    9E              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-record type
    27              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-record type
    2C              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-record type
    29              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-record type
    44              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-record type
    45              // Global Clamp ID
    // Clamp sub-record 22
    03              // FSC Sub-record type
    46              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    0037
    
    // Sensor Record Header
    00DC            // Record ID
    51              // SDR Version
    C0              // Record Type
    32              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    E0              // Fan Profile Support

    // Clamp sub-record 1
    03              // FSC Sub-record type
    94              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-record type
    95              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-record type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-record type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-record type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-record type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-record type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-record type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-record type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-record type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-record type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-record type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-record type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-record type
    14              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-record type
    9E              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-record type
    27              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-record type
    2C              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-record type
    29              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-record type
    44              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-record type
    45              // Global Clamp ID
    // Clamp sub-record 22
    03              // FSC Sub-record type
    46              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    0022
    
    // Sensor Record Header
    00E4            // Record ID
    51              // SDR Version
    C0              // Record Type
    1D              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    18              // FSC Record type

    // Record Body Bytes
    04              // Domain Support
    FF              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    2D              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    13              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1D              // Global Stepwise curve ID
    // Clamp sub-record 1
    03              // FSC Sub-record type
    29              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-record type
    5C              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-record type
    5D              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    0016
    
    // Sensor Record Header
    00E5            // Record ID
    51              // SDR Version
    C0              // Record Type
    11              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    0F              // Fan Profile Support

    // Advanced fan failure sub-record
    04              // FSC Sub-record type
    64              // Domain 0 Fan failure value 
    FF              // Domain 1 Fan failure value 
    FF              // Domain 2 Fan failure value 
    FF              // Domain 3 Fan failure value
    FF              // Domain 4 Fan failure value
    FF              // Domain 5 Fan failure value
    FF              // Domain 6 Fan failure value
    FF              // Domain 7 Fan failure value


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    0016
    
    // Sensor Record Header
    00E6            // Record ID
    51              // SDR Version
    C0              // Record Type
    11              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    18              // FSC Record type

    // Record Body Bytes
    04              // Domain Support
    0F              // Fan Profile Support

    // Advanced fan failure sub-record
    04              // FSC Sub-record type
    FF              // Domain 0 Fan failure value 
    FF              // Domain 1 Fan failure value 
    64              // Domain 2 Fan failure value 
    FF              // Domain 3 Fan failure value
    FF              // Domain 4 Fan failure value
    FF              // Domain 5 Fan failure value
    FF              // Domain 6 Fan failure value
    FF              // Domain 7 Fan failure value


_SDR_TYPE   C0
_SDR_TAG  'EBCP-BNP'
_REC_LEN    0012
    
    // Sensor Record Header
    00E7            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    0F              // Fan Profile Support

    // Fans-off and Low Speed sub-record
    05              // FSC Sub-record type
    C8              // Sensor Number
    C4              // Fans-off control value 
    0A              // Hysteresis
    19              // Fans-off PWM offset


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    014A            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    01              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1E              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    26              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    014B            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    02              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    1F              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    26              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    014C            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    04              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    20              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    26              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    014D            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    08              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    21              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    26              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    014E            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    10              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    22              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    26              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    014F            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    20              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    23              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    26              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0150            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    40              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    24              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    26              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0151            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    80              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    25              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    26              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    0033
    
    // Sensor Record Header
    0152            // Record ID
    51              // SDR Version
    C0              // Record Type
    2E              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    1F              // Fan Profile Support

    // Clamp sub-record 3
    03              // FSC Sub-Record Type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-Record Type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-Record Type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-Record Type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-Record Type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-Record Type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-Record Type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-Record Type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-Record Type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-Record Type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-Record Type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-Record Type
    14              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-Record Type
    9E              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-Record Type
    27              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-Record Type
    2C              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-Record Type
    29              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-Record Type
    44              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-Record Type
    45              // Global Clamp ID
    // Clamp sub-record 22
    03              // FSC Sub-Record Type
    46              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    0033
    
    // Sensor Record Header
    0153            // Record ID
    51              // SDR Version
    C0              // Record Type
    2E              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    E0              // Fan Profile Support

    // Clamp sub-record 3
    03              // FSC Sub-Record Type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-Record Type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-Record Type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-Record Type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-Record Type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-Record Type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-Record Type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-Record Type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-Record Type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-Record Type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-Record Type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-Record Type
    14              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-Record Type
    9E              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-Record Type
    27              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-Record Type
    2C              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-Record Type
    29              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-Record Type
    44              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-Record Type
    45              // Global Clamp ID
    // Clamp sub-record 22
    03              // FSC Sub-Record Type
    46              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    0022
    
    // Sensor Record Header
    0154            // Record ID
    51              // SDR Version
    C0              // Record Type
    1D              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    18              // FSC Record type

    // Record Body Bytes
    04              // Domain Support
    FF              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    2D              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    12              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    08              // Global Stepwise curve ID
    // Clamp sub-record 1
    03              // FSC Sub-Record Type
    29              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-Record Type
    5C              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-Record Type
    5D              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    0016
    
    // Sensor Record Header
    0155            // Record ID
    51              // SDR Version
    C0              // Record Type
    11              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    0F              // Fan Profile Support

    // Advanced fan failure sub-record
    04              // FSC Sub-record type
    64              // Domain 0 Fan failure value 
    FF              // Domain 1 Fan failure value 
    FF              // Domain 2 Fan failure value 
    FF              // Domain 3 Fan failure value
    FF              // Domain 4 Fan failure value
    FF              // Domain 5 Fan failure value
    FF              // Domain 6 Fan failure value
    FF              // Domain 7 Fan failure value


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    0016
    
    // Sensor Record Header
    0156            // Record ID
    51              // SDR Version
    C0              // Record Type
    11              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    18              // FSC Record type

    // Record Body Bytes
    04              // Domain Support
    0F              // Fan Profile Support

    // Advanced fan failure sub-record
    04              // FSC Sub-record type
    FF              // Domain 0 Fan failure value 
    FF              // Domain 1 Fan failure value 
    64              // Domain 2 Fan failure value 
    FF              // Domain 3 Fan failure value
    FF              // Domain 4 Fan failure value
    FF              // Domain 5 Fan failure value
    FF              // Domain 6 Fan failure value
    FF              // Domain 7 Fan failure value


_SDR_TYPE   C0
_SDR_TAG  'BP_X35_LC'
_REC_LEN    0012
    
    // Sensor Record Header
    0157            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    0F              // Fan Profile Support

    // Fans-off and Low Speed sub-record
    05              // FSC Sub-record type
    C8              // Sensor Number
    C4              // Fans-off control value 
    0A              // Hysteresis
    19              // Fans-off PWM offset


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0164            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    01              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    27              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2F              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0165            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    02              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    28              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2F              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0166            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    04              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    29              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2F              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0167            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    08              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2A              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2F              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0168            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    10              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2B              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2F              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0169            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    20              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2C              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2F              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    001C
    
    // Sensor Record Header
    016A            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    40              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2D              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2F              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    001C
    
    // Sensor Record Header
    016B            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    80              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2E              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    2F              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    0033
    
    // Sensor Record Header
    016C            // Record ID
    51              // SDR Version
    C0              // Record Type
    2E              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    1F              // Fan Profile Support

    // Clamp sub-record 3
    03              // FSC Sub-Record Type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-Record Type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-Record Type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-Record Type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-Record Type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-Record Type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-Record Type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-Record Type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-Record Type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-Record Type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-Record Type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-Record Type
    14              // Global Clamp ID
    // Clamp sub-record 15
    03              // FSC Sub-Record Type
    9E              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-Record Type
    27              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-Record Type
    2C              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-Record Type
    29              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-Record Type
    44              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-Record Type
    45              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-Record Type
    46              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    0033
    
    // Sensor Record Header
    016D            // Record ID
    51              // SDR Version
    C0              // Record Type
    2E              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    E0              // Fan Profile Support

    // Clamp sub-record 3
    03              // FSC Sub-Record Type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-Record Type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-Record Type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-Record Type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-Record Type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-Record Type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-Record Type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-Record Type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-Record Type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-Record Type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-Record Type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-Record Type
    14              // Global Clamp ID
    // Clamp sub-record 15
    03              // FSC Sub-Record Type
    9E              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-Record Type
    27              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-Record Type
    2C              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-Record Type
    29              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-Record Type
    44              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-Record Type
    45              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-Record Type
    46              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    0022
    
    // Sensor Record Header
    016E            // Record ID
    51              // SDR Version
    C0              // Record Type
    1D              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    18              // FSC Record type

    // Record Body Bytes
    04              // Domain Support
    FF              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    2D              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    12              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    08              // Global Stepwise curve ID
    // Clamp sub-record 1
    03              // FSC Sub-Record Type
    29              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-Record Type
    5C              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-Record Type
    5D              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    0016
    
    // Sensor Record Header
    016F            // Record ID
    51              // SDR Version
    C0              // Record Type
    11              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    0F              // Fan Profile Support

    // Advanced fan failure sub-record
    04              // FSC Sub-record type
    64              // Domain 0 Fan failure value 
    FF              // Domain 1 Fan failure value 
    FF              // Domain 2 Fan failure value 
    FF              // Domain 3 Fan failure value
    FF              // Domain 4 Fan failure value
    FF              // Domain 5 Fan failure value
    FF              // Domain 6 Fan failure value
    FF              // Domain 7 Fan failure value


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    0016
    
    // Sensor Record Header
    0170            // Record ID
    51              // SDR Version
    C0              // Record Type
    11              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    18              // FSC Record type

    // Record Body Bytes
    04              // Domain Support
    0F              // Fan Profile Support

    // Advanced fan failure sub-record
    04              // FSC Sub-record type
    FF              // Domain 0 Fan failure value 
    FF              // Domain 1 Fan failure value 
    64              // Domain 2 Fan failure value 
    FF              // Domain 3 Fan failure value
    FF              // Domain 4 Fan failure value
    FF              // Domain 5 Fan failure value
    FF              // Domain 6 Fan failure value
    FF              // Domain 7 Fan failure value


_SDR_TYPE   C0
_SDR_TAG  'EBCP-LC'
_REC_LEN    0012
    
    // Sensor Record Header
    0171            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    0F              // Fan Profile Support

    // Fans-off and Low Speed sub-record
    05              // FSC Sub-record type
    C8              // Sensor Number
    C4              // Fans-off control value 
    0A              // Hysteresis
    19              // Fans-off PWM offset

_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    017E            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    01              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    30              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    38              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    017F            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    02              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    31              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    38              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0180            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    04              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    32              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    38              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0181            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    08              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    33              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    38              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0182            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    10              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    34              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    38              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0183            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    20              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    35              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    38              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0184            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    40              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    36              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    38              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    001C
    
    // Sensor Record Header
    0185            // Record ID
    51              // SDR Version
    C0              // Record Type
    17              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    80              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    19              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    37              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    38              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    0033
    
    // Sensor Record Header
    0186            // Record ID
    51              // SDR Version
    C0              // Record Type
    2E              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    1F              // Fan Profile Support

    // Clamp sub-record 3
    03              // FSC Sub-Record Type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-Record Type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-Record Type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-Record Type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-Record Type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-Record Type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-Record Type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-Record Type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-Record Type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-Record Type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-Record Type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-Record Type
    14              // Global Clamp ID
    // Clamp sub-record 15
    03              // FSC Sub-Record Type
    9E              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-Record Type
    27              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-Record Type
    2C              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-Record Type
    29              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-Record Type
    44              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-Record Type
    45              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-Record Type
    46              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    0033
    
    // Sensor Record Header
    0187            // Record ID
    51              // SDR Version
    C0              // Record Type
    2E              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    E0              // Fan Profile Support

    // Clamp sub-record 3
    03              // FSC Sub-Record Type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-Record Type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-Record Type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-Record Type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-Record Type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-Record Type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-Record Type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-Record Type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-Record Type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-Record Type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-Record Type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-Record Type
    14              // Global Clamp ID
    // Clamp sub-record 15
    03              // FSC Sub-Record Type
    9E              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-Record Type
    27              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-Record Type
    2C              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-Record Type
    29              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-Record Type
    44              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-Record Type
    45              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-Record Type
    46              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    0022
    
    // Sensor Record Header
    0188            // Record ID
    51              // SDR Version
    C0              // Record Type
    1D              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    18              // FSC Record type

    // Record Body Bytes
    04              // Domain Support
    FF              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    2D              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    01              // Sensor exclusion count (N)
    2E              // Sensor number
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    12              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    00              // Global Stepwise header ID
    08              // Global Stepwise curve ID
    // Clamp sub-record 1
    03              // FSC Sub-Record Type
    29              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-Record Type
    5C              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-Record Type
    5D              // Global Clamp ID


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    0016
    
    // Sensor Record Header
    0189            // Record ID
    51              // SDR Version
    C0              // Record Type
    11              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    0F              // Fan Profile Support

    // Advanced fan failure sub-record
    04              // FSC Sub-record type
    64              // Domain 0 Fan failure value 
    FF              // Domain 1 Fan failure value 
    FF              // Domain 2 Fan failure value 
    FF              // Domain 3 Fan failure value
    FF              // Domain 4 Fan failure value
    FF              // Domain 5 Fan failure value
    FF              // Domain 6 Fan failure value
    FF              // Domain 7 Fan failure value


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    0016
    
    // Sensor Record Header
    018A            // Record ID
    51              // SDR Version
    C0              // Record Type
    11              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    18              // FSC Record type

    // Record Body Bytes
    04              // Domain Support
    0F              // Fan Profile Support

    // Advanced fan failure sub-record
    04              // FSC Sub-record type
    FF              // Domain 0 Fan failure value 
    FF              // Domain 1 Fan failure value 
    64              // Domain 2 Fan failure value 
    FF              // Domain 3 Fan failure value
    FF              // Domain 4 Fan failure value
    FF              // Domain 5 Fan failure value
    FF              // Domain 6 Fan failure value
    FF              // Domain 7 Fan failure value


_SDR_TYPE   C0
_SDR_TAG  '24HDD_LC'
_REC_LEN    0012
    
    // Sensor Record Header
    018B            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    01              // Domain Support
    0F              // Fan Profile Support

    // Fans-off and Low Speed sub-record
    05              // FSC Sub-record type
    C8              // Sensor Number
    C4              // Fans-off control value 
    0A              // Hysteresis
    19              // Fans-off PWM offset

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0029
    
    // Sensor Record Header
    00F7            // Record ID
    51              // SDR Version
    C0              // Record Type
    24              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    12              // Record Subtype Value
    
    // Aggregate Sensor Configuration Record
    C8              // Aggregate sensor number (C8h = Aggregate Thermal Margin 1)
    0F              // Number of input pairs to follow
    74              // Input 1 sensor number
    FC              // Input 1 margin reference value (-4 = FCh)
    75              // Input 2 sensor number
    FC              // Input 2 margin reference value
    B0              // Input 3 sensor number
    00              // Input 3 margin reference value
    B1              // Input 4 sensor number
    00              // Input 4 margin reference value (70 = 46h)
    B2              // Input 5 sensor number
    00              // Input 5 margin reference value (83 = 53h)
    B3              // Input 6 sensor number
    00              // Input 6 margin reference value (74 = 4Ah)
    22              // Input 7 sensor number
    53              // Input 7 margin reference value (98 = 62h)
    23              // Input 8 sensor number
    4A              // Input 8 margin reference value
    24              // Input 9 sensor number
    69              // Input 9 margin reference value
    25              // Input 10 sensor number
    46              // Input 10 margin reference value
    27              // Input 11 sensor number
    69              // Input 11 margin reference value
    45              // Input 12 sensor number
    69              // Input 12 margin reference value
    46              // Input 13 sensor number
    69              // Input 13 margin reference value
    2E              // Input 14 sensor number
    3C              // Input 14 margin reference value
    2F              // Input 15 sensor number
    62              // Input 15 margin reference value


_SDR_TYPE   C0
_SDR_TAG    '24HDDHSBP'
_REC_LEN    0029
    
    // Sensor Record Header
    00F8            // Record ID
    51              // SDR Version
    C0              // Record Type
    24              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    12              // Record Subtype Value
    
    // Aggregate Sensor Configuration Record
    C8              // Aggregate sensor number (C8h = Aggregate Thermal Margin 1)
    0F              // Number of input pairs to follow
    74              // Input 1 sensor number
    FC              // Input 1 margin reference value (-4 = FCh)
    75              // Input 2 sensor number
    FC              // Input 2 margin reference value
    B0              // Input 3 sensor number
    00              // Input 3 margin reference value
    B1              // Input 4 sensor number
    00              // Input 4 margin reference value (70 = 46h)
    B2              // Input 5 sensor number
    00              // Input 5 margin reference value (83 = 53h)
    B3              // Input 6 sensor number
    00              // Input 6 margin reference value (74 = 4Ah)
    22              // Input 7 sensor number
    53              // Input 7 margin reference value (98 = 62h)
    23              // Input 8 sensor number
    4A              // Input 8 margin reference value
    24              // Input 9 sensor number
    69              // Input 9 margin reference value
    25              // Input 10 sensor number
    46              // Input 10 margin reference value
    27              // Input 11 sensor number
    69              // Input 11 margin reference value
    45              // Input 12 sensor number
    69              // Input 12 margin reference value
    46              // Input 13 sensor number
    69              // Input 13 margin reference value
    2E              // Input 14 sensor number
    3C              // Input 14 margin reference value
    2F              // Input 15 sensor number
    62              // Input 15 margin reference value


_SDR_TYPE   C0
_SDR_TAG    'EBCP-BNP'
_REC_LEN    0029
    
    // Sensor Record Header
    00F8            // Record ID
    51              // SDR Version
    C0              // Record Type
    24              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    12              // Record Subtype Value
    
    // Aggregate Sensor Configuration Record
    C8              // Aggregate sensor number (C8h = Aggregate Thermal Margin 1)
    0F              // Number of input pairs to follow
    74              // Input 1 sensor number
    FC              // Input 1 margin reference value (-4 = FCh)
    75              // Input 2 sensor number
    FC              // Input 2 margin reference value
    B0              // Input 3 sensor number
    00              // Input 3 margin reference value
    B1              // Input 4 sensor number
    00              // Input 4 margin reference value (70 = 46h)
    B2              // Input 5 sensor number
    00              // Input 5 margin reference value (83 = 53h)
    B3              // Input 6 sensor number
    00              // Input 6 margin reference value (74 = 4Ah)
    22              // Input 7 sensor number
    53              // Input 7 margin reference value (98 = 62h)
    23              // Input 8 sensor number
    4A              // Input 8 margin reference value
    24              // Input 9 sensor number
    69              // Input 9 margin reference value
    25              // Input 10 sensor number
    46              // Input 10 margin reference value
    27              // Input 11 sensor number
    69              // Input 11 margin reference value
    45              // Input 12 sensor number
    69              // Input 12 margin reference value
    46              // Input 13 sensor number
    69              // Input 13 margin reference value
    2E              // Input 14 sensor number
    3C              // Input 14 margin reference value
    2F              // Input 15 sensor number
    62              // Input 15 margin reference value


_SDR_TYPE   C0
_SDR_TAG    'BP_X35_LC'
_REC_LEN    0029
    
    // Sensor Record Header
    0157            // Record ID
    51              // SDR Version
    C0              // Record Type
    24              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    12              // Record Subtype Value
    
    // Aggregate Sensor Configuration Record
    C8              // Aggregate sensor number (C8h = Aggregate Thermal Margin 1)
    0F              // Number of input pairs to follow
    74              // Input 1 sensor number
    FC              // Input 1 margin reference value
    75              // Input 2 sensor number
    FC              // Input 2 margin reference value
    B0              // Input 3 sensor number
    00              // Input 3 margin reference value
    B1              // Input 4 sensor number
    00              // Input 4 margin reference value
    B2              // Input 5 sensor number
    00              // Input 5 margin reference value
    B3              // Input 6 sensor number
    00              // Input 6 margin reference value
    22              // Input 7 sensor number
    53              // Input 7 margin reference value
    23              // Input 8 sensor number
    4A              // Input 8 margin reference value
    24              // Input 9 sensor number
    69              // Input 9 margin reference value
    25              // Input 10 sensor number
    46              // Input 10 margin reference value
    27              // Input 11 sensor number
    69              // Input 11 margin reference value
    45              // Input 12 sensor number
    69              // Input 12 margin reference value
    46              // Input 13 sensor number
    69              // Input 13 margin reference value
    2E              // Input 14 sensor number
    3C              // Input 14 margin reference value
    2F              // Input 15 sensor number
    62              // Input 15 margin reference value


_SDR_TYPE   C0
_SDR_TAG    'EBCP-LC'
_REC_LEN    0029
    
    // Sensor Record Header
    016F            // Record ID
    51              // SDR Version
    C0              // Record Type
    24              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    12              // Record Subtype Value
    
    // Aggregate Sensor Configuration Record
    C8              // Aggregate sensor number (C8h = Aggregate Thermal Margin 1)
    0F              // Number of input pairs to follow
    74              // Input 1 sensor number
    FC              // Input 1 margin reference value
    75              // Input 2 sensor number
    FC              // Input 2 margin reference value
    B0              // Input 3 sensor number
    00              // Input 3 margin reference value
    B1              // Input 4 sensor number
    00              // Input 4 margin reference value
    B2              // Input 5 sensor number
    00              // Input 5 margin reference value
    B3              // Input 6 sensor number
    00              // Input 6 margin reference value
    22              // Input 7 sensor number
    53              // Input 7 margin reference value
    23              // Input 8 sensor number
    4A              // Input 8 margin reference value
    24              // Input 9 sensor number
    69              // Input 9 margin reference value
    25              // Input 10 sensor number
    46              // Input 10 margin reference value
    27              // Input 11 sensor number
    69              // Input 11 margin reference value
    45              // Input 12 sensor number
    69              // Input 12 margin reference value
    46              // Input 13 sensor number
    69              // Input 13 margin reference value
    2E              // Input 14 sensor number
    3C              // Input 14 margin reference value
    2F              // Input 15 sensor number
    62              // Input 15 margin reference value


_SDR_TYPE   C0
_SDR_TAG    '24HDD_LC'
_REC_LEN    0029
    
    // Sensor Record Header
    00F8            // Record ID
    51              // SDR Version
    C0              // Record Type
    24              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    12              // Record Subtype Value
    
    // Aggregate Sensor Configuration Record
    C8              // Aggregate sensor number (C8h = Aggregate Thermal Margin 1)
    0F              // Number of input pairs to follow
    74              // Input 1 sensor number
    FC              // Input 1 margin reference value
    75              // Input 2 sensor number
    FC              // Input 2 margin reference value
    B0              // Input 3 sensor number
    00              // Input 3 margin reference value
    B1              // Input 4 sensor number
    00              // Input 4 margin reference value
    B2              // Input 5 sensor number
    00              // Input 5 margin reference value
    B3              // Input 6 sensor number
    00              // Input 6 margin reference value
    22              // Input 7 sensor number
    53              // Input 7 margin reference value
    23              // Input 8 sensor number
    4A              // Input 8 margin reference value
    24              // Input 9 sensor number
    69              // Input 9 margin reference value
    25              // Input 10 sensor number
    46              // Input 10 margin reference value
    27              // Input 11 sensor number
    69              // Input 11 margin reference value
    45              // Input 12 sensor number
    69              // Input 12 margin reference value
    46              // Input 13 sensor number
    69              // Input 13 margin reference value
    2E              // Input 14 sensor number
    3C              // Input 14 margin reference value
    2F              // Input 15 sensor number
    62              // Input 15 margin reference value


_SDR_TYPE   C0
_REC_LEN    001F
    
    // Sensor Record Header
    00F8            // Record ID
    51              // SDR Version
    C0              // Record Type
    1A              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    12              // Record Subtype Value
    
    // Aggregate Sensor Configuration Record
    C9              // Aggregate sensor number (C8h = Aggregate Thermal Margin 1)
    0A              // Number of input pairs to follow
    23              // Input 1 sensor number
    54              // Input 1 margin reference value (-4 = FCh)
    14              // Input 2 sensor number
    64              // Input 2 margin reference value
    25              // Input 3 sensor number
    4B              // Input 3 margin reference value
    22              // Input 4 sensor number
    5D              // Input 4 margin reference value (70 = 46h)
    27              // Input 5 sensor number
    41              // Input 5 margin reference value (83 = 53h)
    2C              // Input 6 sensor number
    41              // Input 6 margin reference value (74 = 4Ah)
    2F              // Input 7 sensor number
    64              // Input 7 margin reference value (98 = 62h)
    2E              // Input 8 sensor number
    4C              // Input 8 margin reference value
    5C              // Input 9 sensor number
    3C              // Input 9 margin reference value
    5D              // Input 10 sensor number
    3C              // Input 10 margin reference value


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0012
    
    // Sensor Record Header
    00F9            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    19              // Record Subtype Value
    
    // Exit Air Record
    0200            // Alpha S LSB first
    1100            // Alpha F LSB first
    05              // Qmin
    16              // Qmax
    05              // P Offset
    07              // Correction factor at Qmin
    09              // Correction factor at Qmax


_SDR_TYPE   C0                                               
_SDR_TAG    'EBCP-BNP'
_REC_LEN    0012
    
    // Sensor Record Header
    00F9            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    19              // Record Subtype Value
    
    // Exit Air Record
    0200            // Alpha S LSB first
    1100            // Alpha F LSB first
    04              // Qmin
    17              // Qmax
    00              // P Offset
    08              // Correction factor at Qmin
    0A              // Correction factor at Qmax


_SDR_TYPE   C0
_SDR_TAG    '24HDDHSBP'
_REC_LEN    0012
    
    // Sensor Record Header
    00FA            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    19              // Record Subtype Value
    
    // Exit Air Record
    0200            // Alpha S LSB first
    1100            // Alpha F LSB first
    04              // Qmin
    17              // Qmax
    00              // P Offset
    08              // Correction factor at Qmin
    0A              // Correction factor at Qmax


_SDR_TYPE   C0
_SDR_TAG    'BP_X35_LC'
_REC_LEN    0012
    
    // Sensor Record Header
    0159            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    19              // Record Subtype Value
    
    // Exit Air Record
    0200            // Alpha S LSB first
    1100            // Alpha F LSB first
    04              // Qmin
    12              // Qmax
    BC              // P Offset
    03              // Correction factor at Qmin
    03              // Correction factor at Qmax


_SDR_TYPE   C0
_SDR_TAG    'EBCP-LC'
_REC_LEN    0012
    
    // Sensor Record Header
    0171            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    19              // Record Subtype Value
    
    // Exit Air Record
    0200            // Alpha S LSB first
    1100            // Alpha F LSB first
    06              // Qmin
    15              // Qmax
    EC              // P Offset
    02              // Correction factor at Qmin
    02              // Correction factor at Qmax


_SDR_TYPE   C0
_SDR_TAG    '24HDD_LC'
_REC_LEN    0012
    
    // Sensor Record Header
    00FA            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    19              // Record Subtype Value
    
    // Exit Air Record
    0200            // Alpha S LSB first
    1100            // Alpha F LSB first
    04              // Qmin
    12              // Qmax
    BC              // P Offset
    03              // Correction factor at Qmin
    03              // Correction factor at Qmax


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0012
    
    // Sensor Record Header
    00FB            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    11              // Record Subtype Value
    
    // Airflow Record
    01              // Domain mask
    2200            // Correction factor 1 (in units of .01) LSB first
    2D00            // Correction factor 2 (in units of .01) LSB first
    1E              // PWM for Correction Factor 1
    64              // PWM for Correction Factor 2
    20              // Max CFM of Fan
    03              // Quantity of fans in this equation


_SDR_TYPE   C0
_SDR_TAG    'EBCP-BNP'
_REC_LEN    0012
    
    // Sensor Record Header
    00FB            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    11              // Record Subtype Value
    
    // Airflow Record
    01              // Domain mask
    2D00            // Correction factor 1 (in units of .01) LSB first
    3400            // Correction factor 2 (in units of .01) LSB first
    1E              // PWM for Correction Factor 1
    64              // PWM for Correction Factor 2
    20              // Max CFM of Fan
    03              // Quantity of fans in this equation


_SDR_TYPE   C0
_SDR_TAG    '24HDDHSBP'
_REC_LEN    0012
    
    // Sensor Record Header
    00FC            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    11              // Record Subtype Value
    
    // Airflow Record
    01              // Domain mask
    2500            // Correction factor 1 (in units of .01) LSB first
    3000            // Correction factor 2 (in units of .01) LSB first
    1E              // PWM for Correction Factor 1
    64              // PWM for Correction Factor 2
    20              // Max CFM of Fan
    03              // Quantity of fans in this equation


_SDR_TYPE   C0
_SDR_TAG    'BP_X35_LC'
_REC_LEN    0012
    
    // Sensor Record Header
    0158            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    11              // Record Subtype Value
    
    // Airflow Record
    01              // Domain mask
    1E00            // Correction factor 1 (in units of .01) LSB first
    2400            // Correction factor 2 (in units of .01) LSB first
    1E              // PWM for Correction Factor 1
    64              // PWM for Correction Factor 2
    20              // Max CFM of Fan
    03              // Quantity of fans in this equation


_SDR_TYPE   C0
_SDR_TAG    'EBCP-LC'
_REC_LEN    0012
    
    // Sensor Record Header
    0170            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    11              // Record Subtype Value
    
    // Airflow Record
    01              // Domain mask
    1E00            // Correction factor 1 (in units of .01) LSB first
    2400            // Correction factor 2 (in units of .01) LSB first
    1E              // PWM for Correction Factor 1
    64              // PWM for Correction Factor 2
    20              // Max CFM of Fan
    03              // Quantity of fans in this equation


_SDR_TYPE   C0
_SDR_TAG    '24HDD_LC'
_REC_LEN    0012
    
    // Sensor Record Header
    0170            // Record ID
    51              // SDR Version
    C0              // Record Type
    0D              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    11              // Record Subtype Value
    
    // Airflow Record
    01              // Domain mask
    2800            // Correction factor 1 (in units of .01) LSB first
    2B00            // Correction factor 2 (in units of .01) LSB first
    1E              // PWM for Correction Factor 1
    64              // PWM for Correction Factor 2
    20              // Max CFM of Fan
    03              // Quantity of fans in this equation


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0010
    
    // Sensor Record Header
    00FA            // Record ID
    51              // SDR Version
    C0              // Record Type
    0B              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    20              // Record Subtype Value

    //Sensor Based Power Limit
    01              //Version
    C9              //Input sensor number
    FB              //Low threshold
    3C              //Low processor limit
    08              //Low memory limit
    00              //High threshold
    28              //High processor limit


_SDR_TYPE   C0
_SDR_TAG    '24HDDHSBP'
_REC_LEN    0010
    
    // Sensor Record Header
    00FA            // Record ID
    51              // SDR Version
    C0              // Record Type
    0B              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    20              // Record Subtype Value

    //Sensor Based Power Limit
    01              //Version
    C9              //Input sensor number
    FB              //Low threshold
    3C              //Low processor limit
    08              //Low memory limit
    00              //High threshold
    28              //High processor limit


_SDR_TYPE   C0
_SDR_TAG    'EBCP-BNP'
_REC_LEN    0010
    
    // Sensor Record Header
    00FA            // Record ID
    51              // SDR Version
    C0              // Record Type
    0B              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    20              // Record Subtype Value

    //Sensor Based Power Limit
    01              //Version
    C9              //Input sensor number
    FB              //Low threshold
    3C              //Low processor limit
    08              //Low memory limit
    00              //High threshold
    28              //High processor limit


_SDR_TYPE   C0
_SDR_TAG    'BP_X35_LC'
_REC_LEN    0010
    
    // Sensor Record Header
    015A            // Record ID
    51              // SDR Version
    C0              // Record Type
    0B              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    20              // Record Subtype Value

    //Sensor Based Power Limit
    01              //Version
    C9              //Input sensor number
    FB              //Low threshold
    3C              //Low processor limit
    08              //Low memory limit
    00              //High threshold
    28              //High processor limit


_SDR_TYPE   C0
_SDR_TAG    'EBCP-LC'
_REC_LEN    0010
    
    // Sensor Record Header
    0172            // Record ID
    51              // SDR Version
    C0              // Record Type
    0B              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    20              // Record Subtype Value

    //Sensor Based Power Limit
    01              //Version
    C9              //Input sensor number
    FB              //Low threshold
    3C              //Low processor limit
    08              //Low memory limit
    00              //High threshold
    28              //High processor limit


_SDR_TYPE   C0
_SDR_TAG    '24HDD_LC'
_REC_LEN    0010
    
    // Sensor Record Header
    0172            // Record ID
    51              // SDR Version
    C0              // Record Type
    0B              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    20              // Record Subtype Value

    //Sensor Based Power Limit
    01              //Version
    C9              //Input sensor number
    FB              //Low threshold
    3C              //Low processor limit
    08              //Low memory limit
    00              //High threshold
    28              //High processor limit


_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0010
    
    // Sensor Record Header
    00FA            // Record ID
    51              // SDR Version
    C0              // Record Type
    0B              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    20              // Record Subtype Value

    //Sensor Based Power Limit
    01              //Version
    C9              //Input sensor number
    FB              //Low threshold
    3C              //Low processor limit
    08              //Low memory limit
    00              //High threshold
    28              //High processor limit


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0018
    
    // Sensor Record Header
    00FD            // Record ID
    51              // SDR Version
    C0              // Record Type
    13              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1A              // Record Subtype Value
    
    // Auto Profile Record
    01              // 70W CPU Multiplier (0Ah = 10 units of 0.1)
    01              // >70W and <105W CPU Multiplier (08h = 8 units of .1)
    01              // >105W and <145W CPU Multiplier(04h = 4 units of .1)
    02              // Memory Multiplier (08h = 8 units of 0.1)
    28              // HDD Multiplier (0Ah = 10 units of 0.1)
    05              // Minimum Performance Profile (06h = 6)
    19              // Profile 0 Threshold (22h = 34 units of 10)
    1E              // Profile 1 Threshold (36h = 54 units of 10)
    28              // Profile 2 Threshold (4Ah = 74 units of 10)
    32              // Profile 3 Threshold (5Dh = 93 units of 10)
    3C              // Profile 4 Threshold (87h = 135 units of 10)
    64              // Profile 5 Threshold (C7h = 199 units of 10)
    96              // Profile 6 Threshold (C8h = 200 units of 10)
    13              // PHI Card Shift/Max Profile [3:0] Card Shift - 4, [7:4] Max Profile - 7
    23              // PHI Shift/Max Profile [3:0] Shift - 7, [7:4] Max Profile - 7


_SDR_TYPE   C0
_SDR_TAG    '24HDDHSBP'
_REC_LEN    0018
    
    // Sensor Record Header
    00FE            // Record ID
    51              // SDR Version
    C0              // Record Type
    13              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1A              // Record Subtype Value
    
    // Auto Profile Record
    01              // 70W CPU Multiplier (0Ah = 10 units of 0.1)
    01              // >70W and <105W CPU Multiplier (08h = 8 units of .1)
    01              // >105W and <145W CPU Multiplier(04h = 4 units of .1)
    02              // Memory Multiplier (08h = 8 units of 0.1)
    14              // HDD Multiplier (0Ah = 10 units of 0.1)
    05              // Minimum Performance Profile (06h = 6)
    28              // Profile 0 Threshold (22h = 34 units of 10)
    2D              // Profile 1 Threshold (36h = 54 units of 10)
    32              // Profile 2 Threshold (4Ah = 74 units of 10)
    3C              // Profile 3 Threshold (5Dh = 93 units of 10)
    46              // Profile 4 Threshold (87h = 135 units of 10)
    64              // Profile 5 Threshold (C7h = 199 units of 10)
    96              // Profile 6 Threshold (C8h = 200 units of 10)
    13              // PHI Card Shift/Max Profile [3:0] Card Shift - 4, [7:4] Max Profile - 7
    23              // PHI Shift/Max Profile [3:0] Shift - 7, [7:4] Max Profile - 7


_SDR_TYPE   C0
_SDR_TAG    'EBCP-BNP'
_REC_LEN    0018
    
    // Sensor Record Header
    00FD            // Record ID
    51              // SDR Version
    C0              // Record Type
    13              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1A              // Record Subtype Value
    
    // Auto Profile Record
    01              // 70W CPU Multiplier (0Ah = 10 units of 0.1)
    01              // >70W and <105W CPU Multiplier (08h = 8 units of .1)
    01              // >105W and <145W CPU Multiplier(04h = 4 units of .1)
    02              // Memory Multiplier (08h = 8 units of 0.1)
    28              // HDD Multiplier (0Ah = 10 units of 0.1)
    05              // Minimum Performance Profile (06h = 6)
    19              // Profile 0 Threshold (22h = 34 units of 10)
    1E              // Profile 1 Threshold (36h = 54 units of 10)
    28              // Profile 2 Threshold (4Ah = 74 units of 10)
    32              // Profile 3 Threshold (5Dh = 93 units of 10)
    3C              // Profile 4 Threshold (87h = 135 units of 10)
    64              // Profile 5 Threshold (C7h = 199 units of 10)
    96              // Profile 6 Threshold (C8h = 200 units of 10)
    13              // PHI Card Shift/Max Profile [3:0] Card Shift - 4, [7:4] Max Profile - 7
    23              // PHI Shift/Max Profile [3:0] Shift - 7, [7:4] Max Profile - 7


_SDR_TYPE   C0
_SDR_TAG    'BP_X35_LC'
_REC_LEN    0018
    
    // Sensor Record Header
    015C            // Record ID
    51              // SDR Version
    C0              // Record Type
    13              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1A              // Record Subtype Value
    
    // Auto Profile Record
    00              // 70W CPU Multiplier
    00              // >70W and <105W CPU Multiplier
    00              // >105W and <145W CPU Multiplier
    02              // Memory Multiplier
    28              // HDD Multiplier
    05              // Minimum Performance Profile
    19              // Profile 0 Threshold
    1E              // Profile 1 Threshold
    28              // Profile 2 Threshold
    32              // Profile 3 Threshold
    3C              // Profile 4 Threshold
    64              // Profile 5 Threshold
    96              // Profile 6 Threshold
    13              // PHI Card Shift/Max Profile [3:0] Card Shift - 4, [7:4] Max Profile - 7
    23              // PHI Shift/Max Profile [3:0] Shift - 7, [7:4] Max Profile - 7


_SDR_TYPE   C0
_SDR_TAG    'EBCP-LC'
_REC_LEN    0018
    
    // Sensor Record Header
    0174            // Record ID
    51              // SDR Version
    C0              // Record Type
    13              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1A              // Record Subtype Value
    
    // Auto Profile Record
    00              // 70W CPU Multiplier
    00              // >70W and <105W CPU Multiplier
    00              // >105W and <145W CPU Multiplier
    02              // Memory Multiplier
    28              // HDD Multiplier
    05              // Minimum Performance Profile
    19              // Profile 0 Threshold
    1E              // Profile 1 Threshold
    28              // Profile 2 Threshold
    32              // Profile 3 Threshold
    3C              // Profile 4 Threshold
    64              // Profile 5 Threshold
    96              // Profile 6 Threshold
    13              // PHI Card Shift/Max Profile [3:0] Card Shift - 4, [7:4] Max Profile - 7
    23              // PHI Shift/Max Profile [3:0] Shift - 7, [7:4] Max Profile - 7


_SDR_TYPE   C0
_SDR_TAG    '24HDD_LC'
_REC_LEN    0018
    
    // Sensor Record Header
    0174            // Record ID
    51              // SDR Version
    C0              // Record Type
    13              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1A              // Record Subtype Value
    
    // Auto Profile Record
    00              // 70W CPU Multiplier
    00              // >70W and <105W CPU Multiplier
    00              // >105W and <145W CPU Multiplier
    02              // Memory Multiplier
    28              // HDD Multiplier
    05              // Minimum Performance Profile
    19              // Profile 0 Threshold
    1E              // Profile 1 Threshold
    28              // Profile 2 Threshold
    32              // Profile 3 Threshold
    3C              // Profile 4 Threshold
    64              // Profile 5 Threshold
    96              // Profile 6 Threshold
    13              // PHI Card Shift/Max Profile [3:0] Card Shift - 4, [7:4] Max Profile - 7
    23              // PHI Shift/Max Profile [3:0] Shift - 7, [7:4] Max Profile - 7


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0017
    
    // Sensor Record Header
    00FF            // Record ID
    51              // SDR Version
    C0              // Record Type
    12              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // Record Version
    03              // FSC Record type
    
    // Fan Sensor Domain Map
    06              // [7:4]Domain number/[3:0]sensor count
    30              // Sensor number Fan Sensor 1
    31              // Sensor number Fan Sensor 2
    32              // Sensor number Fan Sensor 3
    33              // Sensor number Fan Sensor 4
    34              // Sensor number Fan Sensor 5
    35              // Sensor number Fan Sensor 6
    24              // [7:4]Domain number/[3:0]sensor count
    A0              // Sensor number Fan Sensor 1
    A1              // Sensor number Fan Sensor 2
    A4              // Sensor number Fan Sensor 3
    A5              // Sensor number Fan Sensor 4


_SDR_TYPE   C0
_SDR_TAG    'EBCP-BNP'
_REC_LEN    0017
    
    // Sensor Record Header
    00FF            // Record ID
    51              // SDR Version
    C0              // Record Type
    12              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // Record Version
    03              // FSC Record type
    
    // Fan Sensor Domain Map
    06              // [7:4]Domain number/[3:0]sensor count
    30              // Sensor number Fan Sensor 1
    31              // Sensor number Fan Sensor 2
    32              // Sensor number Fan Sensor 3
    33              // Sensor number Fan Sensor 4
    34              // Sensor number Fan Sensor 5
    35              // Sensor number Fan Sensor 6
    24              // [7:4]Domain number/[3:0]sensor count
    A0              // Sensor number Fan Sensor 1
    A1              // Sensor number Fan Sensor 2
    A4              // Sensor number Fan Sensor 3
    A5              // Sensor number Fan Sensor 4


_SDR_TYPE   C0
_SDR_TAG    '24HDDHSBP'
_REC_LEN    0017
    
    // Sensor Record Header
    0100            // Record ID
    51              // SDR Version
    C0              // Record Type
    12              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // Record Version
    03              // FSC Record type
    
    // Fan Sensor Domain Map
    06              // [7:4]Domain number/[3:0]sensor count
    30              // Sensor number Fan Sensor 1
    31              // Sensor number Fan Sensor 2
    32              // Sensor number Fan Sensor 3
    33              // Sensor number Fan Sensor 4
    34              // Sensor number Fan Sensor 5
    35              // Sensor number Fan Sensor 6
    24              // [7:4]Domain number/[3:0]sensor count
    A0              // Sensor number Fan Sensor 1
    A1              // Sensor number Fan Sensor 2
    A4              // Sensor number Fan Sensor 3
    A5              // Sensor number Fan Sensor 4


_SDR_TYPE   C0
_SDR_TAG    'BP_X35_LC'
_REC_LEN    001B
    
    // Sensor Record Header
    015B            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // Record Version
    03              // FSC Record type
    
    // Fan Sensor Domain Map
    06              // [7:4]Domain number/[3:0]sensor count
    30              // Sensor number Fan Sensor 1
    31              // Sensor number Fan Sensor 2
    32              // Sensor number Fan Sensor 3
    33              // Sensor number Fan Sensor 4
    34              // Sensor number Fan Sensor 5
    35              // Sensor number Fan Sensor 6
    24              // [7:4]Domain number/[3:0]sensor count
    A0              // Sensor number Fan Sensor 1
    A1              // Sensor number Fan Sensor 2
    A4              // Sensor number Fan Sensor 3
    A5              // Sensor number Fan Sensor 4
    61              // [7:4]Domain number/[3:0]sensor count
    3C              // Sensor number Fan Sensor 1
    71              // [7:4]Domain number/[3:0]sensor count
    3D              // Sensor number Fan Sensor 1


_SDR_TYPE   C0
_SDR_TAG    'EBCP-LC'
_REC_LEN    001B
    
    // Sensor Record Header
    0173            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // Record Version
    03              // FSC Record type
    
    // Fan Sensor Domain Map
    06              // [7:4]Domain number/[3:0]sensor count
    30              // Sensor number Fan Sensor 1
    31              // Sensor number Fan Sensor 2
    32              // Sensor number Fan Sensor 3
    33              // Sensor number Fan Sensor 4
    34              // Sensor number Fan Sensor 5
    35              // Sensor number Fan Sensor 6
    24              // [7:4]Domain number/[3:0]sensor count
    A0              // Sensor number Fan Sensor 1
    A1              // Sensor number Fan Sensor 2
    A4              // Sensor number Fan Sensor 3
    A5              // Sensor number Fan Sensor 4
    61              // [7:4]Domain number/[3:0]sensor count
    3C              // Sensor number Fan Sensor 1
    71              // [7:4]Domain number/[3:0]sensor count
    3D              // Sensor number Fan Sensor 1


_SDR_TYPE   C0
_SDR_TAG    '24HDD_LC'
_REC_LEN    001B
    
    // Sensor Record Header
    0173            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // Record Version
    03              // FSC Record type
    
    // Fan Sensor Domain Map
    06              // [7:4]Domain number/[3:0]sensor count
    30              // Sensor number Fan Sensor 1
    31              // Sensor number Fan Sensor 2
    32              // Sensor number Fan Sensor 3
    33              // Sensor number Fan Sensor 4
    34              // Sensor number Fan Sensor 5
    35              // Sensor number Fan Sensor 6
    24              // [7:4]Domain number/[3:0]sensor count
    A0              // Sensor number Fan Sensor 1
    A1              // Sensor number Fan Sensor 2
    A4              // Sensor number Fan Sensor 3
    A5              // Sensor number Fan Sensor 4
    61              // [7:4]Domain number/[3:0]sensor count
    3C              // Sensor number Fan Sensor 1
    71              // [7:4]Domain number/[3:0]sensor count
    3D              // Sensor number Fan Sensor 1


_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    001D
    
    // Sensor Record Header
    0109            // Record ID
    51              // SDR Version
    C0              // Record Type
    18              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // Record Version
    03              // FSC Record type
    
    // Fan Sensor Domain Map
    06              // [7:4]Domain number/[3:0]sensor count
    30              // Sensor number Fan Sensor 1
    31              // Sensor number Fan Sensor 2
    32              // Sensor number Fan Sensor 3
    33              // Sensor number Fan Sensor 4
    34              // Sensor number Fan Sensor 5
    35              // Sensor number Fan Sensor 6
    16              // [7:4]Domain number/[3:0]sensor count
    30              // Sensor number Fan Sensor 1
    31              // Sensor number Fan Sensor 2
    32              // Sensor number Fan Sensor 3
    33              // Sensor number Fan Sensor 4
    34              // Sensor number Fan Sensor 5
    35              // Sensor number Fan Sensor 6
    61              // [7:4]Domain number/[3:0]sensor count
    36              // Sensor number Fan Sensor 1
    71              // [7:4]Domain number/[3:0]sensor count
    37              // Sensor number Fan Sensor 1


_SDR_TYPE   C0
_SDR_TAG    'TEST_PLATE'
_REC_LEN    001D
    
    // Sensor Record Header
    0101            // Record ID
    51              // SDR Version
    C0              // Record Type
    18              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // Record Version
    03              // FSC Record type
    
    // Fan Sensor Domain Map
    06              // [7:4]Domain number/[3:0]sensor count
    30              // Sensor number Fan Sensor 1
    31              // Sensor number Fan Sensor 2
    32              // Sensor number Fan Sensor 3
    33              // Sensor number Fan Sensor 4
    34              // Sensor number Fan Sensor 5
    35              // Sensor number Fan Sensor 6
    16              // [7:4]Domain number/[3:0]sensor count
    30              // Sensor number Fan Sensor 1
    31              // Sensor number Fan Sensor 2
    32              // Sensor number Fan Sensor 3
    33              // Sensor number Fan Sensor 4
    34              // Sensor number Fan Sensor 5
    35              // Sensor number Fan Sensor 6
    61              // [7:4]Domain number/[3:0]sensor count
    36              // Sensor number Fan Sensor 1
    71              // [7:4]Domain number/[3:0]sensor count
    37              // Sensor number Fan Sensor 1


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    000A
    
    // Sensor Record Header
    0102            // Record ID
    51              // SDR Version
    C0              // Record Type
    05              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1B              // Record Subtype Value
    16              // Watts


_SDR_TYPE   C0
_SDR_TAG    '24HDDHSBP'
_REC_LEN    000A
    
    // Sensor Record Header
    0103            // Record ID
    51              // SDR Version
    C0              // Record Type
    05              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1B              // Record Subtype Value
    26              // Watts


_SDR_TYPE   C0
_SDR_TAG    'EBCP-BNP'
_REC_LEN    000A
    
    // Sensor Record Header
    0103            // Record ID
    51              // SDR Version
    C0              // Record Type
    05              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1B              // Record Subtype Value
    03              // Watts


_SDR_TYPE   C0
_SDR_TAG    'BP_X35_LC'
_REC_LEN    000A
    
    // Sensor Record Header
    015D            // Record ID
    51              // SDR Version
    C0              // Record Type
    05              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1B              // Record Subtype Value
    16              // Watts


_SDR_TYPE   C0
_SDR_TAG    'EBCP-LC'
_REC_LEN    000A
    
    // Sensor Record Header
    0175            // Record ID
    51              // SDR Version
    C0              // Record Type
    05              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1B              // Record Subtype Value
    03              // Watts


_SDR_TYPE   C0
_SDR_TAG    '24HDD_LC'
_REC_LEN    000A
    
    // Sensor Record Header
    0103            // Record ID
    51              // SDR Version
    C0              // Record Type
    05              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1B              // Record Subtype Value
    26              // Watts


_SDR_TYPE   C0
_SDR_TAG    'DISABLE_NVME_FUNCTIONS'
_REC_LEN    000A
    
    // Sensor Record Header
    0200            // Record ID
    51              // SDR Version
    C0              // Record Type
    05              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    22              // Record Subtype Value (Enable NVMe access)
    
    // Enable NVMe access
    00              // 00 = disable 01 = enable


_SDR_TYPE   C0
_SDR_TAG    'ENABLE_NVME_FUNCTIONS'
_REC_LEN    000A
    
    // Sensor Record Header
    0200            // Record ID
    51              // SDR Version
    C0              // Record Type
    05              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    22              // Record Subtype Value (Enable NVMe access)
    
    // Enable NVMe access
    01              // 00 = disable 01 = enable


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    'EBCP-BNP'
_SDR_TAG    'BP_X35_LC'
_SDR_TAG    'EBCP-LC'
_REC_LEN    000B
    
    // Sensor Record Header
    0201            // Record ID
    51              // SDR Version
    C0              // Record Type
    06              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1D              // Record Subtype Value (SSD Combo HSBP)
    
    // SSD Combo HSBP
    00              // HSBP Index
    00              // HSBP PBA class        


_SDR_TYPE   C0
_SDR_TAG    '24HDDHSBP'
_SDR_TAG    '24HDD_LC'
_REC_LEN    000B
    
    // Sensor Record Header
    0201            // Record ID
    51              // SDR Version
    C0              // Record Type
    06              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1D              // Record Subtype Value (SSD Combo HSBP)
    
    // SSD Combo HSBP
    00              // HSBP Index
    02              // HSBP PBA class


_SDR_TYPE   C0
_SDR_TAG    '24HDDHSBP'
_SDR_TAG    '24HDD_LC'
_REC_LEN    0009
    
    // Sensor Record Header
    0108            // Record ID
    51              // SDR Version
    C0              // Record Type
    04              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1F              // Record Subtype Value (24HDD HSBP)


_SDR_TYPE   C0
_SDR_TAG    'TEST_PLATE'
_REC_LEN    000B
    
    // Sensor Record Header
    0201            // Record ID
    51              // SDR Version
    C0              // Record Type
    06              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1D              // Record Subtype Value (SSD Combo HSBP)
    
    // SSD Combo HSBP
    00              // HSBP Index
    03              // HSBP PBA class (NULL HSBP)


_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    000B
    
    // Sensor Record Header
    0201            // Record ID
    51              // SDR Version
    C0              // Record Type
    06              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    1D              // Record Subtype Value (SSD Combo HSBP)
    
    // SSD Combo HSBP
    00              // HSBP Index
    03              // HSBP PBA class (NULL HSBP)


_SDR_TYPE   C0
_SDR_TAG    'TEST_PLATE'
_REC_LEN    001B
    
    // Sensor Record Header
    0104            // Record ID
    51              // SDR Version
    C0              // Record Type
    16              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    C5              // Domain Support
    FF              // Fan Profile Support

    // Domain Configuration Sub-record
    01              // FSC Sub-record type
    32              // Normal Control Value
    64              // Ramp Step
    01              // Scan Rate
    FF              // Fan fault boost value
    64              // Temperature threshold boost value
    64              // Chassis cover boost value
    00              // Sensor exclusion count (N)
    // Stepwise sub-record (lower clipping curve)
    02              // FSC Sub-record type
    01              // Global Stepwise header ID
    0C              // Global Stepwise curve ID
    // Stepwise sub-record (upper clipping curve)
    02              // FSC Sub-record type
    01              // Global Stepwise header ID
    04              // Global Stepwise curve ID


_SDR_TYPE   C0
_SDR_TAG    'TEST_PLATE'
_REC_LEN    0039
    
    // Sensor Record Header
    0106            // Record ID
    51              // SDR Version
    C0              // Record Type
    34              // Record Length
    
    // Record Key Bytes
    570100          // Manufacturer ID
    0C              // Record Subtype Value
    02              // FSC version
    08              // FSC Record type

    // Record Body Bytes
    C5              // Domain Support
    FF              // Fan Profile Support

    // Clamp sub-record 1
    03              // FSC Sub-record type
    74              // Global Clamp ID
    // Clamp sub-record 2
    03              // FSC Sub-record type
    75              // Global Clamp ID
    // Clamp sub-record 3
    03              // FSC Sub-record type
    B0              // Global Clamp ID
    // Clamp sub-record 4
    03              // FSC Sub-record type
    B1              // Global Clamp ID
    // Clamp sub-record 5
    03              // FSC Sub-record type
    B2              // Global Clamp ID
    // Clamp sub-record 6
    03              // FSC Sub-record type
    B3              // Global Clamp ID
    // Clamp sub-record 7
    03              // FSC Sub-record type
    24              // Global Clamp ID
    // Clamp sub-record 8
    03              // FSC Sub-record type
    23              // Global Clamp ID
    // Clamp sub-record 9
    03              // FSC Sub-record type
    25              // Global Clamp ID
    // Clamp sub-record 10
    03              // FSC Sub-record type
    22              // Global Clamp ID
    // Clamp sub-record 11
    03              // FSC Sub-record type
    26              // Global Clamp ID
    // Clamp sub-record 12
    03              // FSC Sub-record type
    2F              // Global Clamp ID
    // Clamp sub-record 13
    03              // FSC Sub-record type
    2E              // Global Clamp ID
    // Clamp sub-record 14
    03              // FSC Sub-record type
    14              // Global Clamp ID
    // Clamp sub-record 15
    03              // FSC Sub-record type
    9E              // Global Clamp ID
    // Clamp sub-record 16
    03              // FSC Sub-record type
    93              // Global Clamp ID
    // Clamp sub-record 17
    03              // FSC Sub-record type
    27              // Global Clamp ID
    // Clamp sub-record 18
    03              // FSC Sub-record type
    2C              // Global Clamp ID
    // Clamp sub-record 19
    03              // FSC Sub-record type
    29              // Global Clamp ID
    // Clamp sub-record 20
    03              // FSC Sub-record type
    44              // Global Clamp ID
    // Clamp sub-record 21
    03              // FSC Sub-record type
    45              // Global Clamp ID
    // Clamp sub-record 22
    03              // FSC Sub-record type
    46              // Global Clamp ID


_SDR_TYPE   C0
_REC_LEN    0010
    
    // Sensor Record Header
    0000            // Record ID
    51              // SDR Version
    C0              // Record Type
    0B              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    0D              // Record Subtype Value (NM Discovery)
    
    // NM Discovery
    01              // Version number of record subtype
    2C              // NM Device Slave Address ([7:1] - 7-bit address; [0] - reserved)
    60              // [7:4] - channel number (6 for secondary IPMB) [3:2] - reserved [1:0] - sensor owner LUN)
    19              // Node Manager Health Event sensor
    18              // Node Manager Exception Event sensor
    1A              // Node Manager Operational Capabilities sensor
    1B              // Node Manager Threshold Exceeded sensor


_SDR_TYPE   C0
_REC_LEN    0036
    
    // Sensor Record Header
    0130            // Record ID
    51              // SDR Version
    C0              // Record Type
    31              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    11              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    96              // M
    00              // M, Tolerance
    88              // B
    C0              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    C1              // R exp, B exp
    07              // Analog characteristic flags
    E4              // Nominal Reading
    EF              // Normal Maximum
    D9              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    CD              // Lower critical
    D4              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    C4              // Type/Length Code
    'P3V3'          // String Bytes


_SDR_TYPE   C0
_REC_LEN    003E
    
    // Sensor Record Header
    0131            // Record ID
    51              // SDR Version
    C0              // Record Type
    39              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    12              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    B2              // M
    40              // M, Tolerance
    97              // B
    C0              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    B1              // R exp, B exp
    07              // Analog characteristic flags
    DE              // Nominal Reading
    EF              // Normal Maximum
    C1              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    B7              // Lower critical
    BC              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    CC              // Type/Length Code
    'PVNN_PCH_AUX'  // String Bytes


_SDR_TYPE   C0
_REC_LEN    003F
    
    // Sensor Record Header
    0132            // Record ID
    51              // SDR Version
    C0              // Record Type
    3A              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    13              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    C2              // M
    40              // M, Tolerance
    3C              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    B1              // R exp, B exp
    07              // Analog characteristic flags
    E8              // Nominal Reading
    EF              // Normal Maximum
    E1              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    D6              // Lower critical
    DC              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    CD              // Type/Length Code
    'P1V05_PCH_AUX' // String Bytes


_SDR_TYPE   C0
_SDR_TAG    'S2600BPP'
_SDR_TAG    'S2600BPQ'
_SDR_TAG    'S2600BPL'
_REC_LEN    003F
    
    // Sensor Record Header
    0133            // Record ID
    51              // SDR Version
    C0              // Record Type
    3A              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    14              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    64              // M
    40              // M, Tolerance
    DA              // B
    40              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    B0              // R exp, B exp
    07              // Analog characteristic flags
    E8              // Nominal Reading
    EF              // Normal Maximum
    E1              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    D5              // Lower critical
    DC              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    CD              // Type/Length Code
    'P0V83_LAN_AUX' // String Bytes


_SDR_TYPE   C0
_REC_LEN    003A
    
    // Sensor Record Header
    0134            // Record ID
    51              // SDR Version
    C0              // Record Type
    35              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    15              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    37              // M
    00              // M, Tolerance
    26              // B
    C0              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    D0              // R exp, B exp
    07              // Analog characteristic flags
    E0              // Nominal Reading
    EB              // Normal Maximum
    D5              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    C6              // Lower critical
    CC              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    C8              // Type/Length Code
    'P12V_AUX'      // String Bytes


_SDR_TYPE   C0
_REC_LEN    003A
    
    // Sensor Record Header
    0135            // Record ID
    51              // SDR Version
    C0              // Record Type
    35              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    16              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    4D              // M
    00              // M, Tolerance
    B4              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    C0              // R exp, B exp
    07              // Analog characteristic flags
    E7              // Nominal Reading
    EE              // Normal Maximum
    E0              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    D4              // Lower critical
    DA              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    C8              // Type/Length Code
    'P1V8_PCH'      // String Bytes


_SDR_TYPE   C0
_REC_LEN    003D
    
    // Sensor Record Header
    0136            // Record ID
    51              // SDR Version
    C0              // Record Type
    38              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    17              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    56              // M
    00              // M, Tolerance
    87              // B
    C0              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    C0              // R exp, B exp
    07              // Analog characteristic flags
    D3              // Nominal Reading
    EE              // Normal Maximum
    AB              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    A1              // Lower critical
    A6              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    CB              // Type/Length Code
    'PVCCIN_CPU0'   // String Bytes


_SDR_TYPE   C0
_REC_LEN    003D
    
    // Sensor Record Header
    0137            // Record ID
    51              // SDR Version
    C0              // Record Type
    38              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    18              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    56              // M
    00              // M, Tolerance
    87              // B
    C0              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    C0              // R exp, B exp
    07              // Analog characteristic flags
    D3              // Nominal Reading
    EE              // Normal Maximum
    AB              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    A1              // Lower critical
    A6              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    CB              // Type/Length Code
    'PVCCIN_CPU1'   // String Bytes


_SDR_TYPE   C0
_REC_LEN    0040
    
    // Sensor Record Header
    0138            // Record ID
    51              // SDR Version
    C0              // Record Type
    3B              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    19              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    33              // M
    00              // M, Tolerance
    45              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    C0              // R exp, B exp
    07              // Analog characteristic flags
    E8              // Nominal Reading
    EF              // Normal Maximum
    E1              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    D6              // Lower critical
    DC              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    CE              // Type/Length Code
    'PVDDQ_ABC_CPU0'// String Bytes


_SDR_TYPE   C0
_REC_LEN    0040
    
    // Sensor Record Header
    0139            // Record ID
    51              // SDR Version
    C0              // Record Type
    3B              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    1A              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    33              // M
    00              // M, Tolerance
    45              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    C0              // R exp, B exp
    07              // Analog characteristic flags
    E8              // Nominal Reading
    EF              // Normal Maximum
    E1              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    D6              // Lower critical
    DC              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    CE              // Type/Length Code
    'PVDDQ_DEF_CPU0'// String Bytes


_SDR_TYPE   C0
_REC_LEN    0040
    
    // Sensor Record Header
    013A            // Record ID
    51              // SDR Version
    C0              // Record Type
    3B              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    1B              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    33              // M
    00              // M, Tolerance
    45              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    C0              // R exp, B exp
    07              // Analog characteristic flags
    E8              // Nominal Reading
    EF              // Normal Maximum
    E1              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    D6              // Lower critical
    DC              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    CE              // Type/Length Code
    'PVDDQ_ABC_CPU1'// String Bytes


_SDR_TYPE   C0
_REC_LEN    0040
    
    // Sensor Record Header
    013B            // Record ID
    51              // SDR Version
    C0              // Record Type
    3B              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    1C              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    33              // M
    00              // M, Tolerance
    45              // B
    00              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    C0              // R exp, B exp
    07              // Analog characteristic flags
    E8              // Nominal Reading
    EF              // Normal Maximum
    E1              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    D6              // Lower critical
    DC              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    CE              // Type/Length Code
    'PVDDQ_DEF_CPU1'// String Bytes


_SDR_TYPE   C0
_REC_LEN    003D
    
    // Sensor Record Header
    013C            // Record ID
    51              // SDR Version
    C0              // Record Type
    38              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    1D              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    DA              // M
    40              // M, Tolerance
    2D              // B
    C0              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    B0              // R exp, B exp
    07              // Analog characteristic flags
    D4              // Nominal Reading
    EF              // Normal Maximum
    A3              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    9A              // Lower critical
    9F              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    CB              // Type/Length Code
    'PVCCIO_CPU0'   // String Bytes


_SDR_TYPE   C0
_REC_LEN    003D
    
    // Sensor Record Header
    013D            // Record ID
    51              // SDR Version
    C0              // Record Type
    38              // Record Length
    
    // Record body bytes
    570100          // Manufacturer ID
    34              // Record Subtype Value
    
    // Record Key Bytes
    20              // Sensor Owner ID
    00              // Sensor Owner LUN
    1E              // Sensor Number
    
    // Record Body Bytes
    07              // Entity ID
    01              // Entity Instance
    7F              // Sensor Initialization
    68              // Sensor Capabilities
    02              // Sensor Type
    01              // Event / Reading Base Type
    0000            // Assertion Event Mask
    0000            // Deassertion Event Mask
    0000            // Reading Mask & Settable / Readable Threshold Masks
    00              // Sensor Units 1
    04              // Sensor Units 2
    00              // Sensor Units 3
    00              // Linearization
    DA              // M
    40              // M, Tolerance
    2D              // B
    C0              // B, Accuracy
    00              // Accuracy, Accuracy Exp
    B0              // R exp, B exp
    07              // Analog characteristic flags
    D4              // Nominal Reading
    EF              // Normal Maximum
    A3              // Normal Minimum
    FF              // Sensor Maximum Reading
    00              // Sensor Minimum Reading
    FF              // Upper non-recoverable
    FC              // Upper critical
    F5              // Upper non-critical
    00              // Lower non-recoverable
    9A              // Lower critical
    9F              // Lower non-critical
    01              // Positive hysteresis value
    01              // Negative hysteresis value
    45              // OEM
    CB              // Type/Length Code
    'PVCCIO_CPU1'   // String Bytes


_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0015
    
    // Sensor Record Header
    0119            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    'SDR File 1.39'  // String Bytes


_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0018
    
    // Sensor Record Header
    011A            // Record ID
    51              // SDR Version
    C0              // Record Type
    13              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    'SDR Package 1.39'// String Bytes


_SDR_TYPE   C0
_REC_LEN    0015
    
    // Sensor Record Header
    011B            // Record ID
    51              // SDR Version
    C0              // Record Type
    10              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    'SDR File 1.39' // String Bytes


_SDR_TYPE   C0
_REC_LEN    0018
    
    // Sensor Record Header
    011C            // Record ID
    51              // SDR Version
    C0              // Record Type
    13              // Record Length
    
    // Record Body Bytes
    570100          // Manufacturer ID
    'SDR Package 1.39'// String Bytes



)
