# oparesolvehfiport

(Host) Permits the Intel® Omni-Path Fabric Host Software style Intel® Omni-Path Host Fabric Interface (HFI) number and port number arguments to be converted to a Host Software style HFI name and physical port number.

## Syntax

    oparesolvehfiport [-o output] [hfi] [port]

## Options

`--help`

  Produces full help text.

`-o output`

  Specifies the output type.

  `devname`

    Prints the device name, in the format hfiname:portnum (Default).

  `hfinum`

    Prints the hfi number.

`hfi`

  Specifies the HFI, numbered 1..n. Using 0 specifies that the -p port port is a system-wide port number. Default is 0.

`port`

  Specifies the port, numbered 1..n. Using 0 specifies the first active port. Default is 0.

  The HFI and port permit a variety of selections:
  `0 0`

    First active port in system.

  `x 0`

    First active port on HFI x.

  `0 y`

    Port y within system (no matter which ports are active).

  `x y`

    HFI x, port y

## Examples

    oparesolvehfiport 0 1                #Output: hfi1_0:1
    oparesolvehfiport -o devname 0 1     #Output: hfi1_0:1
    oparesolvehfiport -o hfinum 0 1      #Output: 1