================================================================================
Intel(R) Server Board S2600WF, Intel(R) Server System R1000WF Product Family and
Intel(R) Server System R2000WF Product Family Firmware Update Package
for Intel(R) One Boot Flash Update Utility and Windows* Preboot Execution Environment 
================================================================================
Intel(R) Server Boards and Systems
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : 	Oct 16, 2018
TO      : 	Intel(R) Server Board S2600WF Product Family 
			Intel(R) Server System R1000WF Product Family 
			Intel(R) Server System R2000WF Product Family               
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : 00.01.0014
ME     : 04.00.04.340
BMC    : 1.60.56383bef
FRUSDR : 1.60
================================================================================
                           Support Platforms and Dependency
================================================================================
Processors supported: 
Intel(R) Xeon(R) Scalable processors

Microcode versions:
        CPUID           Version       Status
        0x50653        0x01000144     (Xeon Scalable B1)
        0x50654        0x0200004D     (Xeon Scalable H0)

The following update process must be followed to ensure a trouble free update.
1.	BMC firmware
2.	BIOS
3.	Manageability Engine (ME) firmware
4. 	FD
5.	FRUSDR

================================================================================
                             IMPORTANT NOTE!!!                   
================================================================================
 - This Update package must be installed using 
   Intel(R) One-boot Flash Update (OFU) V14.1 Build 14 or later
   
1. Package C-State only works well with Xeon Scalable Family H0 parts, for other Xeon Scalable Family stepping, C6 non-retention is hardcode from BIOS side.
2. BIOS R00.01.0001 does not support online downgrade to any Dxxx or Xxxx BIOS.
3. BIOS R00.01.0001 removed Xeon Scalable Family A1 microcode(m1350651_8000002B) and Xeon Scalable Family B0 microcode(m9750652_80000035).
4. Removed 'UpdateNvram' support for iflash32 tool for security reason of SRA bios.
5. Security revision upgrade to v0002 on BIOS R00.01.0002 will prevent BIOS downgrade via normal mode to R00.01.0001, user can use BIOS recovery mode for BIOS downgrade. Although Intel doesn't recommend downgrading firmware
6. One new production key is integrated onto R0004 BIOS, which will correct an OEM string. 
7. This release include security revision upgrade to version 0004. This will prevent BIOS downgrade via normal mode to previous version with lower security revision, user can use BIOS recovery mode process for BIOS downgrade.
8. System will prevent downgrading ME from 04.00.04.288 to 04.00.04.235 or older version, if system BIOS version is R0009. This is an expected behavior. 
9. Security revision upgrade to 0005 since BIOS R010, it will prevent BIOS downgrade via normal mode to previous version that with lower security revision, user can use BIOS recovery mode for BIOS downgrade.
10. Downgrading BMC below 1.43.660a4315 is not supported due to a security revision change. 
================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   V14.1 Build 14 or later)
 - Windows* Preboot Execution Environment (WinPE)

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from http://downloadcenter.intel.com/
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel(R) OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from http://downloadcenter.intel.com/
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE_x64_Update.bat"
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB flash drive from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB flash drive manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x64 OS, you have to read
OFU release notes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x64_Update.bat" 
for WinPE2.1/3.0 64 bit solution as an example. Please refer to white paper 
"White Paper-Intel Server Utilities Procedure for WinPE.pdf" for details on 
building your own customized WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.1 - built from Windows Server 2008 R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.

================================================================================
                         BIOS R00.01.0014(This release)
================================================================================
Rename BIOS ID from X0149 to R0014.
HSD-ES:1605354891, TPM Update fail on S2600ST and S2600WF
OSS_0008036:       Update Microcode 0x4d for Xeon Scalable H0 and 0x144 for Xeon Scalable B1  
                   Reference code version: 20180612_CP_PURLEY_PRODUCTION_155_R08 
                   [PC Stitching] Update OPA UEFI driver to v1.6.0.0.0 
HSD-ES:1506124820, CCB2334 [PSIRT Factory BMC & BIOS] enabling one-time software update to any version
OSS_0007838,       [PC Stitching]Update ME SPS version to 340
HSD-ES:2103621945, [S2600BP] Windows2016 cannot be installed with SATA port5+port7 RSTe RAID0
HSD-ES:1506125508, Other PCI device's SsidSvid is 0xFFFFFFFF and is different from NIC Controller on SFP+ S2600BP board
HSD-ES:1506122324, Higher security ID from 1.05 to 1.06 because HECI PRT and Backup BIOS PRT patch
HSD-ES:1504762466, BIOS Change for #CCB 2083[Syscfg tool]Add option to configure fan pwm offset in syscfg
HSD-ES:2202640819, System will not boot to IPV4 PXE if UEFI Network Stack disabled for IPV6 PXE in BIOS
HSD-ES:1504784817, CCB2267[BMC+BIOS]Need mechanism for BMC to return MAC addresses for add-in card on demand
HSD-ES:2103622021, Toshiba THNSN5128GPU7 M.2 PCIe SSD can't detect successful under Win2016 OS.
HSD-ES:1504707008, CCB2222 [BIOS] Add Infineon FW update capability support in BIOS and UEFI application
HSD-ES:2007351694, BSOD after warm reboot if HT is enabled with Windows Server 2016 version 17663 and 17666
HSD-ES:2103621261, [S2600WF]SMBIOS Type 8 NIC number does not match motherboard number 
HSD-ES:1504713715, [CCB#2284][S2600WF&S2600BP]Fix system will hang with POST code 0x94 when one riser slot of HOST connects two WRG JBOD nodes with 32 RSSDs
HSD-ES:1406736015, BIOS does not return Type 199 records
HSD-ES:1504707003, CCB1822 Support Relax Ordering and No Snoop in BIOS setup and ITK
HSD-ES:1504749247, [S2600WF]bios_wp protection has not been enabled
HSD-ES:1504749852, CCB2249 Add SMBIOS OEM String modification capability in ITK
HSD-ES:1504771459, After clear CMOS, EWS does not display about CMOS log when boot to BIOS setup
HSD_ES:2103620812, MMIO size set to Auto/1G can't boot to BIOS with NIC Card-XL710 in Legacy mode 
HSD-ES:1504762466, BIOS Change for #CCB 2083 [Syscfg tool]Add option to configure fan pwm offset in syscfg
HSD-ES:2103616363, Inject Memory Address Parity error and no error event occurred in SEL accordingly
HSD-ES:1504630755, Change "CPU Power and Performance Policy" from "Balanced Performance" to "Performance" on the custom BIOS capsule by ITK tool, related items "C1E" can not be changed automatically.
HSD-ES:1504788000, CL541242  5386244: BaseTraceHubInitLibNull references non-existing SkylakeSiPkg
HSD-ES:1504788000, CL547293  5386319: Xeon Scalable 2933 mc transient error
HSD-ES:1504788000, CL556508  5386005: BIOS NTB PPD Option Setup is Reversed
HSD-ES:1504788000, CL558559  5386307: Some validated DIMMs have not been included in the DimmWT4 table
HSD-ES:1504788000, CL558628  5385969: Advanced Memory Test failed at MT_CPGC_READ_WRITE   
HSD-ES:1504788000, CL570837  5386628: HECI_MBAR can be reallocated by ring-0 anywhere in the address map (BIOS vulnerability)
HSD-ES:1504788000, CL569535  5386412: 2 SKT DEBUG build ASSERTs with a Security Violation
HSD-ES:1504788000, CL566239  5386475: System hangs after error injection during DIMM Address Translation
HSD-ES:1504788000, CL571328  5386488: 2006702382: NVDIMM not in memory map when NUMA is disabled
HSD-ES:1504788000, CL576560  5386813: Enable MSR_VIRTUAL_MSR_LLC_PREFETCH reconfiguration on Skylake B-step
HSD-ES:1504788000, CL579507  5386817: Add device IDs for QS/PRQ S LBG SKU
OSS_0006624:       Integration BIOS ACM to 1.3.6 and SINIT to 1.3.3
OSS_0007339:       [PC Stitching] Update ME SPS version to 333
HSD-ES:2202565747, BIOS POST messaging shows no errors when in fact a DIMM is mapped out
HSD-ES:1504788000, CL575833 5386751: Function RemovePsfAccess () is not called with SPS FW binary
HSD-ES:1504788000, CL582692 5386573: IioEarlyInit.c:IioPciePortEWL() swaps link_width and link_speed in EWL
HSD-ES:1504788000, CL558927 5386052: [220586227] Early SEC RC is not properly programming the HPET due to coding bug, causing rogue write to memory [IPS 220586227]
HSD-ES:1504788000, CL 553223 + CL556549 5386074: ACPI table will miss some core with some specific bit mask processor
HSD-ES:1504790255, Clone from 5386949 FW-UEFI-Vuln-2018-008 - "PSIRT-BIOS-2018-008 Additional protection for DCI enable"
HSD-ES:2103617388, When hotplug NVMe HDDs the RSTe GUI location couldn't match actual HDDs location
HSD-ES:1505084878, XL710 show the same boot order name in Boot management
HSD-ES:1505083003, CCB 2161 [BIOS]Support more memory vendor DIMMs -- Apacer,ATP,Hyundai,Innodisk,intelimem,V Color
HSD-ES:1505083055, CCB 2401 [BIOS] BIOS support for WFC, WFD, WFS cluster systems
HSD-ES:2103619811, [S2600BP] Boot manager still show pcie device if disable it on PCIe Port Oprom Control. -->Fix CL552580 side effect
HSD-ES:2103620496, NIC Port Mapping between Chassis and Windows Server OS are inverted on S2600BP SFP+, RJ45 and S2600WFT
OSS_0006929:       [PC Stitching] Update RSTE Drivers to v5.4.0.1039
HSD-ES:2103621959, EWS and SEL viewer shown incorrect ME version when online update ME version
HSD-ES:1504784817, CCB2267 [BMC+BIOS]Need mechanism for BMC to return MAC addresses for add-in card on demand
HSD-ES:1505330637, Add two APIs in fast video ppi and protocol
HSD-ES:2103620418, [S2600WF] After downgrade FD and ME, SUT will halt with beep code 1-5-1-2 when reboot
		
===============================================================================
		BMC v1.60.56383bef - (Release version)
===============================================================================
    1407264248 - [S2600BP] BMC is not reporting redundancy lost by clearing STATUS_INPUT flags from PSU
    1506122908 - [S2600WF]The AIC Product Name information returned is replaced by part MAC address of the third cards when the connected AIC Cards are greater than two.
    1506123447 - BMC User and Network setting will change to default after online update BMC to 1.59.ba077703&AC cycle
    1505567118 - [S2600BT]SSL/TLS use of weak RC4 cipher
    1505573379 - [S2600BT]Birthday attacks against TLS ciphers with 64bit block size vulnerability (Sweet32)
    1506114971 - [S2600ST] Chinese characters are not displayed properly in Event Log page while login Web in Chinese
    1506118999 - Q2'18 #CCB2434 [Purley BMC]Implement 0xD5 return code when user requests power on and system is already on
    1506119149 - Completion code for OEM get sensor reading(platform power consumption) isn't right when no ADM chipset is available.
    1506123447 - BMC User and Network setting will change to default after online update BMC to 1.59.ba077703&AC cycle
    2103620859 - [S2600BT] Media will be unmounted after boot into OS
    2103621752 - [S2600WF] Media will be unmounted after boot into OS
    2103622022 - [S2600BT] Event log page can't be read via IE browser
    2103622102 - [S2600WF] The Event Log shown abnormally on EWS after pressed NMI Button.
    2103622115 - EWS: Use firefox browser to check the system event log, all the information is unreadable code unless clearing the browser cache
    2103622127 - EWS: There is a unreadable character in the system event log
    2103622137 - EWS: When set the language to Chinese, the event log information show unreadable characters
    2103622142 - EWS: It could not establish the session to EWS after setting the https port to customized value
    2103622186 - [S2600BT] BMC can't stuck in Safe mode after execute 4 times BMC watchdog
    2103622241 - [S2600BT] HTTPS Port can't login from other values after HTTPS Port modify 8443
    2203123584 - Remote ipmitool chassis power off returns error when chassis is already off.
    2203745825 - [KVM/VM] Virtual Media redirection fails installing OS and console spews SSL errors
    1504766995 - [S2600BP LCR]Sensors are not correctly display in one cycle when run AC/DC cycle test
    2103622260 - [S2600BT] Enable Remote Debug function command response incorrect via BMC Shared LAN IP

v1.59.ba077703(Internal version)
    1506118927 - Q2'18 #CCB2427  [Purley BMC]Increase KVM timeout to 1+ minutes
    2103614048 - EWS User Enable is blank
    2103621847 - [S2600BT] EWS some information will be abnormal via IE browser
    2103621983 - [S2600ST] There is no display information for DIMM and FRU in system information while login Web by using IE
    2103622082 - [S2600WF] Event log page can't be read via IE browser
    2103622113 - IE: After updating the BMC_1.58.eafa53ef, it could not show the system event log in EWS
    2202696827 - BMC EWS GUI SEL Fails to Finish Loading
    2203669681 - BMC Web console fails to show FRU and Memory information after update to SUP x0135
    1506077858 - [S2600BP LCR]Event log “Sensor failure—HSBP temp -- Asserted” during AC/DC/linpack test
    1504651008 - Sometimes system will generate an abnormal event log about “Sensor failure—HSBP temp -- Asserted” and status LED show green blinking
    220857900 - [S2600BP] 17 of 3456 nodes  ( 9 of 864 system) failed EST for intermittent BMC FW Health unable to read HSBP Temp sensor
    2103620331 - [S2600BT]profile can't be shifted by the riser number
    1505815184 - RKVM can't launch if we have setup port forward from external IP address to internal address
    2103622022 - [S2600BT] Event log page can't be read via IE browser

v1.58.eafa53ef(Internal version)
    2103621764 - [S2600BT] Network configuration will be abnormal on EWS after stress VLAN ID test
    2103621770 - [S2600WF] Network configuration page can't worked on EWS after stress VLAN ID test
    2202676945 - Get Security Version Information returns 00 00, hence no way to know the security revision of the firmware.
    2202770366 - ReadSelfTest command response not as expected and the command missing in EPS
    2202843495 - [KVM/VM] Java pegs the CPUs on Linux when kvm/virtual media loses connection to the BMC
    2203284099 - [KVM] - The TLS ciphers used by KVM (port 5902) and USB (port 627) allow weak encryption algorithms and ciphers

v1.57.ba2942a4(Internal version)
    2103621726 - [VMviewer] The History will shown duplicate messages after mount image files via VMViewer.
    2103621885 - EWS: Use IE browser, it could show the baseboard serial number string
    2202676945 - Get Security Version Information returns 00 00, hence no way to know the security revision of the firmware.
    2202696827 - BMC EWS GUI SEL Fails to Finish Loading
    2202731630 - [EWS] Lower privilege user (operator, user) can update session timeout for all users
    2203103848 - [Redfish] Account Service with user privilege leaks user information

v1.56.18cf2437(Internal version)
    1504745080 - [S2600BP LCR]PS1/PS2 Input Power/Curr Out %/Temperature sensors show no reading or disabled and need unplug/plug nodes to recovery during AC cycling
    2202314699 - RSD 2.2 -TPM setting by PSME via POST command is not implemented yet
    1504716901 - It takes more than 10 second to get MTT CPU1/2 sensor

v1.55.cfacd447(Internal version)
    2103621780 - The name of menu bar is incorrect on KVM
    2202485388 - Redfish - Discrepancy in PATCH body for  BootSourceOverride Action
    2202039060 - MSM PS script 1.13. issue with "debuglog" command
    2103620859 - [S2600BT] Media will be unmounted after boot into OS
    2103621667 - [S2600BT] The login screen of EWS page shown abnormal with OEM customized image
    2103621528 - [S2600BT] The login screen of EWS page shown abnormal
    2103620331 - [S2600BT]profile can't be shifted by the riser number

v1.54.aec2b430(Internal version)
    1504707042 - Q1'18 #CCB2201[Purley BMC]Need OpenLDAP support in BMC
    1504765942 - Setting IPv4 Network is abnormal via EWS
    2103621229 - [S2600WF] The Alerts Destination configuration can't save on EWS when SUT no install OCP card.
    2103621677 - [S2600BT] Setting IPv4 Network is abnormal via EWS
    2103621719 - [S2600BT] Alert Mail delivery failed via EWS settings
    2202534178 - [redfish] several properties are missing from /redfish/v1/Managers/BMC/EthernetInterfaces/1

v1.53.463a2c11(Internal version)
    1504749848 - Q2'18 #CCB2257 Q2'18 [Purley]Add OEM command to provide global reset capability for Syscfg(Graceful shutdown, then automatically power on after powering off)
    2103621462 - [S2600BT] The SEL description is incorrect when trigger the FPGA CATERR.
    2103621525 - Failed in setting up SNMP alert destination with IPv6 address in the SUT's EWS
    2103621597 - [S2600BT] The SEL doesn't "Power off/down" event logged after DC Cycle.
    2103621603 - [S2600WF] User 1(Anonymous) can't be modify in EWS users page.
    2202039060 - MSM PS script 1.13. issue with "debuglog" command
    2202534178 - [redfish] several properties are missing from /redfish/v1/Managers/BMC/EthernetInterfaces/1
    2103621661 - [S2600BT] There are no thermal trip/IERR deasserted events logged on SEL
    2103621582 - [S2600WF] The sensor type of SMI timeout is not match with EPS 1.12
    2202525692 - [redfish] AssetTag is missing from Systems/{ID}

v1.52.0bfa4b80(Internal version)
    1504743210 - EWS will auto login out after click "Clear Event log", and event log can't be cleared by EWS
    2103621502 - [S2600BT] EWS will be forced to logout when click Clear Event Log.
    2103621528 - [S2600BT] The login screen of EWS page shown abnormal
    2202565737 - BMC SEL Incorrectly Reports DIMM Slot with Failed DIMM in CPU2 Slot C1
    
v1.51.f1fd06fa(Internal version)
    2006708660 - BB P1- P2 VR Temp issue during AC Cycling
    2103621270 - Unusual thermal critical events in JBOD BMC log during QRC (AC/DC/Warm reboot) cycling test
    2103621381 - [S2600BT] There are two OEM Sensors in EWS sensor type category
    2103621464 - [S2600BT] EWS will be forced to logout when use Operator and User privilege
    2201838395 - Redfish - Unable to set BootOverrideTarget to Pxe when the BootOverrideMode is UEFI.
    2202420277 - DIMM Enumeration in BMC GUI SEL Display for ECC Entry is 0-based
    2202468321 - KVM window can not be closed by clicking "trash can" symbol in the Web console
    2006679703 - Redfish:  ResetCycle command fails to send graceful restart.

v1.50.0d4c5dee(Internal version)
    1504720141 - Fan values differ substantially before and after cold reset of the BMC under performance mode
    1504731495 - flash BMC will occur 'Error Finish BMC update transfer failed.' when online update BMC 1.48.da6db8b3 to BMC 1.48.da6db8b3

v1.49.ab1470a9(Internal version)
    220891332 - S2600WF BMC GUI Fails to display P4600 NVMe information
    1504707051 - Q1'18 #CCB2118 [Q1'18 Purley BMC] Need to support NVMe 1.2 VPD to correctly identify Cliffdate, Fultdondate and future drives
    1504711379 - [S2600BP LCR]HSBP_PSOC sensor shows no reading when run reboot test.(recovered later automatically)
    1504720124 - [S2600BP]BMC release-notes doesn't contain the new type PSU(PSSF222201A  04A)
    2006710682 - Chassis ID LED needs to be pressed twice to turn off when turned on in EWS

v1.48.da6db8b3(Internal version)
    1504706586 - [FTF]Get DIMM offset command returned unexpected completion code 0x01 during FSC AutoProfileFunc.tcl test
    1504707060 - Q1'18 #CCB1954 [Purley BMC] Remote debug over PECI
    1504718239 - Customize EWS image update failed
    2103620599 - EWS: Occasionally it shows "Exist an effective connect from others" or "Media has been unmounted from others" while mount or unmount the virtual device

v1.47.e54761ed(Internal version)
    1504473313 - [FTF]Fan Boost value do not reach expected value  during running FSC BAT_FSC_Functional_004.tcl test
    1504696854 - Redfish URL redfish/v1/Managers/BMC/NICs NOT align with Redfish Spec
    1504696869 - Redfish API GET redfish/v1/Managers/BMC/ response should contain ServiceEntryPointUUID element
    1504699916 - 2130W PSU predictive failure on S2600BP from across customers and across sites
    1504706039 - Redfish API unable to read system network interfaces
    1504707049 - Q1'18 #CCB2140 [Purley BMC]Get CPU temperature displayed in degree Celsius after executing an “ipmitool sensor”
    2006709919 - IPMI OEM type record cannot use 0x20 on generator ID field
    2103620363 - The ME sensor should not be define in SDR 1.41 file.
    2103620840 - BMC debug console shows abnormal messages about "PcieSwitch_sensors_thread".
    2103620851 - [S2600BT] Failed to update configuration of NM by EWS.
    2201981916 - BMC firmware Update to 1.47.e54761ed clears the BMC LAN Settings

v1.45.ed3c869e(Internal version)
    1604603941 - [FTF]It will report a failure “Unable to program SDR record#52” during SDR and FSC FTF test.
    2103617028 - [S2600WF]Description in HELP page isn't corresponding to the actual EWS page
    2103620512 - [S2600BT] The Power Control shows incorrect in the KVM menu bar
    2103620737 - [S2600BT] The being setting NM policy of memory cannot delete by EWS
    2103619818 - [S2600BT] NM configuration Couldn't display the memory power policy in the EWS

v1.44.889bc937(Internal version)
    1504627444 - #CCB2006: [Cloned CCB 2003] [CLX-WFFR]ERROR_N[1,0] connection request to BMC
    1604595437 - Several Redfish GET commands return errors
    2006689963 - VR-Watchdog - Voltage Fault issues running DC_Cycling
    2006709004 - [S2600BT] Wrong date in event logs with WW51 BKC
    2103617840 - [S2600BT] The time stamp in sellog is incorrect after offline flash BIOS , BMC , set clear CMOS jumper and remove battery.
    2103619526 - It generates some incorrect event logs in the AC cycle stress test
    2103619725 - The sensor reading of "System Airflow" sensor in slave node show 0 CFM.
    2103619818 - [S2600BT] NM configuration Couldn't display the memory power policy in the EWS
    2103619846 - [S2600WF] The VFP LED cannot be changed via SM signal command under MTM 1 or 2 mode.
    2201187649 - S2600WF LNET Router BMC sometimes reports Voltage Fault State - Asserted/Deasserted events during DC and OS cycling
    
v1.43.91f76955 - (Point Release for JAVA certificate expiring)
	1504745080 - [S2600BP]PS1/PS2 Input Power/Curr Out %/Temperature sensors show no reading or disabled and need unplug/plug nodes to recovery during AC cycling
    1505482466 - Point release to unblock customer line down due to Java certificate expiring. 

================================================================================
				FRUSDR 1.60 
================================================================================    

- Enable "PS[x] Fan Fail" for 1600W PSU
- Enable median filter for hidden voltage sensors.
- Add support for 1600W psu.
- Updates to version 30 of FSC spreadsheet
- Adds remote PECI support to the Remote Debug sensor
- HSD 2103619689 - Includes NVMe sensors for 12*3.5 HSBP
- HSD 2202506519 - Updates CPU name in master.cfg display
- Adds processor absolute temp sensor
- Removes unused UPI Fatal sensors
- Updates to version 29 of FSC spreadsheet
- CCB1904 Adds support for Riser 3 temp sensor detection
- Adds FW Security sensor

================================================================================
			SYSTEM HARDWARE & SOFTWARE REQUIREMENTS/REVISIONS
================================================================================
- S2600WFT, S2600WF0, S2600WFQ baseboards only.

  System BIOS  - 00.01.0013 or later
  ME Firmware  - 04.00.04.294 or later
  BMC Firmware - 1.43.660a4315 or later
  FRUSDR       - 1.43  or later

- Front Panel, Hot-swap backplane, and Baseboard FRU data must be available
  for chassis auto-detection to succeed.


===============================================================================
                        KNOWN ISSUES/WORKAROUNDS/REQUIREMENTS
===============================================================================
HSD-ES 2103620418: After downgrade FD and ME, SUT will halt with beep code 1-5-1-2 when reboot. 
       Please use the following WA when online downgrading SW stacks from R010 SUP to previous SUP version: 
       Online downgrade process: flash BIOS -> flash FD -> reset SUT -> flash ME -> flash BMC -> flash FRUSDR -> AC cycle SUT -> SUT can boot up normally.

WARNING: This release has the BMC PCIe bridge disabled. This will cause the 
    majority of operating systems to fail at boot as they stall during video 
    driver initialization
    
    Steps to recover a failing operating system:
    
	Linux variants (one of the below):
        A. Ensure the "modprobe.blacklist=ast" parameter is set in your boot loader (grub)
        B. Ensure you are using a kernel version v4.10 or newer
    For Red Hat* Enterprise Linux* v7.3, please refer to the included "RHEL73_InstallationGuide_Rev1.00.pdf"
	For SUSE* Linux* Enterprise Server v12 SP1 or SP2, please refer to the included "SLES12_InstallationGuide_Rev1.00.pdf"
	
    Windows variants:
        Boot to safe mode, and load aspeed video driver v1.03 or greater and reboot
	For Windows* Server 2016, please refer to the included "WinSrv16_InstallationGuide_Rev1.00.pdf" 
	
=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2018 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.