This release note and the software it accompanies it are copyright (c) 2003, Intel Corporation, and may only be installed and used in accordance with the license that accompanies the software.

File name: SUSE70_drv_204.zip

Driver version 2.04

This download supports SCSI Intel(R) Server RAID Controllers, please verify that this driver has been tested with the RAID controller you have chosen to use.
You can verify compatability on the RAID controller's driver page at http://support.intel.com.

Attention!
===========
This download is created using a zip compression untility and is compatible with a variety of zip programs,  please extract it to floppy diskette keeping the directory structure intact.
Please refer to product and OS documentation for application instructions for this driver.

Contents
=========

File			Version 	Size		Date         	Description		
-----			--------     	----- 		-----        	------------
NET-MOD.GZ		2.04		454KB		6/29/03		Driver
OTHER-MO.GZ		2.04		433KB		6/29/03
SCSI-MOD.GZ		2.04		547KB		10/26/02
README.TXT		n/a	       	3KB	   	10/22/02	This file
License			N/a		13KB

Using This Tool
================
1. Extract the SuSE70_drv_204.zip file to a floppy diskette
2. This diskette contains the Storage RAID Controller modules driver disk of SuSE 7.0. 
* The suse/sus70sys.exe contains the linux driver for the installed linux system.

3.  Boot from the original SuSE Linux 7.0 Bootdisk / CD.
4.  Follow the following sequence during installation (personalise when needed):

	Choose language
	Choose display type
	Choose keyboard map
	Choose Kernel modules (hardware drivers)
	Load SCSI Module
	Choose -- More Modules --
	Please insert the modules disk
	Choose OK
	Select gdth: ICP vortex GDTH Disk Array
	No parameters
	Module "gdth" has been successfully loaded !
	OK
	Kernel Messages
	OK
	CHoose "BACK"
	Choose "Settings"
	Choose "Debug expert"
	Choose "Force rootimage"
	Do you want the rootimage to be loaded into the RAM disk ...
	Choose "No"
	CHoose "BACK"
	CHoose "BACK"
	Start installation / system
	Start installation/update
	Choose source medium e.g. CDROM
	Choose the YaST2 - graphical installer
	Select language
	Select Keyboard layout and timezone
	Select New installation
	Choose hard disk
	Use entire hard disk
	Software Selection e.g. Minimal
	Personalize
	Password for root

	!!! WAIT !!!
	WAIT until... Now booting your system --- DO NOT CONFIRM THIS MESSAGE
	!!! WAIT !!!

	Switch With CTRL-ALT-F2 to the second terminal and insert the floppy
	disk with the system-modules.tgz
	then
	mount /dev/fdo /mnt/mnt
	cp /mnt/mnt/system-modules.tgz /mnt
	cd /mnt
	tar xvfz system-modules.tgz
	mk_initrd /mnt
	chroot /mnt
	lilo
	Switch With CTRL-ALT-F7 to YaST2 and confirm the "Now booting your system"
	message
	


