This release note and the software that accompanies it are copyright (c) 2004, Intel Corporation, and may only be installed and used in accordance with the license that accompanies the software.
This version of firmware is designed for controllers using software stack 1 as listed below, it is not compatible with the SRCU42X, SRCS16, SRCZCRX, SRCU42E, SROMBU42E or later controllers.

Firmware Version = 2.42.02-R07A

This download supports Intel(R) Server RAID Controllers listed below using software stack 2.
SRCU32
SRCZCR
SRCU42L
SRCS14L

Extract this package to a local drive and copy the appropriate firmware file to a diskette.  


Attention!
===========
The Firmware update utility is not incorporated in this download and must be applied using the OS version of the StorCon utility or the firmware update utility (FRUU).

It may not be possible to apply this update using the Xrom (cntl+g) version of StorCon to a controller with firmware 2.36 or older.  
The use of an OS (DOS, Windows, or Linux) version of StorCon or the FRU utility may be used.  

This firmware supports both the "normal" and "recovery" update modes. 
If the RAID controller firmware is corrupted, you must move the recovery jumper on your controller to the recovery position in order to apply this update using the FRUU.
The Intel(R) Server RAID Controller SRCU32 does not have a recovery jumper and the FRUU utility can only be used in normal mode on this controller.


Contents
=========
Name				DAte		Size		Description
src_rxfw.07a			11/30/04	1343KB 		Firmware image file
fw24202R07a_readme.txt		01/05/05	5KB		This file
Web Licence.rtf			07/02/03	13KB		License

Instructions:
=============
To perform an update using the firmware recovery utility, complete the following steps:
1. Download the FRU utility and extract it to a floppy diskette by running the extract.bat file.
2. Download and extract the firmware image file to a floppy diskette.
3. If the recovery option is used, remove power (unplug the power cords) from the target system, move the recovery jumper on the RAID controller from the "normal" position to the "recovery" position, and install in the target system.
4. Re-apply power and boot the target system to the FRU disk mentioned in step 1.
5. The system will present a menu that lists the installed raid card and prompt for the firmware file needed.
6. Insert the firmware diskette mentioned in step 2.
7. Press the number key associated with your RAID controller as displayed on the menu (usually the number 0 unless you have more than one RAID card installed).
8. The Firmware will be programmed into the RAID controller, when complete you will be prompted to exit.
9. If the jumper was changed in step 3, Power down the target system and remove power (unplug the power cords).
10.Move the recovery jumper on the RAID controller back to the "normal" position.
11.Reinstall the RAID controller, re-apply power, and boot the system.

To perform the update using the StorCon Utility, complete the following steps:
1. Boot to an OS and run the OS version of StorCon.
2. Press enter to select the controller.
3. Press the F4 key for advanced functions.
4. Select the Configure controller option.
5. Insert the floppy containing the firmware image file into the floppy drive.
6. Select the update firmware option.
7. Press enter to confirm the  firmware check.
8. Press "Y" to confirm the update.
9. Do not interupt the firmware update process, Reboot the system when the update completes.


Changes
========
1. FW 2.42.01-R078 and later, added SATA enclosure management support including Safte LED activity & fault support via I2C cable from the raid controller to the SATA backplane. Please refer to the SATA cabling guide for additional information, this document may be found on support.intel.com.
2. Added instruction to reset checkpoint to 0 upon completion of rebuild.  See TA-743-1 for additional detail.

*Other names and brands may be claimed as the property of others.	


