Intel® Storage System SSR316MJ2
Release Notes Version 6.0
EBSD Driver for Windows
August 2004

Copyright (c) 2004. All rights reserved.
Thank you for your interest in the EBSD Driver for Windows.
These Release Notes provide
- information about current limitations in this release
- possible workarounds to these limitations

EBSD Driver for Windows
EBSD Snapshots of iSCSI Volumes Can Only Be Mounted On One System At A Time (520)
If you create a snapshot of an iSCSI volume, and change the snapshot type to EBSD, that snapshot can
only be mounted on one system at a time.
Windows User Services Do Not Start Automatically After a Reboot of Windows Server (784)
Application Services and their dependent services, such as Lanmanserver, or Browser, which are
configured in the EBSD Advanced Settings tab, will not start automatically after a reboot of the Windows
server if an EBSD volume is mounted as a Raw disk on the Windows server.
Workaround
Manually start those services after a reboot of the Windows server.
