//****************************************************************************
//                          Intel Corporation
//                    Jones Farm, Hillsboro, Oregon
//                           (503) 696-8080
//
//                Intel Corporation Proprietary Information
//     Copyright (c) 2004 Intel Corporation, All Rights Reserved
//****************************************************************************
//
//  TITLE:  IMMAGCM3.FRU                            DATE CREATED: 07/09/2004
//
//  DESCRIPTION:  Field Replaceable Unit (FRU) information file.  This FRU
//      file is for the Intel GCM NIC Board FRU.
//
//  PVCS INFORMATION:
//
//****************************************************************************
//****************************************************************************

_LF_NAME       'GCM NIC Board'          // Name for this load file
_LF_VERSION    '0.03'                   // Version of this load file
_LF_FMT_VER    '1.50'                   // Version of the load file format
_IPMI_VERSION  '1.50'                   // IPMI format version

_FRU (
_FRU_TITLE     'GCM NIC Board'      // FRU Title
_START_ADDR    0000                     // Start Address
_DATA_LEN      0080                     // Data Length = 128 bytes
_NVS_TYPE      'IMBDEVICE'              // Non-volatile Storage Type
_DEV_ID        02                       // Device ID
_DEV_BUS       FF                       // Device Bus
_DEV_ADDRESS   20                       // Device Address

_SEE_COMMON
   01                                   // Common Header Format Version
   01                                   // Internal Use Area Starting Offset (in multiples of 8 bytes)
   00                                   // Chassis Info Area Starting Offset (in multiples of 8 bytes)
   02                                   // Board Info Area Starting Offset (in multiples of 8 bytes)
   0C                                   // Product Info Area Starting Offset (in multiples of 8 bytes)
   00                                   // MultiRecord Area Starting Offset (in multiples of 8 bytes)
   00                                   // Pad
   F0                                   // Common Header Checksum

_SEE_INTERNAL
   00 00 00 00 00 00                    // First 6 bytes are MAC address, MS byte first
   00 00                                // Last 2 bytes pad the area to 8 bytes

_SEE_BOARD
   01                                   // Board Info Area Format Version Bit Fields
   0A                                   // Board Info Area Length = 80 bytes (10 blocks)
   00                                   // Language Code
   00 00 00                             // Mockup Mfg. Date/Time
   C5                                   // Board Manufacturer type/length byte
   'Intel'                              // Board Manufacturer name
   CD                                   // Board Product Name type/length byte
   'GCM NIC Board'                      // Board Product Name
   D2                                   // Board Serial Number type/length byte
   '..................'                // Mockup Board Serial Number
   CA                                   // Board Part Number type/length byte
   '..........'                         // Mockup Board Part Number
   CC                                   // FRU File ID
   'FRU Ver 0.03'
   C0                                   // Board Custom Field 1
   C0                                   // Board Custom Field 2
   C0                                   // Board Custom Field 3
   C1                                   // No more fields type/length byte

_SEE_PRODUCT
   01                                   // Area Format Version Bit Fields
   04                                   // Area Length = 32 bytes (4 blocks)
   00                                   // Language Code
   C5                 			// Product Manufacturer Name
   'Intel'            			// 5 digit ascii Product Manufacturer name
   C0                                   // Product Name type/length byte
   C0                                   // Product part/model number type/length byte
   C0                                   // Product Version type/length byte
   C0                                   // Product Serial Number type/length byte
   C0                                   // Asset Tag type/length byte
   C0                                   // FRU file ID type/length byte
   C0                                   // Custom Field
   C1                                   // No more fields type/length byte
)
