//****************************************************************************
//                          Intel Corporation
//                    Jones Farm, Hillsboro, Oregon
//                           (503) 696-8080
//
//                Intel Corporation Proprietary Information
//     Copyright (c) 1999-2004 Intel Corporation, All Rights Reserved
//****************************************************************************
//
//  TITLE:  6SATAHS2.FRU                             DATE CREATED:  08/10/2004
//
//  DESCRIPTION:  HSC Field Replaceable Unit (FRU) information file.  This FRU 
//      file is for the Intel HSC SATA Module.
//
//  PVCS INFORMATION:
//      $Workfile: $ 
//      $Author:   $
//      $Revision: $  
//      $Date:     $
//      $Modtime:  $ 
//
//****************************************************************************
//  REVISION HISTORY:
//
//****************************************************************************

//
// File Header Information
//

_LF_NAME       'Hotswap SATA Module' // The name for this load file
_LF_VERSION    '0.2'        // The version of this load file
_LF_FMT_VER    '1.50'       // The version of the load file format
_IPMI_VERSION  '1.50'       // Specifies the IPMI format version #

//
// FRU Area Header 
//

_FRU (                      // FRU data for the HSB Module 
_FRU_TITLE      'Hot Swap Ctlr'  // FRU title
_START_ADDR     0000             // Start Address is 00h
_DATA_LEN       00D8             // Length is 152 bytes
_NVS_TYPE       'IMBDEVICE'      // 256 byte Serial EEPROM used to store FRU
_DEV_ID         00               // Device ID
_DEV_CONTROLLER 20               // Device Controller
_DEV_BUS        00               // IMB device resides behind the HSC
_DEV_ADDRESS    C0

_SEE_COMMON          // NVS Common Header area contents 00-07h (8 bytes)
   01                // Common Header Format Version
   01                // Internal Use Area Offset in multiples of 8 bytes
   00                // Chassis Information Area Starting Offset in multiples of 8 bytes
   02                // Board Area Starting Offset in multiples of 8 bytes
   00                // Product Information Area Starting Offset in multiples of 8 bytes
   00                // MultiRecord Information Area Starting Offset in multiples of 8 bytes
   00                // PAD (1 byte)
   FC                // Common Header Checksum (2's complement)

_SEE_INTERNAL        // NVS Internal Use area contents 08h-0Fh (8 bytes)
   01 00 00 00 00 00 00 02  // 08h - 0Fh

_SEE_BOARD           // NVS Board Info area contents
   01                // Board info area format version
   19                // Board info area length in multiples of 8 bytes
   00                // Unicode country base (00 = use 8-bit latin 1 ascii)
   00 00 00          // Mock-up mfg date / time
   C5                // Board mfr type/length byte
   'Intel'           // Board manufacturer name
   CB                // Board product name type/length byte
   'FXX6SATABRD'  // Board product name
   CC                // 11 001010 board serial number type/length byte
   '............'    // Mock-up 12 digit ascii board serial number
   CA                // 11 001010 board part number type/length byte
   'C55293-203'      // 10-digit part number as 8-bit ascii
   CC                // FRU File ID field is NULL
   'FRU Ver 0.02'
   C0                // Board Custom Field
   C0                // Board Custom Field
   C0                // Board Custom Field
   C0                // Board Custom Field
   C0                // Board Custom Field
   C0                // Board Custom Field
   C1                // No more fields type/length byte
) 

//** End of FRU for HSC ******************************************************

