//****************************************************************************
//                          Intel Corporation
//                    Airport Road, Bangalore, India
//
//                Intel Corporation Proprietary Information
//     Copyright (c) 2003-2004 Intel Corporation, All Rights Reserved
//****************************************************************************
//
//  TITLE: 4SCSIHS2.FRU                               DATE CREATED: 06/30/2004
//
//  DESCRIPTION: HSC Field Replaceable Unit (FRU) information file.
//		     This FRU file is for Intel SC5300 4-Slot SCSI HSC Module.
//
//  PVCS INFORMATION:
//      $Workfile:  $
//      $Author  :  $
//      $Revision:  $  
//
//****************************************************************************
// REVISION HISTORY:
//
//****************************************************************************

//
// File Header Information
//

_LF_NAME       'Hotswap SCSI Module' // The name for this load file
_LF_VERSION    '0.2'   // The version of this load file
_LF_FMT_VER    '1.50'  // The version of the load file format
_IPMI_VERSION  '1.50'  // Specifies the IPMI format version #

//
// FRU Area Header 
//

_FRU (                       // FRU data for the HSB Module
_FRU_TITLE      'Hot Swap Ctlr'  // String Bytes
_START_ADDR     0000         // Start address is 00h
_DATA_LEN       0098         // Length is 152 bytes
_NVS_TYPE       'IMBDEVICE'  // 256 byte Serial EEPROM used to store FRU
_DEV_ID         00           // Device ID
_DEV_CONTROLLER 20           // Device Controller
_DEV_BUS        00           // IMB device bus
_DEV_ADDRESS    C2           // I2C address of 4HDD HSBP on which FRU EEPROM resides.

_SEE_COMMON          // NVS Common Header area contents 00-07h (8 bytes)
   01                // Common Header Format Version
   01                // Internal Use Area Offset in multiples of 8 bytes
   00                // Chassis Information Area Starting Offset in multiples of 8 bytes
   02                // Board Area Starting Offset in multiples of 8 bytes
   00                // Product Information Area Starting Offset in multiples of 8 bytes
   00                // MultiRecord Information Area Starting Offset in multiples of 8 bytes
   00                // PAD (1 byte)
   FC                // Common Header Checksum (2's complement)

_SEE_INTERNAL        // NVS Internal Use area contents 08h-0Fh (8 bytes)
   01 00 00 00 00 00 00 20 // 08h - 0Fh;last 2 bytes=_LF_VERSION

_SEE_BOARD           // NVS Board Info area contents 10h-97h (136 bytes)
   01                // Board info area format version
   11                // Board info area length in multiples of 8 bytes
   00                // Unicode country base (00 = use 8-bit latin 1 ascii)
   00 00 00          // Mock-up mfg date / time
   C5                // Board mfr type/length byte
   'Intel'           // Board manufacturer name
   D5                // 11 010101 Board product name type/length byte
   '4-Slot SCSI Backplane'  // Board product name
   CC                // 11 001100 board serial number type/length byte
   '............'    // Mock-up 12 digit ascii board serial number
   CA                // 11 001010 board part number type/length byte
   '..........'      // 10-digit part number as 8-bit ascii
   CB                // 11 001011 FRU File ID field
   'FRU Ver 0.2'     // FRU version
   C1                // No more fields type/length byte
)

//** End of FRU for HSC ******************************************************
