OBSOLETE Patch-ID# 110842-08
Keywords: new platform hpc3130 note.h hpc3130 attach detach routine
Synopsis: Obsoleted by: 110842-09 SunOS 5.8: hpc3130 driver patch for SUNW,Sun-Fire-880
Date: Jul/22/2002

Install Requirements: Reboot after installation                      
                      See Special Install Instructions                      
                      
Solaris Release: 8

SunOS Release: 5.8

Unbundled Product: 

Unbundled Release: 

Xref: 

Topic: SunOS 5.8: hpc3130 driver patch for SUNW,Sun-Fire-880
	***********************************************************
	NOTE: This patch may contain one or more OEM-specific platform ports.
	      See the appropriate OEM_NOTES file within the patch for
	      information specific to these platforms.
	      DO NOT INSTALL this patch on an OEM system if a corresponding
	      OEM_NOTES file is not present (or is present, but instructs not
	      to install the patch), unless the OEM vendor directs otherwise.
	***********************************************************
	NOTE:   Refer to Special Install Instructions section for
                IMPORTANT specific information on this patch.

Relevant Architectures: sparc

BugId's fixed with this patch: 4369175 4371073 4381743 4403481 4408237 4434341 4465733 4472722 4506746 4514513 4514865 4518973 4520822 4672995

Changes incorporated in this version: 4672995

Patches accumulated and obsoleted by this patch: 110775-01 111757-01

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/etc/driver_aliases
/etc/minor_perm
/etc/name_to_major
/platform/SUNW,Sun-Fire-880/kernel/drv/sparcv9/hpc3130
/usr/platform/sun4u/include/sys/hpc3130_events.h
/usr/platform/sun4u/include/sys/i2c/clients/hpc3130.h

Problem Description:

4672995 Console messages seen (fru: Device busy) scrolls off screen
 
(from 110842-07)
 
4518973 slot reporting from kernel messages shouldn't use "instance" numbers and offsets
4514865 Hotplug inconsistencies when only one power supply exists
 
(from 110842-06)
 
4506746 hpc3130 module id string is too long for modinfo
4403481 front PCI HP indicator LED's do not shut off after Fresh Choice is configured
4520822 DR behaves inconsistently
4514513 hpc3130 driver registers interrupt handler too late, hangs on attach
 
(from 110842-05)
 
4465733 Crystal + Panics running stress attach/detach routine
4472722 hotplug controller sends poll wake up when there is no event
 
(from 110842-04)
 
	This patch revision was generated to accumulate and obsolete
        the feature changes introduced in feature point patch 111757-01.
 
(from 110842-03)
 
4434341 i2c drivers should include "sys/note.h" not "note.h"
 
(from 110842-02)
 
4371073 hpc3130 LED wiring for safari slots is changing in P2 motherboards
 
(from 110842-01)
 
      This patch revision was generated to accumulate and obsolete the
      feature changes introduced in feature point patch 110775-01
 
(from 110775-01)
 
4381743 Add new platform support in Solaris
4369175 pcf8584 generates syslog warning for a non-error condition
 
(from 111757-01)
 
4408237 hotplug is not disabled when only one power supply exists

Patch Installation Instructions:
--------------------------------
 
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7-9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
       example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
       example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
-----------------------------
 
Reboot the system after patch installation.
 
	NOTE:   To get the complete fix for 4408237 (hotplug is not
		disabled when only one power supply exists), one needs
		to install the libpsvcpolicy_psr patch for SUNW,Sun-Fire-880
		110849-06 (or newer).

README -- Last modified date:  Tuesday, January 21, 2003

