                         GRANDEST FLEET CDROM
                            version 6-1-94

Insert disk into CDROM drive.
Switch to drive (i.e. D:)
Type INSTALL and hit return.

After installing game, run SETUP to configure sound drivers.
If you later want to change from SVGA to VGA or visa versa use the
install program on the CDROM.  If you ever change the CDROM's pathname,
run the intallation program again and use the 3rd option.

Runs in SVGA 640 by 480 by 256 color mode (VESA_101). If your video card
is not recognized by the program, load your video card's VESA driver and
try running Grandest Fleet again.

Start game with GFLEET with your Grandest Fleet disk in the CDROM drive.
Use S or M after GFLEET on command line to disable Sound or Music to save memory.


                     QQP
                495 Highway 202
             Flemington, NJ 08822
                (908)-788-2799


Start up line toggles available:
M  to not load music drivers. (saves 40K conventional memory)
S  to not load digitized sound drivers. (saves 29K conventional memory)
P  to not protect sound during palette animation (looks better, but might
    cause problems on some cards...)
X  to bypass the yes-no question when exiting the program.
C  to bypass the cover screens at start up.
W  Used only in VGA mode. Slows down display, but saves 500K expanded memory.
B  to not load big ship pictures. (saves 260K expanded memory)
A  to turn off all palette animation.
D  to use direct calls for palette changes. (use if problems with palette animation)
R  to turn on retrace checking. (use if problems with palette animation)
7  allows only maps up to 70 hexes in width to be used. (saves 25K conventional memory)
6  max map witdth 60 hexes. (saves 50K total conventional memory)
5  max map witdth 50 hexes. (saves 75K total conventional memory)
