
Based on the A4EII amphibious tank which was purchased from Britian in 1935,
the T-37-a had the original balsa wood side floats ommitted and combined
a welded and riveted construction. It had moderate speed and a 20mm gun.
Production ended in 1936, but it was used through 1942.

