
The design requirements of the A10 (Cruiser Tank) called for an infantry-
support tank with thicker armor than the A9, to be built at as low a
cost as possible. As a result, more armor was added to the front and sides, 
and its maximum speed was reduced to improve reliability. The tank came 
equipped with a 2lb anti-tank gun, effective against most early war German 
tanks. 

