Modem INIT string listing.  (COMPREHENSIZE LIST)

First try ATZ in the Clear and INIT string before trying the strings below.

For best performance you will want to disable compression and error 
correction on your modem.  Also set Flow Control to Hardware (CTS/RTS) 
or to NONE (no flow control).  Here are some init strings for popular 
modems that we have found.  Check your modem's documentation to see if the
commands listed are supported by your modem and if they are setting the 
the items mentioned above.

If your system does not run smoothly during MODEM or DIRECT LINK play and 
you are using MIDI music, turn music OFF to increase game speed.  This is 
done by setting your MIDI Music Volume to 0, or by using the alt-m keystroke 
shortcut.

**NOTE:  If you get the message "ERROR IN INIT STRING" you may leave the init 
         string completely blank, WAR2 will skip that step.    
         Also, if this error appears, you can try replacing &M0 with &Q0 
         or replace &Q0 or &Q6 with &M0.  All of these commands select
         Asynchronous Communications Mode.


AT&T Dataport 2001          AT &F%VFX7S62=0%VG9\Q2\N0&W
AT&T Dataport:              AT &F X7 S62=0 \Q2 \N0 &W
AT&T Dataport Express       AT &F &K0 &Q0 
Archtec                     AT &F %C0 \N0
-----------------------------------------------------------------
Best Data                   AT &F &K0 &Q0 %C0 /N0
Boca                        AT &Q6 %C0 &K0
Boca 14.4 Fax/Modem         AT S46=0 S37=9 N0 &Q0 &D2 &K4
Boca 14.4k                  AT S46=0 S37=9 N0 &Q0 &D2 &K0 %C0
Boca 14.4 internal          AT &C0 S37=9 N0 &Q0 &K0 W0 S36=3 S48=128 %C0
Boca 14.4k (external)       AT &F S0=1 S36=0 &K0 &Q6 N0 S37=9 &D2
Boca M1440i (internal)
AT S48=0 S37=9 S46=136 %C0 %E0 %M0 &K0 &Q0 &R1 &C1 &D2 \G0 \N1 N0
----------------------------------------------------------------- 
Cardinal                         AT &F W0 &Q0 &D2
Cardinal 14.4k                   AT &F N0 S37=9 &Q0 &D2 \N1
Computer Peripherals 14.4        AT &F S37=9 S46=0 N0 &Q0 &K0
Creative Labs Modem Blaster      AT %C0 \N0 V1
----------------------------------------------------------------- 
Digicom Systems (DSI) (softmodem)     AT Z \N0 &D2 &K0 S48=48 
Digicom Systems Scout Plus            ATZ*E0*N3*M0*S0*F0&D2 
Digicom connection 96+Softmodem:      AT \N1 &d2 %c0 s37=9 &K0 
Digicom connection 96+Softmodem:      AT Z \N0 &D2 &K0 S48=0 
Digicom connection 96+Softmodem:      ATZ*E0*N3*S0*M0*F0&D2 
----------------------------------------------------------------- 
GVC 14.4k (internal)      AT &F B8 \Q0
Gateway Telepath          AT &F S37=9 %C0 &K0 &Q6 \G0 
Gateway Telepath 14.4k    AT S46=0 S37=9 N0 &Q0 &D2 &K0 %C0 
Gateway Telepath I:       AT S0=2 &N6 &K0 &M0
Gateway Telepath I:       AT &F S37=9 &K0 &Q0 %C0 N0 \G0 &D2 S46=0 S0=2
Gateway Telepath II       AT S0=2 S37=9 %C0 &Q0 &K0
Gateway Telepath II:      AT &F &K0 &M0 &N6 S0=2
Generic 14.4k Fax/Modem   AT S46=0 S37=9 N0 &Q0 &D2 %C0 \G0 &K0 
Generic v.32bis 14.4k     AT \N0 %C0 B8 
----------------------------------------------------------------- 
Hayes 28.8k V.FAST Modem       AT &Q6 &K S37=9 N %C0 \N0
Hayes Optima 28.8/14.4         AT &F S37=9 N0 &Q0 &K0 
----------------------------------------------------------------- 
IBM MWAV (Aptiva)              AT &F M1 V1 X4 S0=1 %C0
Infotel 144I:                  AT &Q0 S37=9 N0 &D2
Intel 14.4k                    AT \N0 %C0 \Q0 B8
Intel 14.4k (internal)         AT Z B8 Q1 \C0 \N1 %C0 \V 
Intel 400/i Fax/Modem:         AT Z \N0 %C0 H0 S31=9 &Q0
----------------------------------------------------------------- 
Macronix                       AT S36=3 S37=9 &K0 %C0 \G0 
Microcom QX/4232bis            AT %C0 \N0
NOKIA ECM 4896M TRELLIS V.32.  AT Z %C0 /N0
Netcomm M7F                    AT &E &K0 B0 \V0 X4 &D2 \N1 \Q0 #J0 #Q9 %C0 
Nokia ECM 4896M Trellis V.32.  AT Z %C0 /N0 
----------------------------------------------------------------- 
Practical Peripherals 14400FX v.32bis   AT S46=0 &Q0 &K0 &D2
Practical Peripherals 14400FX v.32bis   AT Z S46=0 &Q0 &D2 
----------------------------------------------------------------- 
All Supra Modems          AT &F0 N S37=9
------------------------------------------------------------------ 
Telebit 3000/Worldblazer  AT S50=6 S180=0
Telepath 14.4k try Clear: ATZ X4
                   Init:  AT &F1 &MO &KO S0=2 
Turbo Modem Plus          AT &F B8 %C0 /N1 
------------------------------------------------------------------
USR Sportster 9600        AT &M0 &K0 &N6
USR 14.4k                 AT &K0 &H0 &D0 &I0 &R1
USR 14.4k                 AT &F0 B0 S34=1 &N6 &K0 &I0
USR Sportster             AT &F0 &K0 &M0 &B1 S34=1 &N6 &I0 
USR 14.4k                 AT &B1 &M0 S27=16 &H0 &I0 &K0 &N6 
USR 14.4k                 AT &M0 &K0 &N8 &D0 B0
USR 14.4k                 AT &A0 &B0 &D0 &H1 &I0 &K0 &M0 &N6 &R1 S34=1 
USR Courier 16.8:         AT &A0 &M0 &K0& N6 B0 S0=0 X7
USR Courier v.32bis       AT E1 Q0 V1 S7=60 &C1 &D2 &K0 &N6 &A3 &H0 &M0 
USR Sportster 14.4k Baud:  19200  (use 38400 for 28.8k sportsters)
                   Clear:  AT Z X4
                    INIT:  AT &F1 &K0 &M0 X4
                  HangUp:  ATH0
USR Sportster 28.8k  (as above but use 38400 baud)
USR 14.4k Dual Standard   AT B0 X4 Q0 &R1 &B1 &N6 &A0 &D2 &H0 &I0 &K0 &M0 M1 
USR DS v.32bis v.42bis    AT &M0 &N6 &A0 &R1 &H0 &K0 &I0 &S0 &B1 X1
USR Courier HST/DS 16.8k  AT X4 B0 &A0 &B0 &H2 &I0 &K0 &M0 &N6 
------------------------------------------------------------------ 
ViVa 14.4k           AT &F &Q6 \N0 %C0 &D2 N0 S37=9
Viva 14.4 Fax/Modem: AT S11=50 S37=9 S95=52 L0 N0 S46=0 &Q0 &D2 \N1 
------------------------------------------------------------------ 
Wang 14/14 modem:    AT S46=0 S37=9 N0 &K0 %C0 %M0 &Q0 &D2 \N1 
------------------------------------------------------------------ 
Zoom Init            AT &F &Q6 S37=9 N0 &K0 %C0
Zoom Init            AT &F &Q0 S37=9 N0 &K0 S46=0 
Zoom 14.4k VFX       AT &Q6 S37=9 N0 %C0 \N0
Zoom Init            AT &Q6 S37=9 N0 &K0 S46=136 S36=1 S48=128 %C0 
Zoom OEM Modem       AT &Q6 S37=9 N0 &K0
Zoom:                AT &Q6 S37=9 N0 &K0 %C0 
Zoom:                AT &Q6 &K0 &D2 \N0 %C0 
Zyxel (E+):          AT &N3 &K0
Zyxel U-1496E+       AT Z &N4 &K0
