                       LAN Server 3.0

  This document applies to the EtherExpress(tm) 16, 16TP, 16C, FLASH,
  FLASH TP, FLASHC, MCA, and MCA/TP.  The FlashC will work with the
  flash/boot rom disabled.  This document contains notes for installing
  the NDIS driver and does not explain how to configure an EtherExpress
  board.  For instructions about configuring the board, see either the
  Expert's Guide or the Complete Guide.

  INTRODUCTION:
  -------------
  Before you begin, you will need the I/O address of the EtherExpress board.
  You can get this information by running SOFTSET on the EtherExpress 16,
  16TP, 16C, FLASH, FLASH TP, or FlashC card or the IBM SC program on the
  Etherexpress MCA or MCA/TP card.

  This installation does not use OS/2 Extended Services.

  These steps apply to both the file server and the workstation.  After
  installing OS/2, follow the below steps prior to installing LAN Server 3.0
  or the workstation requestor.

  OS/2 2.1 and LAN Server 3.0:
  ----------------------------
  1.  Make sure you have the extended nif file, EXP16.NIF dated later than
      6/18/90.  This file is available on the Intel BBS in the archive
      NDIS16.EXE.

  2.  Copy EXP16.OS2 and EXP16.NIF from the Intel EtherExpress(tm) LAN
      Adapter Driver and Option Diskette or from the downloaded file to the
      C:\IBMCOM\MACS directory.

  3.  Install LAN Adapter and Protocol Support (LAPS) from an OS/2 window.

  4.  After installing the software, select configure LAN transports.  The
      EtherExpress 16 will appear in the Lan Adaptors window.  Select the
      necessary protocols and save the configuration.

  5.  Exit LAPS, shutdown the system and reboot the computer.  The complete
      PROTOCOL.INI file will be created and put in the C:\IBMCOM directory.  The
      CONFIG.SYS and AUTOEXEC.BAT files will be updated.


  SAMPLE PROTOCOL.INI FILE
  ------------------------
  [PROT_MAN]
     DriverName=PROTMAN$

  [IBMLXCFG]
     EXP16_nif = EXP16.nif
     NETBEUI_nif = NETBEUI.nif

  ;*--------------------------------------------------------------------*
  ;*---------------------PROTOCOL SECTION--------------*
  ;*--------------------------------------------------------------------*

  [NETBEUI_nif]
     DriverName = netbeui$
     Bindings = EXP16_nif
     ETHERAND_TYPE = "I"
     USEADDRREV = "YES"
     OS2TRACEMASK = 0x0
     SESSIONS = 40
     NCBS = 95
     NAMES = 21
     SELECTORS = 5
     USEMAXDATAGRAM = "NO"
     ADAPTRATE = 1000
     WINDOWERRORS = 0
     TI = 30000
     T1 = 500
     T2 = 200
     MAXIN = 1
     MAXOUT = 2
     NETBIOSTIMEOUT = 500
     NETBIOSRETRIES = 8
     NAMECACHE = 0
     PIGGYBACKACKS = 1
     DATAGRAMPACKETS = 2
     PACKETS = 350
     LOOPPACKET= 1
     PIPELINE = 5
     MAXTRANSMITS = 6
     MINTRANSMITS = 2
     DLCRETRIES = 5

  ;*---------------------------------------------------------------------*
  ;*---------------------------MAC SECTION--------------------*
  ;*---------------------------------------------------------------------*

  [EXP16_nif]
     DriverName = EXP16$
     IOADDRESS = 0x300




