##
Using a modem

You need to have installed the following modules in order to connect by using a modem:

- Modem driver
- Dial-up network
- TCP/IP
- Dial-up server

Windows 95 does not provide a Dial-up server function. It is necessary to obtain the Dial-up Network 1.3 upgrade module from the Microsoft web download pages. MS Plus also includes the Dialup server function.

Please follow the steps below in order to connect by using a modem:

1. Step 1: TCP/IP
2. Step 2: Dialup Network
3. Step 3: Dialup server
4. Step 4: IP address (Host PC)
5. Step 5: IP address (Guest PC)

### TCP/IP

Check whether TCP/IP is installed.

1. Click on "Start" - "Settings" - "Control panel."
2. Double click on "Networks."
3. Check whether "TCP/IP" is in the list. If it is not, then continue.
4. Click on "Add."
5. Select "Protocol" and click on "Add."
6. Select "Microsoft" as the manufacturer and select "TCP/IP" as the network protocol.
7. Click on "OK" and follow the directions on the screen.

### Installing Windows dial-up network (95/98/NT)

Installing Windows dial-up network

1. Select "Start"-"Programs"-"Accessories."
2. Find "Dial-up network" in the menu. if you do not see it, go to step 2.
3. Click on "Start"-"Settings"-"Control panel."
4. Double-click on "Add/Remove Programs."
5. Select the "Windows Setup" tab.
6. Select "Communications" from the list.
7. Click on "Details."
8. Select "Dial-up networking."

   If you are using Windows 98.,you need to make a check mark next to "Dial-up Server."

9. Click on "OK"and follow the directions on the screen.

> Note: Windows 2000 has dial-up network as a default function.

#### Setting Dial-up RECEIVE on the host PC (Windows NT)

1. Click on "Control Panel."
2. Double-click on "Networks."
3. Click on the "Services" tab and select "Remote Access Service."
4. Double-click on "Configurations."
5. Select "Allow Dial-in."

#### Setting Dial-up RECEIVE on the host PC (Windows 2000)

1. Click on "Start" - "Settings" - "Network and Dial-up Connection"
2. Double Click on "New connection."
3. Select "Dial-up Receive" and click on "Next."
4. Select a device and click on "Next."
5. Choose users and click on "Next."

### Installing the Microsoft Plus! Dial-Up Server

You need to install Microsoft Plus!, if you are using Windows 95 in the host PC. If your host PC's OS is Windows NT, Windows 98, or OS/2 Warp, this function is included in the OS itself.

1. Insert the MS Plus! CD-ROM.
2. Select "Dial-up Server"from the list.
3. Follow the instructions on the screen.
4. After rebooting, select "PPP: Internet, Windows95, Windows NT" as the server and select"Receive a phone call."

### Setting the host PC's IP address

#### Setting the host PC's (Windows 95/98) IP address

1. Click on "Start"-"Settings"-"Control Panel."
2. Double-click on "Networks."
3. In the list, select "TCP/IP -> Dial-Up Adapter."
4. Click on "Properties."
5. Select "Specify an IP address" and type in your IP address; for example, IP address: 10.10.10.10 Sub-net Mask: 255.0.0.0
6. Click on "OK."

#### Setting the host PC's (Windows NT) IP address

1. Click on "Start"-"Settings"-"Control Panel."
2. Double-click on "Networks"and select "TCP/IP protocol."
3. Click on "Properties" and select the "IP address" tab.
4. Select "Specify an IP address" and type in your IP address; for example, IP Address: 10.10.10.10 Sub-net Mask: 255.0.0.0.
5. Click on "OK."

#### Enrolling dial-up users (Windows NT)

1. Click on "Start"- "Programs"- "Administration tools"- "User Manager."
2. Click on "Properties."
3. Click on "Dial-in."
4. Make a check mark next to "Allow Dial-in."
5. Click on "OK."

#### Specifying the IP address of a Guest PC (Windows NT)

Attention: This setting must be done on the host PC.

1. Click on "Start"- "Settings"- "Control Panel."
2. Double-click on "Networks."
3. Click on the "Service"tab and select "Remote access service."
4. Click on "Properties."
5. Click on "Networks" push button.
6. Make check marks next to both TCP/IP items.
7. Click on "Configurations" button.
8. Select "Only this computer."
9. Select "Use static address pool" and specify an address range such as 10.10 10.11 - 10.10.10.20.
10. Click on "OK."

### Setting a guest PC's IP address

#### Setting a guest PC's (Windows 95/98) IP address

1. Click on "Start"-"Programs"-"Accessories"-"Dial-Up Networking."
2. Make a new connection by following the Wizard.
3. Click the right mouse button on the new icon and select "Properties."
4. Click on "Server Types" tab.
5. Select "PPP:Windows95,Windows NT3.5, Internet"as the type of Dial-Up Server and make check marks next to "Enable software compression", "Require encrypted password"and "TCP/IP."
6. Click on"TCP/IP Settings."
7. If the host PC is running Windows 95 or OS/2, select"Specify an IP address "and specify an IP address such as 10.10.10.11. If the slave server is running Windows NT, select "Server-assigned IP address."

#### Setting a guest PC's (Windows 2000) IP address

1. Click on "Start" - "Settings" - "Network and Dial-up Connection"
2. Click right button on an icon which you are going to use.
3. Select TCP/IP on the list.
4. Select "properties."
5. Set the appropriate value on the "Internet protocol( TCP/IP) properties."