=============================================================================
    Intel(R) Server Platform S1400SP FRU/SDR Update Release Notes
=============================================================================

INTEL Enterprise Platform & Services Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA

=============================================================================

DATE:   Sep,08 2012

TO:	    Intel(R) Server Platform S1400SP customers

SUBJECT:    Integrate BMC(R) FRU/SDR update package S1400SP_FRUSDR_06 release notes

=============================================================================
                               LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products.
No license, express or implied, by estoppel or otherwise, to any intellectual
property rights is granted by this document. Except as provided in Intel's
Terms and Conditions of Sale for such products, Intel assumes no liability
whatsoever, and Intel disclaims any express or implied warranty, relating to
sale and/or use of Intel products including liability or warranties relating
to fitness for a particular purpose, merchantability, or infringement of any
patent, copyright or other intellectual property right. Intel Corporation may
have patents or pending patent applications, trademarks, copyrights, or other
intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not
provide any license, express or implied, by estoppel or otherwise, to any
such patents, trademarks, copyrights, or other intellectual property rights.
Intel products are not intended for use in medical, life saving, or life
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation.

*Other names and brands are the property of their respective owners.

Copyright (c) 2012 Intel Corporation.

=============================================================================
                              ABOUT THIS RELEASE
=============================================================================

SDR file version: 1.00
Baseboard FRU file version: 0.01
Master configuration file version: 1.00
FRUSDR Utility:                    11.0-Build 14

=============================================================================
        SYSTEM HARDWARE & SOFTWARE REQUIREMENTS/REVISIONS
=============================================================================

- This FRU/SDR package has only been tested on S1400SP FAB1 baseboards

- BMC firmware rev 01.15 (or later) MUST be preinstalled prior to installing
  this FRU/SDR package

- BIOS R0044 or later
- MB Ver Fab1

=============================================================================
                      IMPORTANT INSTALLATION NOTES
=============================================================================

- None

=============================================================================
            INSTALLATION PROCEDURE
=============================================================================

1. Ensure BMC release 01.16 or later is pre-installed before attempting this
   FRU/SDR update.

2. Copy all of the files in the S1400SP_FRUSDR_04.zip archive to a USB key,
   hard disk drive or floppy drive.
   All of the files in this zip archive must reside in the same directory.

3. Boot to EFI and then run the following command to display the
   contents of the baseboard FRU device:

    FRUSDR /d FRU

   If device is empty(which is the case for all new FAB1 baseboards) or corrupted, then
   execute the following command to program the empty FRU device:

   For S1400SP:
        FRUSDR /fru S1400SP.fru

4. Now execute the following command to bring up the main FRU/SDR load menu:

    FRUSDR /cfg master.cfg


5. Select the option which is applicable to what you want to do. On a brand
   new baseboard I would highly recommend to run option 3 to program both
   the FRU and SDR. By reprogramming the FRU you will be given the option
   to input data from the keyboard into various chassis, board and product
   areas. Ensure that you select the correct chassis from the chassis
   selection menu otherwise your fan sensors will not be configured
   properly.

6. Once the package has finished its installation, I would highly recommend
   to DC power off the system and cycle AC power.

=============================================================================
                           KNOWN ISSUES/WORKAROUNDS
=============================================================================

- None

=============================================================================
                           FEATURES ADDED
=============================================================================
S1400SP_FRUSDR_0100:
- Update the PSU's FRU into the PSU's detection in Master file
- Update the Correction factor C1 and C2 system airflow record

S1400SP_FRUSDR_06:
- Correct the domain mask of Fans-off record for BFP21 Redundant chassis, which is incorrect before
 
S1400SP_FRUSDR_05:
- Modify the P1 VRD Hot sensor to auto-rearm
- Update the feature of auto-detect PSU and HSBP 
- Add the sensor "IO mod Presence" and "SAS Mod Presence"

S1400SP_FRUSDR_04:
- Initial release

=============================================================================
                           ISSUES FIXED
=============================================================================
S1400SP_FRUSDR_0100:
- None

S1400SP_FRUSDR_06:
- None

S1400SP_FRUSDR_05:
- [FW EVL]It can't automatic detect the fru of the power supply.

S1400SP_FRUSDR_04:
- Initial release

=============================================================================
                             REFERENCE MATERIAL
=============================================================================

CONFIG-FSC Rev1.6 datasheet


[END OF RELEASE NOTES]