Intel® Graphics Media Accelerator

Video BIOS Release Document

Microsoft Windows* 7

Intel Confidential

INFORMATION IN THIS DOCUMENT IS PROVIDED IN CONNECTION WITH INTEL PRODUCTS. NO LICENSE, EXPRESS OR IMPLIED, BY ESTOPPEL OR OTHERWISE, TO ANY INTELLECTUAL PROPERTY RIGHTS IS GRANTED BY THIS DOCUMENT. EXCEPT AS PROVIDED IN INTEL'S TERMS AND CONDITIONS OF SALE FOR SUCH PRODUCTS, INTEL ASSUMES NO LIABILITY WHATSOEVER AND INTEL DISCLAIMS ANY EXPRESS OR IMPLIED WARRANTY, RELATING TO SALE AND/OR USE OF INTEL PRODUCTS INCLUDING LIABILITY OR WARRANTIES RELATING TO FITNESS FOR A PARTICULAR PURPOSE, MERCHANTABILITY, OR INFRINGEMENT OF ANY PATENT, COPYRIGHT OR OTHER INTELLECTUAL PROPERTY RIGHT.

UNLESS OTHERWISE AGREED IN WRITING BY INTEL, THE INTEL PRODUCTS ARE NOT DESIGNED NOR INTENDED FOR ANY APPLICATION IN WHICH THE FAILURE OF THE INTEL PRODUCT COULD CREATE A SITUATION WHERE PERSONAL INJURY OR DEATH MAY OCCUR.
Intel may make changes to specifications and product descriptions at any time, without notice. Designers must not rely on the absence or characteristics of any features or instructions marked "reserved" or "undefined." Intel reserves these for future definition and shall have no responsibility whatsoever for conflicts or incompatibilities arising from future changes to them. The information here is subject to change without notice. Do not finalize a design with this information.
The products described in this document may contain design defects or errors known as errata which may cause the product to deviate from published specifications. Current characterized errata are available on request.

Intel and the Intel logo are trademarks of Intel Corporation in the U.S. and other countries.

*Other names and brands may be claimed as the property of others.

Copyright© 2010, Intel Corporation. All rights reserved.

Latest Video BIOS Builds Since: 26/09/2011
Build # | Chipset Family
3072 | Oak Trail
3071 | Oak Trail
3068 | Oak Trail
3062 | Oak Trail
3058 | Oak Trail
3056 | Oak Trail
3049 | Oak Trail
3040 | Oak Trail
3036 | Oak Trail
3034 | Oak Trail
3028 | Oak Trail
3020 | Oak Trail
3013 | Oak Trail
3011 | Oak Trail

Video BIOS Builds

Video BIOS Release Note: 17/08/2011
Sighting# | Bug# | RCR# | DCN# | Description/Issue fixed | Chipset Family Affected | Build
| NA |  |  | Addition of 50Hz option under mode removal table | OakTrail | 3072
| 3904268 |  |  | VBIOS boot time optimized | Oak Trail | 3071
| 3903839 |  |  | While looping VBIOS 3034 extension function 4F02h, the LCD panel shows black screen | Oak Trail | 3068
| 3904307 |  |  | Added support for VIDEO MODE 0F in the VBIOS | Oak Trail | 3062
| 3904226 |  |  | Added ability to remove specific resolution and refresh rate through VBT | Oak Trail | 3058
| 3904128 |  |  | The display goes blank while resuming from S4 | Oak Trail | 3056
| 3904182 |  |  | LVDS clock frequency setting in VBT is not applied | Oak Trail | 3056
| 3903954 |  |  | LVDS clock frequency setting is wrong | Oak Trail | 3049
| 3903927 |  |  | LVDS panel power sequencing was wrong | Oak Trail | 3049
| 3903833 |  |  | Windows logo shifted to the left while system boot up | Oak Trail | 3040
| 3903820 |  |  | Garbage seen on the screen while resuming from S4 | Oak Trail | 3040
| 3903697 |  |  | Removal of modes through VBT(BMP) settings is not working | Oak Trail | 3036
| 3903652 |  |  | System hang occurs when F8 is clicked more than once to enter into safe mode | Oak Trail | 3034
| 3903509 |  |  | No ‘POST’ screen on HDMI | Oak Trail | 3020
| 3903275 |  |  | Function to detect the right display connected implemented | Oak Trail | 3013
| 3903085 |  |  | BMP does not allow VBT settings changes | Oak Trail | 3011
| 3903128 |  |  | Restart fails with or without graphics driver | Oak Trail | 3011
| 3903187 |  |  | LFP backlight is ON when system is booted to HDMI | Oak Trail | 3011