This release note and the software that accompanies it are copyright (c) 2015, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.


==========================
Supported RAID Controllers
==========================
This download supports the following Intel(R) RAID controllers using the SAS software stack: RMS3CC080, RMS3CC040, RMS3HC080, RS3YC, RS3LC, RS3SC008, RS3MC044, RS3DC080, RS3DC040, RS3WC080, RCS25ZB040, RCS25ZB040LX, RS25AB080, RS25SB008, RMS2PB080, RMS25PB040, RMT3PB080, RMS25CB080, RMS25CB080N,MS25PB080N, RMS25CB040, RMT3CB080, RS25NB008, RS25DB080, RS2VB080, RS2VB040, RT3WB080, RS2WC040, RS2WC080, RS2SG240, RS2WG160, RMS2MH080, RMS2AF080, RMS2AF040, RS2MB044, RS2BL080, RS2BL080DE, RS2BL040, RS2PI008DE, RS2PI008.  Please verify that this utility has been tested with the RAID card you have chosen to use by checking the web page for your controller at http://support.intel.com.


===================
Package Information
===================
Version = 1.17.08
OS supported = EFI, FreeBSD, Linux, Linux-ppc, Solaris x86, Ubuntu, VMware, VMware-MN, VMware-NM-NDS, Windows


==================
Known Restrictions
==================
STORCLI PHASE 2.0 Specific Limitations:
1.	User can use both 'raid0' and 'r0' for mentioning the raid level. And user can find both the forms in the help command.
2.	When passing parameter,'set' for CC mode is mandatory. 
3.	The use of comma in between array no and row parameter in the syntax for making ‘pdreplacemissing’ should not be used.
4.	User would not be able to specify ROWs while creating ‘Dedicated Hot Spare’. Instead user needs to use ‘Drive Group ID’ as dgs=N
5.	In ‘Foreign Configuration show’, utility will display VD as ‘Foreign’ instead of showing the VD state.
6.	The success code and description is printed only after complete processing of the command. Success will not be printed unless the entire log is displayed to the output. Hence the success code and description is printed at the end of the log for this particular command.
7.	Any command syntax is still valid, if user uses “-” instead of “/”  for e.g. storcli.exe /c0-vall show.
8.	Show ‘Bus and PCI Slot type’ are not shown as part of the controller information.
9.	While creating a VD using non-Enc-ID Devices, user needs to provide inputs in the format ‘D:SlotID’ as syntax (for eg: Drives=D:1,2,3 where 1,2,3 are the slot ids of the non encID devices)
10.	Tape Drives will be listed only with /c0/sall show all command, /c0/sall show doesn’t list Tape drive but only display the direct attached drives if present or a blank table if none are connected.
11.	Importing Foreign Configuration while Rebuild is in progress then query for Show fall the output would display multiple R60 VDs.
12.	Date and Time of controller is not displayed in proper format in EFI Environment 
13.	JSON is not required in EFI
14.	The sector size of the drives are displayed in “KB” instead of bytes under the PD List table. This is just display error in tabular format but it is displayed correctly in drive details.
15.	The “Eid:slot” column while importing a foreign config is not populated. StorCLI: The VD name cannot contain spaces as allowed in MSM.
16.	Consistency Check cannot be scheduled beyond year-2037AD.
17.	Flashing 9260CV low-level controller firmware is supported only through DOS version of CLI (MegaCLI) and not through EFI version of StorCLI.  Flashing MegaRAID firmware does not have this issue.

Known Behavior:
1.	‘All VD initialization’ command when run through StorCLI utility, shows the error message as failed for cachecaded VD. This is a generic limitation.
2.	While reconstruction is in progress, start of CC/Init/BGI operations on same VD throws an inappropriate error message. This is a generic limitation.
3.	In controller show cc the field CC current state will change only when it meets the schedule CC parameters.
4.	All the unsupported commands for SWR controller if tried to execute may result in unknown behaviour for example – system hang-up. For the list of unsupported commands refer to user guide Appendix C: Unsupported Commands in Embedded RAID.
5.	Output for controller information contains junk characters in VMware ESXi 4.1 update2.  
6.	FDE drives are displayed as secured drives on SWR- SCU controller.
7.	There is no check to see whether user has entered different properties or the same property multiple times in StorCLI command. Hence StorCLI  does not throw syntax error for the command “/c0/dall show all all all”. This issue is because of the implementation of accepting multiple properties in a single command line in some cases.


=======================
Contents on the package
=======================
The following files are included in this zip:

Name						Description
ir3_StorCli_vX.XX.XX_rel-notes.txt		This file
License_v2.pdf					License Agreement
EFI\StorCli.efi					EFI Utility
FreeBSD\StorCli					FreeBSD 32bit Utility
FreeBSD\StorCli64 				FreeBSD 64bit Utility
Linux\storcli-X.XX.XX-X.noarch.rpm		Linux Installation package
Linux-ppc\StorCli64.tar 			Linux-ppc Utility
Solaris\StoCli.pkg				Solaris Installation package
Sparc\StoCli.pkg				Sparc Installation package
Ubuntu\storcli_X.XX.XX_alldeb			Ubuntu Installation package
VMware\StorCli.zip					VMware Utility
VMware-MN\vmware-esx-storcli-X.XX.XX.vib 	VMware-MN utility
VMware-MN-NDS\vmware-esx-storcli-X.XX.XX.vib 	VMware-MN utility
Windows\StorCli.exe				Windows 32bit utility
windows\StorCli64.exe				Windows 64bit utility


==========================
Installation instructions:
==========================

EFI
==========
This utility is an EFI Based command line utility that can be used to query the controller and attached devices for status, Update Firmware, and create/manage logical drive configuration.
Extract DOS folder contents to a user specified location such as = FS0:


FreeBSD
==========
This utility is a FreeBSD Based command line utility that can be used to query the controller and attached devices for status, Update Firmware, and create/manage logical drive configuration.
Extract the FreeBSD folder contents to a user specified location.

In FreeBSD OS, StorCli or StorCli64 application will not function if the user is trying to run it in CSH, the default shell in FreeBSD.
Please ensure that the user has entered the bash shell by executing the command "bash".


Linux
==========
This utility is a Linux Based command line utility that can be used to query the controller and attached devices for status, Update Firmware, and create/manage logical drive configuration.

To install StorCLI, perform the following steps:
1. Unzip the StorCLI package.
2. To install the StorCLI RPM, run the rpm -ivh <StorCLI-x.xx-x.noarch.rpm> command.
3. To upgrade the StorCLI RPM, run the rpm -Uvh <StorCLI-x.xx-x.noarch.rpm> command.


Solaris
==========
This utility is a Solaris Based command line utility that can be used to query the controller and attached devices for status, Update Firmware, and create/manage logical drive configuration.
Extract Solaris folder contents to a user specified location and install the utility pkg.

Requirement for Storcli Execution 

1) Download "libgcc-3.4.6-....-local.gz" from http://www.sunfreeware.com

2) Copy it to the setup and Extract.

3) Install the Package using bellow command.

	pkgadd -d libgcc-3.4.6-....-local.pkg

4) Prior to executing standalone Storcli binary, check the permissions of Storcli binary. 

	"ls -l storcli"

5) If executable permissions are not given, run the below command to change the permissions.

	"chmod +x storcli"

Ubuntu
==========
1. Copy the Package.sh and the Linux Binaries to the ubnutnu server.

2. Run the Package.sh with the version as argument as below. Version should not start with the alphabet.
	./Package.sh x.xx.xx

2. Installing debian Package
	sudo dpkg -i storcli_x.xx.xx_all.deb

3. verifying , if the package is installed successfully or not.
   dpkg -l | grep -i storcli

4. Run the commands    with super user as below.
	sudo /opt/MegaRAID/storcli/storcli adpcount


VMware & Vmware-MN & Vmware-MN-NDS
==========
This utility is a VMWare Based command line utility that can be used to query the controller and attached devices for status, Update Firmware, and create/manage logical drive configuration.
Extract Windows folder contents to a user specified location 

1. The installed VIB Package can be list using command 
	"esxcli software vib list "
 
2. The VIB Package can be installed using the command
	"esxcli software vib install -v=vmware-esx-storcli.vib"

3.The VIB Package can be removed using the command
	"esxcli software vib remove -n=vmware-esx-storcli.vib"


Windows
==========
This utility is a Windows Based command line utility that can be used to query the controller and attached devices for status, Update Firmware, and create/manage logical drive configuration.
Extract Windows folder contents to a user specified location.  

The command prompt needs to have administrative privileges in order to run StorCLI commands.


Supported commands and options
=============================
 
storcli -v 
storcli -h| -help| ? 
storcli -h| -help| ? legacy
storcli show 
storcli show all
storcli show ctrlcount
storcli show file=<filepath>
storcli /cx add vd r[0|1|5|6|00|10|50|60]
	[Size=<VD1_Sz>,<VD2_Sz>,..|all] [name=<VDNAME1>,..] 
	drives=e:s|e:s-x|e:s-x,y,e:s-x,y,z [PDperArray=x][SED]
	[pdcache=on|off|default][pi][DimmerSwitch(ds)=default|automatic(auto)|
	none|maximum(max)|MaximumWithoutCaching(maxnocache)][WT|WB|AWB][nora|ra]
	[direct|cached] [cachevd] [Strip=<8|16|32|64|128|256|512|1024>]
	 [AfterVd=X] [EmulationType=0|1|2] [Spares = [e:]s|[e:]s-x|[e:]s-x,y]
	[force][ExclusiveAccess] [Cbsize=0|1|2 Cbmode=0|1|2|3|4|7] 
storcli /cx add vd each r0 [name=<VDNAME1>,..] [drives=e:s|e:s-x|e:s-x,y]
	[SED] [pdcache=on|off|default][pi] [DimmerSwitch(ds)=default|
	automatic(auto)|none|maximum(max)|MaximumWithoutCaching(maxnocache)] 
	[WT|WB|AWB] [nora|ra] [direct|cached] [EmulationType=0|1|2]
	[Strip=<8|16|32|64|128|256|512|1024>] [ExclusiveAccess]
	[Cbsize=0|1|2 Cbmode=0|1|2|3|4|7]
storcli /cx add VD cachecade|nytrocache r[aid][0,1,10, 1EC] 
	drives = [e:]s|[e:]s-x|[e:]s-x,y [WT|WB] [assignvds = 0,1,2] 
	[BOOTVOLSIZE=x]
storcli /cx add VD cachecade|nytrocache slice r[aid][0,1]
	size=<x> [name=<NytroCacheName>] drives= [e:]s|[e:]s-x|[e:]s-x,y
	[WT|WB][assignvds = 0,1,2]
	size=[<VD1_Sz>,<VD2_Sz>,..] [name=<VDNAME1>,..] [WT|WB] [nora|ra]
	[direct|cached] [CachedBadBBU|NoCachedBadBBU]
	[Strip=<8|16|32|64|128|256|512|1024>] [AfterVd=X]
	[Spares = [e:]s|[e:]s-x|[e:]s-x,y] [force]
storcli /cx/ex show 
storcli /cx/ex show all 
storcli /cx/ex show status 
storcli /cx/ex show phyerrorcounters 
storcli /cx/vx del [cachecade] [discardcache] [force]
storcli /cx delete events
storcli /cx show events [[type= <sincereboot| sinceshutdown| includedeleted|
latest=x| ccincon vd=<0,1,...>] filter=<[info],[warning],[critical],[fatal]>
file=<filepath> [logfile[=filename]]
storcli /cx show eventloginfo
storcli /cx show health [all]
storcli /cx delete securitykey
storcli /cx set securitykey=xxxxxxxx {passphrase=xxxx} {keyid=xxx}
storcli /cx start Diag Duration=<Val> 
storcli /cx set securitykey keyid=xxx
storcli /cx compare securitykey=xxxxxxxxxx
storcli /cx set termlog[=on|off|offthisboot]
storcli /cx show termlog [type=config|contents] [logfile[=filename]] 
storcli /cx delete termlog
storcli /cx set securitykey=xxxxxxxx oldsecuritykey=xxxxxxxx
	{passphrase=xxxx} {keyid=xxx}
storcli /cx set sesmonitoring[=on|off]
storcli /cx show sesmonitoring 
storcli /cx set failpdonsmarterror[=on|off]
storcli /cx show failpdonsmarterror 
storcli /cx/dx show 
storcli /cx/dall show cachecade 
storcli /cx/dx show all 
storcli /cx/dall show mirror 
storcli /cx/dall split mirror 
storcli /cx/dall add mirror src=<val> [force] 
storcli /cx show freespace
storcli /cx/fall show [all] [securityKey = xxx]
storcli /cx/fall del|delete [securityKey = xxx]
storcli /cx/fall import [preview] [securityKey = xxx]
storcli /cx/vx set ssdcaching=on|off
storcli /cx/vx set hidden=on|off
storcli /cx/dx set hidden=on|off
storcli /cx/dx set security=on
storcli /cx/vx show expansion
storcli /cx show fshinting
storcli /cx/vx set fshinting=<value>
storcli /cx/vx expand Size=<xx> [expandarray]
storcli /cx[/ex]/sx show 
storcli /cx[/ex]/sx show all
storcli /cx[/ex]/sx start rebuild 
storcli /cx[/ex]/sx stop rebuild 
storcli /cx[/ex]/sx pause rebuild 
storcli /cx[/ex]/sx resume rebuild 
storcli /cx[/ex]/sx show rebuild 
storcli /cx[/ex]/sx show health 
storcli /cx[/ex]/sx show smart 
storcli /cx[/ex]/sx start copyback target=e:s 
storcli /cx[/ex]/sx stop copyback 
storcli /cx[/ex]/sx pause copyback 
storcli /cx[/ex]/sx resume copyback 
storcli /cx[/ex]/sx reset phyerrorcounters 
storcli /cx[/ex]/sx show copyback 
storcli /cx[/ex]/sx show phyerrorcounters 
storcli /cx[/ex]/sx start initialization  
storcli /cx[/ex]/sx stop initialization  
storcli /cx[/ex]/sx show initialization  
storcli /cx[/ex]/sx start locate  
storcli /cx[/ex]/sx stop locate  
storcli /cx[/ex]/sx show securitykey keyid 
storcli /cx[/ex]/sx add hotsparedrive [DGs=<N|0,1,2...>] [enclaffinity]
	[nonrevertible]
storcli /cx[/ex]/sx delete hotsparedrive
storcli /cx[/ex]/sx spinup
storcli /cx[/ex]/sx spindown
storcli /cx[/ex]/sx set online 
storcli /cx[/ex]/sx set offline 
storcli /cx[/ex]/sx set missing 
storcli /cx[/ex]/sx set jbod 
storcli /cx[/ex]/sx set security=on 
storcli /cx[/ex]/sx set good [force]  
storcli /cx[/ex]/sx insert dg=A array=B row=C 
storcli /cx/vx set emulationType=0|1|2
storcli /cx/vx set cbsize=0|1|2 cbmode=0|1|2|3|4|7 
storcli /cx/vx set wrcache=WT|WB|AWB
storcli /cx/vx set rdcache=RA|NoRA
storcli /cx/vx set iopolicy=Cached|Direct
storcli /cx/vx set accesspolicy=RW|RO|Blocked|RmvBlkd
storcli /cx/vx set pdcache=On|Off|Default
storcli /cx/vx set name=<NameString>
storcli /cx/vx set HostAccess=ExclusiveAccess|SharedAccess
storcli /cx/vx set ds=Default|Auto|None|Max|MaxNoCache
storcli /cx/vx set autobgi=On|Off
storcli /cx/vx set pi=Off
storcli /cx/vx show
storcli /cx/vx show all [logfile[=filename]]
storcli /cx/vx show init
storcli /cx/vx show cc
storcli /cx/vx show erase
storcli /cx/vx show migrate
storcli /cx/vx show bgi
storcli /cx/vx show autobgi
storcli /cx/vx show trim
storcli /cx set consistencycheck|cc=[off|seq|conc] [delay=value]
	starttime=yyyy/mm/dd hh] [excludevd=x-y,z]
storcli /cx show cc|consistencycheck
storcli /cx show ocr 
storcli /cx set ocr=<on|off>
storcli /cx/vx start init[Full][Force]
storcli /cx/vx start erase [simple|normal|thorough|standard][patternA=<val>]
[patternB=<val>]
storcli /cx/vx start cc[Force]
storcli /cx/vx start migrate type=raidx [option=add|remove 
	drives=[e:]s|[e:]s-x|[e:]s-x,y] [Force] 
storcli /cx/vx stop init
storcli /cx/vx stop erase
storcli /cx/vx stop cc
storcli /cx/vx stop bgi
storcli /cx/vx pause cc
storcli /cx/vx pause bgi
storcli /cx/vx resume cc
storcli /cx/vx resume bgi
storcli /cx show 
storcli /cx show all [logfile[=filename]]
storcli /cx show preservedcache 
storcli /cx/vx delete preservedcache[force] 
storcli /cx[/ex]/sx download src=<filepath> [satabridge] [mode= 5|7]
storcli /cx/ex download src=<filepath> [forceActivate] 
storcli /cx[/ex]/sx secureerase [force]  
storcli /cx[/ex]/sx start erase [simple| normal| thorough | standard| threepass]
   [patternA=<val>] [patternB=<val>]
storcli /cx[/ex]/sx stop erase 
storcli /cx[/ex]/sx show erase 
storcli /cx[/ex]/sx show rawdata pageaddr=<pageaddress in hex> file=<filename> 
storcli /cx[/ex]/sx set bootdrive=<on|off> 
storcli /cx/vx set bootdrive=<on|off>
storcli /cx show bootdrive
storcli /cx show bootwithpinnedcache
storcli /cx set bootwithpinnedcache=<on|off>
storcli /cx show activityforlocate
storcli /cx set activityforlocate=<on|off>
storcli /cx show copyback
storcli /cx set copyback=<on|off> type=smartssd|smarthdd|all 
storcli /cx show jbod
storcli /cx set jbod=<on|off> [force]
storcli /cx set autorebuild=<on|off> 
storcli /cx set ldlimit=<default|max> 
storcli /cx show autorebuild
storcli /cx set autopdcache=<off|[on|sscr0]|r0|wbr0> [immediate]
storcli /cx show autopdcache
storcli /cx show cachebypass
storcli /cx set cachebypass=<on|off> 
storcli /cx show usefdeonlyencrypt
storcli /cx set usefdeonlyencrypt=<on|off>
storcli /cx show prcorrectunconfiguredareas
storcli /cx set prcorrectunconfiguredareas=<on|off> 
storcli /cx show batterywarning
storcli /cx set batterywarning=<on|off> 
storcli /cx show abortcconerror
storcli /cx set abortcconerror=<on|off> 
storcli /cx show ncq
storcli /cx show configautobalance 
storcli /cx set ncq=<on|off> 
storcli /cx set configautobalance=<on|off> 
storcli /cx show maintainpdfailhistory
storcli /cx set maintainpdfailhistory=<on|off> 
storcli /cx show restorehotspare
storcli /cx set restorehotspare=<on|off> 
storcli /cx set bios [state=<on|off>] [Mode=<SOE|PE|IE|SME>] [abs=<on|off>]
       [DeviceExposure=<value>]
storcli /cx show bios 
storcli /cx show alarm
storcli /cx set alarm=<on|off|silence> 
storcli /cx show foreignautoimport
storcli /cx set foreignautoimport=<on|off> 
storcli /cx show directpdmapping
storcli /cx set directpdmapping=<on|off> 
storcli /cx show rebuildrate
storcli /cx set rebuildrate=<value> 
storcli /cx show loadbalancemode
storcli /cx set loadbalancemode=<on|off> 
storcli /cx show eghs
storcli /cx set eghs [state=<on|off>] [eug=<on|off>] [smarter=<on|off>] 
storcli /cx show cacheflushint
storcli /cx set cacheflushint=<value> 
storcli /cx show prrate
storcli /cx set prrate=<value> 
storcli /cx show ccrate
storcli /cx set ccrate=<value> 
storcli /cx show bgirate
storcli /cx set bgirate =<value> 
storcli /cx show dpm 
storcli /cx set dpm =<on|off> 
storcli /cx show sgpioforce 
storcli /cx set sgpioforce =<on|off> 
storcli /cx set supportssdpatrolread =<on|off> 
storcli /cx show migraterate
storcli /cx set migraterate=<value> 
storcli /cx show spinupdrivecount
storcli /cx show wbsupport
storcli /cx set spinupdrivecount=<value> 
storcli /cx show spinupdelay
storcli /cx set spinupdelay=<value> 
storcli /cx show coercion
storcli /cx set coercion=<value> 
storcli /cx show limitMaxRateSATA
storcli /cx set limitMaxRateSATA=on|off 
storcli /cx show HDDThermalPollInterval
storcli /cx set HDDThermalPollInterval=<value> 
storcli /cx show SSDThermalPollInterval
storcli /cx set SSDThermalPollInterval=<value> 
storcli /cx show smartpollinterval
storcli /cx set smartpollinterval=<value> 
storcli /cx show eccbucketsize
storcli /cx set eccbucketsize=<value> 
storcli /cx show eccbucketleakrate
storcli /cx set eccbucketleakrate=<value> 
storcli /cx show backplane
storcli /cx set backplane mode=<value> expose=<on/off> 
storcli /cx show perfmode
storcli /cx set perfmode=<value> [maxflushlines=<value> numiostoorder=<value>]
storcli /cx show perfmodevalues
storcli /cx show pi
storcli /cx set pi [state=<on|off>] [import=<on|off>]
storcli /cx show time
storcli /cx set time=<yyyymmdd hh:mm:ss | systemtime> 
storcli /cx show ds
storcli /cx set ds=OFF type=1|2|3|4
storcli /cx set ds=ON type=1|2 [properties]
storcli /cx set ds=ON type=3|4 DefaultLdType=<val> [properties]
storcli /cx set ds [properties] 
storcli /cx show safeid
storcli /cx show rehostinfo
storcli /cx show pci
storcli /cx show ASO
storcli /cx set aso key=<key value> preview
storcli /cx set aso key=<key value>
storcli /cx set aso transfertovault
storcli /cx set aso rehostcomplete
storcli /cx set aso deactivatetrialkey
storcli /cx set factory defaults
storcli /cx download file=<filepath> [fwtype=<val>] [ResetNow] [nosigchk] 
	[noverchk] [force]
storcli /cx flush|flushcache
storcli /cx [start] flush|flushcache [cachecade | nytrocache | ALL]
storcli /cx stop flush|flushcache cachecade|nytrocache
storcli /cx show flush|flushcache cachecade|nytrocache 
storcli /cx/px show 
storcli /cx/px show all
storcli /cx/px set linkspeed=0|1.5|3|6|12 
storcli /cx/bbu show 
storcli /cx/bbu show all 
storcli /cx/bbu show status 
storcli /cx/bbu show properties 
storcli /cx/bbu show learn 
storcli /cx/bbu show gasgauge Offset=xxxx Numbytes=n 
storcli /cx/bbu start learn 
storcli /cx/bbu show modes 
storcli /cx/bbu set [ learnDelayInterval=<val> | bbuMode=<val>  
	|learnStartTime=[DDD HH | off] | autolearnmode=<val> | 
	powermode=sleep | writeaccess=sealed ] 
storcli /cx/cv set SCAPVPD file=<input file path> VPDPage=<SCapVPDFixed>
storcli /cx/cv show 
storcli /cx/cv show all 
storcli /cx/cv show status 
storcli /cx/cv show learn 
storcli /cx/cv show SCAPVPD file=<output file path> VPDPage=<SCapVPDFixed>
storcli /cx/cv start learn 
storcli /cx show securitykey keyid 
storcli /cx start patrolread
storcli /cx stop patrolread
storcli /cx pause patrolread
storcli /cx resume patrolread
storcli /cx show patrolRead
storcli /cx show powermonitoringinfo
storcli /cx show ldlimit
storcli /cx set patrolread = {{on mode=<auto|manual> }|{off}}
storcli /cx set patrolread [starttime=< yyyy/mm/dd hh>] 
	[maxconcurrentpd =<value>] [includessds=<on|onlymixed|off>]
	[uncfgareas=on|off]
storcli /cx set patrolread delay = <value>
storcli /cx[/ex]/sx show diag paniclog [Query] | [ExtractSlot=x] 
                                         | [EraseSlot=x] [file=filepath]
storcli /cx[/ex]/sx show diag smartlog [file=filepath] 
storcli /cx[/ex]/sx show diag errorlog [file=filepath] 
storcli /cx del Nytrocache [force]
storcli /cx show badblocks
storcli /cx flasherase 
storcli /cx shutdown 
storcli /cx/mx set mode=<Internal | External | Auto> 
storcli /cx/mx show 
storcli /cx transform iMR 
storcli /cx restart 
storcli /cx/vx show BBMT
storcli /cx/vx delete BBMT
storcli /cx[/ex]/sx start format [thorough] 
storcli /cx show dequeuelog file=<filepath>
storcli /cx show maintenance
storcli /cx set maintenance mode=normal|nodevices 
storcli /cx show personality
storcli /cx set personality=RAID|HBA 
storcli /cx show jbodwritecache
storcli /cx set jbodwritecache=on|off|default 
storcli /cx show immediateio
storcli /cx show driveactivityled
storcli /cx set immediateio=<on|off>
storcli /cx show largeiosupport
storcli /cx set largeiosupport=<on|off>
storcli /cx set driveactivityled=<on|off>
storcli /cx show pdfailevents [lastoneday] [lastseqnum=<val>] [file=<filepath>] 
storcli /cx show pdfaileventoptions
storcli /cx set pdfaileventoptions [detectionType=<val>] [correctiveaction=<val>] [errorThreshold=<val>] 
storcli /cx show AliLog [logfile[=filename]]
storcli /cx get config file=<fileName>
storcli /cx set config file=<fileName>
storcli /cx show flushwriteverify
storcli /cx set flushwriteverify=<on|off>


~~~~~~~~~~~~~~~
Legacy CMDTool2 commands: 

 NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

storcli -v 
storcli -help|-h|? 
storcli -adpCount 
storcli -AdpSetProp {CacheFlushInterval -val} | { RebuildRate -val} 
    | {PatrolReadRate -val} | {BgiRate -val} | {CCRate -val} 
    | {ReconRate -val} | {SpinupDriveCount -val} | {SpinupDelay -val} 
    | {CoercionMode -val} | {ClusterEnable -val} | {PredFailPollInterval -val} 
    | {BatWarnDsbl -val} | {EccBucketSize -val} | {EccBucketLeakRate -val} 
    | {AbortCCOnError -val} | AlarmEnbl | AlarmDsbl | AlarmSilence 
    | {SMARTCpyBkEnbl -val} | {SSDSMARTCpyBkEnbl -val} | NCQEnbl | NCQDsbl 
    | {MaintainPdFailHistoryEnbl -val} | {RstrHotSpareOnInsert -val} 
    | {DisableOCR -val} | {BootWithPinnedCache -val} | {enblPI -val} | {PreventPIImport -val} 
    | {EnblSpinDownUnConfigDrvs -val} | {UseDiskActivityforLocate -val} -aN|-a0,1,2|-aALL 
    | AutoEnhancedImportEnbl | AutoEnhancedImportDsbl -aN|-a0,1,2|-aALL 
    | {ExposeEnclDevicesEnbl -val} -aN|-a0,1,2|-aALL 
    | {DsblSpinDownHsp -val} -aN|-a0,1,2|-aALL 
    | {SpinDownTime -val} | {Perfmode -val} | {EnableVC -val} -aN|-a0,1,2|-aALL 
    | {PerfMode -val –MaxFlushLines -val –NumIOsToOrder -val} -aN|-a0,1,2|-aALL 
    | {useDiskActivityForLocate -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDrvCnt -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDelay -val} -aN|-a0,1,2|-aALL 
storcli -AdpSetProp -AutoDetectBackPlaneDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Auto Detect of SGPIO and i2c SEP. 
             1=Disable Auto Detect of SGPIO. 
             2=Disable Auto Detect of i2c SEP. 
             3=Disable Auto Detect of SGPIO and i2c SEP. 
storcli -AdpSetProp -CopyBackDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Copyback. 
             1=Disable Copyback. 
storcli -AdpSetProp -EnableJBOD -val -aN|-a0,1,2|-aALL 
       val - 0=Disable JBOD mode. 
             1=Enable JBOD mode. 
storcli -AdpSetProp -DsblCacheBypass -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Cache Bypass. 
             1=Disable Cache Bypass. 
storcli -AdpSetProp -LoadBalanceMode -val -aN|-a0,1,2|-aALL 
       val - 0=Auto Load balance mode. 
             1=Disable Load balance mode. 
storcli -AdpSetProp -UseFDEOnlyEncrypt -val -aN|-a0,1,2|-aALL 
       val - 0=FDE and controller encryption (if HW supports) is allowed. 
             1=Only support FDE encryption, disallow controller encryption. 
storcli -AdpSetProp -PrCorrectUncfgdAreas -val -aN|-a0,1,2|-aALL 
       val - 0= Correcting Media error during PR is disabled. 
             1=Correcting Media error during PR is allowed. 
storcli -AdpSetProp -DefaultSnapshotSpace -X% -aN|-a0,1,2|-aALL 
       where X is the percentage of the source VD size. 
storcli -AdpSetProp -DefaultViewSpace -X% -aN|-a0,1,2|-aALL 
       where X is the percentage of the source VD size. 
storcli -AdpSetProp -AutoSnapshotSpace -X% -aN|-a0,1,2|-aALL 
       where X is the percentage of the source VD size. 
storcli -AdpSetProp -DefaultLdPSPolicy -Automatic| -None | -Maximum| -MaximumWithoutCaching -aN|-a0,1,2|-aALL 
storcli -AdpSetProp -DisableLdPS -interval n1 -time n2 -aN|-a0,1,2|-aALL 
       where n1 is the number of hours beginning at time n2 
       where n2 is the number of minutes from 12:00am 
storcli -AdpSetProp -ENABLEEGHSP -val -aN|-a0,1,2|-aALL 
       val - 0= Disabled Emergency GHSP. 
             1= Enabled Emergency GHSP. 
storcli -AdpSetProp -ENABLEEUG -val -aN|-a0,1,2|-aALL 
       val - 0= Disabled Emergency UG as Spare. 
             1= Enabled Emergency UG as Spare. 
storcli -AdpSetProp -ENABLEESMARTER -val -aN|-a0,1,2|-aALL 
       val - 0= Disabled Emergency Spare as Smarter. 
             1= Enabled Emergency Spare as Smarter. 
storcli -AdpSetProp -DPMenable -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Drive Performance Monitoring . 
             1=Enable Drive Performance Monitoring. 
storcli -AdpSetProp -limitMaxRateSATA -val -aN|-a0,1,2|-aALL 
       val - 0=Disables Max limit Rate for SATA to 3G . 
             1=Enable Max limit Rate for SATA to 3G. 
storcli -AdpGetProp CacheFlushInterval | RebuildRate | PatrolReadRate 
    | BgiRate | CCRate | ReconRate | SpinupDriveCount | SpinupDelay 
    | CoercionMode | ClusterEnable | PredFailPollInterval | BatWarnDsbl 
    | EccBucketSize | EccBucketLeakRate | EccBucketCount | AbortCCOnError 
    | AlarmDsply | SMARTCpyBkEnbl | SSDSMARTCpyBkEnbl | NCQDsply 
    | MaintainPdFailHistoryEnbl | RstrHotSpareOnInsert 
    | EnblSpinDownUnConfigDrvs  | DisableOCR 
    | BootWithPinnedCache |enblPI  | PreventPIImport | AutoEnhancedImportDsply | AutoDetectBackPlaneDsbl 
    | CopyBackDsbl | LoadBalanceMode | UseFDEOnlyEncrypt | WBSupport | EnableJBOD 
    | DsblCacheBypass | ExposeEnclDevicesEnbl | DsblSpinDownHsp | SpinDownTime | useDiskActivityForLocate 
    | DefaultLdPSPolicy | DisableLdPsInterval | DisableLdPsTime | SpinUpEncDrvCnt | SpinUpEncDelay  
    | PrCorrectUncfgdAreas | ENABLEEGHSP | ENABLEEUG | ENABLEESMARTER  -aN|-a0,1,2|-aALL 
    | -DPMenable -| Perfmode | PerfModeValues | limitMaxRateSATA aN|-a0,1,2|-aALL 
    | DefaultSnapshotSpace -aN|-a0,1,2|-aALL 
    | DefaultViewSpace -aN|-a0,1,2|-aALL 
    | AutoSnapshotSpace -aN|-a0,1,2|-aALL 
storcli -AdpAllInfo -aN|-a0,1,2|-aALL  
storcli -AdpGetTime -aN|-a0,1,2|-aALL  
storcli -AdpSetTime yyyymmdd hh:mm:ss -aN   
storcli -AdpBIOS -Enbl |-Dsbl | -SOE | -PE | -IE | -SME | EnblAutoSelectBootLd | DsblAutoSelectBootLd | -Dsply -aN|-a0,1,2|-aALL 
storcli -AdpBootDrive {-Set {-Lx | -physdrv[E0:S0]}} | {-Unset {-Lx | -physdrv[E0:S0]}} |-Get -aN|-a0,1,2|-aALL 
storcli -AdpAutoRbld -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL
storcli -AdpCacheFlush -aN|-a0,1,2|-aALL
storcli -AdpPR -Dsbl|EnblAuto|EnblMan|Start|Suspend|Resume|Stop|Info 
         |{SetDelay Val}|{-SetStartTime yyyymmdd hh}|{maxConcurrentPD Val} -aN|-a0,1,2|-aALL
storcli -AdpCcSched -Dsbl|-Info|{-ModeConc | -ModeSeq [-ExcludeLD -LN|-L0,1,2]
   [-SetStartTime yyyymmdd hh ] [-SetDelay val ] } -aN|-a0,1,2|-aALL
storcli -AdpCcSched -SetStartTime yyyymmdd hh -aN|-a0,1,2|-aALL
storcli -AdpCcSched -SetDelay val  -aN|-a0,1,2|-aALL
storcli -FwTermLog -BBUoff|BBUoffTemp|BBUon|BBUGet|Dsply|Clear -aN|-a0,1,2|-aALL
storcli -AdpAlILog -aN|-a0,1,2|-aALL 
storcli -AdpDiag [val] -aN|-a0,1,2|-aALL
          val - Time in second.
storcli -AdpShutDown -aN|-a0,1,2|-aALL
storcli -AdpDowngrade -aN|-a0,1,2|-aALL
storcli -PDList -aN|-a0,1,2|-aALL 
storcli -PDGetNum -aN|-a0,1,2|-aALL 
storcli -pdInfo -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
storcli -PDOnline  -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
storcli -PDOffline -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
storcli -PDMakeGood -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
storcli -PDMakeJBOD -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
storcli -PDHSP {-Set [-Dedicated [-ArrayN|-Array0,1,2...]] [-EnclAffinity] [-nonRevertible]} 
     |-Rmv -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
storcli -PDRbld -Start|-Stop|-Suspend|-Resume|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
storcli -PDClear -Start|-Stop|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
storcli -PdLocate {[-start] | -stop} -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
storcli -PdMarkMissing -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
storcli -PdGetMissing -aN|-a0,1,2|-aALL 
storcli -PdReplaceMissing -physdrv[E0:S0] -arrayA, -rowB -aN 
storcli -PdPrpRmv [-UnDo] -physdrv[E0:S0] -aN|-a0,1,2|-aALL  
storcli -EncInfo -aN|-a0,1,2|-aALL 
storcli -EncStatus -aN|-a0,1,2|-aALL 
storcli -PhyInfo -phyM -aN|-a0,1,2|-aALL  
storcli -PhySetLinkSpeed -phyM -speed -aN|-a0,1,2|-aALL
storcli -PdFwDownload [offline][ForceActivate] {[-SataBridge] -PhysDrv[0:1] }|{-EncdevId[devId1]} -f <filename> -aN|-a0,1,2|-aALL  
storcli -LDInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
storcli -LDSetProp  {-Name LdNamestring} | -RW|RO|Blocked|RemoveBlocked | WT|WB|ForcedWB [-Immediate]|RA|NORA | DsblPI 
        | Cached|Direct | -EnDskCache|DisDskCache | CachedBadBBU|NoCachedBadBBU | -[ExclusiveAccess|SharedAccess] 
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
storcli -LDSetPowerPolicy -Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching 
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
storcli -LDGetProp  -Cache | -Access | -Name | -DskCache | -PSPolicy | Consistency | [ExclusiveAccess] -Lx|-L0,1,2|-LALL  
        -aN|-a0,1,2|-aALL 
storcli -LDInit {-Start [-full]}|-Abort|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
storcli -LDCC -Start|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
storcli -LDBI -Enbl|-Dsbl|-getSetting|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL  
storcli -LDRecon {-Start -rX [{-Add | -Rmv} -Physdrv[E0:S0,...]]}|-ShowProg|-ProgDsply 
        -Lx -aN 
storcli -LdPdInfo -aN|-a0,1,2|-aALL 
storcli -LDGetNum -aN|-a0,1,2|-aALL 
storcli -LDBBMClr -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
storcli -getLdExpansionInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
storcli -LdExpansion -pN -dontExpandArray -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
storcli -GetBbtEntries -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
storcli -Cachecade -assign|-remove -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL
storcli -CfgLdAdd -rX[E0:S0,E1:S1,...] [WT|WB] [NORA|RA] [Direct|Cached]
        [CachedBadBBU|NoCachedBadBBU] [-szXXX [-szYYY ...]]
        [-strpszM] [-Hsp[E0:S0,...]] [-AfterLdX] [-Force]|[FDE|CtrlBased]  
        [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-Cache] [-ExclusiveAccess] [-enblPI] -aN 
storcli -CfgCacheCadeAdd [-rX] -Physdrv[E0:S0,...] {-Name LdNamestring} [WT|WB|ForcedWB] [-assign -LX|L0,2,5..|LALL] -aN|-a0,1,2|-aALL 
storcli -CfgEachDskRaid0 [WT|WB] [NORA|RA] [Direct|Cached] [-enblPI] 
        [CachedBadBBU|NoCachedBadBBU] [-strpszM]|[FDE|CtrlBased] [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-Cache] [-ExclusiveAccess] [-enblPI] -aN|-a0,1,2|-aALL
storcli -CfgClr [-Force] -aN|-a0,1,2|-aALL 
storcli -CfgDsply -aN|-a0,1,2|-aALL 
storcli -CfgCacheCadeDsply -aN|-a0,1,2|-aALL 
storcli -CfgLdDel -LX|-L0,2,5...|-LALL [-Force] -aN|-a0,1,2|-aALL 
storcli -CfgCacheCadeDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
storcli -CfgFreeSpaceinfo -aN|-a0,1,2|-aALL 
storcli -CfgSpanAdd -r10 -Array0[E0:S0,E1:S1] -Array1[E0:S0,E1:S1] [-ArrayX[E0:S0,E1:S1] ...] 
        [WT|WB] [NORA|RA] [Direct|Cached] [CachedBadBBU|NoCachedBadBBU]
        [-szXXX[-szYYY ...]][-strpszM][-AfterLdX][-Force]|[FDE|CtrlBased] 
        [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-Cache] [-ExclusiveAccess] [-enblPI] -aN 
storcli -CfgSpanAdd -r50 -Array0[E0:S0,E1:S1,E2:S2,...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,...] ...][WT|WB][NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-szXXX[-szYYY ...]][-strpszM][-AfterLdX][-Force]| 
        [FDE|CtrlBased]  
        [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-Cache] [-ExclusiveAccess] [-enblPI] -aN 
storcli -CfgSpanAdd -r60 -Array0[E0:S0,E1:S1,E2:S2,E3,S3...] -Array1[E0:S0,E1:S1,E2:S2,E3,S3...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,E3,S3...] ...][WT|WB][NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-szXXX[-szYYY ...]][-strpszM][-AfterLdX][-Force]| 
        [FDE|CtrlBased]  
        [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-Cache] [-ExclusiveAccess] [-enblPI] -aN 
storcli -CfgAllFreeDrv -rX [-SATAOnly] [-SpanCount XXX] [WT|WB] [NORA|RA] 
        [Direct|Cached] [CachedBadBBU|NoCachedBadBBU] [-strpszM]
        [-HspCount XX [-HspType -Dedicated|-EnclAffinity|-nonRevertible]] | 
        [FDE|CtrlBased]  
        [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-Cache] [-ExclusiveAccess] [-enblPI] -aN 
storcli -CfgSave -f filename -aN   
storcli -CfgRestore -f filename -aN   
storcli -CfgForeign -Scan | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
storcli -CfgForeign -Dsply [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
storcli -CfgForeign -Preview [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
storcli -CfgForeign -Import [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
storcli -CfgForeign -Clear [x]|[-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
        x - index of foreign configurations. Optional. All by default. 
storcli -AdpEventLog -GetEventLogInfo -aN|-a0,1,2|-aALL 
storcli -AdpEventLog -GetEvents {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
storcli -AdpEventLog -GetSinceShutdown {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
storcli -AdpEventLog -GetSinceReboot {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
storcli -AdpEventLog -IncludeDeleted {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
storcli -AdpEventLog -GetLatest n {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
storcli -AdpEventLog -GetCCIncon -f <fileName> -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
storcli -AdpEventLog -Clear -aN|-a0,1,2|-aALL 
storcli -AdpBbuCmd -aN|-a0,1,2|-aALL  
storcli -AdpBbuCmd -GetBbuStatus -aN|-a0,1,2|-aALL  
storcli -AdpBbuCmd -GetBbuCapacityInfo -aN|-a0,1,2|-aALL  
storcli -AdpBbuCmd -GetBbuDesignInfo -aN|-a0,1,2|-aALL  
storcli -AdpBbuCmd -GetBbuProperties -aN|-a0,1,2|-aALL  
storcli -AdpBbuCmd -BbuLearn -aN|-a0,1,2|-aALL  
storcli -AdpBbuCmd -BbuMfgSleep -aN|-a0,1,2|-aALL  
storcli -AdpBbuCmd -BbuMfgSeal -aN|-a0,1,2|-aALL  
storcli -AdpBbuCmd -getBbumodes  -aN|-a0,1,2|-aALL  
storcli -AdpBbuCmd -SetBbuProperties -f <fileName> -aN|-a0,1,2|-aALL 
storcli -AdpBbuCmd -ScheduleLearn -Dsbl|-Info|[-STARTTIME DDD hh] -aN|-a0,1,2|-aALL 
storcli -AdpFacDefSet -aN 
storcli -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
storcli -AdpFwFlash -f filename [-ResetNow] [-NoSigChk] [-NoVerChk] [-FWTYPE n] -aN|-a0,1,2|-aALL  
storcli -AdpGetConnectorMode -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
storcli -AdpSetConnectorMode -Internal|-External|-Auto -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
storcli -PhyErrorCounters -aN|-a0,1,2|-aALL  
storcli -DirectPdMapping -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL  
storcli -PDCpyBk -Start -PhysDrv[E0:S0,E1:S1] -aN|-a0,1,2|-aALL 
storcli -PDCpyBk -Stop|-Suspend|-Resume|-ShowProg|-ProgDsply -PhysDrv[E0:S0] -aN|-a0,1,2|-aALL 
storcli -PDInstantSecureErase -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
storcli -CfgSpanAdd -rX -array0[E0:S1,E1:S1.....] array1[E0:S1,E1:S1.....] -szxxx -enblPI -aN|-a0,1,2|-aALL 
storcli -LDMakeSecure -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
storcli -Version -Cli|-Ctrl|-Driver|-Pd -aN|-a0,1,2|-aALL 
storcli -DestroySecurityKey | [-Force] -aN 
storcli -CreateSecurityKey -SecurityKey sssssssssss | [-Passphrase sssssssssss] |[-KeyID kkkkkkkkkkk] -aN 
storcli -CreateSecurityKey useEKMS -aN 
storcli -ChangeSecurityKey -OldSecurityKey sssssssssss | -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
storcli -ChangeSecurityKey -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
storcli -ChangeSecurityKey useEKMS -OldSecurityKey sssssssssss -aN
storcli -ChangeSecurityKey -useEKMS -aN
storcli -GetKeyID [-PhysDrv[E0:S0]] -aN 
storcli -SetKeyID -KeyID kkkkkkkkkkk -aN 
storcli -VerifySecurityKey -SecurityKey sssssssssss -aN 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
storcli -GetPreservedCacheList -aN|-a0,1,2|-aALL 
storcli -DiscardPreservedCache -Lx|-L0,1,2|-Lall -force -aN|-a0,1,2|-aALL 
storcli -Snapshot -Enbl -szXXX SnapshotRepositoryLD N [-AutoSnapshot] [-AutoDeleteOldestSnapshot] -Lx -aN|-a0,1,2|-aALL
storcli -Snapshot -Setprop {-AutoSnapshot -val} | {-AutoDeleteOldestSnapshot -val} -Lx -aN|-a0,1,2|-aALL
storcli -Snapshot -Dsbl -Lx -aN|-a0,1,2|-aALL
storcli -Snapshot -TakeSnapshot [-SnapshotName NameString] [-CreateView [-viewName NameString] [-RW|RO|Blocked] -szXXX] -Lx|-L0,1,2 -aN|-a0,1,2|-aALL
storcli -Snapshot -DeleteSnapshot -SnapshotTime yyyymmdd hh:mm:ss | -all [-Force|-Y] -Lx|L0,1,2 -aN|-a0,1,2|-aALL
storcli -Snapshot -CreateView -SnapshotTime yyyymmdd hh:mm:ss [-viewName NameString] [-RW|RO|Blocked] -szXXX -Lx -aN|-a0,1,2|-aALL
storcli -Snapshot -DeleteView [-SnapshotTime yyyymmdd hh:mm:ss] -Lx -aN|-a0,1,2|-aALL
storcli -Snapshot -Info [-SnapshotTime yyyymmdd hh:mm:ss | -ViewTime yyyymmdd hh:mm:ss] -Lx -aN|-a0,1,2|-aALL
storcli -Snapshot -Clean  -Lx -aN|-a0,1,2|-aALL
storcli -Snapshot -GetViewInfo [-ViewTargetId N ] -aN|-a0,1,2|-aALL
storcli -ShowSummary [-f filename] -aN
storcli -ELF -GetSafeId -aN|-a0,1,2|-aALL
storcli -ELF -ControllerFeatures -aN|-a0,1,2|-aALL
storcli -ELF -Applykey key <val> [Preview] -aN|-a0,1,2|-aALL
storcli -ELF -TransferToVault -aN|-a0,1,2|-aALL
storcli -ELF -DeactivateTrialKey -aN|-a0,1,2|-aALL
storcli -ELF -ReHostInfo -aN|-a0,1,2|-aALL
storcli -ELF -ReHostComplete -aN|-a0,1,2|-aALL
storcli -LDViewMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
storcli -LDJoinMirror -DataSrc <val>[-force] -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
storcli -SecureErase 
	Start[
		Simple|
		[Normal   [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]|
		[Thorough [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]]
	| Stop
	| ShowProg
	| ProgDsply 
	[-PhysDrv [E0:S0,E1:S1,...] | -Lx|-L0,1,2|-LALL] -aN|-a0,1,2|-aALL
storcli -Perfmon {-start -interval <val>} | {stop} | {-getresults -f <Filename>} -aN 
storcli -DpmStat -Dsply {lct | hist | ra | ext } [-physdrv[E0:S0]] -aN|-a0,1,2|-aALL  
storcli -DpmStat -Clear {lct | hist | ra | ext } -aN|-a0,1,2|-aALL  

    Note: The directly connected drives can be specified as [:S] 

    Wildcard '?' can be used to specify the enclosure ID for the drive in the 
      only enclosure without direct connected device or the direct connected 
      drives with no enclosure in the system.

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 


=============
Fixes/Updates
=============
v1.17.08 (MR6.9)
	SCGCQ00845688 - (Closed) - MR_6.8_storcli: Fails to get phyerrorcounters of the expander phys for the enclosures which are in daisy chain
	SCGCQ00853174 - (Closed) - Storcli writes "no CC errors were logged " instead of "no pd events" in a file, when fire a command pdfailevents.
	SCGCQ00857748 - (Closed) - On executing storcli cmd to dump alilog, it posts an error message and also doesnt list all the information
	SCGCQ00857760 - (Closed) - Alignment of logs in the log file for the controller info is not proper
	SCGCQ00863767 - (Closed) - Fixed all the resource leaks, Null pointer deferences and error handling issues.
	SCGCQ00865020 - (Closed) - The Design Info field is partially populated for CV in StorCLI Ver 1.17.01 as compared to the previous releases.
	SCGCQ00874043 - (Closed) - StorCLI returns confusing message when flashing incompatible FW image(16MB)
	SCGCQ00880288 - (Closed) - storcli command "/c0 show alilog" takes more than 2 mins.
	SCGCQ00880959 - (Closed) - Coverity defect fixes in Storcli 6.9
	SCGCQ00884900 - (Closed) - Coverity defects in 6.9 Storlci
	SCGCQ00894452 - (Closed) - Storcli displays wrong message while deleting a CCVD
	SCGCQ00894601 - (Closed) - StorCLI : output string needs to be change for largeIO support command
	SCGCQ00845602 - (Closed) - Alpha 6.8: Storcli command ./storcli /cx/fall show not displaying proper error message for non importable VD.
	SCGCQ00859728 - (Closed) - Need to change the message if identified an OS or file system on VD
	SCGCQ00867587 - (Closed) - Check for OS on any Jbod while disabling JBOD on the controller
	SCGCQ00914834 - (Closed) - Updating storcli as per the API changes for LargeIOSupport
	SCGCQ00860801 - (Closed) - Coverity defects for 6.9
	SCGCQ00863669 - (Closed) - Coverity fixes in MR6.9
	SCGCQ00865464 - (Closed) - Incorrect error message displays BBU instead of CV
	SCGCQ00874608 - (Resolved) - misspelled word in storcli message
	SCGCQ00893958 - (Resolved) - MR_Intruder: Incomplete help file provided for the command storcli /cx set autopdcache=<off|[on|sscr0]|r0|wbr0> [immediate]
	SCGCQ00865804 - (Closed) - PERCCLI shows storccli during help command
	SCGCQ00865971 - (Closed) - StorCLI saves a degraded config but does not restore it.
	SCGCQ00873650 - (Closed) - Dereferencing the null pointer
	SCGCQ00855390 - (Closed) - Adding NULL Check to avoid referencing a NULL
	SCGCQ00860822 - (Closed) - If connector index is 0xFF display connector name as "Internal"
	SCGCQ00864791 - (Closed) - Coverity defects(Adding NULL Checks and Error messages in failure cases)
	SCGCQ00853185 - (Closed) - Storcli fails to dump lastoneday pdfailevents in a file.
	SCGCQ00855389 - (Closed) - Remove unused variables in flash Cp.
	SCGCQ00877894 - (Closed) - Disable SSD caching fails from Storcli in OEL 7.
	SCGCQ00873620 - (Closed) - StorCLI does not find enclosures in multipath environment
	SCGCQ00851795 - (Implemented) - Implemented commands to save/restore the configuration on the controller.
	SCGCQ00867424 - (Implemented) - Incorrect message displayed when performing Auto configuration raid 0 with SSD drives.
	SCGCQ00828030 - (Implemented) - Add support to detect that an OS is installed on a JBOD and to block it from being changed to Unconfigured Good
	SCGCQ00894103 - (Closed) - StorCLI : Add support to enable/Disable of Large IO Support - 1 MB IO
	SCGCQ00854620 - (Implemented) - Provide a more descriptive port enumeration
	SCGCQ00833594 - (Closed) - added new command /c0 show swalilog equivalent to adpalilog
	SCGCQ00850619 - (Closed) - Added support for flashing the FW on intruder and new Dev-ID's of Invader are added f
	SCGCQ00853554 - (Port_Complete) - OEM requesting to do a WRITE VERIFY prior to flushing cache.
	SCGCQ00864789 - (Port_Complete) - Spelling mistake in storcli output command pdfaileventoption

v1.16.06 (MR6.8)
	SCGCQ00355536 - (Closed) - MegaCli and StorCli can not manage both Liberator (and prior) and TB controllers in the same system under FreeBSD with the mf
	SCGCQ00357948 - (Closed) - StorCLI does not display drive information behind the Blackjack (Alta) interposer correctly
	SCGCQ00359629 - (Closed) - In paged view the text " Press Enter to continue" should be changed to " Press any key to Continue"
	SCGCQ00359998 - (Closed) - Code clean up in libmods and sysefi files are added
	SCGCQ00360814 - (Closed) - StorCLI: Not able to set pr property includessds as onlymixed on Liberator cacheoffload controller
	SCGCQ00362216 - (Closed) - iMr_Fury_StorCli:4K Drive size shown wrong in Esxi4.1U3
	SCGCQ00362717 - (Closed) - storcli /c0/d0 show " in that legend missing for "Dgrd/pdgd/Onln/ofLn/Rbld"
	SCGCQ00363455 - (Closed) - The legend for the PD List table exceeds 80 char limit.
	SCGCQ00363522 - (Closed) - storcli query for displaying controller properties is showing status , as failure.
	SCGCQ00364248 - (Closed) - StorCLI failed to delete a VD that is just created under Windows 2008
	SCGCQ00364622 - (Closed) - Reports wrong diskgroup size while querying controller level properties
	SCGCQ00364735 - (Closed) - UEFI, the O/P of <storcli /c0 show all>"Current Controller Date/Time" & "Current System Date/time" are not in proper format
	SCGCQ00371445 - (Closed) - Vmware CLI fails to set the phy linkspeed
	SCGCQ00378828 - (Closed) - StorCLI-Legacy:'adpbootdrive get' fails to get bootdrive information.
	SCGCQ00381100 - (Closed) - MR: not able to create PRL11 using 96 drives.
	SCGCQ00408070 - (Closed) - StorCLI does not show both "Current Write Policy" and "Default Write Policy" for VD
	SCGCQ00413789 - (Closed) - storcli crashes on having a non PI drive and trying to create pi vd on all the drive
	SCGCQ00438350 - (Closed) - Megacli crashes after invoking any command in SGI system with one 9280-8e and 2 quad port qlogic FC cards.
	SCGCQ00475583 - (Closed) - Raptor_Galaxy_Tencent:Tencent Storcli detecting the card.
	SCGCQ00479843 - (Closed) - Storcli internal errors should return with 1001, but its coming as -1
	SCGCQ00481474 - (Closed) - Some Numeric values in CLI o/p comes in Hex format
	SCGCQ00484560 - (Closed) - Try to create a Exclusive VD, but after creation it still shows as Shared VD.
	SCGCQ00505771 - (Closed) - Wrong size of CacheCade VD is getting displayed after making one PD offline
	SCGCQ00518543 - (Closed) - PCLI Sparc(1.07.02):" Cli show all" command fails with error msg "Error! App exec failed in FW PCLIError! Internal".
	SCGCQ00568073 - (Closed) - Storclio_1.09.00:Fails to set SubOEMID on Solaris OS .
	SCGCQ00574835 - (Closed) - MR_Inv_6.3_PPC:Storcli- Retreiving LDBBM info through storcli is failing on SLES11 SP2 PPC64
	SCGCQ00579658 - (Closed) - PPC64 :: MR Liberator :: All commands of StorCli is failing with segmentation fault after creating a GlobalHotSpare
	SCGCQ00644123 - (Closed) - "/cx/ex show phyerrorcounters" gives core dump on freeBSD 32 and 64 bit.
	SCGCQ00653742 - (Closed) - Storlib header file checkin and make compatible changes in CLI code.
	SCGCQ00690355 - (Closed) - Storcli shows two controllers in the system though you have only one cotntroller in the system.
	SCGCQ00712982 - (Closed) - Verify StorCLI warns on destructive operations - R0 with 2 x SED drives Deleted with no warning.
	SCGCQ00716584 - (Closed) - /c0 show all page are having some incorrectness in controller information
	SCGCQ00725192 - (Closed) - H330: Firmware Crash is hit while creating the Raid1 vd without drives selected
	SCGCQ00730505 - (Closed) - After Rebuilding, DHS and Expand VD operations failed to update as per VD properties
	SCGCQ00756647 - (Closed) - 6.6_StorCli: StorCli lists all cascaded enclosures at position 0.
	SCGCQ00758770 - (Closed) - FW breaks in iMR when excluding VD's from CC
	SCGCQ00759183 - (Closed) - SED adapterOperation detailed is not shown in detailed show controller properties
	SCGCQ00759187 - (Closed) - Boot Volume details is shown in Megacli but not with storcli.
	SCGCQ00759969 - (Closed) - Adapters are not listed in sorted order.
	SCGCQ00760752 - (Closed) - /c0 show all does not list hwCfg information as compared to MegaCLI.
	SCGCQ00762663 - (Closed) - Storclio : Different error code is coming for 'set pcilinkspeed' in VMware 4.1U3
	SCGCQ00765712 - (Closed) - StorCLI is not updated with the error Message for all new MFI_STAT added in mfistat.h
	SCGCQ00765759 - (Closed) - StorCLI shows wrong "Number of blocks" for a 65.5TB VD size
	SCGCQ00765762 - (Closed) - StorCLI VMware Binary not displaying detailed description for phyerrorcounters of enclosures
	SCGCQ00772243 - (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a VD which is associated with a CacheCade VD
	SCGCQ00779789 - (Closed) - Active operation(s) is coming as none when virtual drive erase is in progress.
	SCGCQ00779806 - (Closed) - ASO count mismatch in show ASO w.r.t ASO in storcli show all cmd
	SCGCQ00782882 - (Closed) - MR6.6:StorCLI shows incorrect information about "Cache Vault Flash Size"
	SCGCQ00784808 - (Closed) - "cpybck" help is not coming in Legends
	SCGCQ00792202 - (Closed) - Readability : Output string need to be updated for supportForceTo512e in show all command
	SCGCQ00792232 - (Closed) - MFCdefaults : DisableHII option needs to be include in getShowDefaults()
	SCGCQ00793374 - (Closed) - Comparing an array to null is not useful: "rawSmartData != NULL"
	SCGCQ00794394 - (Closed) - MR_6.7_STROCLI: Command "./storcli64 /c0/ex/sx reset phyerrorcounters" fails in RHEL6.6 PPC64
	SCGCQ00802031 - (Closed) - Deallocation of the same memory more than 
	SCGCQ00804554 - (Closed) - emory not freed which can cause leak
	SCGCQ00804588 - (Closed) - Memory leak happening in failure case since not freeing before returning error code.
	SCGCQ00818653 - (Closed) - Copyright value still shows 2014
	SCGCQ00827049 - (Closed) - Storcli cannot create R10 in iMR with 6 or 8 drives per span.
	SCGCQ00827299 - (Closed) - Storcli crashes instead of showing error message on enabling caching on Source VDs and C
	SCGCQ00833223 - (Closed) - Not displaying the timePeriod for event MR_EVT_PD_DEGRADED_MEDIA_POOR_PERFORMANCE
	SCGCQ00833224 - (Closed) - setting vfmap with PF/wrong VF is throwing error
	SCGCQ00839797 - (Closed) - Segmentation Fault observed, when trying to create R1 CCVD using 3/5 drives
	SCGCQ00840948 - (Closed) - Storcli throws syntax error,when setting errorThreshold.
	SCGCQ00853174 - (Closed) - Storcli writes "no CC errors were logged " instead of "no pd events" in a file, when fire a command pdfailevents.
	SCGCQ00360040 - (Closed) - Storcli is returning error with show
	SCGCQ00362070 - (Closed) - iMr_Fury_StorCLi:SectorSize show as "512KB" for 512Bytes drives
	SCGCQ00362421 - (Closed) - StorCLI: Not able to detect Liberator Controller on FreeBSD 9.0(64-bit)
	SCGCQ00364097 - (Closed) - iMR_Inv_6.1:StoreCLI- StoreCLI reports wrong Emulation type for VDs
	SCGCQ00365632 - (Closed) - PCI Info for FreeBSD needs to be indicated as "N/A"
	SCGCQ00372155 - (Closed) - Certain controller features displayed under "show all" exceeds 80-char limit.
	SCGCQ00374735 - (Closed) - StorCLI crashed when run on a Windows 2008 64-bit with 24GB of RAM and 66 drives attached
	SCGCQ00374979 - (Closed) - Storcli ld info command displays R10 vd Span Depth to 1.
	SCGCQ00378135 - (Closed) - portings of AdpRestart command
	SCGCQ00379104 - (Closed) - Not able to get paged view of StorCLI output on VM-Ware Platform
	SCGCQ00396665 - (Closed) - StorcLi_5.7: Remove the description for "Ra=Read Ahead Adaptive" in VD show info.
	SCGCQ00424978 - (Closed) - MR6.1: Hamlin: Is VD Emulated=Yes when emulationType=1
	SCGCQ00442610 - (Closed) - Onfi_patch_6.0:Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
	SCGCQ00442652 - (Closed) - SWR_1.34 - Serial number field is blank in controller information and the same could be updated with N/A in StorCli
	SCGCQ00490620 - (Closed) - Unable to insert a drive after setting a drive as 'Missing' .
	SCGCQ00503981 - (Closed) - Command "./Storcli /call/eall/sx set offline" fails with ERRcode1001 and ERRmsg drive not found.
	SCGCQ00504585 - (Closed) - Some sparc structures missing for storcli.
	SCGCQ00567761 - (Closed) - MR Liberator : PPC SERVERGY Server : MonTask: line 541 in file ../../raid/raidpci.c
	SCGCQ00644545 - (Closed) - storecli reports wrong size on 3000MB VD
	SCGCQ00649324 - (Closed) - MR6.4_StorCLI_240VD: StorCLI crashes on issuing /c1 set cc=conc delay=10 starttime=2014/12/12 12 excludevd=0
	SCGCQ00649962 - (Closed) - Cannot create a VD smaller than 800MB with 4K drives
	SCGCQ00653672 - (Closed) - MR6.4: Storcli show command does not display all the controllers plugged into the server
	SCGCQ00757358 - (Closed) - Add adapterOperation support details in /c0 show all for cachebypassMode.
	SCGCQ00758101 - (Closed) - MR_6.6_Storcli: Storcli reports supercap state 'unknown' while learn is happening on the controller.
	SCGCQ00758924 - (Closed) - Exception with command /co show badblocks or "storcli /cx flasherase"
	SCGCQ00759178 - (Closed) - SupportMaxRate SATA is not listed in PD allowed operations.
	SCGCQ00759181 - (Closed) - Add adapterOperation support details in /c0 show all for Emulationtype.
	SCGCQ00759862 - (Closed) - OEMID is coming as "Unknown" for /c0 show all
	SCGCQ00759959 - (Closed) - Support details are not shown in /c0 show all for discard cache (stalling LD deletion)
	SCGCQ00760385 - (Closed) - MR_6.6: StorCLI showing incorrect value for next Schedule time for consistency check after disabling the CC
	SCGCQ00760398 - (Closed) - MR6.6: Segmentation fault (Core Dumped) in CLI when setting any invalid value for PR start time
	SCGCQ00761937 - (Closed) - MR 6.6 Prealpha2 Storcli:Similar PCI address(BDF number) is displayed for multiple controllers connected to FreeBSD 9.3.
	SCGCQ00764658 - (Closed) - StorCLI /c0 show all command does not reflect the discard vd delete filed
	SCGCQ00765714 - (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a CacheCade VD
	SCGCQ00767363 - (Closed) - Showing wrong creation date for Autoconfigured virtual drives
	SCGCQ00771626 - (Closed) - Storcli errors are printing in a different line.
	SCGCQ00772302 - (Closed) - Storcli has option to set PR maxconcurrentpd but show is not present
	SCGCQ00772332 - (Closed) - vpdpage should be read from 4 bytes to get serial number of drive
	SCGCQ00778577 - (Closed) - GB scale to be added while showing CacheCade size in CLI
	SCGCQ00779800 - (Closed) - MR6.6_CLI_FreeBSD: Displaying incorrect Driver name
	SCGCQ00783357 - (Closed) - CTRL-R:2 iMR Card in same System hitting Montask
	SCGCQ00785918 - (Closed) - Reviewing the Code AdataMfi, RmDataMf and VdDataMf files.
	SCGCQ00792200 - (Closed) - supportCPLDUpdate support bit needs to be updated in contoller detailed information
	SCGCQ00793761 - (Closed) - The HDD firmware revision is shown blank for few drives connected.
	SCGCQ00794393 - (Closed) - MR_6.7_STROCLI: "./storcli64 /c0/ex show phyerrorcounters" gives segmentation fault in RHEL6.6 PPC64
	SCGCQ00795335 - (Closed) - Explicit null dereferenced in rmdatamf.cpp causing wrong result
	SCGCQ00796206 - (Closed) - fisResBuffer memory allocation is not considering the failure case
	SCGCQ00803420 - (Closed) - Storcli displays wrong native driver version on ESXi5.5 when quered .
	SCGCQ00804745 - (Closed) - Resource leak - Leak of memory or pointers to system resources
	SCGCQ00805547 - (Closed) - MR_6.7_ Storcli: "Storcli /cx/eall/sall show " gives no enclosure found if two enclosures are connected in multipath scenario
	SCGCQ00806966 - (Resolved) - IDA show incorrect RAID controller type information
	SCGCQ00814939 - (Closed) - MR_6.7: Storcli Command "./storcli /c0/v2 set accesspolicy=RmvBlkd " fails for a blocked source VD.
	SCGCQ00819880 - (Closed) - Gas Gauge Update + StorCLI ResetNow Op
	SCGCQ00837197 - (Closed) - MR_6.8_Storcli: Cachevault flash size shows differently for different commands in storcli under RHEL6.6 PPC64
	SCGCQ00837339 - (Closed) - "/c0/cv show all" shows "CacheVault Flash Size" as 0KB for TB.
	SCGCQ00837342 - (Closed) - New PD_Degraded media events are not logging correctly in PPC
	SCGCQ00840408 - (Closed) - Storcli gives wrong message for '/c1 /eall show phyerrorcounters' on IMR controller with no enclosures
	SCGCQ00357263 - (Closed) - MegaCLI adpgetpciinfo returns a static Bus Number value "17d0"
	SCGCQ00366000 - (Closed) - Storcli displays incomplete serial number for some SSDs
	SCGCQ00377364 - (Closed) - StorCli shows Power Saving Option as enabled, despite IBM Flatwood controller having power saving option completely disabled.
	SCGCQ00383043 - (Closed) - StorCLI-Invader : The "coercion" mode is not in sync with the legacy values.
	SCGCQ00454971 - (Closed) - storcli /c0 show is not listinf SWR controller
	SCGCQ00475562 - (Resolved) Storcli - DFF firmware download fails with config ID mismatch on ESXi5.1
	SCGCQ00475815 - (Closed) - debug prints are present when issuing /co/eall show
	SCGCQ00499067 - (Closed) - Storcli reports VD Type as "Rec1" during reconstruction on SPARC.
	SCGCQ00518579 - (Closed) - Unable to make R10 through Ctrl R using 4k drives
	SCGCQ00529763 - (Closed) - Some characters missing while querying for VD properties with having 64 VD's on a controller.
	SCGCQ00572800 - (Closed) - MR_Inv_6.3_PPC:Storcli-WWN is showing blank for SAS PDs on SLES11 SP2 PPC64
	SCGCQ00581416 - (Closed) - PPC64 :: MR Liberator :: ./storcli64 /c0 show dequeuelog file command failing with segmentation fault
	SCGCQ00601775 - (Closed) - MR : on querying PR status, storcli hits segmentation fault.
	SCGCQ00609942 - (Closed) - storelib header file changes porting
	SCGCQ00645195 - (Closed) - Storcli : unable to set patrol read delay
	SCGCQ00674023 - (Closed) - MR_6.4_StorCli_EFI: Storcli.efi crashes for iMR card.
	SCGCQ00674969 - (Closed) - Storcli doesn't show SN of Samsung SSD 200/400/800 in SWRAID version 1.32
	SCGCQ00695070 - (Closed) - storcli /c0 show all is not displaying "support vd hide" and "support HOQrebuild" feilds and legends are not displayed for HD
	SCGCQ00729691 - (Closed) - MR6.5alpha:Segmentation fault(coredump) observed on executing ./storcli /c1/v63 show all for 64th cachecade VD in ubuntu14.04
	SCGCQ00752000 - (Closed) - In Windows and Linux only controller grouping is working but not sorting
	SCGCQ00755063 - (Closed) - Add support bits for uneven-span and SSHA support
	SCGCQ00759290 - (Closed) - SSM-FLASh drives property is displayed for regular drives.
	SCGCQ00767347 - (Closed) - Patrol read delay is showing wrong value when set to continuous
	SCGCQ00785400 - (Closed) - VD level hide/unhide is not possible through storcli in PPC
	SCGCQ00792264 - (Closed) - Missing the Display of the property temperatureCtrl.
	SCGCQ00794760 - (Closed) - When Supercap SOH is reported bad, CLI still see the Supercap status as "Optimal"
	SCGCQ00799426 - (Closed) - Command /cx/ex show phyerrorcounters gives bus error in Orcale Enterprise Linux
	SCGCQ00804650 - (Closed) - Varailble need to be freed before returning in all failure case
	SCGCQ00809736 - (Closed) - FW hangs during SVD and CCVD migration based on DDR Size
	SCGCQ00830544 - (Closed) - Adpalilog is failing with storcli
	SCGCQ00838307 - (Closed) - Maintainer name being populated while querying for storcli version from OS
	SCGCQ00840372 - (Closed) - Read policy should be 'NORA' for IMR controller instead of 'none'
	SCGCQ00842237 - (Closed) - storcli exits with legacy syntax for pdfwdownload
	SCGCQ00357913 - (Closed) - Update VD emulation feature in StorCLI Libmods module to sync with latest APIs.
	SCGCQ00360745 - (Closed) - StorCLI does not provide command to set HSM or HCOE SCGCQ00358662
	SCGCQ00364332 - (Closed) - iMR_Inv_6.1:StoreCLI-StoreCLI does not give proper message while trying to create 33rd VD on iMR FURY controller
	SCGCQ00365950 - (Closed) - StorCLI cannot displays information for controller in Safe mode
	SCGCQ00374336 - (Closed) - System halts on issuing storcli commands in EFI Environment.
	SCGCQ00384644 - (Closed) - iMR_Inv_6.1:StorCLI- StorCLI does not show 'Unsupported/Blocked' state for 4K drives even though FW is not supporting 4K
	SCGCQ00396303 - (Resolved) - Cfgclr command fails without force option in Sparc OS
	SCGCQ00397663 - (Closed) - StorCli_MR: While creating VD using default values FW allows read policy as"Ra=Read Ahead Adaptive" as against PR-317400
	SCGCQ00465956 - (Closed) - No of blocks displayed for a VD remains same for all VD sizes.
	SCGCQ00467502 - (Closed) - State of the Shielded Drive is not displayed using storcli command
	SCGCQ00569935 - (Closed) - PPC64 :: MR Liberator :: Storcli Version 1.09.01 is showing wrong Creation Date and Time in VD properties
	SCGCQ00574287 - (Closed) - MR_Inv_6.3_PPC:Storcli- Storcli gives 'Segmentation fault' while retriving 'advanced software options' on SLES11 SP2 PPC64
	SCGCQ00627672 - (Closed) - MR6.4_StorCLI: c0 show controller health is failing
	SCGCQ00674131 - (Closed) - StorCLIO_1.09.09 : Not able to set subOEMid in Rhel 5.10 x64 bit.
	SCGCQ00712171 - (Closed) - While creating cachecade vd with one SAS-SSD;Raid 1 option is also enabled
	SCGCQ00787705 - (Closed) - CPLD - userCodeDefinition should be shown as part of /c0 show all command
	SCGCQ00792233 - (Closed) - CPLD UPDATE : cpld upgradableCPLD support bit need to add under hardware configuration
	SCGCQ00796227 - (Closed) - rlListPtr is not handled properly in failure case
	SCGCQ00804680 - (Closed) - Out-of-bounds access and array delete misuse
	SCGCQ00819603 - (Closed) - With command "/c0 start diag" duration should be an optional param.
	SCGCQ00820392 - (Closed) - Segmentation fault while querying for GHSP/DHSP while drive is going in shield-HSP state.
	SCGCQ00827192 - (Closed) - PD fail events are not logging into the file properly in EFI environment
	SCGCQ00830435 - (Closed) - LDViewMirror is giving segmentation fault
	SCGCQ00839321 - (Closed) - Storcli gives wrong error code with respect to FW state while converting JBOD to UG
	SCGCQ00423832 - (Closed) - EFI_ Storcli: Cannot set vpd file on controller, EFI hangs and cannot proceed for further operations until reboot
	SCGCQ00448094 - (Closed) - core dump while issuing storcli command ./storcli /c0/fall show 
	SCGCQ00471116 - (Closed) - Pcli: Pcli crashes while try to set securitykey for controller.
	SCGCQ00493491 - (Closed) - Storcli /c0 show ASO fails and delay in displaying
	SCGCQ00521999 - (Closed) - CSET: storelib header file checkin for the latest changes done by storelib - (SCGCQ00521999)
	SCGCQ00523370 - (Closed) - StorCLI reports controller status as 'OK' when Arctrus controller(9361-8i) booted in safe mode
	SCGCQ00792211 - (Closed) - supportDrvActivityLEDSetting supported bit need to be update in Supported adapater Operations
	SCGCQ00793354 - (Closed) - Incorrect sizeof expression in dcmdprm
	SCGCQ00804663 - (Closed) - Variable going out of scope without freeing which causes memory leak
	SCGCQ00813314 - (Closed) - Not able add new VD in Drive Group
	SCGCQ00830269 - (Closed) - storcli /call show all fails with "command invalid"
	SCGCQ00835758 - (Closed) - Storcli shows caching is enabled on Source VD when CCVD is in offline state
	SCGCQ00348911 - (Closed) - Adapter 0: Failed to start SecureErase on Virtual Drive 0 in VMware_ESXi_5.1
	SCGCQ00394883 - (Closed) - StorCli_MR: While Creating RAID1 with four drives command facing the "C0:BAIL_OUT at line 1354" on Flatwood Board
	SCGCQ00436107 - (Closed) - The bootwithpinnedcache logic is backwards, both storcli and the FW are affected
	SCGCQ00518201 - (Closed) - MR6.2 : Storcli shows incorrect "Bus" information when "/c0 show all" is run
	SCGCQ00564008 - (Closed) - StorCli: Segmantation fault appearing in storcli when issuing /c0/fall show
	SCGCQ00622605 - (Closed) - CS2.0: Ctrl-R Domain Id is not showing in controller properties
	SCGCQ00789402 - (Closed) - Remove the code related to enableVCor feild this was used for ASD and now it is not used any more.
	SCGCQ00792205 - (Closed) - supportForceFlash needs to add under suported adapter operations
	SCGCQ00795334 - (Closed) - Operands don't affect result in pddatamf.cpp causing wrong result
	SCGCQ00811117 - (Closed) - LibMod changes for CTLR+R to read Disk Write Cache settings of PD.
	SCGCQ00477037 - (Closed) - CLI reporting Large VD (56TB) size slightly smaller than other apps (by .001)
	SCGCQ00603174 - (Closed) - /c0 set cc=conc command fails with iMR card.
	SCGCQ00795342 - (Closed) - Unchecked return value in rmdatamf.cpp (getControllerStatus)
	SCGCQ00801311 - (Closed) - MR_6.7_Storcli: Storcli reports wrong tmm and scap date of manufacture under scap properties in RHEL6.6 PPC64
	SCGCQ00853185 - (Closed) - Storcli fails to dump lastoneday pdfailevents in a file.
	SCGCQ00792085 - (Closed) - StorCLI :supportDisableImmediateIO adapter properties need to be added under show all command
	SCGCQ00792234 - (Closed) - Firmware error code status MFI_STAT_SECURE_SYSTEM_PD_EXISTS needs to be update in code
	SCGCQ00793361 - (Closed) - Non-array delete for objects in rmdatamf
	SCGCQ00793363 - (Closed) - Resource leak in VdDataMf scanPartitions
	SCGCQ00795336 - (Closed) - Explicit null dereferenced in vddatamf.cpp (getVdDetldInfo)
	SCGCQ00804672 - (Resolved) - Non-array delete for objects: destructors will not be called for objects in the array leading to unexpected beh
	SCGCQ00351234 - (Implemented) - Provide a way to enable or disable 512E using Applicaions
	SCGCQ00632240 - (Implemented) - SED/FDE changes for storcli Synchro
	SCGCQ00685007 - (Closed) - Added the library functions for the new MR API bits and LD operations.
	SCGCQ00685010 - (Closed) - Added the library functions for the new MR API bits and LD operations.
	SCGCQ00696872 - (Closed) - Consistent Sorting of Controllers for End Users in Customer Facing Tools
	SCGCQ00735171 - (Closed) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
	SCGCQ00818101 - (Implemented) - Add set "Fail PD on SMARTer" property feature to StorCLI
	SCGCQ00829204 - (Implemented) - LibMods: Increase maximum cache size for Cachecade to 2048GB. This will be named CC 2.5
	SCGCQ00525321 - (Closed) - Implemented the diag results to print on console
	SCGCQ00564477 - (Implemented) - Display the NCQ enabled/disabled status of every SATA disk drive in the output of StorCLI and MegaCLI
	SCGCQ00642230 - (Closed) - Allow VMWARE version of STORCLI cannot be run from any directory
	SCGCQ00726019 - (Implemented) - Add set "Fail PD on SMARTer" property feature to StorCLI
	SCGCQ00755527 - (Closed) - Enable SED on JBOD
	SCGCQ00350668 - (Implemented) - Create Spanned R0 array (00) in StorCLI
	SCGCQ00369742 - (Implemented) - MWCLI. R10, R50, R60, R00 VD creation
	SCGCQ00558815 - (Closed) - MR 4.12: Big endian architecture support for MR Linux driver and StorCli
	SCGCQ00787923 - (Implemented) - OEL Support for SPARC
	SCGCQ00352120 - (Implemented) - MWCLI. Add HA support into storcli
	SCGCQ00564474 - (Implemented) - Request RAID CLI to display the Patrol Read Start Time
	SCGCQ00621287 - (Closed) - STORCLI will support MR controller management without UEFI BootServiceDriver Driver and also has retain functionality of existing see- adapter-through-driver functionality.
	SCGCQ00750164 - (Closed) - RRB 71 - enable SED support for iMR JBOB
	SCGCQ00757473 - (Closed) - LD Deletion stalling all IOs on 12.12.0-0178
	SCGCQ00818987 - (Closed) - LimMod changes related to CtrlH & MSM Mismatch on write-back options - UI Inconsistancy issue
	SCGCQ00828476 - (Closed) - Storcli Should display SAS Address N/A if its invalid and change Host interface type names from PCIX, PCIE to PCI-X, PCI-E
	SCGCQ00333209 - (Closed) - Implemented 128 drive support by using the new ENCL_INFO structures
	SCGCQ00349548 - (Closed) - Uneven span support is added in StorCLI.
	SCGCQ00349599 - (Implemented) - Refer attached design doc
	SCGCQ00433703 - (Implemented) - Megacli/storcli support for lmrc driver
	SCGCQ00467863 - (Implemented) - ASD- StorCLI - Libmod changes to support PD caching.
	SCGCQ00632051 - (Closed) - Added the OEM-NEC check for getting default disk-cache policy in Libmods as Disable.
	SCGCQ00827663 - (Closed) - Implemented the VD-VF mapping related commands in factory tool
	SCGCQ00827665 - (Closed) - Implemented the VD-VF mapping related commands in factory tool
	SCGCQ00381093 - (Implemented) - PR SCGCQ00319011: Rebuild time res
	SCGCQ00665081 - (Closed) - If any error that is returned as negative we return it s 0xFF from CLI to shell else FW returned error status will be returned to shell.
	SCGCQ00693042 - (Implemented) - Complete 240VD support for utilities
	SCGCQ00794841 - (Closed) - Functionality to extract field value from new API changes
	SCGCQ00795150 - (Opened) - UDK Support for EFI
	SCGCQ00816344 - (Implemented) - Utilities/Applications should not assume that expanders are enclosures as this is not always the case.
	SCGCQ00817977 - (Closed) - Monitoring Drive performance and predictive failure
	SCGCQ00817980 - (Closed) - Storcli: Monitoring Drive performance and predictive failure
	SCGCQ00342399 - (Implemented) - CSET: (Tbolt PR 211180) Punctured Block Logging Improvements
	SCGCQ00381311 - (Implemented) - dcmd path chagnes for supporting the new cachevault a

v1.15.05 (MR6.7)
	SCGCQ00808112 - (Closed) - PDFwDownload with legacy syntax fails
	SCGCQ00806973 - (Closed) - Not able to create VD using cfgcachecade add legacy syntax
	SCGCQ00806493 - (Closed) - MR6.7:StorCLI throws error message as "Older Ver Image", when trying to Flash 4MB file from MR 6.7 Pack6 to Pack7
	SCGCQ00804568 - (Closed) - Resource Leak : The system resource will not be reclaimed and reused, reducing the future availability of the resource
	SCGCQ00804302 - (Closed) - Resource leak: Variable going out of scope leaks the storage it points to.
	SCGCQ00803053 - (Closed) - storcli crashes on trying to flash the CPLD
	SCGCQ00799098 - (Closed) - Smartpollinterval range to be changed from '1 to 65535' to '0 to 65535'
	SCGCQ00797172 - (Closed) - Logically dead code in SwEvt.cpp
	SCGCQ00797168 - (Closed) - Non-array delete for scalars SnpShtCp.cpp
	SCGCQ00797143 - (Closed) - Resource Leak in LdRecn.cpp
	SCGCQ00797088 - (Closed) - Structurally dead code in foreigncp.cpp (process_show)
	SCGCQ00797085 - (Closed) - Explicit null dereferenced in ctcfpgcp.cpp (write_config_page)
	SCGCQ00796128 - (Closed) - Memory leak due to Pdlist pointer
	SCGCQ00795465 - (Closed) - Resource leak in cfgssccp.cpp(associateVDsToCachePool)
	SCGCQ00795437 - (Closed) - Dereference before null check pdremfp.cpp
	SCGCQ00795144 - (Closed) - Memory leak as UnCfgdVdOnFreeSpOnPd Class object is not freed
	SCGCQ00795130 - (Closed) - storcli /c0 set cc doesnot have option to include all VD's.
	SCGCQ00793707 - (Closed) - Set Supercap VPD information fails on PPC
	SCGCQ00793396 - (Closed) - Comparing an array to null is not useful: "NULL != fspHdrList"
	SCGCQ00793393 - (Closed) - Non-array delete for objects in trmlgcp.cpp
	SCGCQ00793378 - (Closed) - Non-array delete for objects cfgechcp.cpp in associateVDsToCachePool
	SCGCQ00793375 - (Closed) - Resource leak adpvpdcp.cpp in AdpSetVPD
	SCGCQ00793372 - (Closed) - Non-array delete for objects adhwrcp.cpp handleReadSuboption
	SCGCQ00790062 - (Closed) - "./storcli64 /c0 show cc" fails in RHEL 6.6 PPC64 with more than 64 VDs present
	SCGCQ00790032 - (Closed) - "./storcli64 /c0 show eghs" fails on RHEL 6.6 PPC64
	SCGCQ00789389 - (Closed) - autopdcache detailed help dose not have immediate option
	SCGCQ00782882 - (Closed) - MR6.6:StorCLI shows incorrect information about "Cache Vault Flash Size"
	SCGCQ00779806 - (Closed) - ASO count mismatch in show ASO w.r.t ASO in storcli show all cmd
	SCGCQ00779789 - (Closed) - Active operation(s) is coming as none when virtual drive erase is in progress.
	SCGCQ00772243 - (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a VD which is associated with a CacheCade VD
	SCGCQ00765762 - (Closed) - StorCLI VMware Binary not displaying detailed description for phyerrorcounters of enclosures
	SCGCQ00765759 - (Closed) - StorCLI shows wrong "Number of blocks" for a 65.5TB VD size
	SCGCQ00765712 - (Closed) - StorCLI is not updated with the error Message for all new MFI_STAT added in mfistat.h
	SCGCQ00762663 - (Closed) - Storclio : Different error code is coming for 'set pcilinkspeed' in VMware 4.1U3
	SCGCQ00760752 - (Closed) - /c0 show all does not list hwCfg information as compared to MegaCLI.
	SCGCQ00759969 - (Closed) - Adapters are not listed in sorted order.
	SCGCQ00759187 - (Closed) - Boot Volume details is shown in Megacli but not with storcli.
	SCGCQ00759183 - (Closed) - SED adapterOperation detailed is not shown in detailed show controller properties
	SCGCQ00758770 - (Closed) - FW breaks in iMR when excluding VD's from CC
	SCGCQ00756647 - (Closed) - 6.6_StorCli: StorCli lists all cascaded enclosures at position 0.
	SCGCQ00730505 - (Closed) - After Rebuilding, DHS and Expand VD operations failed to update as per VD properties
	SCGCQ00725192 - (Closed) - Firmware Crash is hit while creating the Raid1 vd without drives selected
	SCGCQ00716584 - (Closed) - /c0 show all page are having some incorrectness in controller information
	SCGCQ00712982 - (Closed) - Verify StorCLI warns on destructive operations - R0 with 2 x SED drives Deleted with no warning.
	SCGCQ00690355 - (Closed) - Storcli shows two controllers in the system though you have only one cotntroller in the system.
	SCGCQ00653742 - (Closed) - Storlib header file checkin and make compatible changes in CLI code.
	SCGCQ00644123 - (Closed) - "/cx/ex show phyerrorcounters" gives core dump on freeBSD 32 and 64 bit.
	SCGCQ00579658 - (Closed) - PPC64 :: MR Liberator :: All commands of StorCli is failing with segmentation fault after creating a GlobalHotSpare
	SCGCQ00574835 - (Closed) - MR_Inv_6.3_PPC:Storcli- Retreiving LDBBM info through storcli is failing on SLES11 SP2 PPC64
	SCGCQ00568073 - (Closed) - Storclio_1.09.00:Fails to set SubOEMID on Solaris OS .
	SCGCQ00518543 - (Closed) - PCLI Sparc(1.07.02):" Cli show all" command fails with error msg "Error! App exec failed in FW PCLIError! Internal".
	SCGCQ00505771 - (Closed) - Wrong size of CacheCade VD is getting displayed after making one PD offline
	SCGCQ00484560 - (Closed) - Try to create a Exclusive VD, but after creation it still shows as Shared VD.
	SCGCQ00481474 - (Closed) - Some Numeric values in CLI o/p comes in Hex format
	SCGCQ00479843 - (Closed) - Storcli internal errors should return with 1001, but its coming as -1
	SCGCQ00355536 - (Closed) - MegaCli and StorCli can not manage both Liberato(and prior) and TB controllers in the same system under FreeBSD with the mf
	SCGCQ00357948 - (Closed) - StorCLI does not display drive information behind the Blackjack (Alta) interposer correctly
	SCGCQ00359629 - (Closed) - In paged view the text " Press Enter to continue" should be changed to " Press any key to Continue"
	SCGCQ00359998 - (Closed) - Code clean up in libmods and sysefi files are added
	SCGCQ00360814 - (Closed) - StorCLI: Not able to set pr property includessds as onlymixed on Liberator cacheoffload controller
	SCGCQ00362216 - (Closed) - iMr_Fury_StorCli:4K Drive size shown wrong in Esxi4.1U3
	SCGCQ00362717 - (Closed) - storcli /c0/d0 show " in that legend missing for "Dgrd/pdgd/Onln/ofLn/Rbld"
	SCGCQ00363455 - (Closed) - The legend for the PD List table exceeds 80 char limit.
	SCGCQ00363522 - (Closed) - storcli query for displaying controller properties is showing status , as failure.
	SCGCQ00364248 - (Closed) - StorCLI failed to delete a VD that is just created under Windows 2008
	SCGCQ00364622 - (Closed) - Reports wrong diskgroup size while querying controller level properties
	SCGCQ00364735 - (Closed) - UEFI, the O/P of <storcli /c0 show all>"Current Controller Date/Time" & "Current System Date/time" are not in proper format
	SCGCQ00371445 - (Closed) - Vmware CLI fails to set the phy linkspeed
	SCGCQ00378828 - (Closed) - StorCLI-Legacy:'adpbootdrive get' fails to get bootdrive information.
	SCGCQ00381100 - (Closed) - MR: not able to create PRL11 using 96 drives.
	SCGCQ00408070 - (Closed) - StorCLI does not show both "Current Write Policy" and "Default Write Policy" for VD
	SCGCQ00413789 - (Closed) - storcli crashes on having a non PI drive and trying to create pi vd on all the drive
	SCGCQ00438350 - (Closed) - Megacli crashes after invoking any command in SGI system with one 9280-8e and 2 quad port qlogic FC cards.
	SCGCQ00475583 - (Closed) - Storcli detecting the controller
	SCGCQ00810266 - (Closed) - MR6.7-Misspellingof Minutes with storcli
	SCGCQ00808109 - (Closed) - storcli -DpmStat -dsply hist physdrv[252:2] a0 fails
	SCGCQ00804748 - (Closed) - Referring a pointer which was already freed.
	SCGCQ00804578 - (Closed) - Variable not freed after allocating memory
	SCGCQ00803754 - (Closed) - CCVD is creating with max array size where it has to be limited to 1TB
	SCGCQ00803404 - (Closed) - After flashing expander firmware storcli is not displaying expected message .
	SCGCQ00797137 - (Closed) - Dereference before null check in pdremfcp.cpp(validateExtractMaxLBAFromDriveCfgFile)
	SCGCQ00797136 - (Closed) - Logically dead code in pddffprovcp.cpp(SendSTPCmd)
	SCGCQ00797091 - (Closed) - Resource leak in ldaddcp.cpp(cfgOnNewArray)
	SCGCQ00797087 - (Closed) - Use after free in expandvdcp.cpp (process_show)
	SCGCQ00795892 - (Closed) - Memory leak as the pointer is not getting deleted when we return a failure.
	SCGCQ00795434 - (Closed) - Dereference before null check in pddffdiagp.cpp
	SCGCQ00795410 - (Closed) - No help provided for the command to uninstall storcli in ubuntu
	SCGCQ00795147 - (Closed) - pdlist pointer is not getting deleted in failure case
	SCGCQ00793729 - (Closed) - Some of the Design info parameters are missing for supercap
	SCGCQ00793385 - (Closed) - Resource leak in encinfcp.cpp (process)
	SCGCQ00793381 - (Closed) - Non-array delete for objects in deqlgcp.cpp (process)
	SCGCQ00793379 - (Closed) - Resource leak in cfgssccp.cpp
	SCGCQ00793373 - (Closed) - Array delete misuse - pdrmps.cpp
	SCGCQ00790043 - (Closed) - "./storcli64 /c0 flasherase " fails in RHEL 6.6 PPC64
	SCGCQ00789416 - (Closed) - StorCLI Code removal for removed ASD feilds in mr.h
	SCGCQ00783357 - (Closed) - CTRL-R:2 iMR Card in same System hitting Montask
	SCGCQ00779800 - (Closed) - MR6.6_CLI_FreeBSD: Displaying incorrect Driver name
	SCGCQ00778577 - (Closed) - GB scale to be added while showing CacheCade size in CLI
	SCGCQ00772332 - (Closed) - vpdpage should be read from 4 bytes to get serial number of drive
	SCGCQ00772302 - (Closed) - Storcli has option to set PR maxconcurrentpd but show is not present
	SCGCQ00771626 - (Closed) - Storcli errors are printing in a different line.
	SCGCQ00767363 - (Closed) - Showing wrong creation date for Autoconfigured virtual drives
	SCGCQ00765714 - (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a CacheCade VD
	SCGCQ00764658 - (Closed) - StorCLI /c0 show all command does not reflect the discard vd delete filed
	SCGCQ00761937 - (Closed) - MR 6.6 Prealpha2 Storcli:Similar PCI address(BDF number) is displayed for multiple controllers connected to FreeBSD 9.3.
	SCGCQ00760398 - (Closed) - MR6.6: Segmentation fault (Core Dumped) in CLI when setting any invalid value for PR start time
	SCGCQ00760385 - (Closed) - MR_6.6: StorCLI showing incorrect value for next Schedule time for consistency check after disabling the CC
	SCGCQ00759959 - (Closed) - Support details are not shown in /c0 show all for discard cache (stalling LD deletion)
	SCGCQ00759862 - (Closed) - OEMID is coming as "Unknown" for /c0 show all
	SCGCQ00759181 - (Closed) - Add adapterOperation support details in /c0 show all for Emulationtype.
	SCGCQ00759178 - (Closed) - SupportMaxRate SATA is not listed in PD allowed operations.
	SCGCQ00758924 - (Closed) - Exception with command /co show badblocks or "storcli /cx flasherase"
	SCGCQ00758101 - (Closed) - MR_6.6_Storcli: Storcli reports supercap state 'unknown' while learn is happening on the controller.
	SCGCQ00757358 - (Closed) - Add adapterOperation support details in /c0 show all for cachebypassMode.
	SCGCQ00649962 - (Closed) - Cannot create a VD smaller than 800MB with 4K drives
	SCGCQ00649324 - (Closed) - MR6.4_StorCLI_240VD: StorCLI crashes on issuing /c1 set cc=conc delay=10 starttime=2014/12/12 12 excludevd=0
	SCGCQ00644545 - (Closed) - storecli reports wrong size on 3000MB VD
	SCGCQ00567761 - (Closed) - MR Liberator : PPC SERVERGY Server : MonTask: line 541 in file ../../raid/raidpci.c
	SCGCQ00504585 - (Closed) - Some sparc structures missing for storcli.
	SCGCQ00503981 - (Closed) - Command "./Storcli /call/eall/sx set offline" fails with ERRcode1001 and ERRmsg drive not found.
	SCGCQ00490620 - (Closed) - Unable to insert a drive after setting a drive as 'Missing' .
	SCGCQ00360040 - (Closed) - Storcli is returning error with show
	SCGCQ00362070 - (Closed) - iMr_Fury_StorCLi:SectorSize show as "512KB" for 512Bytes drives
	SCGCQ00362421 - (Closed) - StorCLI: Not able to detect Liberator Controller on FreeBSD 9.0(64-bit?
	SCGCQ00364097 - (Closed) - iMR_Inv_6.1:StoreCLI- StoreCLI reports wrong Emulation type for VDs
	SCGCQ00365632 - (Closed) - PCI Info for FreeBSD needs to be indicated as "N/A"
	SCGCQ00372155 - (Closed) - Certain controller features displayed under "show all" exceeds 80-char limit.
	SCGCQ00374735 - (Closed) - StorCLI crashed when run on a Windows 2008 64-bit with 24GB of RAM and 66 drives attached
	SCGCQ00374979 - (Closed) - Storcli ld info command displays R10 vd Span Depth to 1.
	SCGCQ00378135 - (Closed) - portings of AdpRestart command
	SCGCQ00379104 - (Closed) - Not able to get paged view of StorCLI output on VM-Ware Platform
	SCGCQ00396665 - (Closed) - StorcLi_5.7: Remove the description for "Ra=Read Ahead Adaptive" in VD show info.
	SCGCQ00424978 - (Closed) - MR6.1 Is VD Emulated=Yes when emulationType=1
	SCGCQ00442610 - (Closed) - Onfi_patch_6.0:Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
	SCGCQ00442652 - (Closed) - SWR_1.34 - Serial number field is blank in controller information and the same could be updated with N/A in StorCli
	SCGCQ00653672 - (Closed) - MR6.4: Storcli show command does not display all the controllers plugged into the server
	SCGCQ00804712 - (Closed) - Resource leak - The system resource will not be reclaimed and reused.
	SCGCQ00804666 - (Closed) - Variable not freed after allocating memory
	SCGCQ00804583 - (Closed) - Resource leak in objects in Storcli: Constructor allocates memory but destructor does not free it.
	SCGCQ00800414 - (Closed) - Coverity 13595 Unchecked return value
	SCGCQ00800403 - (Closed) - Removing logically dead code performing actions that cannot occur
	SCGCQ00795463 - (Closed) - Operands don't affect result in addevscp.cpp (setHSP)
	SCGCQ00795439 - (Closed) - Dereference before null check in cfgsscdp.cpp
	SCGCQ00794039 - (Closed) - Explicit null dereferenced (FORWARD_NULL) assign_zero: Assigning: "drvListPtr" = 0.
	SCGCQ00793371 - (Closed) - Non-array delete for objects in adalogcp.cpp
	SCGCQ00790050 - (Closed) - "./storcli64 /c0 show all page" shows "cachevault flash size = 8.0 ZB
	SCGCQ00785400 - (Closed) - VD level hide/unhide is not possible through storcli in PPC
	SCGCQ00767347 - (Closed) - Patrol read delay is showing wrong value when set to continuous
	SCGCQ00759290 - (Closed) - SSM-FLASh drives property is displayed for regular drives.
	SCGCQ00755063 - (Closed) - Add support bits for uneven-span and SSHA support
	SCGCQ00752000 - (Closed) - In Windows and Linux only controller grouping is working but not sorting
	SCGCQ00729691 - (Closed) - MR6.5alpha:Segmentation fault(coredump) observed on executing ./storcli /c1/v63 show all for 64th cachecade VD in ubuntu14.04
	SCGCQ00695070 - (Closed) - storcli /c0 show all is not displaying "support vd hide" and "support HOQrebuild" feilds and legends are not displayed for HD
	SCGCQ00674969 - (Closed) - Storcli doesn't show SN of Samsung SSD 200/400/800 in SWRAID version 1.32
	SCGCQ00674023 - (Closed) - MR_6.4_StorCli_EFI: Storcli.efi crashes for iMR card.
	SCGCQ00645195 - (Closed) - Storcli : unable to set patrol read delay
	SCGCQ00609942 - (Closed) - storelib header file changes porting
	SCGCQ00601775 - (Closed) - MR : on querying PR status, storcli hits segmentation fault?
	SCGCQ00581416 - (Closed) - PPC64 :: MR Liberator :: ./storcli64 /c0 show dequeuelog file command failing with segmentation fault
	SCGCQ00572800 - (Closed) - MR_Inv_6.3_PPC:Storcli-WWN is showing blank for SAS PDs on SLES11 SP2 PPC64
	SCGCQ00529763 - (Closed) - Some characters missing while querying for VD properties with having 64 VD's on a controller.
	SCGCQ00518579 - (Closed) - Unable to make R10 through Ctrl R using 4k drives
	SCGCQ00499067 - (Closed) - Storcli reports VD Type as "Rec1" during reconstruction on SPARC.
	SCGCQ00475815 - (Closed) - debug prints are present when issuing /co/eall show
	SCGCQ00357263 - (Closed) - MegaCLI adpgetpciinfo returns a static Bus Number value "17d0"
	SCGCQ00366000 - (Closed) - Storcli displays incomplete serial number for some SSDs
	SCGCQ00377364 - (Closed) - StorCli shows Power Saving Option as enabled, despite IBM Flatwood controller having power saving option completely disabled.
	SCGCQ00383043 - (Closed) - StorCLI-Invader : The "coercion" mode is not in sync with the legacy values.
	SCGCQ00454971 - (Closed) - storcli /c0 show is not listinf SWR controller
	SCGCQ00475562 - (Resolved) - Storcli - DFF firmware download fails with config ID mismatch on ESXi5.1
	SCGCQ00807557 - (Closed) - Segmentation fault observed while trying to set JBOD as boot drive through legacy command in UBUNTU 14.10.
	SCGCQ00804768 - (Closed) - Mesgptr is not getting deleted.
	SCGCQ00804713 - (Closed) - LdTargetIdList is not getting freed in failure case
	SCGCQ00796126 - (Closed) - fixing memory leak in bbu class
	SCGCQ00793627 - (Closed) - Set autopdcache fails in PPC
	SCGCQ00793394 - (Closed) - Non-array delete for objects in ttylogcp.cpp
	SCGCQ00793386 - (Closed) - Non-array delete for objects in pdonlncp.cpp - (pdGetNissing)
	SCGCQ00787431 - (Closed) - Dimmerswitch settings different in ctrl+r and storcli
	SCGCQ00712171 - (Closed) - While creating cachecade vd with one SAS-SSD;Raid 1 option is also enabled
	SCGCQ00674131 - (Closed) - StorCLIO_1.09.09 : Not able to set subOEMid in Rhel 5.10 x64 bit.
	SCGCQ00627672 - (Closed) - MR6.4_StorCLI: c0 show controller health is failing
	SCGCQ00574287 - (Closed) - MR_Inv_6.3_PPC:Storcli- Storcli gives 'Segmentation fault' while retriving 'advanced software options' on SLES11 SP2 PPC64
	SCGCQ00569935 - (Closed) - PPC64 :: MR Liberator :: Storcli Version 1.09.01 is showing wrong Creation Date and Time in VD properties
	SCGCQ00357913 - (Closed) - Update VD emulation feature in StorCLI Libmods module to sync with latest APIs.
	SCGCQ00360745 - (Closed) - StorCLI does not provide command to set HSM or HCOE SCGCQ0035866
	SCGCQ00364332 - (Closed) - iMR_Inv_6.1:StoreCLI-StoreCLI does not give proper message while trying to create 33rd VD on iMR FURY controller
	SCGCQ00365950 - (Closed) - StorCLI cannot displays information for controller in Safe mode
	SCGCQ00374336 - (Closed) - System halts on issuing storcli commands in EFI Environment.
	SCGCQ00384644 - (Closed) - iMR_Inv_6.1:StorCLI- StorCLI does not show 'Unsupported/Blocked' state for 4K drives even though FW is not supporting 4K
	SCGCQ00396303 - (Resolved) - Cfgclr command fails without force option in Sparc OS
	SCGCQ00397663 - (Closed) - StorCli_MR: While creating VD using default values FW allows read policy as"Ra=Read Ahead Adaptive" as against PR-317400
	SCGCQ00465956 - (Closed) - No of blocks displayed for a VD remains same for all VD sizes.
	SCGCQ00467502 - (Closed) - State of the Shielded Drive is not displayed using storcli command
	SCGCQ00810638 - (Closed) - Added the condition to check the raid level and fail it if the drives given are lesser than the needed drives
	SCGCQ00797139 - (Closed) - Structurally dead code in prfmoncp.cpp(process)
	SCGCQ00797090 - (Closed) - Resource leak in ldaddcp.cpp(associateVDsToCachePool)
	SCGCQ00793360 - (Closed) - Unchecked return value in appverp.cpp
	SCGCQ00790022 - (Closed) - ./storcli64 /c0 show pr gives segmentation fault on PPC with more than 64 VDs
	SCGCQ00523370 - (Closed) - StorCLI reports controller status as 'OK' when Arctrus controller(9361-8i) booted in safe mode
	SCGCQ00521999 - (Closed) - CSET: storelib header file checkin for the latest changes done by storelib - (SCGCQ00521999)
	SCGCQ00493491 - (Closed) - Storcli /c0 show ASO fails and delay in displaying .
	SCGCQ00471116 - (Closed) - Pcli: Pcli crashes while try to set securitykey for controller.
	SCGCQ00423832 - (Closed) - EFI_ Storcli: Cannot set vpd file on controller, EFI hangs and cannot proceed for further operations until reboot
	SCGCQ00448094 - (Closed) - core dump while issuing storcli command ./storcli /c0/fall show all.
	SCGCQ00348911 - (Closed) - Adapter 0: Failed to start SecureErase on Virtual Drive 0 in VMware_ESXi_5.1
	SCGCQ00804725 - (Closed) - userPdListPtr is not handled properly in failure case
	SCGCQ00804682 - (Closed) - Resource Leak : This could cause an immediate crash or incorrect values might be read subsequently resulting in incorrect com
	SCGCQ00800228 - (Closed) - Out of bounds access which can cause memory corruptions
	SCGCQ00797165 - (Closed) - Non-array delete for scalars ShwSumCp.cpp
	SCGCQ00622605 - (Closed) - CS2.0: Ctrl-R Domain Id is not showing in controller properties
	SCGCQ00564008 - (Closed) - StorCli: Segmantation fault appearing in storcli when issuing /c0/fall show
	SCGCQ00518201 - (Closed) - MR6.2 : Storcli shows incorrect "Bus" information when "/c0 show all" is run
	SCGCQ00394883 - (Closed) - StorCli_MR: While Creating RAID1 with four drives command facing the "C0:BAIL_OUT at line 1354" on Flatwood Board
	SCGCQ00436107 - (Closed) - The bootwithpinnedcache logic is backwards, both storcli and the FW are affected
	SCGCQ00793689 - (Closed) - Reading Supercap VPD information fails on RHEL 6.6 PPC64
	SCGCQ00603174 - (Closed) - /c0 set cc=conc command fails with iMR card.
	SCGCQ00477037 - (Closed) - CLI reporting Large VD (56TB) size slightly smaller than other apps 
	SCGCQ00796453 - (Implemented) - MR 6.7 - If execute delete CCVD force, StorCLI throws error code 0x3 MFI_STAT message but FW throws a proper message
	SCGCQ00781004 - (Implemented) - Write-back caching support for non-RAID disks
	SCGCQ00780967 - (Implemented) - Mechanism to set disk write cache on non-RAID disks - to enable / disable
	SCGCQ00735171 - (Closed) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
	SCGCQ00696872 - (Closed) - Consistent Sorting of Controllers for End Users in Customer Facing Tools
	SCGCQ00685010 - (Closed) - Added the library functions for the new MR API bits and LD operations.
	SCGCQ00685007 - (Closed) - Added the library functions for the new MR API bits and LD operations.
	SCGCQ00632240 - (Implemented) - SED/FDE changes for storcli Synchro
	SCGCQ00351234 - (Implemented) - Provide a way to enable or disable 512E using Applications
	SCGCQ00790434 - (Closed) - Added a message to wait for some time after expander FW flash is success.
	SCGCQ00787963 - (Implemented) - Address BBU/Supercap inconsistent Behavior across HSW apps.
	SCGCQ00755527 - (Closed) - Enable SED on JBOD
	SCGCQ00642230 - (Closed) - Allow VMWARE version of STORCLI cannot be run from any directory
	SCGCQ00564477 - (Implemented) - Display the NCQ enabled/disabled status of every SATA disk drive in the output of StorCLI and MegaCLI
	SCGCQ00525321 - (Closed) - Implemented the diag results to print on console
	SCGCQ00787940 - (Implemented) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
	SCGCQ00558815 - (Closed) - MR 4.12: Big endian architecture support for MR Linux driver and StorCli
	SCGCQ00350668 - (Implemented) - Create Spanned R0 array (00) in StorCLI
	SCGCQ00369742 - (Implemented) - MWCLI. R10, R50, R60, R00 VD creation
	SCGCQ00762265 - (Implemented) - Online Capacity Expansion by adding spans to RAID 10.
	SCGCQ00757473 - (Closed) - LD Deletion stalling all IOs on Niwot HBA 12.12.0-0178
	SCGCQ00750164 - (Closed) - RRB 71 - enable SED support for iMR JBOD
	SCGCQ00621287 - (Closed) - STORCLI will support MR controller management without UEFI BootServiceDriver Driver and also has retain functionality of existing see- adapter-through-driver functionality.
	SCGCQ00564474 - (Implemented) - Request RAID CLI to display the Patrol Read Start Time
	SCGCQ00352120 - (Implemented) - MWCLI. Add HA support into storcli
	SCGCQ00333209 - (Closed) - Implemented 128 drive support by using the new ENCL_INFO structures
	SCGCQ00632051 - (Closed) - Added the OEM-NEC check for getting default disk-cache policy in Libmods as Disable.
	SCGCQ00349548 - (Closed) - Uneven span support is added in StorCLI.
	SCGCQ00349599 - (Implemented) - Refer attached design doc
	SCGCQ00433703 - (Implemented) - Megacli/storcli support for lmrc driver
	SCGCQ00467863 - (Implemented) - ASD- StorCLI - Libmod changes to support PD caching.
	SCGCQ00693042 - (Implemented) - Complete 240VD support for utilities
	SCGCQ00796453 - (Implemented) - MR 6.7 - If execute delete CCVD force, StorCLI throws error code 0x3 MFI_STAT message but FW throws a proper message
	SCGCQ00781004 - (Implemented) - Write-back caching support for non-RAID disks
	SCGCQ00780967 - (Implemented) - Mechanism to set disk write cache on non-RAID disks - to enable / disable
	SCGCQ00735171 - (Closed) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
	SCGCQ00696872 - (Closed) - Consistent Sorting of Controllers for End Users in Customer Facing Tools
	SCGCQ00685010 - (Closed) - Added the library functions for the new MR API bits and LD operations.
	SCGCQ00685007 - (Closed) - Added the library functions for the new MR API bits and LD operations.
	SCGCQ00632240 - (Implemented) - SED/FDE changes for storcli Synchro
	SCGCQ00351234 - (Implemented) - Provide a way to enable or disable 512E using Applications
	SCGCQ00790434 - (Closed) - Added a message to wait for some time after expander FW flash is success.
	SCGCQ00787963 - (Implemented) - Address BBU/Supercap inconsistent Behavior across HSW apps.
	SCGCQ00755527 - (Closed) - Enable SED on JBOD
	SCGCQ00642230 - (Closed) - Allow VMWARE version of STORCLI cannot be run from any directory
	SCGCQ00564477 - (Implemented) - Display the NCQ enabled/disabled status of every SATA disk drive in the output of StorCLI and MegaCLI
	SCGCQ00525321 - (Closed) - Implemented the diag results to print on console
	SCGCQ00787940 - (Implemented) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
	SCGCQ00558815 - (Closed) - MR 4.12: Big endian architecture support for MR Linux driver and StorCli
	SCGCQ00350668 - (Implemented) - Create Spanned R0 array (00) in StorCLI
	SCGCQ00369742 - (Implemented) - MWCLI. R10, R50, R60, R00 VD creation
	SCGCQ00762265 - (Implemented) - Online Capacity Expansion by adding spans to RAID 10.
	SCGCQ00757473 - (Closed) - LD Deletion stalling all IOs on Niwot HBA 12.12.0-0178
	SCGCQ00750164 - (Closed) - RRB 71 - enable SED support for iMR JBOD
	SCGCQ00621287 - (Closed) - STORCLI will support MR controller management without UEFI BootServiceDriver Driver and also has retain functionality of existing see- adapter-through-driver functionality.
	SCGCQ00564474 - (Implemented) - Request RAID CLI to display the Patrol Read Start Time
	SCGCQ00352120 - (Implemented) - MWCLI. Add HA support into storcli
	SCGCQ00333209 - (Closed) - Implemented 128 drive support by using the new ENCL_INFO structures
	SCGCQ00632051 - (Closed) - Added the OEM-NEC check for getting default disk-cache policy in Libmods as Disable.
	SCGCQ00349548 - (Closed) - Uneven span support is added in StorCLI.
	SCGCQ00349599 - (Implemented) - Refer attached design doc
	SCGCQ00433703 - (Implemented) - Megacli/storcli support for lmrc driver
	SCGCQ00467863 - (Implemented) - ASD- StorCLI - Libmod changes to support PD caching.
	SCGCQ00693042 - (Implemented) - Complete 240VD support for utilities
	SCGCQ00665081 - (Closed) - If any error that is returned as negative we return it s 0xFF from CLI to shell else FW returned error status will be returned to shell.
	SCGCQ00381093 - (Implemented) - PR SCGCQ00319011: Rebuild time reset
	SCGCQ00436228 - (Opened) -
	SCGCQ00342399 - (Implemented) - CSET: (Tbolt PR 211180) Punctured Block Logging Improvements
	SCGCQ00381311 - (Implemented) - dcmd path chagnes for supporting the new cachevault api
	SCGCQ00518387 - (Port_Complete) - Storcli(1.07.01): Serial number is not displayed for Seagnus(9361-8i) card in RHEL 6.4 32 bit operating system.
	SCGCQ00579103 - (Port_Complete) - Added the code to add the VD when there are missing drives on the array.
	SCGCQ00602371 - (Active) - Need to display controller memory in Control-R
	SCGCQ00758707 - (Port_Complete) - MR6.5_storCLI: VD property" Exposure to OS" equals to yes even after hidding the Virtual Drive.
	SCGCQ00758750 - (Active) - Libmods changes for defect SCGCQ00726485: Commands for unintended controller during OCR.
	SCGCQ00778747 - (Port_Complete) - Storcli get adpbootdrive legacy syntax fails
	SCGCQ00614802 - (Port_Complete) - ASD- StorCLI- Libmod related changes for porting Virtual cache feature
	SCGCQ00660804 - (Port_Complete) - Libmod changes for ER:SCGCQ00658772
	SCGCQ00732058 - (Port_Complete) - CLI command to access/modify Drive Activity LED
	SCGCQ00758689 - (Active) - Libmods: SES Management Suspend Mode for Expanders
	SCGCQ00766164 - (Port_Complete) - Displaying entire 8-byte HDD drive firmware version.
	SCGCQ00413856 - (Port_Complete) - remove the "Drive write cache" policy from Pd information.
	SCGCQ00468257 - (Port_Complete) - SWR_SLES_11_SP3_GM Release validation : In storCli " serial number and FW package Build " fields are showing blank
	SCGCQ00558869 - (Port_Complete) - Implemented the deviceExposure as a BIOS option to set /c0 set BIOS deviceExposure=<value>
	SCGCQ00578945 - (Port_Complete) - Driver version is displayed as blank for Vmware split driver in CLI 1.08.01.
	SCGCQ00653736 - (Port_Complete) - EnhancementRequest SCGCQ00650090: Add disable/enable BGI option in create VD dialog to CTRL-R
	SCGCQ00688356 - (Port_Complete) - CTRL-R- Max config- Unable to create Raid10 VD using 192 Physical drives.
	SCGCQ00732019 - (Active) - CLI command to access/modify Immediate IO
	SCGCQ00738979 - (Port_Complete) - Implemented the storcli command to print the smart data of SATA drives.
	SCGCQ00469194 - (Port_Complete) - Aligning with FW for strip calculation for 4K drives(LIBMOD)
	SCGCQ00498804 - (Port_Complete) - Unable to set PI to on/off .
	SCGCQ00616621 - (Port_Complete) - Libmods changes for OP and Remanufacture NMR1.8
	SCGCQ00678664 - (Port_Complete) - Libmod changes for defect SCGCQ00666029
	SCGCQ00687252 - (Port_Complete) - Set MFC data using ini file fails for controller
	SCGCQ00736025 - (Active) - MR6.5_RHEL5.10 : StorCLI crashing in *** glibc detected *** on trying to clear configuration on RHEL 5.10
	SCGCQ00758122 - (Port_Complete) - Libmods: Display of CacheVault Flash Memory size
	SCGCQ00793742 - (Port_Complete) - Reading Supercap VPD information fails on RHEL 6.6 PPC64
	SCGCQ00412593 - (Port_Complete) - Resolving compiler errors for Ctrl-R
	SCGCQ00469169 - (Port_Complete) - In virtual drives information the Cac filed values are incorrect with regular VD's
	SCGCQ00477845 - (Port_Complete) - Checking in tab changes
	SCGCQ00498784 - (Port_Complete) - RAID type is displayed as RAID0 for R5 VD on executing command "cli /fall show all" and "cli /fall import preview"
	SCGCQ00643707 - (Port_Complete) - Perccli crashes on displaying controller information when there is a foreign config.
	SCGCQ00694663 - (Port_Complete) - Simulator files check-in with changes in new API.
	SCGCQ00699269 - (Port_Complete) - storcli is displaying only information of one enclosure when all option is given for phyerrorcounters, on multiple enclosures
	SCGCQ00788882 - (Port_Complete) - MegaRAID CPLD update improvements
	SCGCQ00790078 - (Port_Complete) - "./storcli64 /c0 show eghs" fails on RHEL 6.6 PPC64
	SCGCQ00413017 - (Port_Complete) - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
	SCGCQ00437065 - (Port_Complete) - Driver Version is not shown in PercCli
	SCGCQ00595789 - (Port_Complete) - StorcliF Application Error when running AdpDiags in WinPE
	SCGCQ00610099 - (Port_Complete) - implemented the below commands for supporting limitsatato3G.
	SCGCQ00631408 - (Port_Complete) - Added the library calls for supporting the personality mgmt.
	SCGCQ00719102 - (Port_Complete) - Date Created field in storCLI display is incorrect after creating a VD in MSM using SWR versio 1.34 on ALM2-16
	SCGCQ00756644 - (Active) - StorCLI : BBB Phase 1 - 128k threshold plus CLI enable/disable
	SCGCQ00797738 - (Port_Complete) - SuperCap Capacitance from same system is showed inconsistent in -adpbbucmd and /cv show
	SCGCQ00376240 - (Port_Complete) - System halts on issuing storcli commands in EFI Environment.
	SCGCQ00414383 - (Port_Complete) - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
	SCGCQ00468241 - (Port_Complete) - Slow to create VD in HA Linux
	SCGCQ00498801 - (Port_Complete) - Unable to create cachecade VD with WT property .
	SCGCQ00578944 - (Port_Complete) - Wrong driver name is displayed for Vmware split driver in CLI 1.08.01.
	SCGCQ00692501 - (Port_Complete) - Firmware crash (TLB) seen during removal of SAS cable form enclosure connected in multipath.
	SCGCQ00789404 - (Port_Complete) - Remove the code related to enableVCor feild this was used for ASD and now it is not used any more.
	SCGCQ00794454 - (Port_Complete) - Dimmerswitch settings different in ctrl+r and storcli
	SCGCQ00576457 - (Port_Complete) - Multi CC cannot running concurrent even the setting is Concurrent
	SCGCQ00589544 - (Port_Complete) - storcli incorrectly handle set SOE/stoponerror and set with opposite value
	SCGCQ00518387 - (Port_Complete) - Storcli(1.07.01): Serial number is not displayed for Seagnus(9361-8i) card in RHEL 6.4 32 bit operating system.
	SCGCQ00579103 - (Port_Complete) - Added the code to add the VD when there are missing drives on the array.
	SCGCQ00602371 - (Active) - Need to display controller memory in Control-R
	SCGCQ00758707 - (Port_Complete) - MR6.5_storCLI: VD property" Exposure to OS" equals to yes even after hidding the Virtual Drive.
	SCGCQ00758750 - (Active) - Libmods changes for defect SCGCQ00726485: Commands for unintended controller during OCR.
	SCGCQ00778747 - (Port_Complete) - Storcli get adpbootdrive legacy syntax fails
	SCGCQ00614802 - (Port_Complete) - ASD- StorCLI- Libmod related changes for porting Virtual cache feature
	SCGCQ00660804 - (Port_Complete) - Libmod changes for ER:SCGCQ00658772
	SCGCQ00732058 - (Port_Complete) - CLI command to access/modify Drive Activity LED
	SCGCQ00758689 - (Active) - Libmods: SES Management Suspend Mode for Expanders
	SCGCQ00766164 - (Port_Complete) - Displaying entire 8-byte HDD drive firmware version.
	SCGCQ00413856 - (Port_Complete) - remove the "Drive write cache" policy from Pd information.
	SCGCQ00468257 - (Port_Complete) - SWR_SLES_11_SP3_GM Release validation : In storCli " serial number and FW package Build " fields are showing blank
	SCGCQ00558869 - (Port_Complete) - Implemented the deviceExposure as a BIOS option to set /c0 set BIOS deviceExposure=<value>
	SCGCQ00578945 - (Port_Complete) - Driver version is displayed as blank for Vmware split driver in PercCLI 1.08.01.
	SCGCQ00653736 - (Port_Complete) - EnhancementRequest SCGCQ00650090: Add disable/enable BGI option in create VD dialog to CTRL-R
	SCGCQ00688356 - (Port_Complete) - CTRL-R- Max config- Unable to create Raid10 VD using 192 Physical drives.
	SCGCQ00732019 - (Active) - CLI command to access/modify Immediate IO
	SCGCQ00738979 - (Port_Complete) - Implemented the storcli command to print the smart data of SATA drives.
	SCGCQ00469194 - (Port_Complete) - Aligning with FW for strip calculation for 4K drives(LIBMOD)
	SCGCQ00498804 - (Port_Complete) - Unable to set PI to on/off .
	SCGCQ00616621 - (Port_Complete) - Libmods changes for OP and Remanufacture NMR1.8
	SCGCQ00678664 - (Port_Complete) - Libmod changes for defect SCGCQ00666029
	SCGCQ00687252 - (Port_Complete) - Set MFC data using ini file fails for Softlayer controller
	SCGCQ00736025 - (Active) - MR6.5_RHEL5.10 : StorCLI crashing in *** glibc detected *** on trying to clear configuration on RHEL 5.10
	SCGCQ00758122 - (Port_Complete) - Libmods: Display of CacheVault Flash Memory size
	SCGCQ00793742 - (Port_Complete) - Reading Supercap VPD information fails on RHEL 6.6 PPC64
	SCGCQ00412593 - (Port_Complete) - Resolving compiler errors for Ctrl-R
	SCGCQ00469169 - (Port_Complete) - In virtual drives information the Cac filed values are incorrect with regular VD's
	SCGCQ00477845 - (Port_Complete) - Checking in tab changes
	SCGCQ00498784 - (Port_Complete) - RAID type is displayed as RAID0 for R5 VD on executing command "cli /fall show all" and "cli /fall import preview"
	SCGCQ00643707 - (Port_Complete) - Perccli crashes on displaying controller information when there is a foreign config.
	SCGCQ00694663 - (Port_Complete) - Simulator files check-in with changes in new API.
	SCGCQ00699269 - (Port_Complete) - storcli is displaying only information of one enclosure when all option is given for phyerrorcounters, on multiple enclosures
	SCGCQ00788882 - (Port_Complete) - MegaRAID CPLD update improvements
	SCGCQ00790078 - (Port_Complete) - "./storcli64 /c0 show eghs" fails on RHEL 6.6 PPC64
	SCGCQ00413017 - (Port_Complete) - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
	SCGCQ00437065 - (Port_Complete) - Driver Version is not shown in PercCli
	SCGCQ00595789 - (Port_Complete) - StorcliF Application Error when running AdpDiags in WinPE
	SCGCQ00610099 - (Port_Complete) - implemented the below commands for supporting limitsatato3G.
	SCGCQ00631408 - (Port_Complete) - Added the library calls for supporting the personality mgmt.
	SCGCQ00719102 - (Port_Complete) - Date Created field in storCLI display is incorrect after creating a VD in MSM using SWR versio 1.34 on ALM2-16
	SCGCQ00756644 - (Active) - StorCLI : BBB Phase 1 - 128k threshold plus CLI enable/disable
	SCGCQ00797738 - (Port_Complete) - SuperCap Capacitance from same system is showed inconsistent in -adpbbucmd and /cv show
	SCGCQ00376240 - (Port_Complete) - System halts on issuing storcli commands in EFI Environment.
	SCGCQ00414383 - (Port_Complete) - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
	SCGCQ00468241 - (Port_Complete) - Slow to create VD in HA Linux
	SCGCQ00498801 - (Port_Complete) - Unable to create cachecade VD with WT property .
	SCGCQ00578944 - (Port_Complete) - Wrong driver name is displayed for Vmware split driver in PercCLI 1.08.01.
	SCGCQ00692501 - (Port_Complete) - Firmware crash (TLB) seen during removal of SAS cable form enclosure connected in multipath.
	SCGCQ00789404 - (Port_Complete) - Remove the code related to enableVCor feild this was used for ASD and now it is not used any more.
	SCGCQ00794454 - (Port_Complete) - Dimmerswitch settings different in ctrl+r and storcli
	SCGCQ00576457 - (Port_Complete) - Multi CC cannot running concurrent even the setting is Concurrent
	SCGCQ00589544 - (Port_Complete) - storcli incorrectly handle set SOE/stoponerror and set with opposite value
	SCGCQ00593831 - (Port_Not_Required) - Inconsistency LDBBM status shown in storcli.
	SCGCQ00611867 - (Port_Complete) - Implemented the commands for ThermalPoll interval for SSD and HDD
	SCGCQ00647256 - (Port_Complete) - ASD- MR 6.4 - NytroXD compilation related fix
	SCGCQ00789418 - (Port_Complete) - StorCLI Code removal for removed ASD feilds in mr.h
	SCGCQ00790077 - (Port_Complete) - "./storcli64 /c0 flasherase " fails in RHEL 6.6 PPC64


v1.14.12 (MR6.6)
	SCGCQ00696870 (Closed) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
	SCGCQ00755055 (Closed) - Not able to flash Firware
	SCGCQ00757356 (Closed) - Show cc (ExcludeVD property) results in memory overwrite with 240VD support.
	SCGCQ00757358 (Closed) - Add adapterOperation support details in /c0 show all for cachebypassMode.
	SCGCQ00758079 (Closed) - MR 6.6 Prealpha:Incorrect Storcli version is displayed for MR 6.6 FreeBSD binary.
	SCGCQ00758739 (Closed) - StorCLI while executing SED command the syntax fails with unsupported token
	SCGCQ00758756 (Closed) - Imporper detailed help command discription for set security JBOD command
	SCGCQ00757497 (Closed) - LD Deletion stalling all IOs on Niwot HBA 12.12.0-0178
	SCGCQ00725192 (Closed) - Firmware Crash is hit while creating the Raid1 vd without drives selected
	SCGCQ00730505 (Closed) - After Rebuilding, DHS and Expand VD operations failed to update as per VD properties
	SCGCQ00752000 (Closed) - In Windows and Linux only controller grouping is working but not sorting
	SCGCQ00755063 (Closed) - Add support bits for uneven-span and SSHA support
	SCGCQ00756647 (Closed) - 6.6_StorCli: StorCli lists all cascaded enclosures at position 0.
	SCGCQ00757755 (Closed) - MR6.6_StorCLI: Displaying"BBU Not Present" for Cache vault in iMR Fury Controller
	SCGCQ00758920 (Closed) - "Storcli.exe has stopped working" when issuing command to see controller badblocks.
	SCGCQ00758924 (Closed) - Exception with command /co show badblocks or "storcli /cx flasherase"
	SCGCQ00759178 (Closed) - SupportMaxRate SATA is not listed in PD allowed operations.
	SCGCQ00759181 (Closed) - Add adapterOperation support details in /c0 show all for Emulationtype.
	SCGCQ00759183 (Closed) - SED adapterOperation detailed is not shown in detailed show controller properties
	SCGCQ00759187 (Closed) - Boot Volume details is shown in Megacli but not with storcli.
	SCGCQ00759213 (Closed) - Unused errors present in foreign command processor
	SCGCQ00759218 (Closed) - Memset is used only for 4 bytes where it has to be reset for the size of buffer we create.
	SCGCQ00759290 (Closed) - SSM-FLASh drives property is displayed for regular drives.
	SCGCQ00759862 (Closed) - OEMID is coming as "Unknown" for /c0 show all
	SCGCQ00759959 (Closed) - Support details are not shown in /c0 show all for discard cache (stalling LD deletion)
	SCGCQ00759969 (Closed) - Adapters are not listed in sorted order.
	SCGCQ00760214 (Closed) - /c0 show health all command does not show health for all drives
	SCGCQ00760215 (Closed) - show health command for drives is failing with error code 61
	SCGCQ00760255 (Closed) - Storcli_Patch_6.4 : Detailed help file is not generating for MFG
	SCGCQ00760385 (Closed) - MR_6.6: StorCLI showing incorrect value for next Schedule time for consistency check after disabling the CC
	SCGCQ00760398 (Closed) - MR6.6: Segmentation fault (Core Dumped) in CLI when setting any invalid value for PR start time
	SCGCQ00760752 (Closed) - /c0 show all does not list hwCfg information as compared to MegaCLI.
	SCGCQ00760757 (Closed) - add vd help is exceeding 80 character per line limit.
	SCGCQ00761937 (Closed) - MR 6.6 Prealpha2 Storcli:Similar PCI address(BDF number) is displayed for multiple controllers connected to FreeBSD 9.3.
	SCGCQ00762663 (Closed) - Storclio : Different error code is coming for 'set pcilinkspeed' in VMware 4.1U3
	SCGCQ00763998 (Closed) - Help missing for set sesmonitoring command
	SCGCQ00764636 (Closed) - StorCLI:Vd delete discardcache option for delete virtual drive should not support for Liberator & TB
	SCGCQ00764658 (Closed) - StorCLI /c0 show all command does not reflect the discard vd delete filed
	SCGCQ00764794 (Closed) - storcli crash when trying to import 240+64 vd at once
	SCGCQ00765712 (Closed) - StorCLI is not updated with the error Message for all new MFI_STAT added in mfistat.h
	SCGCQ00765714 (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a CacheCade VD
	SCGCQ00765759 (Closed) - StorCLI shows wrong "Number of blocks" for a 65.5TB VD size
	SCGCQ00766153 (Closed) - BBMT entries corrected and uncorrected error counters are rounding off after max is reached.
	SCGCQ00766154 (Closed) - BadBlock count displayed with below commands are rounding off after max is reached.
	SCGCQ00767040 (Closed) - help content is wrong for command /c0 set pcilinspeed
	SCGCQ00767061 (Closed) - MBOX values for set pcilinkspeed are not aligned with MR API.
	SCGCQ00767868 (Closed) - StorCLI: Detailed Help for coercion command should have the description for thier Value as [ 0, 1 , 2]
	SCGCQ00758101 (Closed) - MR_6.6_Storcli: Storcli reports supercap state 'unknown' while learn is happening on the controller.
	SCGCQ00758770 (Closed) - FW breaks in iMR when excluding VD's from CC
	SCGCQ00723935 (Closed) - Enclosure connector name not displaying properly
	SCGCQ00749743 (Closed) - Syncro SSHA : StorCLI /c0 show loadbalancemode show Load Balance OFF eventhought the fearure is ON
	SCGCQ00770875 (Closed) - MR 6.6 : Storcli for FreeBSD gives wrong version
	SCGCQ00775217 (Closed) - MR6.6_StorCLI: Showing BBU_Prop for cache vault instead of CacheVault_Prop for MR Controller card
	SCGCQ00776897 (Closed) - MR_6.6_StorCLI: Incorrectness in the Error message while deactivating the trial Key.
	SCGCQ00777800 (Closed) - storcli reports CCVD deleted even though its still under deletion process by FW
	SCGCQ00779800 (Closed) - MR6.6_CLI_FreeBSD: Displaying incorrect Driver name
	SCGCQ00780082 (Closed) - Segmentation fault while trying to flash GasGauge file with "noverchk" switch.
	SCGCQ00780773 (Closed) - MR6.6:StorCLI shows incorrect information about "Cache Vault Flash Size"
	SCGCQ00782882 (Closed) - MR6.6:StorCLI shows incorrect information about "Cache Vault Flash Size"
	SCGCQ00783289 (Closed) - Firmware returns an error for DCMD MR_DCMD_SCAN_FOR_FOREIGN_CONFIGS, but storcli still goes ahead and fires import.
	SCGCQ00783693 (Closed) - Storcli running legacy Cli command for encinfo does not display the reults in the correct format
	SCGCQ00787431 (Closed) - Dimmerswitch settings different in ctrl+r and storcli
	SCGCQ00794013 (Closed) - too many bytes for ioctl, given [ffff], max [ff44]
	SCGCQ00795836 (Closed) - storcli /c0/eall show is giving segmentation on TB FW
	SCGCQ00413396 (Closed) - MR_Inv_6.1:StoreCLI- Reports CTRL+R is disabled (controller boot properties) but actually it is enabled
	SCGCQ00797068 (Closed) - SATA SSD Model string is truncated to 8 bytes in StorCLI /cx/sx/ex show all Device Attributes section
	SCGCQ00797277 (Closed) - SuperCap Capacitance from same system is showed inconsistent in -adpbbucmd and /cv show
	SCGCQ00797726 (Closed) - EFI Storcli is not show the PD information on Grantley server

v1.13.08 (MR6.5 patch)
	EPSD100243493 - Cmdtool2 & StorCLI -adpalilog causes seg faults under Linux

v1.13.06 (MR6.5)
	SCGCQ00617622 - (Closed) - Storcli- Gives Seg fault for './storcli /c0 show all' if a foreign Secured VD is present on the controller
	SCGCQ00637551 - (Closed) - storcli.efi /c0 set migraterate is setting values even if the value is out of range
	SCGCQ00648409 - (Closed) - Value not popped up for successful completion of autopdcache=r0 command.
	SCGCQ00649340 - (Closed) - Store add VD help should display R1 EC as supported raid level
	SCGCQ00657399 - (Closed) - query for multiple enclosure properties is failing in storcli version-1.12.05
	SCGCQ00659228 - (Closed) - storcli show file=***.rom displaying only firmware version
	SCGCQ00668210 - (Closed) - Inconsistent scheduled learn time.
	SCGCQ00672888 - (Closed) - Junk Characters observed in EFI storcli version : 1.12.07
	SCGCQ00678562 - (Closed) - the phy number dosent come properly on querying the phy error counter
	SCGCQ00606774 - (Closed) - command "set patrolread delay" showing negative time delay
	SCGCQ00622402 - (Closed) - Changing the MR_MFC_DEFAULTS->biosContinueOnError behavior for StorCLI as per PDMs
	SCGCQ00624834 - (Closed) - fw is not able create vd on all drive as r0 using storcli command without an option immediate
	SCGCQ00624991 - (Closed) - there is no syntax for storcli64.exe /cx/ex show
	SCGCQ00629272 - (Closed) - storcli /c0/v2-256 show results in segmentation fault
	SCGCQ00644238 - (Closed) - improper statment for emulationType 0 in help & detailed help
	SCGCQ00647260 - (Closed) - a failure message is displayed for a successful operation
	SCGCQ00653749 - (Closed) - "cfgcachecadedsply" command is not showing any CC VD details [when creating using EVS + CCVD]
	SCGCQ00611955 - (Closed) - Update the storcli help file for this command ./stocli /c0 set eccbucketleakrate
	SCGCQ00616901 - (Closed) - seeing junk characters for command "show termlog"
	SCGCQ00626582 - (Resolved) - not able to create WB cachecade-VD
	SCGCQ00627824 - (Closed) - High Availability Properties alignment properly in adpallinfo detail.
	SCGCQ00627826 - (Closed) - not able set emergency hotspare field in storcli
	SCGCQ00646216 - (Closed) - Help not displayed for diag when tagged with paniclog,smartlog and errorlog.
	SCGCQ00647107 - (Closed) - LD emulation type set to 512e even though there only 512n drives are used during creation
	SCGCQ00682484 - (Closed) - help file needs to be updated  for /cx/dx add mirror src=2
	SCGCQ00684010 - (Closed) - For iBBU battery typeiBBU09 the Next Learn time value is not correct in the output of storCLI command storcli64 /c0/bbu show
	SCGCQ00691917 - (Closed) - on querying for backplane/controller PHY, errors get reported
	SCGCQ00645141 - (Closed) - Storcli reports VD state as offline if pinned cache is generated through CC VD removal
	SCGCQ00646223 - (Closed) - adding mirror by setting src value to 0 will start rebuild on online drive
	SCGCQ00649337 - (Closed) - Junk characters seen in storcli.efi –adpallinfo –a0 and storcli.efi /c0 show all
	SCGCQ00695247 - (Closed) - on querying the PHY info for the drive,storcli gives the junk data
	SCGCQ00666644 - (Closed) - using option 2 i.e ./storcli /c0/d0 add mirror src=2 give success but no operation is performed
	SCGCQ00694027 - (Closed) - on querying the phy error counter for controller, storcli dosent fail the cmd
	SCGCQ00615654 - (Closed) - Battery serial number is not coming properly as per termlogs
	SCGCQ00627716 - (Closed) - unable to create VD using Storcli
	SCGCQ00646344 - (Closed) - verall Health of a controller is displayed as ERROR if there is no VD present.
	SCGCQ00658427 - (Closed) - Need to handle the failed cases and junk/invalid image file scenario for storcli show file=<filename> command
	SCGCQ00675388 - (Closed) - Storcli won't set cacheflushinterval to a value greater >= 10 using old megacli syntax
	SCGCQ00670246 - (Closed) - add vd each type=r0 creation leads to Segmentation Fault
	SCGCQ00678558 - (Closed) - the out put for phyerror counter goes beyound the limit of wordcount.
	SCGCQ00678616 - (Closed) - Status of storcli controller show health command on Python card Failed
	SCGCQ00621291 - (Closed) - Add storCLI command to read phy error counters (target, expander, controller)
	SCGCQ00625566 - (Closed) - Add a feature to read and display the FW version from the .rom file for MegaRAID FW package
	SCGCQ00634751 - (Closed) - Requirement for 512e implementation changes
	SCGCQ00673086 - (Closed) - Add SSHA support to StorCLI
	SCGCQ00610100 - (Port_Complete) - implemented the below commands for supporting limitsatato3G
	SCGCQ00615523 - (Port_Complete) - doesn't have proper keyword to set the Dimmer switch property for DisableLDPS.
	SCGCQ00631409 - (Port_Complete) - Add support bit check for flash-erase.
	SCGCQ00654713 - (Port_Complete) - Help not displayed for diag when tagged with paniclog,smartlog and errorlog.
	SCGCQ00615522 - (Port_Complete) - displays 'Model' information incorrectly using show
	SCGCQ00626649 - (Port_Complete) - storcli /253-255 show gives segmentation fault.
	SCGCQ00630127 - (Active) - Changing the MR_MFC_DEFAULTS->biosContinueOnError behavior for StorCLI as per PDMs
	SCGCQ00660446 - (Port_Complete) - WB CCVD is created eventhough WT is specified in Slice nytro Cache create option
	SCGCQ00629199 - (Port_Complete) - unable to create VD using Storcli
	SCGCQ00615442 - (Port_Complete) - Porting OverProvisioning and Remanufacture to StorCli5.9 for NMR 1.8
	SCGCQ00631330 - (Port_Complete) - set batterywarning command sets inproperly.
	SCGCQ00631410 - (Port_Complete) - SSDThermalPollInterval value range starts from 1 not from 0
	SCGCQ00614724 - (Port_Complete) - add VD nytrocache command displays a wrong error message if the CCVD is already present
	SCGCQ00614177 - (Port_Complete) - StorCli Displays Incorrect Information for BatteryWarning versus MagaCli
	SCGCQ00631411 - (Port_Complete) - Implemented the personality mgmt to set either HBA/RAID mode.
	SCGCQ00670865 - (Port_Complete) - Storcli shows success message on creating EC CCVD in WT mode
	SCGCQ00691901 - (Port_Complete) - Not able to enable security on DG which are eligible for secured Drive Group
	SCGCQ00690877 - (Port_Complete) - Advance Software options is not displaying any value for MegaRAID CacheCade Pro2.0
	SCGCQ00611864 - (Port_Complete) - Porting megaSCu syntax to perccli for limitMaxRateSATAto3G
	SCGCQ00611866 - (Port_Complete) - Implemented the commands for ThermalPoll interval for SSD and HDD
	SCGCQ00615271 - (Port_Complete) - StorCLIF and StorCLIO - Porting VC features
	SCGCQ00670863 - (Port_Complete) - Source VD association failed and Storcli application crashed while associating sourceVD to CCVD

V1.12.13
	SCGCQ00617622 - (Closed) - Storcli- Gives Seg fault for './storcli /c0 show all' if a foreign Secured VD is present on the controller
	SCGCQ00637551 - (Closed) - storcli.efi /c0 set migrate rate is setting values even if the value is out of range
	SCGCQ00648409 - (Closed) - Value not popped up for successful completion of autopdcache=r0 command.
	SCGCQ00649340 - (Closed) - Store add VD help should display R1 EC as supported raid level
	SCGCQ00657399 - (Closed) - query for multiple enclosure properties is failing in storcli version-1.12.05
	SCGCQ00659228 - (Closed) - storcli show file=***.rom displaying only firmware version
	SCGCQ00668210 - (Closed) - Inconsistent scheduled learn time.
	SCGCQ00672888 - (Closed) - Junk Characters observed in EFI storcli version : 1.12.07
	SCGCQ00678562 - (Closed) - the phy number dosent come properly on querying the phy error counter
	SCGCQ00606774 - (Closed) - command "set patrolread delay" showing negative time delay
	SCGCQ00622402 - (Closed) - Changing the MR_MFC_DEFAULTS->biosContinueOnError behaviour for StorCLI as per PDMs
	SCGCQ00624834 - (Closed) - fw is not able create vd on all drive as r0 using storcli command without an option immediate
	SCGCQ00624991 - (Closed) - there is no syntax for storcli64.exe /cx/ex show
	SCGCQ00629272 - (Closed) - storcli /c0/v2-256 show results in segmentation fault
	SCGCQ00644238 - (Closed) - improper statement for emulationType 0 in help & detailed help
	SCGCQ00647260 - (Closed) - Storcli-1.12.03-a failure message is displayed for a successful operation
	SCGCQ00653749 - (Closed) - "cfgcachecadedsply" command is not showing any CC VD details [when creating using EVS + CCVD]
	SCGCQ00611955 - (Closed) - Update the storcli help file for this command ./stocli /c0 set eccbucketleakrate
	SCGCQ00616901 - (Closed) - seeing junk characters for command "show termlog"
	SCGCQ00626582 - (Resolved) - not able to create WB cachecade-VD
	SCGCQ00627824 - (Closed) - -High Availability Properties alignment properly in adpallinfo detail.
	SCGCQ00627826 - (Closed) - not able set emergency hotspare field in storcli
	SCGCQ00646216 - (Closed) - Help not displayed for diag when tagged with paniclog,smartlog and errorlog.
	SCGCQ00647107 - (Closed) - LD emulation type set to 512e even though there only 512n drives are used during creation
	SCGCQ00682484 - (Closed) - help file needs to be updated  for /cx/dx add mirror src=2
	SCGCQ00684010 - (Closed) - For iBBU battery typeiBBU09 the Next Learn time value is not correct in the output of storCLI command storcli64 /c0/bbu show
	SCGCQ00691917 - (Closed) - on querying for backplane/controller PHY, errors get reported
	SCGCQ00645141 - (Closed) - Storcli reports VD state as offline if pinned cache is generated through CC VD removal
	SCGCQ00646223 - (Closed) - adding mirror by setting src value to 0 will start rebuild on online drive
	SCGCQ00649337 - (Closed) - Junk characters seen in storcli.efi –adpallinfo –a0 and storcli.efi /c0 show all
	SCGCQ00695247 - (Closed) - on querying the PHY info for the drive, storcli gives the junk data
	SCGCQ00666644 - (Closed) - using option 2 i.e ./storcli /c0/d0 add mirror src=2 give success but no operation is performed
	SCGCQ00694027 - (Closed) - on querying the phy error counter for controller, storcli doesn't fail the cmd
	SCGCQ00615654 - (Closed) - Battery serial number is not coming properly as per termlogs
	SCGCQ00627716 - (Closed) - unable to create VD using Storcli
	SCGCQ00646344 - (Closed) - Overall Health of a controller is displayed as ERROR if there is no VD present.
	SCGCQ00658427 - (Closed) - Need to handle the failed cases and junk/invalid image file scenario for storcli show file=<filename> command
	SCGCQ00675388 - (Closed) - Storcli won't set cacheflushinterval to a value greater >= 10 using old megacli syntax
	SCGCQ00670246 - (Closed) - add vd each type=r0 creation leads to Segmentation Fault
	SCGCQ00678558 - (Closed) - the out put for phyerror counter goes beyond the limit of wordcount.
	SCGCQ00678616 - (Closed) - Status of storcli controller show health command on card Failed
	SCGCQ00621291 - (Closed) - Add storCLI command to read phy error counters (target, expander, controller)
	SCGCQ00625566 - (Closed) - Add a feature to read and display the FW version from the .rom file for MegaRAID FW package
	SCGCQ00634751 - (Closed) - Requirement for 512e implementation changes
	SCGCQ00673086 - (Closed) - OAdd SSHA support to StorCLI
	SCGCQ00610100 - (Port_Complete) - implemented the below commands for supporting limitsatato3G
	SCGCQ00615523 - (Port_Complete) - doesn't have proper keyword to set the Dimmer switch property for DisableLDPS.
	SCGCQ00631409 - (Port_Complete) - Add support bit check for flash-erase.
	SCGCQ00654713 - (Port_Complete) - Help not displayed for diag when tagged with paniclog,smartlog and errorlog. - (SCGCQ00646216) --Updating review comments
	SCGCQ00615522 - (Port_Complete) - displays 'Model' information incorrectly using PercCLI show
	SCGCQ00626649 - (Port_Complete) - storcli /253-255 show gives segmentation fault.
	SCGCQ00660446 - (Port_Complete) - WB CCVD is created even though WT is specified in Slice nytro Cache create option
	SCGCQ00629199 - (Port_Complete) -  unable to create VD using Storcli
	SCGCQ00615442 - (Port_Complete) - Porting OverProvisioning and Remanufacture to StorCli5.9 for NMR 1.8
	SCGCQ00631330 - (Port_Complete) - set batterywarning command sets improperly.
	SCGCQ00631410 - (Port_Complete) - SSDThermalPollInterval value range starts from 1 not from 0
	SCGCQ00614724 - (Port_Complete) - add VD nytrocache command displays a wrong error message if the CCVD is already present
	SCGCQ00614177 - (Port_Complete) - StorCli Displays Incorrect Information for BatteryWarning versus MagaCli
	SCGCQ00631411 - (Port_Complete) - Implemented the personality mgmt to set either HBA/RAID mode.
	SCGCQ00670865 - (Port_Complete) - NMR1.8-Storcli shows success message on creating EC CCVD in WT mode
	SCGCQ00691901 - (Port_Complete) - Not able to enable security on DG which are eligible for secured Drive Group
	SCGCQ00690877 - (Port_Complete) - Advance Software options is not displaying any value for MegaRAID CacheCade Pro2.0
	SCGCQ00611864 - (Port_Complete) - Porting megaSCu syntax to perccli for limitMaxRateSATAto3G
	SCGCQ00611866 - (Port_Complete) - Implemented the commands for ThermalPoll interval for SSD and HDD
	SCGCQ00615271 - (Port_Complete) - StorCLIF and StorCLIO - Porting VC features
	SCGCQ00670863 - (Port_Complete) - Source VD association failed and Storcli application crashed while associating sourceVD to CCVD

v1.09.13
	SCGCQ00681802 - (Completed) - GG firmware update patch (GG firmware update support for following OSes: Windows, Linux, EFI, Ubuntu)
	SCGCQ00681722 - (Closed) - storcli (megacli style) output difference in pdlist command
	SCGCQ00682462 - (Closed) - Help file should be updated
	SCGCQ00655156 - (Closed) - "storcli -AdpBIOS -BE -a0" no longer works
	SCGCQ00682485 - (Closed) - status of the command id getting success with invalid GG file.
	SCGCQ00682477 - (Closed) - option "Resetnow" should be blocked when flashing Gasguage
	SCGCQ00698740 - (Closed) - Card with Empty module version doesn't update firmware if option "noverchk" is provided.
	SCGCQ00683236 - (Closed) - In Rhel OS seeing wrong error code.
	SCGCQ00658495 - (Port_Complete) - set batterywarning command sets improperly.
	SCGCQ00659836 - (Port_Complete) - StorCli Displays Incorrect Information for BatteryWarning versus MagaCli

v1.09.08
	SCGCQ00567786 - not able get enclosure status
	SCGCQ00571823 - Added a condition to check for no VDs in StrtDrCp
	SCGCQ00573703 - Storcli shows wrong VD size for 4K VDs during foreign config import
	SCGCQ00574165 - compare factorysettings is a factory command but works in storcli
	SCGCQ00579423 - storcli - issung "storcli /c0/v256" command generating coredump segmentation fault
	SCGCQ00600059 - Storcli creates configuration not using the OEM default value for Disk Cache Policy
	SCGCQ00471826 - StorCli mbox value needs to be changed for the command "storcli /c0/bbu show gasgauge offset=1 numbytes=1"
	SCGCQ00571832 - Added a condition to check for no VDs
	SCGCQ00574325 - Storcli 'show ds' command fails with message "LD Power saving is unsupported"
	SCGCQ00598687 - for bbu command In properties schedule time is showing twice
	SCGCQ00599761 - storcli /c0/e1,2,3 show is showing enclouser properties multiple times.
	SCGCQ00622402 - Changing the MR_MFC_DEFAULTS->biosContinueOnError behaviour for StorCLI as per PDMs
	SCGCQ00484361 - Removed the option all from tokenizer as it is not supported for enclosure firmware download.
	SCGCQ00563031 - Even though there are no drive groups, the command storcli /c0/dxxx set security=on is getting success
	SCGCQ00565409 - while Rebuild was going on Storcli was allows to create a partial VD on the same drive group
	SCGCQ00576233 -  ./storcli64 /c0/bbu set learnstarttime command is failing with segmentation fault
	SCGCQ00595061 - Storcli shows wrong estimated time for a rebuilding drive.
	SCGCQ00602401 - ./storcli64 /c0/e252 show status displays success message
	SCGCQ00581367 - MOn issuing command Adpalilog -a0 the Storcli throws an error 0x0c on PPC server
	SCGCQ00601834 - The SCAPVPD commands are described as BBU instead of CV.
	SCGCQ00559492 - Storcli displays the cc estimated time left out for the vd's where the operation is not in progress
	SCGCQ00573720 - Need to display skipped images by storcil package flashing
	SCGCQ00574205 - ./storcli64 /c252 show is displaying controller information of 1st controller
	SCGCQ00601212 - Detailed help for storcli /c0/v0 set hostaccess is not showing
	SCGCQ00581982 - Difference in behaviour across windows and linux platform after flashing FW from storclif
	SCGCQ00598488 - storcli /c256 show is showing O/P as wrong syntax.
	SCGCQ00600176 - command "/c0/p8 show" causing cli crash in windows OS
	SCGCQ00602926 - when we query help for set perfmode the range is not mentioned for maxflush lines & numiostoorder.
	SCGCQ00606117 - storlib library depended Make file flags check in
	SCGCQ00577682 - MR Liberator :: ./storcli64 /c0 show dequeuelog file command failing with segmentation fault
	SCGCQ00588916 - ./storcli64 /c0/sall show rebuild command shows success status
	SCGCQ00598788 - "show termlog" command description is coming after displaying the logs.
	SCGCQ00627716 - unable to create VD using Storcli
	SCGCQ00553006 - Updated Help syntax for add vd w.r.t AWB
	SCGCQ00572149 - Added the help changes for break and join mirror.
	SCGCQ00601568 - nolog option is not working in MegaCLI
	SCGCQ00526855 - Link libstdc++ statically to Linux versions of Strcli, storclio and storclif
	SCGCQ00602432 - Linux-ppc 32-bit minimum driver version supported by storcli 06.603.04.00.
	SCGCQ00554055 - Big endian architecture support for MR Linux driver and StorCli
	SCGCQ00555468 - Added OEM based help and displaying it.
	SCGCQ00568855 - Added new commands for join mirror
	SCGCQ00550374 - Added new commands for break mirror
	SCGCQ00569363 - Implemented the below CS syncro commands
	SCGCQ00564470 - Request RAID CLI to display the Patrol Read Start Time
	SCGCQ00523846 - Storcli to flash 16 and 32 MB images
	SCGCQ00593583 - In Storcli, appropriate error description to be logged when FW flash is failed
	SCGCQ00601765 - Storcli shows wrong estimated time for a rebuilding drive.
	SCGCQ00576453 - Found storli will show incorrect Next starttime after changing CC from Automatic to OFF.
	SCGCQ00592293 - Unable to replace failed drive
	SCGCQ00598800 - StorCLI adpalilog command crashes in Windows 2012 R2 Build 9600 - version 1.06.03 and version 1.03.46
	SCGCQ00558870 - Implemented the deviceExposure as a BIOS option to set /c0 set BIOS deviceExposure=n
	SCGCQ00564130 - Added a condition to check for number of drives.
	SCGCQ00604174 - BiosContinueOnError IssueWebBIOS for SAS9265-8i controller incorrectly reports "Pause on errors" instead of "Bypass Error"
	SCGCQ00593384 - SCSI bus reset while collecting TFF smart logs
	SCGCQ00593417 - 1.05.56 rpm installation failed saying "scriptlet failed, exit status 1"
	SCGCQ00593572 - TFF firmware upgrade succeeded with mode 7 on Eagle board
	SCGCQ00567735 - not showing DS3 enable properties.
	SCGCQ00578982 - and storclif mention "nytrocache" in help message not an OEM feature
	SCGCQ00593226 - When attempting to update DFF firmware, update fails with error "Failure 1001 failed to get ssd Controller type.
	SCGCQ00593386 - 'start format' command form stocli on unconfigured drive deletes all the vds configured
	SCGCQ00598815 - StorCLI adpalilog command crashes in Windows 2012 R2 Build 9600 - version 1.06.03 and version 1.03.46
	SCGCQ00563046 - storcli64.exe /c0/cv start learn option is not present
	SCGCQ00575400 - Getting segmentation fault when executed the command /c0 compare factorysettings file= file name
	SCGCQ00555931 - storclif 1.07.06 does not have memory scrub test available
	SCGCQ00567476 - getting segmentation fault when executed the command /c0 set factory file=filename
	SCGCQ00578979 - space present in command compare factorysettings between words factorysettings
	SCGCQ00593402 - Successful command execution depicted as a "failure" for the command: "add each vd type=r0"
	SCGCQ00593571 - Storcli doesn't provide "Description" in output when extract paniclog is issued on all the TFFs.
	SCGCQ00593568 - Storcli does not prompt the user to reboot the host after changing the link speed of a TFF.

v1.07.07
	SCGCQ00493418 - FW breaks to MegaMon on executing "Cli /eall/sall show all" command.
	SCGCQ00501866 - Time Left is not show correctly by sparc storcli
	SCGCQ00521869 - /call/eall show not providing details of enclosure connected to the second controller
	SCGCQ00526799 - Not able to flash PD firmware of 4TB Drive using storcli
	SCGCQ00485777 - FW breaks to Megamon, after creating 16 R0 VD's and on executing command "cli /vall show all" from PCLI.
	SCGCQ00501376 - "/c0 show dequeuelog file=_____" command is not working in OS OEL_5.9
	SCGCQ00503993 - Command "./storcli /call/eall/sall show" fails for second controller with description drive not found.
	SCGCQ00505348 - The help file for "/c0 start Diag duration=___" is missing
	SCGCQ00503359 - Wrong PCLI version with junk characters are displayed under GetControllerInfo.
	SCGCQ00498965 - "/c0/bbu start learn" command starts battery learn cycle on supercap battery.
	SCGCQ00518133 - LSI_MR Controllers fails to set "FACTORY SETTINGS"
	SCGCQ00526503 - Flashing of FW in UEFI mode using storcli.efi is issuing File read error.
	SCGCQ00501383 - "/c0 show dequeuelog file=_____" command is missing in main help file
	SCGCQ00501414 - Online firmware update is not triggered on flashing FW
	SCGCQ00524047 - Segmentation fault occures while converting binary to text file of DQlogs
	SCGCQ00526385 - Unable to create cachecade VD with WT property .
	SCGCQ00522666 - Command "cli /sall show all" 
	SCGCQ00524755 - Storcli- Gives incomplete message while clearing config when CC VD is present on the controller
	SCGCQ00493544 - "Error! App exec failed in FW PCLIError! Internal" is displayed on executing "Cli /eall/sall spindown" command with 25 drives.
	SCGCQ00501437 - StorCLI - MR 6.2 StorCLI help syntax is wrong
	SCGCQ00518372 - Displaying the Adapter health status in storcli show.
	SCGCQ00501561 - Implemented the diag results to print on console
	SCGCQ00484168 - Implemented the AWB for VD creations
	SCGCQ00526393 - Implementation of "MegaCli adpbbucmd schedulelearn [options.....] an" equivalent command in storcli
	SCGCQ00304999 - SWR- Retrieval of controller information fails .
	SCGCQ00305001 - storcli command- show DS displays wrong information for type4 and DS off
	SCGCQ00307493 - (RW LSIP200233165) Storcli: Reocurance should be spelled as reoccurrence in controller show all properties for PR and CC
	SCGCQ00307495 - Displaying the correct operating system for Windows 2012 Server
	SCGCQ00308671 - StorCLI is not showing correct driver version in Solaris 11
	SCGCQ00309347 - StorCli-SATA Drives "PRODUCT ID" its not showing properly.
	SCGCQ00312089 - Storcli- Not able to perform erase operation on a PD on VMWare 4.1 update 2
	SCGCQ00312319 - Storcli- Status of /pall set linkspeed is showing success even though the operation is failure on ESX 4.1 update 2
	SCGCQ00314106 - Remove all negative error codes
	SCGCQ00314585 - StorCli - Cache cade VD information page doesn't have any details for associated VDs.
	SCGCQ00322316 - Defect: Storcli-Controller show/set help page in that last line execute with Storcli Directory.
	SCGCQ00328184 - StorCLI2.0: "endCtlrPropUpdate failed 4" when changing the properties of patrolread
	SCGCQ00335239 - Virtual Drive properties(stripe size and size) got changed when VD is degraded
	SCGCQ00338301 - StorCLI : Not able to set BBU modes using legacy syntax in EFI Environment
	SCGCQ00341488 - stocli_EFI- In paged view the next line after "press enter to continue " should be displayed in next line
	SCGCQ00342056 - StorCLI - in command "./storcli show " 2 fields are not getting displayed ( 1. Host Name , 2. Operating System )
	SCGCQ00342074 - storcli should not depend on MFC_FEATURES instead check the other bits which indicates whether a particular feature is supported
	SCGCQ00342549 - spelling mistake of initialization in (background initialization)
	SCGCQ00343721 - (Cloned_EnhReq) - Drive /c0/ex/sx Hot Spare Information, displays array info under Dedicated Drive Group(s) = 0, 1
	SCGCQ00343907 - StorCLI_EFI: System halts while performing import preview with securitykey in EFI Environment
	SCGCQ00345525 - On performing an "add vd" with size provided in TB a decimal value is truncated to whole number as input.
	SCGCQ00349419 - storcli /c0 show all -----> driver version and driver name field is missing
	SCGCQ00350744 - ./storcli /c0/dall show -----> In the drive group info the alignment for global hot spare drive is improper.
	SCGCQ00352569 - Buffer overflow
	SCGCQ00360745 - StorCLI does not provide command to set HSM or HCOE SCGCQ00358662
	SCGCQ00362717 - storcli /c0/d0 show " in that legend missing for "Dgrd/pdgd/Onln/ofLn/Rbld"
	SCGCQ00363522 - storcli query for displaying controller properties is showing status , as failure.
	SCGCQ00364248 - StorCLI failed to delete a VD that is just created under Windows 2008
	SCGCQ00364622 - Reports wrong diskgroup size while querying controller level properties
	SCGCQ00381100 - MR: not able to create PRL11 using 96 drives.
	SCGCQ00462959 - Slow to create VD in HA Linux
	SCGCQ00464708 - Storcli display total number of VDs in a individual drive group properties.
	SCGCQ00466519 - StorCLI_6.1:The help file for "/c0 compare securitykey h" is missing
	SCGCQ00467119 - SWR_SLES_11_SP3_GM Release validation : In storCli " serial number and FW package Build " fields are showing blank
	SCGCQ00481532 - Msg comes for all /c0 show commands.
	SCGCQ00305002 - Storcli:Unable to update PD Firmware using Storcli in Vmware 5.0
	SCGCQ00310308 - Storcli -Format for Date/Time varies in show|show all controller properties .
	SCGCQ00313759 - Storcli:Unable to create Cachecade VD in Windows 8
	SCGCQ00314602 - StorCli - Cachecade VD information page should not display stripe size.
	SCGCQ00316677 - Logical and Physical sector size must be hidden when 512E feature is not supported
	SCGCQ00322262 - iMR_Inv:37 drives shown as unconfigured good in MegaCLI when "enable JBOD=0" in Ubuntu 12.04 32 bit OS
	SCGCQ00324797 - Serial Number of controller is not displayed for some controllers.
	SCGCQ00332212 - libsysfs custom implementation issue.
	SCGCQ00341418 - In the command O/P of <./storcli /c0 show all>"Driver Name" and "Driver Version"are NOT matching with actual name and version
	SCGCQ00342723 - It is displaying the driver version as driver name
	SCGCQ00344992 - In the command O/P of <./storcli /c0 show all>, ErrMsg 255 Failed to get Bus Info is displayed
	SCGCQ00348911 - Adapter 0: Failed to start SecureErase on Virtual Drive 0 in VMware_ESXi_5.1
	SCGCQ00353679 - StorCli-"/c0/eall/sall show"in that need to be describe the GHS/Onln/Offln/F
	SCGCQ00355536 - MegaCli and StorCli can not manage both Liberator (and prior) and TB controllers in the same system under FreeBSD with the mfi adn mrsas driver.
	SCGCQ00357653 - Removing static memory allocation and allocating memory dynamically in function stricmp in file Cutils.cpp
	SCGCQ00357913 - Update VD emulation feature in StorCLI Libmods module to sync with latest APIs.
	SCGCQ00359998 - Code clean up in libmods and sysefi files are added
	SCGCQ00360814 - StorCLI: Not able to set pr property includessds as onlymixed on Liberator cacheoffload controller
	SCGCQ00362421 - StorCLI: Not able to detect Liberator Controller on FreeBSD 9.0(64-bit)
	SCGCQ00364097 - iMR_Inv_6.1:StoreCLI- StoreCLI reports wrong Emulation type for VDs
	SCGCQ00366000 - Storcli displays incomplete serial number for some SSDs
	SCGCQ00374979 - Storcli ld info command displays R10 vd Span Depth to 1.
	SCGCQ00469162 - In virtual drives information the Cac filed values are incorrect with regular VD's
	SCGCQ00476030 - while running I/O ,It's taking time to load the controller information.
	SCGCQ00312928 - Storcli- Abbreviation of UID should be mentioned in the output for /cx/fall show all
	SCGCQ00314122 - Missing characters in PD model display
	SCGCQ00317649 - Defect: StorCli-VD state "Dgrd'' is changed in the description-''dgrd''
	SCGCQ00326862 - FreeBSD support for MegaWare Cli
	SCGCQ00338688 - Storcli spelling mistakes and typos
	SCGCQ00343593 - Description for different Drive "State" like DHS, Ugood, Online need to be provided under Show Drive Information
	SCGCQ00363455 - The legend for the PD List table exceeds 80 char limit.
	SCGCQ00364735 - UEFI, the O/P of <storcli /c0 show all>"Current Controller Date/Time" & "Current System Date/time" are not in proper format
	SCGCQ00371445 - Vmware CLI fails to set the phy linkspeed
	SCGCQ00377364 - StorCli shows Power Saving Option as enabled, despite controller having power saving option completely disabled.
	SCGCQ00383043 - StorCLI-Invader : The "coercion" mode is not in sync with the legacy values.
	SCGCQ00394883 - StorCli_MR: While Creating RAID1 with four drives command facing the "C0:BAIL_OUT at line 1354"
	SCGCQ00396303 - Cfgclr command fails without force option in Sparc OS
	SCGCQ00460861 - MR_Inv_6.1:StorCLI- Gives wrong message after battery retention test command is issued for Supercap FBU03
	SCGCQ00462885 - Need to remove storcli /cx show clusterenable and storcli /cx set clusterenable=<value> since FW did not support this in HA
	SCGCQ00466038 - MR_Inv_6.1:StoreCLI- StorCLI reports retention time as 0 for supercap FBU02 and FBU03
	SCGCQ00466251 - HA : StorCLI crash when update drive firmware
	SCGCQ00471042 - PCLI:Cant able to set securitykey for Controller and also VD name for VD(Takes as uppercharacter even if name given in lower)
	SCGCQ00485270 - StorCLI- unsupported CV operations for SuperCap 'set' needs to be removed
	SCGCQ00311990 - Removed unsupported property "Ra=Read Ahead Adaptive" from VD information.
	SCGCQ00314114 - sector size of PDs are shown as 512 KB which is wrong.
	SCGCQ00314128 - Add abbreviation description to all the PD states
	SCGCQ00318435 - (Cloned_EnhReq) - Porting of 1.0 PRs to storcli phase 2.5 (Libmods)
	SCGCQ00345372 - Storcli command "/cx show all" must display ROC temperature.
	SCGCQ00359629 - In paged view the text " Press Enter to continue" should be changed to " Press any key to Continue"
	SCGCQ00365950 - StorCLI cannot displays information for controller in Safe mode
	SCGCQ00442610 - Onfi_patch_6.0:Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
	SCGCQ00469179 - Aligning with FW for strip calculation for 4K drives
	SCGCQ00337962 - StorCLI: not able to save events in txt file in EFI environment
	SCGCQ00362216 - iMr_Fury_StorCli:4K Drive size shown wrong in Esxi4.1U3
	SCGCQ00365632 - PCI Info for FreeBSD needs to be indicated as "N/A"
	SCGCQ00379104 - Not able to get paged view of StorCLI output on VM-Ware Platform
	SCGCQ00438350 - Megacli crashes after invoking any command in SGI system with one 9280-8e and 2 quad port qlogic FC cards.
	SCGCQ00485561 - storclio set and get vpd gives a wrong output in failure case.
	SCGCQ00493690 - /var/tmp//installobaWVe/checkinstallrbaWVe: line 11: syntax error at line 22
	SCGCQ00481039 - option -v doesn't work with preboot storcli
	SCGCQ00311436 - Storcli-SWR- Controller serial number display is different in show/showall controller properties .
	SCGCQ00360040 - Storcli is returning error with show
	SCGCQ00408070 - StorCLI does not show both "Current Write Policy" and "Default Write Policy" for VD
	SCGCQ00423832 - EFI_ Storcli: Cannot set vpd file on controller, EFI hangs and cannot proceed for further operations until reboot
	SCGCQ00470976 - Storcli shows irrelevant information about Nytro cache VD when user types "CfgCacheCadeDsply"
	SCGCQ00484372 - Storcli:Help file modification required for command ''/cx set eghs''
	SCGCQ00357263 - MegaCLI adpgetpciinfo returns a static Bus Number value "17d0"
	SCGCQ00362070 - iMr_Fury_StorCLi:SectorSize show as "512KB" for 512Bytes drives
	SCGCQ00396665 - StorcLi_5.7: Remove the description for "Ra=Read Ahead Adaptive" in VD show info.
	SCGCQ00397663 - StorCli_MR: While creating VD using default values FW allows read policy as"Ra=Read Ahead Adaptive" as against PR-317400
	SCGCQ00424978 - Is VD Emulated=Yes when emulationType=1
	SCGCQ00436107 - The bootwithpinnedcache logic is backwards, both storcli and the FW are affected
	SCGCQ00448094 - core dump while issuing storcli command ./storcli /c0/fall show all.
	SCGCQ00454971 - storcli /c0 show is not listinf SWR controller
	SCGCQ00471978 - Storcli does not show firmware version using Megacli syntax
	SCGCQ00472000 - Storcli:"storcli /c0/v0 del help" does not show information on normal vd delete
	SCGCQ00314119 - "Drive NCQ setting" field Removed
	SCGCQ00357948 - StorCLI does not display drive information behind the Blackjack (Alta) interposer correctly
	SCGCQ00384644 - iMR_Inv_6.1:StorCLI- StorCLI does not show 'Unsupported/Blocked' state for 4K drives even though FW is not supporting 4K
	SCGCQ00413789 - storcli crashes on having a non PI drive and trying to create pi vd on all the drive
	SCGCQ00442652 - SWR_1.34 - Serial number field is blank in controller information and the same could be updated with N/A in StorCli
	SCGCQ00484230 - "Cli /ex/sx set offline" fails with errcd -1 and message enclosure ID not found.
	SCGCQ00495121 - Unable to set pnpid using the ini file with captal letters mixed in the string
	SCGCQ00330250 - StorCLI compliance with OSSRB recommendation
	SCGCQ00342399 - CSET: (Tbolt PR 211180) Punctured Block Logging Improvements
	SCGCQ00329470 - Implemented the StorCLI commands to erase contents from NVCache
	SCGCQ00488282 - Add ability to change/program PCIDATA in StorClio (CLI for OEMs)
	SCGCQ00501189 - MWCLI. Add command /cX/vX locate
	SCGCQ00323426 - Porting of Vogel 1.0 PRs to storcli phase 2.5 [Libmods]
	SCGCQ00349599 - Refer attached design doc
	SCGCQ00352120 - MWCLI. Add HA support into storcli
	SCGCQ00329469 - Implemented the StorCLI commands to scrub memory on controllers
	SCGCQ00332606 - Display Drive Model number, Serial Number and Firmware Revision as in MSM
	SCGCQ00349548 - Uneven span support is added in StorCLI.
	SCGCQ00351234 - Provide a way to enable or disable 512E using Applications
	SCGCQ00479543 - MWCLI: Need MegaOEM for Solaris x86 and Solaris SPARC
	SCGCQ00333213 - Implemented 128 drive support by using the new ENCL_INFO structures
	SCGCQ00322837 - Printing multiple json objects from different controllers as a single Array
	SCGCQ00332600 - StorCLI compliance with OSSRB recommendation
	SCGCQ00350668 - Create Spanned R0 array (00) in StorCLI
	SCGCQ00381311 - dcmd path changes for supporting the new cachevault api
	SCGCQ00369742 - MWCLI. R10, R50, R60, R00 VD creation
	SCGCQ00381093 - PR SCGCQ00319011: Rebuild time reset
	SCGCQ00433703 - Megacli/storcli support for lmrc driver
	SCGCQ00413856 - remove the "Drive write cache" policy from Pd information.
	SCGCQ00469192 - Aligning with FW for strip calculation for 4K drives
	SCGCQ00471590 - Need to remove storcli /cx show clusterenable and storcli /cx set clusterenable=<value> since FW did not support this in HA
	SCGCQ00504584 - Command "./storcli /call/eall/sall show" fails for second controller with description drive not found.
	SCGCQ00413017 - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
	SCGCQ00376240 - System halts on issuing storcli commands in EFI Environment.
	SCGCQ00437065 - Driver Version is not shown
	SCGCQ00473065 - StorCli_6.1: The SATA drive is dropped while creating a R1 vd using mix of SAS and SATA drives
	SCGCQ00478786 - (v 1.04.11) get a good return code (0) even when it failed
	SCGCQ00471582 - Storclio:Spelling mistake during execution of command 'compare factorysettings'
	SCGCQ00475598 - Storcli:4K -Wrong size updated after performing OCE on 4K Drives .
	SCGCQ00475601 - storcli crash while using the command /cx/vx expand size=xx expandarray
	SCGCQ00414383 - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
	SCGCQ00481849 - StorCLI- StorCLI reports wrong capacitance value for supercap FBU03
	SCGCQ00412593 - Resolving compiler errors for Ctrl-R
	SCGCQ00471048 - HA : StorCLI crash when update drive firmware
	SCGCQ00469390 - MR_Inv_6.1:StoreCLI- StorCLI reports retention time as 0 for supercap FBU02 and FBU03

v1.05.07
	SCGCQ00009501 - MPI2_FW_IMAGE_HEADER is 16 bits too long
	SCGCQ00183867 - MPI2: IO Unit Page 10 structure incorrect
	SCGCQ00364332 - iMR_Inv_6.1:StoreCLI-StoreCLI does not give proper message while trying to create 33rd VD on iMR FURY controller
	SCGCQ00374336 - System halts on issuing storcli commands in EFI Environment.
	SCGCQ00374732 - StorCLI cannot set "bypasserror" or "be"
	SCGCQ00374733 - Storcli does not show 512 strip size in the online help
	SCGCQ00378124 - Porting of AdpRestart Command
	SCGCQ00379046 - MegaCLI help shows Storcli in generic help command
	SCGCQ00379112 - storcli-legacy: The helpfile for "adpfwflash" needs to be updated for "NoVerChk"
	SCGCQ00381383 - Storcli_Invader: "/c0 pause pr" Description message should be sync with command
	SCGCQ00394588 - storcli only displays 1 vd when 7 present on DG view
	SCGCQ00397280 - StorCli_MR:Need to modify the "DIMMER SWITCH" Help Description
	SCGCQ00397877 - SWR: EFI:"Press any key to continue" displays twice.
	SCGCQ00397893 - SWR: EFI: Operating system details shows nothing.
	SCGCQ00399897 - BBU GasGauge Status information should not get printed for TMMC
	SCGCQ00400429 - Storcli help lists unsupported /Fx option for foreign commands
	SCGCQ00406358 - CLI does not provide appropriate error message and error code when secure erase is not supported
	SCGCQ00414300 - StorCli_6.0-The help file for "storcli /cx/fx " is missing.
	SCGCQ00415814 - storcli only associates 38 out of 48 VDs
	SCGCQ00418295 - size=0 VD is getting created with remaining free space, when a VD is present in Drive Group.
	SCGCQ00421114 - Storcli/Storclif/storclio:Help file for Legacy commands displays mrcli instead storcli.
	SCGCQ00421282 - StorCLIO : not able to get or set hwdevice information with storCLIO
	SCGCQ00423757 - EFI: Storcli : Not able to get and set vpd information on TMM module or Supercap
	SCGCQ00435852 - misspelled word in storcli.efi message
	SCGCQ00437754 - Help syntax is not aligned with 80 char per line limits.
	SCGCQ00449926 - Power Shell support for megacli syntax for windows _ Porting
	SCGCQ00450496 - StorcliF : output for the command /c0 compare factorysettings is not in sync with the legacy output.
	SCGCQ00456135 - Unable to create Cachecade VD by referring the syntax in Help file for ''add vd'' .
	SCGCQ00462959 - Slow to create VD in HA Linux
	SCGCQ00466519 - StorCLI_6.1:The help file for "/c0 compare securitykey h" is missing
	SCGCQ00372155 - Certain controller features displayed under "show all" exceeds 80-char limit.
	SCGCQ00374118 - StorCli-"/c0/dall show all "in FreeSpaceDetails legend missing for "ID/VD/AfterVD"
	SCGCQ00374979 - Storcli ld info command displays R10 vd Span Depth to 1.
	SCGCQ00376643 - Fail to set/disable the Disk Cache Policy along with the vd creation.
	SCGCQ00378135 - portings of AdpRestart command
	SCGCQ00378828 - StorCLI-Legacy:'adpbootdrive get' fails to get bootdrive information.
	SCGCQ00385101 - StorCli implementation of AdpRestart Command
	SCGCQ00386429 - StorCLI help file shows /cx/dx show cachecade instead of /cx/dall show cachecade
	SCGCQ00391731 - storcli displays message as firmware flash successfully completed even the flashing is failed.
	SCGCQ00397014 - With one VD as foreign, StorCLI shows all VDs as foreign.
	SCGCQ00397269 - StorCli_5.7: On SuperCap battery ''strat learn" operation is not allowed
	SCGCQ00399002 - handleTokens(tokenListPtr);
	SCGCQ00399387 - Not able to find range for Perf Mode value
	SCGCQ00401663 - help text not working for the command set securitykey
	SCGCQ00412827 - CV (CacheVault) does not support changing bbu mode but StorCLI show option to change bbu mode
	SCGCQ00417435 - StorCLIF : the command /cx get hwdevice fails to get VPD information.
	SCGCQ00417973 - Storclio/Storclif-Detailed help for the command start diag required .
	SCGCQ00423781 - StorCLIF : getting wrong values for get gas gauge information.
	SCGCQ00441696 - StoreCLI- Inconsistent behaviour across different application when creating cachecade VD
	SCGCQ00466251 - HA : StorCLI crash when update drive firmware
	SCGCQ00467119 - SWR_SLES_11_SP3_GM Release validation : In storCli " serial number and FW package Build " fields are showing blank
	SCGCQ00469179 - Aligning with FW for strip calculation for 4K drives
	SCGCQ00372264 - StorCLI: The legend for "phy Error Counters" exceeds the 80-char limit.
	SCGCQ00374377 - GetGGEEPData equivalent syntax is not present in storcli
	SCGCQ00374418 - Storcli : controller information query is displaying the status as failure.
	SCGCQ00375757 - "StorCLI /cx/bbu show modes" show the bbu modes description without the actual bbu mode number
	SCGCQ00377364 - StorCli shows Power Saving Option as enabled, despite controller having power saving option completely disabled.
	SCGCQ00380889 - Not able to set securitykey on controller
	SCGCQ00381100 - MR: not able to create PRL11 using 96 drives.
	SCGCQ00383043 - StorCLI-Invader : The "coercion" mode is not in sync with the legacy values.
	SCGCQ00384644 - iMR_Inv_6.1:StorCLI- StorCLI does not show 'Unsupported/Blocked' state for 4K drives even though FW is not supporting 4K
	SCGCQ00386586 - include support for SWR controllers in non LSI verison of storcli.
	SCGCQ00394127 - Added the command to DOS SCU
	SCGCQ00394883 - StorCli_MR: While Creating RAID1 with four drives command facing the "C0:BAIL_OUT at line 1354"
	SCGCQ00396303 - Cfgclr command fails without force option in Sparc OS
	SCGCQ00400019 - "storcli /c0/dall show" command not working
	SCGCQ00411501 - StorCli_MR: Cache vault Strart learn command displaying twice in the hep file "/c0/cv h"
	SCGCQ00414328 - Perf mode value not getting set when executed along with the other parameters
	SCGCQ00414731 - Checking in StorcliF & storcli0 changes
	SCGCQ00415454 - StorCLI help file does not display "add vd spanned array"
	SCGCQ00420040 - StorCLIF : Not able to read or write factory settings with adpsettings command (legacy command )
	SCGCQ00436928 - Illusive/Bad Data Extracted
	SCGCQ00437762 - Exit code coming as 1 for adpbios (Megacli Syntax)
	SCGCQ00443072 - SWR: In Store Cli if we start any background operation Estimated time left field showing Blank
	SCGCQ00447686 - Storecli does not display complete information for the command ./storecli /c0/p0-x show.
	SCGCQ00456501 - StorcliF: StorcliF and StorcliO crashes when given invalid file for the command /c0 set factorysettings file=filename
	SCGCQ00460861 - MR_Inv_6.1:StorCLI- Gives wrong message after battery retention test command is issued for Supercap FBU03
	SCGCQ00466038 - MR_Inv_6.1:StoreCLI- StorCLI reports retention time as 0 for supercap FBU02 and FBU03
	SCGCQ00469162 - In virtual drives information the Cac filed values are incorrect with regular VD's
	SCGCQ00379157 - StorCLI: the help file for "storcli /cx transform iMR" is missing
	SCGCQ00380143 - The set phy linkspeed operation needs to have the unit(GB/s) mentioned and the Description" column is blank for set and Show.
	SCGCQ00394952 - Segmentation fault hitting while executing the command "/c0 set bgi h "
	SCGCQ00398246 - VD create syntax display improper output.
	SCGCQ00398992 - Command displayed in the same line after "Press any key to continue".
	SCGCQ00402499 - Storecli /c0 show eventloginfo 
	SCGCQ00403335 - Mismatch of "Start Copyback " command in global help file and particular help file of copyback .
	SCGCQ00436538 - pd version is not listing all if PDs are missing
	SCGCQ00442610 - Onfi_patch_6.0:Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
	SCGCQ00447972 - Storcli : adpgetprop command for enableeug/enableeghsp showing success and not getting reflected when we give wrong flag
	SCGCQ00451393 - Megascu adpm0flash command hangs for Dell controllers.
	SCGCQ00462885 - Need to remove storcli /cx show clusterenable and storcli /cx set clusterenable=<value> since FW did not support this in HA
	SCGCQ00364097 - iMR_Inv_6.1:StoreCLI- StoreCLI reports wrong Emulation type for VDs
	SCGCQ00375625 - StorCLI : Displaying failure in the output for querying Dimmer switch information
	SCGCQ00379104 - Not able to get paged view of StorCLI output on VM-Ware Platform
	SCGCQ00390777 - iMR_Inv_6.1:StorCLI- VD creation command does not give any message if we tried to create a PI VD using normal PDs
	SCGCQ00392598 - Pause operation should be sync with in show status of the PR.
	SCGCQ00392686 - For the perfmode command in the help file we are displaying the storcli.exe /cx set perfmode = <value> syntax
	SCGCQ00393442 - Spelling mistake in keyword headlessSafeMode
	SCGCQ00406580 - Adprestart command fails
	SCGCQ00413803 - Factory Command /c0/bbu start retentiontest should not be supported in storcli
	SCGCQ00438350 - Megacli crashes after invoking any command in system with one 9280-8e and 2 quad port qlogic FC cards.
	SCGCQ00457906 - storcli_6.1:The help file for"./storcli /cx/mx set h " is missing
	SCGCQ00374735 - StorCLI crashed when run on a Windows 2008 64-bit with 24GB of RAM and 66 drives attached
	SCGCQ00380746 - Error handling for Drive FW download when the hardware is not supported.
	SCGCQ00384729 - Storcli-Inv-multiple VD's in same DG, setting security using /cx/vall set security=on is Failing for every VD except 1st VD
	SCGCQ00392501 - StorCli_5.7 : "/c0/bbu start learn h " is not showing.
	SCGCQ00394005 - Enabling OCR from StorCLI actually disables the controller property.
	SCGCQ00394375 - Adprestart command fails
	SCGCQ00397920 - StorCli_MR: BBU Strart learn command displaying twice in the "/c0/bbu h"
	SCGCQ00400025 - Storcli shows inaccurate Elapsed Time as recon progresses
	SCGCQ00400640 - Copyright information is showing wrongly
	SCGCQ00408070 - StorCLI does not show both "Current Write Policy" and "Default Write Policy" for VD
	SCGCQ00423347 - Storclif :Segmentation Fault with execution of legacy command BBUMFGSET .
	SCGCQ00423832 - EFI_ Storcli: Cannot set vpd file on controller, EFI hangs and cannot proceed for further operations until reboot
	SCGCQ00433513 - StorcliF : Not able to get or set connector mode on cassiopeia controller
	SCGCQ00436931 - CLI displays VPD data for TMM and Battery/Supercap = ONLY TMM Data Extracted but NOT Supercap Data
	SCGCQ00449134 - Battery Over-temp is not showing correctly.
	SCGCQ00454427 - Storcli_6.1:"press any key to continue" showing twice in the lagacy command
	SCGCQ00464708 - Storcli display total number of VDs in a individual drive group properties.
	SCGCQ00369258 - Description is shown as "None" when using verchk option while flashing fw.
	SCGCQ00392053 - MegaCLI and StorCLI should display "Estimated Time Left" in hours, days and minutes format.
	SCGCQ00396665 - StorcLi_5.7: Remove the description for "Ra=Read Ahead Adaptive" in VD show info.
	SCGCQ00397663 - StorCli_MR: While creating VD using default values FW allows read policy as"Ra=Read Ahead Adaptive" as against PR-317400
	SCGCQ00399443 - StorCLI App Crash while execution of event info for vd ccincon
	SCGCQ00402910 - StorCli_6.0:Raid level can be created even without delimiter(i.e size=1gb1gb1gb1gb)
	SCGCQ00424978 - Is VD Emulated=Yes when emulationType=1
	SCGCQ00436107 - The bootwithpinnedcache logic is backwards, both storcli and the FW are affected
	SCGCQ00448094 - core dump while issuing storcli command ./storcli /c0/fall show all.
	SCGCQ00454971 - storcli /c0 show is not listinf SWR controller
	SCGCQ00378448 - StorCLI reports incorrect message when download a firmware image to the controller with pinned cache
	SCGCQ00395178 - storcli doesn't support legacy MegaCli elf commands
	SCGCQ00400139 - StorCLI shows date of manufacture in non-convention format
	SCGCQ00413789 - storcli crashes on having a non PI drive and trying to create pi vd on all the drive
	SCGCQ00422006 - Storcli crashes when given wrong in put file to set VPD on controller
	SCGCQ00442444 - MR_Inv_6.1:StoreCLI- StorCLI gives wrong info when preserved cache is generated on 4K VD (./storcli /c0 show preservedcache).
	SCGCQ00442652 - SWR_1.34 - Serial number field is blank in controller information and the same could be updated with N/A in StorCli
	SCGCQ00066241 - MPI 2.5: Power Management
	SCGCQ00308453 - MPI2: IR reporting Elapsed Seconds
	SCGCQ00299943 - MPI2: add IOCExceptions bit for Partial Memory Failure
	SCGCQ00250721 - MPI2: Update Hard Reset Algorithm with new timings
	SCGCQ00209048 - MPI2: Return Port info in the SAS Device Status Change Event
	SCGCQ00201727 - MPI2: Add spin-up disable bit to SAS IO Unit Page 4
	SCGCQ00201203 - MPI2: Remove/Obsolete MPI Power Management Control Feature PCIE_LINK
	SCGCQ00194293 - MPI2: product specific range for extended image type
	SCGCQ00116336 - Gen 3: method to enable/disable FastPath capability on a per-device basis
	SCGCQ00125672 - Gen 3: add 12Gb/s option for link rate
	SCGCQ00125683 - MPI2: add Link Rate of UNSUPPORTED_PHY_ATTACHED
	SCGCQ00136677 - Gen3: add optional vendor-unique region to MPI25_SCSI_IO_REQUEST structure
	SCGCQ00137514 - MPI2: add PCI Device ID for Warhawk
	SCGCQ00138259 - MPI2: add alternative defines for SGE Direction bit
	SCGCQ00140397 - MPI2: modify Host Based Discovery Action Request
	SCGCQ00141834 - MPI2: ability to disable SATA NCQ on a per-device basis
	SCGCQ00155192 - MPI 2.5: update PCI Device Ids for Invader / Fury
	SCGCQ00157968 - MPI2: Add new Config Page Type - Extended Manufacturing
	SCGCQ00159010 - MPI2: MFG 7 update: method to link ISTWI devices, GPIO, PHYs of a SAS connector
	SCGCQ00160485 - MPI2: Change MPI Simple SGE Local bit description and IEEE Chain Flags to match HW
	SCGCQ00161661 - MPI2: Add IOC Temperature Monitoring Capability
	SCGCQ00162562 - MPI2: rework Pinout field of ConnectorInfo for MFG Page 7
	SCGCQ00162597 - MPI2: reserve some FWDownload ImageType values for product-specific use
	SCGCQ00163413 - MPI2: IOUnit page 7: Add new fields for Board temperature
	SCGCQ00163641 - MPI 2.5: SCSI Initiator I/O path counters (SAS IO Unit Page 16)
	SCGCQ00164407 - MPI 2.5: review SGE Flags for Local bit and Data Location Address Space changes
	SCGCQ00166171 - MPI2: new event for NOTIFY(Enable Spinup)
	SCGCQ00176893 - MPI 2.5: new Power Performance Change Event to report changes to global power management mode
	SCGCQ00177635 - MPI 2.5: report offset of first EEDP error in SCSI IO Reply
	SCGCQ00268818 - Allow for MPI 2.5 IEEE Chain Element in SATA Passthrough Request
	SCGCQ00283196 - Toolbox Diagnostic CLI Request now uses IEEE SGL, including chain elements
	SCGCQ00378774 - new storcli object is added to storcli to represent cachevault
	SCGCQ00413314 - Implement storclif commands - get/set hwdevice and configpage
	SCGCQ00413317 - Implementation of StorCLIF command for AdpSetSubOEMId XX -aN and AdpGetSubOEMId -aN
	SCGCQ00421090 - Added the HA code to MR5.8 stream
	SCGCQ00425077 - Set factory default command in StorCLI
	SCGCQ00283198 - MPI2: Toolbox Diagnostic CLI Tool Request may now use chain elements in the SGL
	SCGCQ00258327 - MPI2: Reserve Product Specific range for Event codes
	SCGCQ00229719 - MPI2: BIOS Page 1 additions for UEFI HII
	SCGCQ00228572 - MPI2: add 4K sectors supported bit to IOC Page 6 CapabilitiesFlags field
	SCGCQ00203886 - MPI2: New RAID Action (COMPATIBILITY_CHECK)
	SCGCQ00194461 - MPI2: Add auto reserve and 8-kbit seeprom support to ISTWII
	SCGCQ00128142 - Gen 3: update MPI v2.5 header files
	SCGCQ00132183 - MPI2: add optional vendor-unique region to MPI2_SCSI_IO_REQUEST structure
	SCGCQ00136201 - MPI2 - additional IR status information
	SCGCQ00142578 - MPI2: obsolete MPI2_IOUNITPAGE1_MULTI_PATHING
	SCGCQ00169936 - MPI 2.5: remove Command Determines Data Direction bit from SCSI IO
	SCGCQ00172984 - MPI2: for SRIOV, allow PF to access config pages for other VFs
	SCGCQ00175997 - MPI2: Add IO Unit Page 10 - Host Credit Balancing
	SCGCQ00218764 - MPI2: new name for SCSI IO Request Control bits
	SCGCQ00227491 - MPI 2.5: IR - new Raid Action to enable the Fast Path
	SCGCQ00209055 - MPI2: create product-specific range for RAID Action Request
	SCGCQ00125496 - Gen 3: remove Release On Full option for diag trace buffer
	SCGCQ00159395 - MPI 2.5: Obsolete MPI2_RAID_VOL_CREATION_BACKGROUND_INIT
	SCGCQ00175743 - MPI2: method to communicate between hosts on virtual functions
	SCGCQ00433477 - Mapping of MegaCLI(DPMenable(set/get) & ForceSGPIO(get/set) command to StorCLI( (show/set -> DPM) & (show/set SGPIOforce))
	SCGCQ00438735 - Changed the storcli syntaxes as Suggested by PDM's and FAE's.
	SCGCQ00157982 - MPI 2.5: Chain SGL Segment sizes
	SCGCQ00399602 - storcli support for LSI and OEM, factory
	SCGCQ00412981 - implementation of StorcliF commands for adpsetsasa,adpdiag,adpshutdown
	SCGCQ00435665 - storcli mapping for the missing legacy commands
	SCGCQ00125662 - MPI2: review Task Set Full handling
	SCGCQ00353002 - Signed FW Update
	SCGCQ00375811 - Need MegaSCU for changes in MFC
	SCGCQ00380155 - Undo - blocking firmware update for drives behind ALTA
	SCGCQ00413337 - MWCLI. storcli builds for LSI and OEM factory, please check description.
	SCGCQ00137489 - MPI2: bring Diagnostic Data Upload Tool forward from MPI v1.5
	SCGCQ00379169 - Remove support for flashing firmware on PDs behind ALTA
	SCGCQ00413064 - Implementation of MegaSCU commands in storcli syntax
	SCGCQ00413432 - Implementation of commands mentioned in the desc below
	SCGCQ00441143 - Implementing Bad block management related commands in storcli.
	SCGCQ00369601 - MWCLI. Add -adpbattest capability to EFI CLI
	SCGCQ00369604 - Rebuild time reset
	SCGCQ00381311 - dcmd path chagnes for supporting the new cachevault api
	SCGCQ00419161 - Implementation of StorCLIO command for ADPMFGSET -f file a0 in storcli
	SCGCQ00419336 - Implementation of setPcilinkspeed command in storCLIF
	SCGCQ00423256 - RRB 45 - CLI Reporting of TMM VPD
	SCGCQ00369742 - MWCLI. R10, R50, R60, R00 VD creation
	SCGCQ00381093 - PR SCGCQ00319011: Rebuild time reset
	SCGCQ00433703 - Megacli/storcli support for lmrc driver
	SCGCQ00434744 - Equivalent storcli command implementation of MegaCLI -AdpGetPciInfo -aN|-a0,1,2|-aALL
	SCGCQ00447069 - Implementation of StorCLIO command for Adpnvram clear a0 in storclio as well as support legacy command
	SCGCQ00413330 - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
	SCGCQ00413856 - remove the "Drive write cache" policy from Pd information.
	SCGCQ00417917 - UEFI StorCli doesn't show the correct UEFI Driver Version
	SCGCQ00413017 - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
	SCGCQ00413888 - StorCli_6.0-The help file for "storcli /cx/dx set security " is missing
	SCGCQ00376240 - System halts on issuing storcli commands in EFI Environment.
	SCGCQ00411384 - Unable to start migration from R0 to R5
	SCGCQ00411614 - hits segmentation fault while creating multiple Vd's on Raid 10.
	SCGCQ00413311 - Cannot change or update controller date and time in MegaSCU
	SCGCQ00437065 - Driver Version is not shown
	SCGCQ00375839 - StorCLI: The legend for "phy Error Counters" exceeds the 80-char limit.
	SCGCQ00411449 - Improper output when configure R10 VD.
	SCGCQ00414863 - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
	SCGCQ00413041 - Getting error message while installing or upgrading on Linux platform
	SCGCQ00458499 - Block configuration with unsupported strip element sizes
	SCGCQ00414383 - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
	SCGCQ00391744 - StorCli-"show ctrlcount" help is not displaying.
	SCGCQ00412593 - Resolving compiler errors for Ctrl-R
	SCGCQ00425263 - storcli /c0 show all : did not have HA information+request to add additional info


v1.04.07
	SCGCQ00364332 - StoreCLI does not give proper message while trying to create 33rd VD on iMR FURY controller
	SCGCQ00374336 - System halts on issuing storcli commands in EFI Environment.
	SCGCQ00374732 - StorCLI cannot set "bypasserror" or "be"
	SCGCQ00374733 - Storcli does not show 512 strip size in the online help
	SCGCQ00378124 - Porting of AdpRestart Command
	SCGCQ00372155 - Certain controller features displayed under "show all" exceeds 80-char limit.
	SCGCQ00374118 - StorCli-"/c0/dall show all "in FreeSpaceDetails legend missing for "ID/VD/AfterVD"
	SCGCQ00378135 - portings of AdpRestart command
	SCGCQ00378828 - StorCLI-Legacy:'adpbootdrive get' fails to get bootdrive information.
	SCGCQ00372264 - StorCLI: The legend for "phy Error Counters" exceeds the 80-char limit.
	SCGCQ00374418 - Storcli : controller information query for OEM controller is displaying the status as failure.
	SCGCQ00375757 - "StorCLI /cx/bbu show modes" show the bbu modes description without the actual bbu mode number
	SCGCQ00374735 - StorCLI crashed when run on a Windows 2008 64-bit with 24GB of RAM and 66 drives attached
	SCGCQ00380746 - Error handling for Drive FW download when the hardware is not supported.
	SCGCQ00369258 - Description is shown as "None" when using verchk option while flashing fw.
	SCGCQ00378448 - StorCLI reports incorrect message when download a firmware image to the controller with pinned cache
	SCGCQ00375811 - Need MegaSCU for changes in MFC
	SCGCQ00380155 - Undo - blocking firmware update for drives behind interposer
	SCGCQ00379169 - Remove support for flashing firmware on PDs behind interposer
	SCGCQ00375839 - StorCLI: The legend for "phy Error Counters" exceeds the 80-char limit.

v1.03.11 - Initial release

*Third-party trademarks are the property of their respective owners.
