Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_lapic_reg_t Struct Reference
SoC Registers (SE)

APIC register block type. More...

`#include <qm_soc_regs.h>`

## Data Fields
QM_RW apic_reg_pad_t | id
| LAPIC ID.
QM_RW apic_reg_pad_t | version
| LAPIC version.
QM_RW apic_reg_pad_t | tpr
| Task priority.
QM_RW apic_reg_pad_t | apr
| Arbitration priority.
QM_RW apic_reg_pad_t | ppr
| Processor priority.
QM_RW apic_reg_pad_t | eoi
| End of interrupt.
QM_RW apic_reg_pad_t | rrd
| Remote read.
QM_RW apic_reg_pad_t | ldr
| Logical destination.
QM_RW apic_reg_pad_t | dfr
| Destination format.
QM_RW apic_reg_pad_t | svr
| Spurious vector.
QM_RW apic_reg_pad_t | isr [8]
| In-service.
QM_RW apic_reg_pad_t | tmr [8]
| Trigger mode.
QM_RW apic_reg_pad_t | irr [8]
| Interrupt request.
QM_RW apic_reg_pad_t | esr
| Error status.
QM_RW apic_reg_pad_t | lvtcmci
| Corrected Machine Check vector.
QM_RW apic_reg_pad_t | icr [2]
| Interrupt command.
QM_RW apic_reg_pad_t | lvttimer
| Timer vector.
QM_RW apic_reg_pad_t | lvtts
| Thermal sensor vector.
QM_RW apic_reg_pad_t | lvtpmcr
| Perfmon counter vector.
QM_RW apic_reg_pad_t | lvtlint0
| Local interrupt 0 vector.
QM_RW apic_reg_pad_t | lvtlint1
| Local interrupt 1 vector.
QM_RW apic_reg_pad_t | lvterr
| Error vector.
QM_RW apic_reg_pad_t | timer_icr
| Timer initial count.
QM_RW apic_reg_pad_t | timer_ccr
| Timer current count.
QM_RW apic_reg_pad_t | timer_dcr
| Timer divide configuration.

## Detailed Description

APIC register block type.

Definition at line 224 of file qm_soc_regs.h.