Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_aonpt_config_t Struct Reference
Always-on Counters

QM Always-on Periodic Timer configuration type. More...

`#include <qm_aon_counters.h>`

## Data Fields
uint32_t | count
| Time to count down from in clock cycles. More...
bool | int_en
| Enable/disable the interrupts. More...
void(* | callback )(void *data)
| User callback. More...
void * | callback_data
| Callback data. More...

## Detailed Description

QM Always-on Periodic Timer configuration type.

Definition at line 40 of file qm_aon_counters.h.

## Field Documentation

void(* qm_aonpt_config_t::callback)(void *data)

User callback.

Parameters

  [in] | data | User defined data.

Definition at line 49 of file qm_aon_counters.h.

Referenced by qm_aonpt_set_config().

void* qm_aonpt_config_t::callback_data

Callback data.

Definition at line 50 of file qm_aon_counters.h.

Referenced by qm_aonpt_set_config().

uint32_t qm_aonpt_config_t::count

Time to count down from in clock cycles.

Definition at line 41 of file qm_aon_counters.h.

Referenced by qm_aonpt_set_config().

bool qm_aonpt_config_t::int_en

Enable/disable the interrupts.

Definition at line 42 of file qm_aon_counters.h.

Referenced by qm_aonpt_set_config().