Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- File List

qm_pin_functions.h
1 /*
2 * {% copyright %}
3 */
4
5 #ifndef __QM_PIN_FUNCTIONS_H__
6 #define __QM_PIN_FUNCTIONS_H__
7
8 /**
9 * SoC Pins definition.
10 *
11 * @defgroup group SOC_PINS
12 * @{
13 */
14
15 #include "qm_common.h"
16
17 /*
18 * This file provides an abstraction layer for pin numbers and pin functions.
19 */
20
21 /* Package pins to pin IDs. */
22
23 /* BGA144 package. */
24 #define QM_PIN_ID_BGA144_D12 QM_PIN_ID_0
25 #define QM_PIN_ID_BGA144_E10 QM_PIN_ID_1
26 #define QM_PIN_ID_BGA144_E11 QM_PIN_ID_2
27 #define QM_PIN_ID_BGA144_E12 QM_PIN_ID_3
28 #define QM_PIN_ID_BGA144_F9 QM_PIN_ID_4
29 #define QM_PIN_ID_BGA144_F10 QM_PIN_ID_5
30 #define QM_PIN_ID_BGA144_L9 QM_PIN_ID_6
31 #define QM_PIN_ID_BGA144_K8 QM_PIN_ID_7
32 #define QM_PIN_ID_BGA144_F11 QM_PIN_ID_8
33 #define QM_PIN_ID_BGA144_F12 QM_PIN_ID_9
34 #define QM_PIN_ID_BGA144_G9 QM_PIN_ID_10
35 #define QM_PIN_ID_BGA144_G10 QM_PIN_ID_11
36 #define QM_PIN_ID_BGA144_G11 QM_PIN_ID_12
37 #define QM_PIN_ID_BGA144_G12 QM_PIN_ID_13
38 #define QM_PIN_ID_BGA144_K10 QM_PIN_ID_14
39 #define QM_PIN_ID_BGA144_K9 QM_PIN_ID_15
40 #define QM_PIN_ID_BGA144_H11 QM_PIN_ID_16
41 #define QM_PIN_ID_BGA144_H12 QM_PIN_ID_17
42 #define QM_PIN_ID_BGA144_E8 QM_PIN_ID_18
43 #define QM_PIN_ID_BGA144_E9 QM_PIN_ID_19
44 #define QM_PIN_ID_BGA144_C12 QM_PIN_ID_20
45 #define QM_PIN_ID_BGA144_B12 QM_PIN_ID_21
46 #define QM_PIN_ID_BGA144_D11 QM_PIN_ID_22
47 #define QM_PIN_ID_BGA144_C11 QM_PIN_ID_23
48 #define QM_PIN_ID_BGA144_A11 QM_PIN_ID_24
49 #define QM_PIN_ID_BGA144_B11 QM_PIN_ID_25
50 #define QM_PIN_ID_BGA144_C10 QM_PIN_ID_26
51 #define QM_PIN_ID_BGA144_D10 QM_PIN_ID_27
52 #define QM_PIN_ID_BGA144_A10 QM_PIN_ID_28
53 #define QM_PIN_ID_BGA144_B10 QM_PIN_ID_29
54 #define QM_PIN_ID_BGA144_C9 QM_PIN_ID_30
55 #define QM_PIN_ID_BGA144_A9 QM_PIN_ID_31
56 #define QM_PIN_ID_BGA144_D9 QM_PIN_ID_32
57 #define QM_PIN_ID_BGA144_B9 QM_PIN_ID_33
58 #define QM_PIN_ID_BGA144_C8 QM_PIN_ID_34
59 #define QM_PIN_ID_BGA144_A8 QM_PIN_ID_35
60 #define QM_PIN_ID_BGA144_B7 QM_PIN_ID_36
61 #define QM_PIN_ID_BGA144_B8 QM_PIN_ID_37
62 #define QM_PIN_ID_BGA144_C7 QM_PIN_ID_38
63 #define QM_PIN_ID_BGA144_A7 QM_PIN_ID_39
64 #define QM_PIN_ID_BGA144_D8 QM_PIN_ID_40
65 #define QM_PIN_ID_BGA144_D7 QM_PIN_ID_41
66 #define QM_PIN_ID_BGA144_D6 QM_PIN_ID_42
67 #define QM_PIN_ID_BGA144_B6 QM_PIN_ID_43
68 #define QM_PIN_ID_BGA144_A6 QM_PIN_ID_44
69 #define QM_PIN_ID_BGA144_C6 QM_PIN_ID_45
70 #define QM_PIN_ID_BGA144_B5 QM_PIN_ID_46
71 #define QM_PIN_ID_BGA144_A5 QM_PIN_ID_47
72 #define QM_PIN_ID_BGA144_D5 QM_PIN_ID_48
73 #define QM_PIN_ID_BGA144_C5 QM_PIN_ID_49
74 #define QM_PIN_ID_BGA144_B4 QM_PIN_ID_50
75 #define QM_PIN_ID_BGA144_D4 QM_PIN_ID_51
76 #define QM_PIN_ID_BGA144_A4 QM_PIN_ID_52
77 #define QM_PIN_ID_BGA144_C4 QM_PIN_ID_53
78 #define QM_PIN_ID_BGA144_B3 QM_PIN_ID_54
79 #define QM_PIN_ID_BGA144_A3 QM_PIN_ID_55
80 #define QM_PIN_ID_BGA144_C3 QM_PIN_ID_56
81 #define QM_PIN_ID_BGA144_D3 QM_PIN_ID_57
82 #define QM_PIN_ID_BGA144_E4 QM_PIN_ID_58
83 #define QM_PIN_ID_BGA144_E3 QM_PIN_ID_59
84 #define QM_PIN_ID_BGA144_B2 QM_PIN_ID_60
85 #define QM_PIN_ID_BGA144_Q2 QM_PIN_ID_61
86 #define QM_PIN_ID_BGA144_C2 QM_PIN_ID_62
87 #define QM_PIN_ID_BGA144_D2 QM_PIN_ID_63
88 #define QM_PIN_ID_BGA144_B1 QM_PIN_ID_64
89 #define QM_PIN_ID_BGA144_E2 QM_PIN_ID_65
90 #define QM_PIN_ID_BGA144_C1 QM_PIN_ID_66
91 #define QM_PIN_ID_BGA144_D1 QM_PIN_ID_67
92 #define QM_PIN_ID_BGA144_E1 QM_PIN_ID_68
93
94 /* WLCSP144 package. */
95 #define QM_PIN_ID_WLCSP144_F2 QM_PIN_ID_0
96 #define QM_PIN_ID_WLCSP144_G4 QM_PIN_ID_1
97 #define QM_PIN_ID_WLCSP144_H5 QM_PIN_ID_2
98 #define QM_PIN_ID_WLCSP144_J6 QM_PIN_ID_3
99 #define QM_PIN_ID_WLCSP144_K6 QM_PIN_ID_4
100 #define QM_PIN_ID_WLCSP144_L6 QM_PIN_ID_5
101 #define QM_PIN_ID_WLCSP144_H4 QM_PIN_ID_6
102 #define QM_PIN_ID_WLCSP144_G3 QM_PIN_ID_7
103 #define QM_PIN_ID_WLCSP144_L5 QM_PIN_ID_8
104 #define QM_PIN_ID_WLCSP144_M5 QM_PIN_ID_9
105 #define QM_PIN_ID_WLCSP144_K5 QM_PIN_ID_10
106 #define QM_PIN_ID_WLCSP144_G1 QM_PIN_ID_11
107 #define QM_PIN_ID_WLCSP144_J4 QM_PIN_ID_12
108 #define QM_PIN_ID_WLCSP144_G2 QM_PIN_ID_13
109 #define QM_PIN_ID_WLCSP144_F1 QM_PIN_ID_14
110 #define QM_PIN_ID_WLCSP144_J5 QM_PIN_ID_15
111 #define QM_PIN_ID_WLCSP144_l4 QM_PIN_ID_16
112 #define QM_PIN_ID_WLCSP144_M4 QM_PIN_ID_17
113 #define QM_PIN_ID_WLCSP144_K4 QM_PIN_ID_18
114 #define QM_PIN_ID_WLCSP144_B2 QM_PIN_ID_19
115 #define QM_PIN_ID_WLCSP144_C1 QM_PIN_ID_20
116 #define QM_PIN_ID_WLCSP144_C2 QM_PIN_ID_21
117 #define QM_PIN_ID_WLCSP144_D1 QM_PIN_ID_22
118 #define QM_PIN_ID_WLCSP144_D2 QM_PIN_ID_23
119 #define QM_PIN_ID_WLCSP144_E1 QM_PIN_ID_24
120 #define QM_PIN_ID_WLCSP144_E2 QM_PIN_ID_25
121 #define QM_PIN_ID_WLCSP144_B3 QM_PIN_ID_26
122 #define QM_PIN_ID_WLCSP144_A3 QM_PIN_ID_27
123 #define QM_PIN_ID_WLCSP144_C3 QM_PIN_ID_28
124 #define QM_PIN_ID_WLCSP144_E3 QM_PIN_ID_29
125 #define QM_PIN_ID_WLCSP144_D3 QM_PIN_ID_30
126 #define QM_PIN_ID_WLCSP144_D4 QM_PIN_ID_31
127 #define QM_PIN_ID_WLCSP144_C4 QM_PIN_ID_32
128 #define QM_PIN_ID_WLCSP144_B4 QM_PIN_ID_33
129 #define QM_PIN_ID_WLCSP144_A4 QM_PIN_ID_34
130 #define QM_PIN_ID_WLCSP144_B5 QM_PIN_ID_35
131 #define QM_PIN_ID_WLCSP144_C5 QM_PIN_ID_36
132 #define QM_PIN_ID_WLCSP144_D5 QM_PIN_ID_37
133 #define QM_PIN_ID_WLCSP144_E5 QM_PIN_ID_38
134 #define QM_PIN_ID_WLCSP144_E4 QM_PIN_ID_39
135 #define QM_PIN_ID_WLCSP144_A6 QM_PIN_ID_40
136 #define QM_PIN_ID_WLCSP144_B6 QM_PIN_ID_41
137 #define QM_PIN_ID_WLCSP144_C6 QM_PIN_ID_42
138 #define QM_PIN_ID_WLCSP144_D6 QM_PIN_ID_43
139 #define QM_PIN_ID_WLCSP144_E6 QM_PIN_ID_44
140 #define QM_PIN_ID_WLCSP144_D7 QM_PIN_ID_45
141 #define QM_PIN_ID_WLCSP144_C7 QM_PIN_ID_46
142 #define QM_PIN_ID_WLCSP144_B7 QM_PIN_ID_47
143 #define QM_PIN_ID_WLCSP144_A7 QM_PIN_ID_48
144 #define QM_PIN_ID_WLCSP144_B8 QM_PIN_ID_49
145 #define QM_PIN_ID_WLCSP144_A8 QM_PIN_ID_50
146 #define QM_PIN_ID_WLCSP144_B9 QM_PIN_ID_51
147 #define QM_PIN_ID_WLCSP144_A9 QM_PIN_ID_52
148 #define QM_PIN_ID_WLCSP144_C9 QM_PIN_ID_53
149 #define QM_PIN_ID_WLCSP144_D9 QM_PIN_ID_54
150 #define QM_PIN_ID_WLCSP144_D8 QM_PIN_ID_55
151 #define QM_PIN_ID_WLCSP144_E7 QM_PIN_ID_56
152 #define QM_PIN_ID_WLCSP144_E9 QM_PIN_ID_57
153 #define QM_PIN_ID_WLCSP144_E8 QM_PIN_ID_58
154 #define QM_PIN_ID_WLCSP144_A10 QM_PIN_ID_59
155 #define QM_PIN_ID_WLCSP144_B10 QM_PIN_ID_60
156 #define QM_PIN_ID_WLCSP144_C10 QM_PIN_ID_61
157 #define QM_PIN_ID_WLCSP144_D10 QM_PIN_ID_62
158 #define QM_PIN_ID_WLCSP144_E10 QM_PIN_ID_63
159 #define QM_PIN_ID_WLCSP144_D11 QM_PIN_ID_64
160 #define QM_PIN_ID_WLCSP144_C11 QM_PIN_ID_65
161 #define QM_PIN_ID_WLCSP144_B11 QM_PIN_ID_66
162 #define QM_PIN_ID_WLCSP144_D12 QM_PIN_ID_67
163 #define QM_PIN_ID_WLCSP144_C12 QM_PIN_ID_68
164
165 /* Pin function name to pin function number. */
166
167 /* Pin ID 0. */
168 #define QM_PIN_0_FN_GPIO_0 QM_PMUX_FN_0
169 #define QM_PIN_0_FN_AIN_0 QM_PMUX_FN_1
170 #define QM_PIN_0_FN_SPI_S_CS_B QM_PMUX_FN_2
171
172 /* Pin ID 1. */
173 #define QM_PIN_1_FN_GPIO_1 QM_PMUX_FN_0
174 #define QM_PIN_1_FN_AIN_1 QM_PMUX_FN_1
175 #define QM_PIN_1_FN_SPI_S_MISO QM_PMUX_FN_2
176
177 /* Pin ID 2. */
178 #define QM_PIN_2_FN_GPIO_2 QM_PMUX_FN_0
179 #define QM_PIN_2_FN_AIN_2 QM_PMUX_FN_1
180 #define QM_PIN_2_FN_SPI_S_SCK QM_PMUX_FN_2
181
182 /* Pin ID 3. */
183 #define QM_PIN_3_FN_GPIO_3 QM_PMUX_FN_0
184 #define QM_PIN_3_FN_AIN_3 QM_PMUX_FN_1
185 #define QM_PIN_3_FN_SPI_S_MOSI QM_PMUX_FN_2
186
187 /* Pin ID 4. */
188 #define QM_PIN_4_FN_GPIO_4 QM_PMUX_FN_0
189 #define QM_PIN_4_FN_AIN_4 QM_PMUX_FN_1
190
191 /* Pin ID 5. */
192 #define QM_PIN_5_FN_GPIO_5 QM_PMUX_FN_0
193 #define QM_PIN_5_FN_AIN_5 QM_PMUX_FN_1
194
195 /* Pin ID 6. */
196 #define QM_PIN_6_FN_GPIO_6 QM_PMUX_FN_0
197 #define QM_PIN_6_FN_AIN_6 QM_PMUX_FN_1
198
199 /* Pin ID 7. */
200 #define QM_PIN_7_FN_GPIO_7 QM_PMUX_FN_0
201 #define QM_PIN_7_FN_AIN_7 QM_PMUX_FN_1
202
203 /* Pin ID 8. */
204 #define QM_PIN_8_FN_GPIO_SS_0 QM_PMUX_FN_0
205 #define QM_PIN_8_FN_AIN_8 QM_PMUX_FN_1
206 #define QM_PIN_8_FN_UART1_CTS QM_PMUX_FN_2
207
208 /* Pin ID 9. */
209 #define QM_PIN_9_FN_GPIO_SS_1 QM_PMUX_FN_0
210 #define QM_PIN_9_FN_AIN_9 QM_PMUX_FN_1
211 #define QM_PIN_9_FN_UART1_RTS QM_PMUX_FN_2
212
213 /* Pin ID 10. */
214 #define QM_PIN_10_FN_GPIO_SS_2 QM_PMUX_FN_0
215 #define QM_PIN_10_FN_AIN_10 QM_PMUX_FN_1
216
217 /* Pin ID 11. */
218 #define QM_PIN_11_FN_GPIO_SS_3 QM_PMUX_FN_0
219 #define QM_PIN_11_FN_AIN_11 QM_PMUX_FN_1
220
221 /* Pin ID 12. */
222 #define QM_PIN_12_FN_GPIO_SS_4 QM_PMUX_FN_0
223 #define QM_PIN_12_FN_AIN_12 QM_PMUX_FN_1
224
225 /* Pin ID 13. */
226 #define QM_PIN_13_FN_GPIO_SS_5 QM_PMUX_FN_0
227 #define QM_PIN_13_FN_AIN_13 QM_PMUX_FN_1
228
229 /* Pin ID 14. */
230 #define QM_PIN_14_FN_GPIO_SS_6 QM_PMUX_FN_0
231 #define QM_PIN_14_FN_AIN_14 QM_PMUX_FN_1
232
233 /* Pin ID 15. */
234 #define QM_PIN_15_FN_GPIO_SS_7 QM_PMUX_FN_0
235 #define QM_PIN_15_FN_AIN_15 QM_PMUX_FN_1
236
237 /* Pin ID 16. */
238 #define QM_PIN_16_FN_GPIO_SS_8 QM_PMUX_FN_0
239 #define QM_PIN_16_FN_AIN_16 QM_PMUX_FN_1
240 #define QM_PIN_16_FN_UART1_TXD QM_PMUX_FN_2
241
242 /* Pin ID 17. */
243 #define QM_PIN_17_FN_GPIO_SS_9 QM_PMUX_FN_0
244 #define QM_PIN_17_FN_AIN_17 QM_PMUX_FN_1
245 #define QM_PIN_17_FN_UART1_RXD QM_PMUX_FN_2
246
247 /* Pin ID 18. */
248 #define QM_PIN_18_FN_UART0_RXD QM_PMUX_FN_0
249 #define QM_PIN_18_FN_AIN_18 QM_PMUX_FN_1
250
251 /* Pin ID 19. */
252 #define QM_PIN_19_FN_UART0_TXD QM_PMUX_FN_0
253 #define QM_PIN_19_FN_GPIO_31 QM_PMUX_FN_1
254
255 /* Pin ID 20. */
256 #define QM_PIN_20_FN_I2C0_SCL QM_PMUX_FN_0
257
258 /* Pin ID 21. */
259 #define QM_PIN_21_FN_I2C0_SDA QM_PMUX_FN_0
260
261 /* Pin ID 22. */
262 #define QM_PIN_22_FN_I2C1_SCL QM_PMUX_FN_0
263
264 /* Pin ID 23. */
265 #define QM_PIN_23_FN_I2C1_SDA QM_PMUX_FN_0
266
267 /* Pin ID 24. */
268 #define QM_PIN_24_FN_I2C0_SS_SDA QM_PMUX_FN_0
269
270 /* Pin ID 25. */
271 #define QM_PIN_25_FN_I2C0_SS_SCL QM_PMUX_FN_0
272
273 /* Pin ID 26. */
274 #define QM_PIN_26_FN_I2C1_SS_SDA QM_PMUX_FN_0
275
276 /* Pin ID 27. */
277 #define QM_PIN_27_FN_I2C1_SS_SCL QM_PMUX_FN_0
278
279 /* Pin ID 28. */
280 #define QM_PIN_28_FN_SPI0_SS_MISO QM_PMUX_FN_0
281
282 /* Pin ID 29. */
283 #define QM_PIN_29_FN_SPI0_SS_MOSI QM_PMUX_FN_0
284
285 /* Pin ID 30. */
286 #define QM_PIN_30_FN_SPI0_SS_SCK QM_PMUX_FN_0
287
288 /* Pin ID 31. */
289 #define QM_PIN_31_FN_SPI0_SS_CS_B_0 QM_PMUX_FN_0
290
291 /* Pin ID 32. */
292 #define QM_PIN_32_FN_SPI0_SS_CS_B_1 QM_PMUX_FN_0
293
294 /* Pin ID 33. */
295 #define QM_PIN_33_FN_SPI0_SS_CS_B_2 QM_PMUX_FN_0
296 #define QM_PIN_33_FN_GPIO_29 QM_PMUX_FN_1
297
298 /* Pin ID 34. */
299 #define QM_PIN_34_FN_SPI0_SS_CS_B_3 QM_PMUX_FN_0
300 #define QM_PIN_34_FN_GPIO_30 QM_PMUX_FN_1
301
302 /* Pin ID 35. */
303 #define QM_PIN_35_FN_SPI1_SS_MISO QM_PMUX_FN_0
304
305 /* Pin ID 36. */
306 #define QM_PIN_36_FN_SPI1_SS_MOSI QM_PMUX_FN_0
307
308 /* Pin ID 37. */
309 #define QM_PIN_37_FN_SPI1_SS_SCK QM_PMUX_FN_0
310
311 /* Pin ID 38. */
312 #define QM_PIN_38_FN_SPI1_SS_CS_B_0 QM_PMUX_FN_0
313
314 /* Pin ID 39. */
315 #define QM_PIN_39_FN_SPI1_SS_CS_B_1 QM_PMUX_FN_0
316
317 /* Pin ID 40. */
318 #define QM_PIN_40_FN_SPI1_SS_CS_B_2 QM_PMUX_FN_0
319 #define QM_PIN_40_FN_UART0_CTS_B QM_PMUX_FN_1
320
321 /* Pin ID 41. */
322 #define QM_PIN_41_FN_SPI1_SS_CS_B_3 QM_PMUX_FN_0
323 #define QM_PIN_41_FN_UART0_RTS_B QM_PMUX_FN_1
324
325 /* Pin ID 42. */
326 #define QM_PIN_42_FN_GPIO_8 QM_PMUX_FN_0
327 #define QM_PIN_42_FN_SPI1_M_SCK QM_PMUX_FN_1
328
329 /* Pin ID 43. */
330 #define QM_PIN_43_FN_GPIO_9 QM_PMUX_FN_0
331 #define QM_PIN_43_FN_SPI1_M_MISO QM_PMUX_FN_1
332
333 /* Pin ID 44. */
334 #define QM_PIN_44_FN_GPIO_10 QM_PMUX_FN_0
335 #define QM_PIN_44_FN_SPI1_M_MOSI QM_PMUX_FN_1
336
337 /* Pin ID 45. */
338 #define QM_PIN_45_FN_GPIO_11 QM_PMUX_FN_0
339 #define QM_PIN_45_FN_SPI1_M_CS_B_0 QM_PMUX_FN_1
340
341 /* Pin ID 46. */
342 #define QM_PIN_46_FN_GPIO_12 QM_PMUX_FN_0
343 #define QM_PIN_46_FN_SPI1_M_CS_B_1 QM_PMUX_FN_1
344
345 /* Pin ID 47. */
346 #define QM_PIN_47_FN_GPIO_13 QM_PMUX_FN_0
347 #define QM_PIN_47_FN_SPI1_M_CS_B_2 QM_PMUX_FN_1
348
349 /* Pin ID 48. */
350 #define QM_PIN_48_FN_GPIO_14 QM_PMUX_FN_0
351 #define QM_PIN_48_FN_SPI1_M_CS_B_3 QM_PMUX_FN_1
352
353 /* Pin ID 49. */
354 #define QM_PIN_49_FN_GPIO_15 QM_PMUX_FN_0
355 #define QM_PIN_49_FN_I2S_RXD QM_PMUX_FN_1
356
357 /* Pin ID 50. */
358 #define QM_PIN_50_FN_GPIO_16 QM_PMUX_FN_0
359 #define QM_PIN_50_FN_I2S_RSCK QM_PMUX_FN_1
360
361 /* Pin ID 51. */
362 #define QM_PIN_51_FN_GPIO_17 QM_PMUX_FN_0
363 #define QM_PIN_51_FN_I2S_RWS QM_PMUX_FN_1
364
365 /* Pin ID 52. */
366 #define QM_PIN_52_FN_GPIO_18 QM_PMUX_FN_0
367 #define QM_PIN_52_FN_I2S_TSCK QM_PMUX_FN_1
368
369 /* Pin ID 53. */
370 #define QM_PIN_53_FN_GPIO_19 QM_PMUX_FN_0
371 #define QM_PIN_53_FN_I2S_TWS QM_PMUX_FN_1
372
373 /* Pin ID 54. */
374 #define QM_PIN_54_FN_GPIO_20 QM_PMUX_FN_0
375 #define QM_PIN_54_FN_I2S_TXD QM_PMUX_FN_1
376
377 /* Pin ID 55. */
378 #define QM_PIN_55_FN_GPIO_21 QM_PMUX_FN_0
379 #define QM_PIN_55_FN_SPI0_M_SCK QM_PMUX_FN_1
380
381 /* Pin ID 56. */
382 #define QM_PIN_56_FN_GPIO_22 QM_PMUX_FN_0
383 #define QM_PIN_56_FN_SPI0_M_MISO QM_PMUX_FN_1
384
385 /* Pin ID 57. */
386 #define QM_PIN_57_FN_GPIO_23 QM_PMUX_FN_0
387 #define QM_PIN_57_FN_SPI0_M_MOSI QM_PMUX_FN_1
388
389 /* Pin ID 58. */
390 #define QM_PIN_58_FN_GPIO_24 QM_PMUX_FN_0
391 #define QM_PIN_58_FN_SPI0_M_CS_B_0 QM_PMUX_FN_1
392
393 /* Pin ID 59. */
394 #define QM_PIN_59_FN_GPIO_25 QM_PMUX_FN_0
395 #define QM_PIN_59_FN_SPI0_M_CS_B_1 QM_PMUX_FN_1
396
397 /* Pin ID 60. */
398 #define QM_PIN_60_FN_GPIO_26 QM_PMUX_FN_0
399 #define QM_PIN_60_FN_SPI0_M_CS_B_2 QM_PMUX_FN_1
400
401 /* Pin ID 61. */
402 #define QM_PIN_61_FN_GPIO_27 QM_PMUX_FN_0
403 #define QM_PIN_61_FN_SPI0_M_CS_B_3 QM_PMUX_FN_1
404
405 /* Pin ID 62. */
406 #define QM_PIN_62_FN_GPIO_28 QM_PMUX_FN_0
407
408 /* Pin ID 63. */
409 #define QM_PIN_63_FN_GPIO_SS_10 QM_PMUX_FN_0
410 #define QM_PIN_63_FN_PWM_0 QM_PMUX_FN_1
411
412 /* Pin ID 64. */
413 #define QM_PIN_64_FN_GPIO_SS_11 QM_PMUX_FN_0
414 #define QM_PIN_64_FN_PWM_1 QM_PMUX_FN_1
415
416 /* Pin ID 65. */
417 #define QM_PIN_65_FN_GPIO_SS_12 QM_PMUX_FN_0
418 #define QM_PIN_65_FN_PWM_2 QM_PMUX_FN_1
419
420 /* Pin ID 66. */
421 #define QM_PIN_66_FN_GPIO_SS_13 QM_PMUX_FN_0
422 #define QM_PIN_66_FN_PWM_3 QM_PMUX_FN_1
423
424 /* Pin ID 67. */
425 #define QM_PIN_67_FN_GPIO_SS_14 QM_PMUX_FN_0
426 #define QM_PIN_67_FN_PLT_CLK_0 QM_PMUX_FN_1
427
428 /* Pin ID 68. */
429 #define QM_PIN_68_FN_GPIO_SS_15 QM_PMUX_FN_0
430 #define QM_PIN_68_FN_PLT_CLK_1 QM_PMUX_FN_1
431
432 /**
433 * @}
434 */
435
436 #endif /* __QM_PIN_FUNCTIONS_H__ */