Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_dma_context_t Struct Reference
SoC Registers (SE)

DMA context type. More...

`#include <qm_soc_regs.h>`

## Data Fields
uint32_t | misc_cfg_low
| DMA Configuration. More...
uint32_t | ctrl_low
| Channel Control Lower. More...
uint32_t | cfg_low
| Channel Configuration Lower. More...
uint32_t | cfg_high
| Channel Configuration Upper. More...
uint32_t | llp_low
| Channel Linked List Pointer. More...

## Detailed Description

DMA context type.

Applications should not modify the content. This structure is only intended to be used by the qm_dma_save_context and qm_dma_restore_context functions.

Definition at line 1911 of file qm_soc_regs.h.

## Field Documentation

uint32_t qm_dma_context_t::cfg_high

Channel Configuration Upper.

Definition at line 1915 of file qm_soc_regs.h.

Referenced by qm_dma_restore_context(), and qm_dma_save_context().

uint32_t qm_dma_context_t::cfg_low

Channel Configuration Lower.

Definition at line 1914 of file qm_soc_regs.h.

Referenced by qm_dma_restore_context(), and qm_dma_save_context().

uint32_t qm_dma_context_t::ctrl_low

Channel Control Lower.

Definition at line 1913 of file qm_soc_regs.h.

Referenced by qm_dma_restore_context(), and qm_dma_save_context().

uint32_t qm_dma_context_t::llp_low

Channel Linked List Pointer.

Definition at line 1916 of file qm_soc_regs.h.

Referenced by qm_dma_restore_context(), and qm_dma_save_context().

uint32_t qm_dma_context_t::misc_cfg_low

DMA Configuration.

Definition at line 1918 of file qm_soc_regs.h.

Referenced by qm_dma_restore_context(), and qm_dma_save_context().