Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

Enumerations
Mailbox Definitions

Mailbox definitions. More...

## Enumerations
enum | qm_mbox_ch_t { QM_MBOX_CH_0 = 0, QM_MBOX_CH_1, QM_MBOX_CH_2, QM_MBOX_CH_3, QM_MBOX_CH_4, QM_MBOX_CH_5, QM_MBOX_CH_6, QM_MBOX_CH_7 }
| Mailbox channel identifiers. More...
enum | qm_mbox_destination_t { , QM_MBOX_TO_LMT, QM_MBOX_TO_SS }
| Definition of the mailbox direction of operation The direction of communication for each channel is configurable by the user. More...

## Detailed Description

Mailbox definitions.

## Enumeration Type Documentation

enum qm_mbox_ch_t

Mailbox channel identifiers.

Enumerator
QM_MBOX_CH_0 | Channel 0.
QM_MBOX_CH_1 | Channel 1.
QM_MBOX_CH_2 | Channel 2.
QM_MBOX_CH_3 | Channel 3.
QM_MBOX_CH_4 | Channel 4.
QM_MBOX_CH_5 | Channel 5.
QM_MBOX_CH_6 | Channel 6.
QM_MBOX_CH_7 | Channel 7.

Definition at line 18 of file qm_mailbox_defs.h.

enum qm_mbox_destination_t

Definition of the mailbox direction of operation The direction of communication for each channel is configurable by the user.

The list below describes the possible communication directions for each channel.

Enumerator
QM_MBOX_TO_LMT | Lakemont core as destination.
QM_MBOX_TO_SS | Sensor Sub-System core as destination.

Definition at line 35 of file qm_mailbox_defs.h.