Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_ss_spi_context_t Struct Reference
SoC Registers (Sensor Subsystem)

Sensor Subsystem SPI context type. More...

`#include <qm_sensor_regs.h>`

## Data Fields
uint32_t | spi_ctrl
| Control Register. More...
uint32_t | spi_spien
| SPI Enable Register. More...
uint32_t | spi_timing
| Timing Register. More...

## Detailed Description

Sensor Subsystem SPI context type.

Applications should not modify the content. This structure is only intended to be used by the qm_ss_spi_save_context and qm_ss_spi_restore_context functions.

Definition at line 697 of file qm_sensor_regs.h.

## Field Documentation

uint32_t qm_ss_spi_context_t::spi_ctrl

Control Register.

Definition at line 698 of file qm_sensor_regs.h.

Referenced by qm_ss_spi_restore_context(), and qm_ss_spi_save_context().

uint32_t qm_ss_spi_context_t::spi_spien

SPI Enable Register.

Definition at line 699 of file qm_sensor_regs.h.

Referenced by qm_ss_spi_restore_context(), and qm_ss_spi_save_context().

uint32_t qm_ss_spi_context_t::spi_timing

Timing Register.

Definition at line 700 of file qm_sensor_regs.h.

Referenced by qm_ss_spi_restore_context(), and qm_ss_spi_save_context().