Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_mvic_reg_t Struct Reference
SoC Registers (D2000)

MVIC register map. More...

`#include <qm_soc_regs.h>`

## Data Fields
QM_RW mvic_reg_pad_t | tpr
| Task priority. More...
QM_RW mvic_reg_pad_t | ppr
| Processor priority. More...
QM_RW mvic_reg_pad_t | eoi
| End of interrupt. More...
QM_RW mvic_reg_pad_t | sivr
| Spurious vector. More...
QM_RW mvic_reg_pad_t | isr
| In-service. More...
QM_RW mvic_reg_pad_t | irr
| Interrupt request. More...
QM_RW mvic_reg_pad_t | lvttimer
| Timer vector. More...
QM_RW mvic_reg_pad_t | icr
| Timer initial count. More...
QM_RW mvic_reg_pad_t | ccr
| Timer current count. More...

## Detailed Description

MVIC register map.

Definition at line 1415 of file qm_soc_regs.h.

## Field Documentation

QM_RW mvic_reg_pad_t qm_mvic_reg_t::ccr

Timer current count.

Definition at line 1430 of file qm_soc_regs.h.

QM_RW mvic_reg_pad_t qm_mvic_reg_t::eoi

End of interrupt.

Definition at line 1419 of file qm_soc_regs.h.

QM_RW mvic_reg_pad_t qm_mvic_reg_t::icr

Timer initial count.

Definition at line 1429 of file qm_soc_regs.h.

QM_RW mvic_reg_pad_t qm_mvic_reg_t::irr

Interrupt request.

Definition at line 1425 of file qm_soc_regs.h.

QM_RW mvic_reg_pad_t qm_mvic_reg_t::isr

In-service.

Definition at line 1423 of file qm_soc_regs.h.

QM_RW mvic_reg_pad_t qm_mvic_reg_t::lvttimer

Timer vector.

Definition at line 1427 of file qm_soc_regs.h.

QM_RW mvic_reg_pad_t qm_mvic_reg_t::ppr

Processor priority.

Definition at line 1418 of file qm_soc_regs.h.

QM_RW mvic_reg_pad_t qm_mvic_reg_t::sivr

Spurious vector.

Definition at line 1421 of file qm_soc_regs.h.

QM_RW mvic_reg_pad_t qm_mvic_reg_t::tpr

Task priority.

Definition at line 1416 of file qm_soc_regs.h.