Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_pic_timer_context_t Struct Reference
SoC Registers (SE)

PIC TIMER context type. More...

`#include <qm_soc_regs.h>`

## Data Fields
uint32_t | timer_icr
| Initial Count Register. More...
uint32_t | timer_dcr
| Divide Configuration Register. More...
uint32_t | lvttimer
| Timer Entry in Local Vector Table. More...

## Detailed Description

PIC TIMER context type.

Applications should not modify the content. This structure is only intended to be used by the qm_pic_timer_save_context and qm_pic_timer_restore_context functions.

Definition at line 283 of file qm_soc_regs.h.

## Field Documentation

uint32_t qm_pic_timer_context_t::lvttimer

Timer Entry in Local Vector Table.

Definition at line 286 of file qm_soc_regs.h.

Referenced by qm_pic_timer_restore_context(), and qm_pic_timer_save_context().

uint32_t qm_pic_timer_context_t::timer_dcr

Divide Configuration Register.

Definition at line 285 of file qm_soc_regs.h.

Referenced by qm_pic_timer_restore_context(), and qm_pic_timer_save_context().

uint32_t qm_pic_timer_context_t::timer_icr

Initial Count Register.

Definition at line 284 of file qm_soc_regs.h.

Referenced by qm_pic_timer_restore_context(), and qm_pic_timer_save_context().