Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_pwm_channel_t Struct Reference
SoC Registers (D2000) | SoC Registers (SE)

PWM / Timer channel register map. More...

`#include <qm_soc_regs.h>`

## Data Fields
QM_RW uint32_t | loadcount
| Load Coun.t. More...
QM_RW uint32_t | currentvalue
| Current Value. More...
QM_RW uint32_t | controlreg
| Control. More...
QM_RW uint32_t | eoi
| End Of Interrupt. More...
QM_RW uint32_t | intstatus
| Interrupt Status. More...

## Detailed Description

PWM / Timer channel register map.

Definition at line 389 of file qm_soc_regs.h.

## Field Documentation

QM_RW uint32_t qm_pwm_channel_t::controlreg

Control.

Definition at line 392 of file qm_soc_regs.h.

Referenced by qm_pwm_restore_context(), qm_pwm_save_context(), qm_pwm_set_config(), qm_pwm_start(), and qm_pwm_stop().

QM_RW uint32_t qm_pwm_channel_t::currentvalue

Current Value.

Definition at line 391 of file qm_soc_regs.h.

QM_RW uint32_t qm_pwm_channel_t::eoi

End Of Interrupt.

Definition at line 393 of file qm_soc_regs.h.

Referenced by QM_ISR_DECLARE().

QM_RW uint32_t qm_pwm_channel_t::intstatus

Interrupt Status.

Definition at line 394 of file qm_soc_regs.h.

QM_RW uint32_t qm_pwm_channel_t::loadcount

Load Coun.t.

Load Count.

Definition at line 390 of file qm_soc_regs.h.

Referenced by qm_pwm_get(), qm_pwm_restore_context(), qm_pwm_save_context(), qm_pwm_set(), and qm_pwm_set_config().