Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

qm_pwm_context_t Struct Reference
SoC Registers (SE)

PWM context type. More...

`#include <qm_soc_regs.h>`

## Detailed Description

PWM context type.

Applications should not modify the content. This structure is only intended to be used by the qm_pwm_save_context and qm_pwm_restore_context functions.

Definition at line 702 of file qm_soc_regs.h.

## Field Documentation

uint32_t qm_pwm_context_t::controlreg

Control Register.

Definition at line 706 of file qm_soc_regs.h.

Referenced by qm_pwm_restore_context(), and qm_pwm_save_context().

uint32_t qm_pwm_context_t::loadcount

Load Count 1.

Definition at line 704 of file qm_soc_regs.h.

Referenced by qm_pwm_restore_context(), and qm_pwm_save_context().

uint32_t qm_pwm_context_t::loadcount2

Load Count 2.

Definition at line 705 of file qm_soc_regs.h.

Referenced by qm_pwm_restore_context(), and qm_pwm_save_context().