=============================================================================
 Intel(R) Server Board S2600KPR FRU Header Factory Mismatch Correction Readme
=============================================================================

INTEL Enterprise Platform & Services Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA

=============================================================================

DATE:     July 26, 2016

TO:       Intel(R) Server Board S2600KPR customers

SUBJECT:  FRU header factory mismatch correction package S2600KPR_FRUFIX_113

=============================================================================
                               LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products.
No license, express or implied, by estoppel or otherwise, to any intellectual
property rights is granted by this document. Except as provided in Intel's
Terms and Conditions of Sale for such products, Intel assumes no liability
whatsoever, and Intel disclaims any express or implied warranty, relating to
sale and/or use of Intel products including liability or warranties relating
to fitness for a particular purpose, merchantability, or infringement of any
patent, copyright or other intellectual property right. Intel Corporation may
have patents or pending patent applications, trademarks, copyrights, or other
intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not
provide any license, express or implied, by estoppel or otherwise, to any
such patents, trademarks, copyrights, or other intellectual property rights.
Intel products are not intended for use in medical, life saving, or life
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation.

*Other names and brands are the property of their respective owners.

Copyright (c) 2016 Intel Corporation.

=============================================================================
                      ABOUT THIS RELEASE PACKAGE
=============================================================================

SDR file version:                    1.13
Baseboard FRU file version:          1.00
Master configuration file version:   113
FRUSDR loader version:               13.1 Build 8

=============================================================================
        SYSTEM HARDWARE & SOFTWARE REQUIREMENTS/REVISIONS
=============================================================================

- S2600KPR baseboard PBA #H13888-361 only

- Haswell processor C1 stepping or higher

- BMC FW 01.37 or later

- BIOS R01.01.0014 or later

- Hot-swap backplane, and Baseboard FRU data must be available
  for chassis auto-detection to succeed

- Please, refer to TA #1111-01 for more information  

=============================================================================
                      IMPORTANT INSTALLATION NOTES
=============================================================================

NOTE: If you updated BIOS and did not clear CMOS RAM, you should do that before
      installing this package.
	  
NOTE: You need to have ME FW 3.05 or later installed for the SSB Temp sensor to work properly.

=============================================================================
                           INSTALLATION PROCEDURE - EFI SHELL
=============================================================================

Note: Ensure BMC FW release 01.37.9235 or later and BIOS D0064 or later are
      pre-installed before attempting this FRU/SDR update.

1. Copy the entire contents of the Package file to the HDD or USB flash drive

2. Execute the following script that's located inside the "EFI" subfolder:

     frufix.nsh

3. The package should do the fix automatically. On completion, the system
   should be able to perform FRU/SDR updates without a FRU header factory
   mismatch warning. The FRU header now matches new FRU/SDR releases.

=============================================================================
                           INSTALLATION PROCEDURE - Linux OS
=============================================================================

Note: Ensure BMC FW release 01.37.9235 or later and BIOS D0064 or later are
      pre-installed before attempting this FRU/SDR update.

1. Copy the entire contents of the Package file to the HDD or USB flash drive

2. Use the One-Boot Flash Update Utility(OFU) to perform the correction. The
   OFU tool can be found at http://downloadcenter.intel.com/

3. Execute the following command using the master.cfg file that's located 
   inside the "Linux" subfolder:

     flashupdt -u ./master.cfg

4. The package should do the fix automatically. On completion, the system
   should be able to perform FRU/SDR updates without a FRU header factory
   mismatch warning. The FRU header now matches new FRU/SDR releases.
   
=============================================================================
                           KNOWN ISSUES AND WORKAROUNDS
=============================================================================

In the event you receive the error "The FRU Headers for System FRU and file _
FRU are not matching" when running the fix (Either on EFI Shell or Linux),
it is due to two reasons:

	1. A different PBA than H13888-361 was used with the fix tool
	2. A second run of the fix has been made

=============================================================================
                           ISSUES FIXED
=============================================================================

S2600KPR baseboard PBA #H13888-361 FRU header factory mismatch corrected.


[END OF README]
