//****************************************************************************
//                            INTEL CONFIDENTIAL
//                     Copyright 2010 Intel Corporation
//                           All Rights Reserved.
//
// The source code contained or described herein and all documents related to
// the source code ("Material") are owned by Intel Corporation or its
// suppliers or licensors. Title to the Material remains with Intel
// Corporation or its suppliers and licensors. The Material contains trade
// secrets and proprietary and confidential information of Intel or its
// suppliers and licensors. The Material is protected by worldwide copyright
// and trade secret laws and treaty provisions. No part of the Material may be
// used, copied, reproduced, modified, published, uploaded, posted,
// transmitted, distributed, or disclosed in any way without Intel's prior
// express written permission.
//
// No license under any patent, copyright, trade secret or other intellectual
// property right is granted to or conferred upon you by disclosure or
// delivery of the Materials, either expressly, by implication, inducement,
// estoppel or otherwise. Any license under such intellectual property rights
// must be express and approved by Intel in writing.
//
//****************************************************************************
//
//  Date:  12/20/2010
//  Description:  Field Replaceable Unit (FRU) data file for the Intel
//  S2600JF baseboard.
//
//****************************************************************************


_LF_NAME       'JP_BMC.fru'          // Name for this load file
_LF_VERSION    '0.01'                // Version of this load file
_LF_FMT_VER    '1.50'                // Version of the load file format
_IPMI_VERSION  '1.00'                // IPMI format version

_FRU (
_FRU_TITLE     'Baseboard FRU'       // FRU Title
_START_ADDR    0000                  // Start Address
_DATA_LEN      0120                  // Data Length
_NVS_TYPE      'IMBDEVICE'           // Non-volatile Storage Type
_DEV_BUS       FF                    // Device Bus
_DEV_ADDRESS   20                    // Device Address

_SEE_COMMON
   01                                // Common Header Format Version
   01                                // Internal Use Area Starting Offset (in multiples of 8 bytes)
   02                                // Chassis Info Area Starting Offset (in multiples of 8 bytes)
   0C                                // Board Info Area Starting Offset (in multiples of 8 bytes)
   16                                // Product Info Area Starting Offset (in multiples of 8 bytes)
   00                                // MultiRecord Area Starting Offset (in multiples of 8 bytes)
   00                                // Pad
   DA                                // Common Header Checksum

_SEE_INTERNAL
   01                                // Internal Use Format Version
   00
   00
   00
   00
   00
   00
   01

_SEE_CHASSIS
   01                                // Chassis Info Area Format Version Bit Fields
   0A                                // Chassis Info Area Length (in multiples of 8 bytes)
   11                                // Chassis Type (Main Server Chassis)
   D2                                // Chassis Part Number
   '..................'
   D2                                // Chassis Serial Number
   '..................'
   DE                                // Custom Chassis Info type/length byte
   '..............................'  // Custom Chassis Info Field (For OEM use)
   C1                                // End of field marker

_SEE_BOARD
   01                                // Board Info Area Format Version Bit Fields
   0A                                // Board Info Area Length (in multiples of 8 bytes)
   00                                // Language Code
   000000                            // Mfg. Date/Time
   D1                                // Board Manufacturer
   'Intel Corporation'
   C7                                // Board Product Name. Currently unknown at the time of this FRU file creation.
   'S2600JF'
   CC                                // Board Serial Number
   '............'
   CA                                // Board Part Number (Contains the PBA#)
   '..........'
   CC                                // FRU File version ID string
   'FRU Ver 0.01'
   C1                                // End of field marker


_SEE_PRODUCT
   01                                // Product Info Area Format Version Bit Fields
   0D                                // Product Info Area Length (in multiples of 8 bytes)
   00                                // Language Code
   D1                                // Product Manufacturer Name
   'Intel Corporation'
   C7                                // Board Product Name. Currently unknown at the time of this FRU file creation
   'S2600JF'
   CA                                // Product Part Number (Contains the Top Assembly (TA)#)
   '..........'
   D4                                // Product Version (Available for OEM use)
   '....................'
   CC                                // Product Serial Number
   '............'
   D4                                // Asset Tag (Available for OEM use)
   '....................'
   C0                                // FRU File ID (Not used)
   C1                                // End of field marker
)
