(c) Copyright 1994-2017 Intel Corp. All rights reserved.

****************************************************
RunTest PCT process control utility       5.05.1.0001 01/24/17
****************************************************


		HELP For BYO Platform Confidence Tests
QUICK TEST option
   Quick test is designed to perform a quick test of the CPU module, Memory, 
   Cache and hard disk units. It is not a complete test of these units.

   The Quick Test package takes between 2 and 5 minutes, depending upon the 
   amount memory that is installed.

   The following is a list of the test modules that are run in Quick Test:

	Power On Self Test     CPU
	SMP Processor Test     Hard Disk 
	Cache Memory           Memory


COMPREHENSIVE TEST option
   The Comprehensive test is designed to perform a complete test the server 
   system.

   Run time for the Comprehensive Test package is between 15 and 20 minutes, 
   depending upon the amount memory that is installed.

   The following is a list of the test modules that are run in Comprehensive
   Test:

    Power On Self Test			CPU
    Math FPU				Cache Memory
    SMP Processor Test			Lindenhurst Chipset
    Memory				Memory Stress Testing
    Primary Interrupt Controller	Programmable Interrupt Controller
    Keyboard Self Test			Mouse Interface
    Real Time Clock			PCI Bus Controller
    PCIe Bus Controller			Intel Pro 1000 NIC Controller
    Super I/O Controller		ATI Video Adapter
    Direct Memory Access Controller	Mini Baseboard Management Controller
    IMM Card (if installed)             BMC (if IMM card installed)
    Comm Port 1 Controller		LSI SCSI Controller
    Parallel Port Controller		Hard Disk Controller and Drives    
    Floppy A Controller			IDE Controller
    MCH Chipset North Bridge            ICH Chipset South Bridge
    PXHD Chipset PCI Bridge             
                                             

COMPREHENSIVE TEST With Continuous Looping option
   The Comprehensive test with continuous looping performs the same test list 
   as the Comprehensive Test Package but runs continuously until stopped.

   To stop the tests press CRTL+BREAK. The test menu will display the pass 
   count.

   Run time for the Comprehensive Test with continuous looping is between 
   15 and 20 minutes per pass, depending upon the amount memory that is 
   installed.

DISPLAY HELP TEXT option

   Display this help text file.

EXIT option

   Exit to DOS.

   
   
To stop the tests at any time and return to 
Test Selection Menu press CTRL+BREAK.

