You are here: Defining Intel AMT Profiles > Defining Active Directory Integration > Defining Additional Object Attributes

# Defining Additional Object Attributes

The object created for the Intel AMT device is automatically assigned all the attributes and values necessary for AD integration. If necessary, you can also define additional attributes and values for the AD object.

Note:
You can only define attributes of the “String” type.

To define additional object attributes:

1. Click Advanced. This additional field is shown:

2. In the text field, define the list of attributes and values that you want to add to the object. Each line in the list must contain only one attribute, entered in the Lightweight Directory Interchange Format (LIDF) described in RFC 2849.

   For example:

   attributeName1: attributeValue1

   attributeName2: attributeValue2

3. When the list is complete, click Next to continue. If the list contains invalid entries, an error message will show the lines with the invalid syntax.

Note:
All the attributes in the list must exist in the AD schema, and the specified values must be valid The Distinguished Name attribute must NOT be defined in this list Invalid entries in this list will cause configuration to fail. The list is not validated against the AD schema. If the list includes attributes configured by Intel SCS, the value defined in the list will replace the value usually configured by Intel SCS.