You are here: Using the Configurator > Maintaining Configured Systems

# Maintaining Configured Systems

Command | MaintainAMT
Description | Runs specific maintenance tasks on Intel AMT, based on settings in the <filename> XML file.
Syntax | ACUConfig.exe [global options] MaintainAMT <filename> <task> [<task>...] [/DecryptionPassword <password>] [/AdminPassword <password>] [/NetworkSettingsFile <file>] {[/FileToRun <filename>] [/FileHash <SHA256 hash>] [/FileUser <username>] [/FilePassword <password>]}
Parameters
[global options] | See CLI Global Options
<filename> | The XML file containing the original configuration settings that were used to configure Intel AMT. Settings in the XML file not related to the specified maintenance tasks are ignored.
<task> | Define at least one of these maintenance tasks: SyncAMTTime – Synchronizes the clock of the Intel AMT device with the clock of the host. This task is performed automatically when any of the other tasks are performed. SyncNetworkSettings – Synchronizes network settings of the Intel AMT device as defined in the <NetworkSettings> tag of the <filename> XML file (see Defining IP and FQDN Settings) ReissueCertificates – Reissues the certificates stored in the Intel AMT device. If the device contains 802.1x certificates, the RenewADPassword task is automatically done as well. RenewADPassword – Changes the password of the Active Directory object representing the Intel AMT system. RenewAdminPassword – Changes the password of the default Digest admin user in the Intel AMT device according to the password setting defined in the profile. AutoMaintain – Automatically does only the maintenance tasks (listed here) that are necessary for this Intel AMT system. For more information, see: About Maintenance Tasks Manual/Automatic Maintenance using the CLI
/DecryptionPassword <password> | Mandatory if any of the files that the Configurator will use are encrypted (see File Encryption)
/AdminPassword <password> | The current password of the default Digest admin user defined in the Intel AMT device. This parameter is NOT necessary if any of these are true: The XML profile contains the Digest admin password The user account running the Configurator is a Kerberos account that is configured in the Intel AMT device with administrator permissions
/NetworkSettingsFile <file> | The path to a file that contains the network settings (FQDN and/or IP) to put in the Intel AMT device. Only use this parameter if you defined the source for at least one of these settings as a dedicated network settings file. For more information, see Defining IP and FQDN Settings.
/FileToRun /FileHash /FileUser /FilePassword | The Configurator can use these parameters to run a script after the command has completed successfully. For more information, see Scripts Run by the Configurator.