System Firmware Update Package(SFUP)README instructions 

Instructions

Intel highly recommends reading this document in its entirety before performing the system update. Verifying that your system meets the documented requirements will ensure a successful update and provide the most reliable system functionality after the update has completed.

Released - March 26, 2018

********************************************************************************
This update package includes the following production level system software updates:

System BIOS  - R01.03.0018
ME Firmware  - 03.01.03.030.0
BMC Firmware - 01.14.11110 
FRUSDR       - 1.30


--- Supported Products ---

Intel(R) Server Board S7200AP and S7200APR Product Families

Contact Intel for Production hardware support requirements

IMPORTANT NOTES: 
- Prior to installation, read the BIOS RELEASE NOTES.txt document and pay close attention to the IMPORTANT NOTES and KNOWN ISSUES for this specific release.

- This unified firmware package supports BOTH the S7200AP and S7200APR board and compute module products. All associated Intel® Xeon Phi™ x200(Formerly KNL) or X205 (Formerly KNM) CPUs are also supported. 

- All updates provided in this package are installed using the OS update method in conjunction with One Flash Update (OFU) tool.

- Do not modify any of the script files.  The scripts as written will provide the most reliable update experience. 

*****************************************************************
	               SYSTEM HARDWARE AND SOFTWARE REQUIREMENTS
*****************************************************************
S7200AP Product Family
- S7200AP baseboard PBA ending in -304 and higher.
- Production versions of Intel® Xeon Phi™ x200(Formerly KNL)up to 230W TDP.
- System BIOS- R01.02.0001 or greater 
- BMC Firmware - Version 01.00.10304 or greater

S7200APR Product Family
- S7200APR baseboard PBA ending in -250 and higher.
- Production versions of Intel® Xeon Phi™ x200(Formerly KNL)and Intel® Xeon Phi™ x205(Formerly KNM) Processors up to 320W TDP.
- System BIOS- R01.03.0001 or greater 
- BMC Firmware - Version 01.09.10985 or greater


- Front Panel, Hot-swap backplane, and Baseboard FRU data must be available for chassis auto-detection to succeed.
*****************************************************************
                           UPDATE PROCEDURE
*****************************************************************

- Follow the instructions in the "OFU Linux Quick Installation and Firmware Update Instructions" and/or in the "Intel_OFU_UserGuideV1.0"


***   Warning:  *** 
!! Do NOT interrupt or reboot or remove power from your system during the update process.
Doing so may render your system inoperable. !!

!! Do not attempt to down rev the system software once loaded on to the system.
Doing so may render your system inoperable. !!



