# Supported Intel® PRO/1000 Server Adapters for Intel® Itanium™-based Systems

This driver software is designed to operate with the following Intel PRO/1000 Server Adapters:

Product Name | Distinguishing Features | LEDs† | Board ID #†† | Controller
--- | --- | --- | --- | ---
PRO/1000 F Server Adapter | SC Fiber connector, Full Duplex | 4 | 738640-xxx A38888-xxx | 82543
PRO/1000 T Server Adapter | Copper RJ45 connector, supports 10/100/1000 | 3 | A19845-xxx A33948-xxx | 82543
PRO/1000 XT Server Adapter | Copper RJ45 connector, supports 10/100/1000 | 2 | A51580-xxx | 82544GC
PRO/1000 XF Server Adapter | SC Fiber connector, Full Duplex | 3 | A50484-xxx | 82544EI
PRO/1000 MT Server Adapter | Copper RJ45 connector, supports 10/100/1000 | 2 | A92165-xxx | 82545EM
PRO/1000 MT Dual Port Server Adapter | Two ports, copper RJ45 connectors, supports 10/100/1000 | 4 | A92111-xxx | 82545EB
PRO/1000 MT Quad Port Server Adapter | Four ports, copper RJ45 connectors, supports 10/100/1000 | 2/port | C32199-xxx | 82546EB
PRO/1000 MF Server Adapter | LC Fiber connector, 1000BASE-SX, Full Duplex | 2 | A91622-xxx | 82546EM
PRO/1000 MF Server (LX) Adapter | LC Fiber connector, 1000BASE-SX, Full Duplex | 2 | A91624-xxx | 82546EM
PRO/1000 MF Dual Port Server Adapter | Two ports, LC Fiber connectors, Full Duplex | 2 | A91620-xxx | 82546EB
PRO/1000 MB Dual Port Server Adapter | Two ports, SerDes Backplane network connectivity | 4 |  | 82546GB
PRO/1000 MB Server Connection | SerDes Backplane network connectivity |  |  | 82545GM
PRO/1000 MT Server Connection | Copper RJ45 connectors, 1000BASE-T |  |  | 82545GM
PRO/1000 MF Dual Port Network Connection | Two ports, LC Fiber connectors, Full Duplex |  |  | 82546EB
PRO/1000 MT Network Connection | Copper RJ45 connectors |  |  | 82545EM
PRO/1000 MB Dual Port Server Connection | Two ports, SerDes Backplane network connectivity |  |  | 82546GB
PRO/1000 MB Dual Port Network Connection | Two ports, SerDes Backplane network connectivity |  |  | 82546GB
PRO/1000 CT Network Connection | Copper RJ45 connectors, supports 10/100/1000, Communications Streaming Architecture, LOM |  |  | 82547GI

Intel(R) PRO/1000 MB Dual Port Server Connection | Two ports, SerDes Backplane network connectivity |  |  | 82546GB

†LED = The number of LEDs visible on the adapter. If a number is not indicated for the product, it is a LAN On Motherboard device (LOM). In other words, the device resides on the motherboard of the system. Since the vendor configures the LEDs, the number of LEDs visible varies from one vendor to another.

††Board ID # = A 6-digit code with a 3-digit extension; printed on barcode sticker on the front of the card.

For detailed information on these Intel adapters, see the Adapter & Driver ID Guide: http://support.intel.com/support/network

`Last modified on 9/10/03 3:23p Revision 11`