//****************************************************************************
//                          Intel Corporation
//                    Jones Farm, Hillsboro, Oregon
//                           (503) 696-8080
//
//                Intel Corporation Proprietary Information
//     Copyright (c) 2004 Intel Corporation, All Rights Reserved
//****************************************************************************
//
//  TITLE:  IMMABMC4.FRU                            DATE CREATED: 06/04/2004
//
//  DESCRIPTION:  Field Replaceable Unit (FRU) information file.  This FRU
//  file is for the Intel(R) Management Module - Advanced Edition FRU.
//
//****************************************************************************

_LF_NAME       'IMM Advanced Board FRU' 		// Name for this load file
_LF_VERSION    '0.04'                   		// Version of this load file
_LF_FMT_VER    '1.50'                   		// Version of the load file format
_IPMI_VERSION  '1.50'                   		// IPMI format version

_FRU (
_FRU_TITLE     'IMM Adv Board'					// FRU Title
_START_ADDR    0000                     		// Start Address
_DATA_LEN      00A8                     		// Data Length = 168 bytes
_NVS_TYPE      'IMBDEVICE'              		// Non-volatile Storage Type
_DEV_ID        01                       		// Device ID
_DEV_BUS       FF                       		// Device Bus
_DEV_ADDRESS   20                       		// Device Address

_SEE_COMMON
   01                                   		// Common Header Format Version
   01                                   		// Internal Use Area Starting Offset (in multiples of 8 bytes)
   00                                   		// Chassis Info Area Starting Offset (in multiples of 8 bytes)
   04                                   		// Board Info Area Starting Offset (in multiples of 8 bytes)
   11                                   		// Product Info Area Starting Offset (in multiples of 8 bytes)
   00                                   		// MultiRecord Area Starting Offset (in multiples of 8 bytes)
   00                                   		// Pad
   E9                                   		// Common Header Checksum

_SEE_INTERNAL
   01 00 00 00 00 00 00 00				// 24 byte internal use area
   00 00 00 00 00 00 00 00
   00 00 00 00 00 00 00 00				

_SEE_BOARD
   01                                   		// Board Info Area Format Version Bit Fields
   0D                                   		// Board Info Area Length = 104 bytes (13 blocks)
   00                                   		// Language Code
   00 00 00                             		// Mockup Mfg. Date/Time
   C5                                   		// Board Manufacturer type/length byte
   'Intel'                              		// Board Manufacturer name
   ED                                   		// Board Product Name type/length byte
   'Intel(R) Management Module - Advanced Edition'	// Board Product Name
   CC                                   		// Board Serial Number type/length byte
   '............'                       		// Mockup Board Serial Number
   CA                                   		// Board Part Number type/length byte
   '..........'                         		// Mockup Board Serial Number
   CC                                   		// FRU File ID
   'FRU Ver 0.04'								// FRU file version number
   C0                                   		// Board Custom Field 1
   C0                                   		// Board Custom Field 2
   C0                                   		// Board Custom Field 3
   C1                                   		// No more fields type/length byte

_SEE_PRODUCT
   01                                   		// Area Format Version Bit Fields
   04                                   		// Area Length = 32 bytes (4 blocks)
   00                                   		// Language Code
   C5                 					// Product Manufacturer Name
   'Intel'            					// 5 digit ascii Product Manufacturer name
   C0                                   		// Product Name type/length byte
   C0                                   		// Product part/model number type/length byte
   C0                                   		// Product Version type/length byte
   C0                                   		// Product Serial Number type/length byte
   C0                                   		// Asset Tag type/length byte
   C0                                   		// FRU file ID type/length byte
   C0                                   		// Custom Field
   C1                                   		// No more fields type/length byte
)
