//****************************************************************************
//                          Intel Corporation
//                    Jones Farm, Hillsboro, Oregon
//                           (503) 696-8080
//
//                Intel Corporation Proprietary Information
//     Copyright (c) 1999-2004 Intel Corporation, All Rights Reserved
//****************************************************************************
//
//  TITLE: SAFmBMC2.FRU                     DATE CREATED:  11/08/2004
//
//  DESCRIPTION:  miniBMC Field Replaceable Unit (FRU) information file.  This FRU 
//      file is for the SE7520AF20 product.  
//
//  PVCS INFORMATION:
//      $Workfile:   SAFmBMC2.FRU  $   
//      $Author:     $
//      $Revision:   $
//      $Date:       $
//      $Modtime:    $
//
//****************************************************************************
//
//******************************************************************************

//
// File Header Information
//

_LF_NAME       'SAF2 Baseboard' // The name for this load file
_LF_VERSION    '0.2'            // Version of this load file
_LF_FMT_VER    '1.50'       // Version of the load file format
_IPMI_VERSION  '1.50'       // IPMI format version

//
// FRU Area Header 
//

_FRU (                      // FRU data for the Baseboard 
_FRU_TITLE 'Basbrd Mgmt Ctlr'     // FRU title
_START_ADDR 0000                     // Start Address
_DATA_LEN 00F8                         // Data Length
_NVS_TYPE   'MBMC_FRU'        // Mini BMC FRU device
_MBMC_SIZE_ADRS 38            // Address of fru size configuration byte
_MBMC_SIZE_DATA FF            // data to program for FRU size
_DEV_BUS FE                           // SMBus
_DEV_ADDRESS 84                  // Device Address = mBMC


_SEE_COMMON
   01                 // Common Header Format Version
   01                 // Internal Use Area Starting Offset (in multiples of 8 bytes)
   02                 // Chassis Info Area Starting Offset (in multiples of 8 bytes)
   09                 // Board Info Area Starting Offset (in multiples of 8 bytes)
   13                 // Product Info Area Starting Offset (in multiples of 8 bytes)
   00                 // MultiRecord Area Starting Offset (in multiples of 8 bytes)
   00                 // Pad
   E0                 // Common Header Checksum

_SEE_INTERNAL
   01 00 21 00 00 00 00 00 // 00h - 07h

_SEE_CHASSIS
   01                 // Chassis Info Area Format Version Bit Fields
   07                 // Chassis Info Area Length (in multiples of 8 bytes)
   17                 // Chassis Type = rack
   C0                 // Chassis Part Number
   C0                 // Chassis Serial Number
   C0                 // Chassis Custom Field - SMaRT Tool chassis name
   C1                 // End of field marker

_SEE_BOARD
   01                 // Board Info Area Format Version Bit Fields
   0A                 // Board Info Area Length (in multiples of 8 bytes)
   00                 // Language Code
   00 00 00           // Mfg. Date/Time
   C5                 // Board Manufacturer
   'Intel'            // 5 digit ascii Board Manufacturer name
   CA                 // Board Product Name
   'SE7520AF20'        // Ascii Board Product name
   CC                 // Board Serial Number
   '............'     // Mock-up 12 digit ascii board serial number
   CA                 // Board Part Number
   '..........'       // Mock-up 10 digit ascii board part number
   CB                 // FRU File ID
   'FRU Ver 0.2'      // FRU file version string
   C0                 // Board Custom Field
   C1                 // End of field marker

_SEE_PRODUCT
   01                 // Product Info Area Format Version Bit Fields
   0C                 // Product Info Area Length (in multiples of 8 bytes)
   00                 // Language Code
   C5                 // Product Manufacturer Name
   'Intel'            // 5 digit ascii Product Manufacturer name
   C0                 // Product Name
   C0                 // Product Part/Model Number
   C0                 // Product Version
   C0                 // Product Serial Number
   C0                 // Asset Tag
   C0                 // FRU File ID
   C0                 // Product Custom Field
   C1                 // End of field marker

)

//** End of FRU for miniBMC ******************************************************
