Return to Zork CD-ROM version 1.2 READ.ME file

9/29/94

This file contains additional information which may not be in the
printed Return to Zork CD-ROM documentation.

To print this file on your printer, type:

    COPY READ.ME PRN

All company or product names are trademarks or registered trademarks
or service marks of their respective owners.

 
 1. ACTIVISION/INFOCOM PRODUCT DEMOS

    The Return to Zork CD-ROM includes a demo of one of our 
    products:  MechWarrior 2:  The Clans. 

    After you have installed Return to Zork CD-ROM, you will be able
    to start the demo from the Return to Zork CD-ROM game
    directory.

    To see the MechWarrior 2:  The Clans demo, type MECH2 at the
    prompt.  MechWarrior 2 will be available on both floppy disk and
    CD-ROM formats for the IBM in 1995.

    For additional information on this and other Activision
    titles, please contact your local retailer, or in the U.S. call
    1 (800) 477-3650.
 

 2. INSTALLING UNDER 386MAX

    If the 386MAX memory manager is active, the installer may run
    very slowly.  You might want to disable 386MAX before running
    INSTALL.


 3. RUNNING UNDER QEMM 7.0

    Do not use the "UMB" option in the "DOS=" line in CONFIG.SYS.

    Change "LOADHIGH" to "LOADHI" wherever it occurs in RTZ.BAT.

    Adding the "RH:N" option to the "QEMM386.SYS" line in CONFIG.SYS
    may prevent memory problems while playing the game.


 4. RUNNING UNDER DR DOS

    Change "LOADHIGH" to "HILOAD" wherever it occurs in RTZ.BAT.


 5. ADDITIONAL MADECD.EXE COMMAND-LINE SWITCHES

    -L  Move video buffers into XMS or EMS memory.  Using this is
        highly recommended, as it reduces the amount of conventional
        memory required by about 64K bytes.  Using this switch may
        result in slightly decreased performance.


 6. CD SPEED TEST

    For Return to Zork CD-ROM to operate properly, your CD-ROM drive
    must be able to maintain a minimum level of data throughput.  To
    verify CD-ROM drive performance, a utility called TESTCD has been
    provided.

    To invoke the utility, insert the Return to Zork CD-ROM disc and
    type:

        TESTCD x:

    where "x" is the letter of the CD-ROM drive.  TESTCD will
    determine the speed of the drive and report it to you.

    If the reported speed is below 150 kilobytes per second, the
    quality of the walk through movies in the game may be affected.
    In this case, you may prefer to disable these movies.  See your
    Return to Zork CD-ROM user's manual for instructions.

    If the reported speed is below 100 kilobytes per second, the
    quality of the character conversations in the game may be
    affected.


 7. OPENING MOVIE SOUNDTRACK SELECTION

    On certain systems, such as those with poor CD-ROM throughput,
    low processor speed, or slow VGA adapters, you may detect jumps
    in the soundtrack during the opening and final movies.

    To eliminate this problem, run the Return to Zork CD-ROM
    installer and answer "NO" to the question, "Do you want to play a
    digital soundtrack during the opening movie?"  This will cause a
    MIDI soundtrack to be played instead.

 
 8. ADLIB USERS

    Return to Zork CD-ROM requires a sound card that supports digital
    audio as well as music.  As the AdLib card only supports music,
    you will need to add a digital audio card or device to your
    computer system.  We offer the low-cost LifeSize Sound Enhancer, 
    which attaches to your printer port for digital audio.  Please
    contact the customer service number found in your manual for more
    information.

 
 9. ADLIB GOLD USERS

    You may experience clicking or popping sounds while playing
    Return to Zork CD-ROM with this audio card.  Return to Zork
    CD-ROM supports the DigPak sound system which is supported by
    AdLib products.  Please contact the manufacturer of your card to
    determine the availability of updated DigPak drivers.  When you
    receive a new DigPak driver, copy it into the DRIVERS
    subdirectory.


10. ADVANCED GRAVIS ULTRASOUND USERS
 
    Do not use the Sound Blaster emulation driver (SBOS).  The
    drivers supplied with Return to Zork CD-ROM will use your
    equipment directly.

    If you are experiencing divide errors, look for the file 
    VOICEOOH.PAT in the ULTRASND\MIDI subdirectory. If this file is 
    not available, please contact Gravis for a patch update.


11. DISK COMPRESSION UTILITIES

    You may experience difficulty installing or running Return to
    Zork CD-ROM if you use any disk compression utilities such as
    DoubleDisk, Stacker, DoubleSpace, etc.  If you experience such
    a problem, try deleting all the files in the new Return to Zork
    CD-ROM subdirectory (often called \RTZ-CD).  Then run a
    defragmentation program and try installing again.


12. CUSTOMER SERVICE INFORMATION.
    
    To purchase this and other Activision/Infocom titles, 
    please contact your local retailer, or in the U.S. call
    1 (800) 477-3650.
 
    If you have any comments, questions or suggestions about Return to 
    Zork or any other Activision product, you can contact us at 
    (310) 479-5644 between the hours of 9:00 a.m. and 5:00 p.m.
    Pacific Time, Monday through Friday, (except closed on holidays)
    or you can contact a customer service representative through the 
    following on-line services:

    Activision BBS: (310) 479-1335
      *   Available 24 hours a day
      *   Up to 14,400 Baud
      *   Settings: 8 Bits, No Parity, 1 Stop bit (8,N,1)

    CompuServe: 76004,2122 or [GO GAMEPUB] in the Game Publishers 
    Forum B

    Prodigy: ACTI10B

    GEnie: ACTIVISION

    America OnLine: MEDIAJAKE or use keyword "ACTIVISION" to locate the
    Activision Forum

    Internet: support@activision.com


13. LIST OF FILES

    Following is a description of all files distributed with or
    created by Return to Zork CD-ROM.  Some of the files may not
    appear in your copy of the game.

    If your disk is low on space, you might want to delete some of
    the files that are not required for game operation.  However, in
    many cases, the only way to restore a deleted file is to run
    INSTALL from the distribution media again.  Your saved games will
    not be lost.

    CDPLAY.EXE
        CD audio player.  Optional.

    DISK.ID
        Distribution disk identification file.  Not copied to the
        hard disk.

    GAME.001
    GAME.002
    GAME.003
    etc.
        Saved games.  GAME.001 contains saved game #1, GAME.002
        contains saved game #2, etc.

    INSTALL.DAT
        Installer instruction file.  Required when reconfiguring
        Return to Zork CD-ROM.

    INSTALL.EXE
        Installer program.  Required when reconfiguring Return to
        Zork CD-ROM.

    MADECD.EXE
        Program required to play Return to Zork CD-ROM.  Required.

    RTZ.BAT
        Batch file for starting up Return to Zork CD-ROM.  Recreated
        each time you run INSTALL.  Required.

    RTZ.CFG
        Configuration file.  Recreated each time you run INSTALL.
        Optional.

    RTZ.GRP
        Windows group file.  Initially required for launching Return
        to Zork CD-ROM from Windows.  If you move Return to Zork
        CD-ROM into a different program group, you can delete this
        file.

    RTZ.ICO
        Windows icon file.  Optional.

    RTZ.PIF
        Windows Program Information File.  Required when launching
        Return to Zork CD-ROM from Windows.

    RTZCD.DAT
        Data file for Return to Zork CD-ROM.  Required.

    RTZCD.PRJ
        Project file containing Return to Zork CD-ROM art, sounds,
        and music.  Optionally copied to the hard disk.

    RTZCD.RED
        Game distribution library.  Not copied to the hard disk.

    RTZCDDRV.RED
        Driver distribution library.  Not copied to the hard disk.

    SAMPLE.AD
    SAMPLE.OPL
        Files for several music drivers.  Required.

    TESTCD.EXE
        CD throughput test program.  Optional.

    The following files are installed into a subdirectory called
    DRIVERS.  Only those files that are needed to support your system
    hardware are required.

    ADLIB.ADV
        Music driver for the AdLib, Sound Blaster, Sound Blaster Pro,
        Sound Blaster 16, Pro AudioSpectrum, Logitech SoundMan, and
        compatible cards.

    ADLIBG.ADV
        Music driver for the AdLib Gold card.

    ADLIBG.COM
        Sound driver for the AdLib Gold card.

    GF166.COM
        Sound driver for the Advanced Gravis UltraSound card.

    GF1MIDI.ADV
        Music driver for the Advanced Gravis UltraSound card.

    LSIZE.COM
        Sound driver for the LifeSize Sound Enhancer digital audio
        device.

    MT32.INI
        Initialization file for the Advanced Gravis UltraSound card.

    MT32MPU.ADV
        Music driver for the Roland LAPC-I, MPU-401 MIDI, and MT-32
        synthesizers.

    PAS16.COM
        Sound driver for the Pro AudioSpectrum 16 card.

    PAUDIO.COM
        Sound driver for the Pro AudioSpectrum card.

    PCSPKR.ADV
        Music driver for the PC internal speaker.

    SB16.COM
        Sound driver for the Sound Blaster 16 card.

    SBCLONE.COM
        Sound driver for Sound Blaster-compatible cards.

    SBLASTER.COM
        Sound driver for the Sound Blaster card.

    SBPRO.COM
        Sound driver for the Sound Blaster Pro and Logitech SoundMan
        cards.

    SNDSYS.COM
        Sound driver for the Windows Sound System card.

    SOURCE.COM
        Sound driver for the Disney Sound Source.

    TANSLTL.COM
        Sound driver for the Tandy SL/TL & Sensation.

    ULTRAMID.EXE
        Driver for the Advanced Gravis UltraSound card.


--------------------- END OF FILE ---------------------
