
                  OS/2 PRINT SUBSYSTEM PRINTER DRIVER
                   FOR OS/2 WARP v2.11 AND ABOVE

                              IMPORTANT
                              ---------
    PLEASE READ THE FOLLOWING TERMS AND CONDITIONS. DOWNLOADING
    THE FIX THAT FOLLOWS, INDICATES YOUR ACCEPTANCE OF THE
    FOLLOWING TERMS AND CONDITIONS:

    - YOU MUST BE, AND YOU AGREE THAT YOU ARE, A PRIOR LICENSEE OF OS/2
      WARP VERSION 4.00
    - YOU MAY MAKE COPIES OF THE OS/2 WARP VERSION 4.00 SERVICE FIX EQUAL TO
      THE NUMBER OF LICENSED COPIES OF OS/2 WARP VERSION 4.00 YOU POSSESS
    - YOU MAY ONLY USE THIS SERVICE FIX FOR MAINTENANCE PURPOSES
    - ALL OTHER TERMS AND CONDITIONS OF YOUR OS/2 WARP VERSION 4.00 LICENSE
      AGREEMENT APPLY TO THIS SERVICE FIX; HOWEVER, THIS DOES NOT EXTEND ANY
      WARRANTY OUTLINED IN SUCH AGREEMENT.


PRINTER DRIVER LEVEL = 30.734
-----------------------------


FILES INCLUDED IN THIS FIXPAK ARE:
---------------------------------
README       - INSTALLATION INSTRUCTIONS (THIS FILE)
PSCRIPT.DRV  - PSCRIPT DRIVER
PSCRIPT.EA   - PSCRIPT DRIVER EAs.
PSCRIPT.SYM  - PSCRIPT DRIVER SYMBOL FILE (FOR DEBUGGING ONLY)
PSCRIPT.HLP  - PSCRIPT DRIVER HELP FILE
PSCRIPT.LST  - LIST OF ALL DEVICES SUPPORTED
LICENSE      - IBM LICENSE AGREEMENT
PRINTER1.PAK - PSCRIPT DRIVER DEVICE DATA


TO INSTALL THIS FIX PERFORM THE FOLLOWING STEPS:
-----------------------------------------------

 Use these printer drivers as you would your original printer driver

 - Open the printer object(s) and deselect all drivers you have
   acquired this fix for and select another driver file as default.
 - Close the printer object.
 - Reboot the system without letting any print jobs print.
 - Point to a printer object
 - Click Mouse Button 2
 - Select properties
 - Select the printer driver tab
 - Point to one of the printer driver objects
 - Click mouse button 2
 - Select the install printer driver
 - The "Install New Printer Driver" dialog will appear.
 - Select "Other OS/2 Printer Driver" and enter the drive and/or
   directory that you have put the driver files into for the install.
 - Press Refresh button to refresh the driver list that is installed on
   the diskette.
 - Select the driver to install and press Install button
 - Select OK to close the "Install New Printer Driver" dialog and
   select the correct driver for the print object
 - Close print object.
 ***
 - A Second Method of installing is to select the printer object in the source directory
 - Pick the printer object you want to install by dragging and droping onto the desktop.

You will now be ready to print using the driver.  If you need additional
help installing the printer driver, please refer to the on-line help
facility.


Note 1:
------
If you are in a network environment, we suggest that you match printer
driver levels between both the server and the requestors.

The Font manager in the network environment is fully functional only if
downloaded fonts are available for both server and client and are in the
same path.


PRINTER DEVICES ADDED SINCE Ver 30.730
--------------------------------------
Brother HL-1650/70N
HP Laserjet 4100
HP Laserjet 1200
HP Laserjet 2200
HP Laserjet 3200
Kyocera Mita FS-1000+
Minolta QMS Magicolor 2200